# Android Camera HAL3.2 Properties

## Table of Contents

# Properties

Property Name | Type | Description | Units | Range | HIDL HAL version | Tags
--- | --- | --- | --- | --- | --- | ---
colorCorrection
controls
Property Name | Type | Description | Units | Range | Initial HIDL HAL version | Tags
android.colorCorrection.mode | byte [public] [full] TRANSFORM_MATRIX (v3.2) Use the android.colorCorrection.transform matrix and android.colorCorrection.gains to do color conversion. All advanced white balance adjustments (not specified by our white balance pipeline) must be disabled. If AWB is enabled with `android.control.awbMode != OFF`, then TRANSFORM_MATRIX is ignored. The camera device will override this value to either FAST or HIGH_QUALITY. FAST (v3.2) Color correction processing must not slow down capture rate relative to sensor raw output. Advanced white balance adjustments above and beyond the specified white balance pipeline may be applied. If AWB is enabled with `android.control.awbMode != OFF`, then the camera device uses the last frame's AWB values (or defaults if AWB has never been run). HIGH_QUALITY (v3.2) Color correction processing operates at improved quality but the capture rate might be reduced (relative to sensor raw output rate) Advanced white balance adjustments above and beyond the specified white balance pipeline may be applied. If AWB is enabled with `android.control.awbMode != OFF`, then the camera device uses the last frame's AWB values (or defaults if AWB has never been run). | The mode control selects how the image data is converted from the sensor's native color into linear sRGB color. |  |  | 3.2 |
Details
When auto-white balance (AWB) is enabled with android.control.awbMode, this control is overridden by the AWB routine. When AWB is disabled, the application controls how the color mapping is performed. We define the expected processing pipeline below. For consistency across devices, this is always the case with TRANSFORM_MATRIX. When either FAST or HIGH_QUALITY is used, the camera device may do additional processing but android.colorCorrection.gains and android.colorCorrection.transform will still be provided by the camera device (in the results) and be roughly correct. Switching to TRANSFORM_MATRIX and using the data provided from FAST or HIGH_QUALITY will yield a picture with the same white point as what was produced by the camera device in the earlier frame. The expected processing pipeline is as follows: The white balance is encoded by two values, a 4-channel white-balance gain vector (applied in the Bayer domain), and a 3x3 color transform matrix (applied after demosaic). The 4-channel white-balance gains are defined as:
    android.colorCorrection.gains = [ R G_even G_odd B ]
where `G_even` is the gain for green pixels on even rows of the output, and `G_odd` is the gain for green pixels on the odd rows. These may be identical for a given camera device implementation; if the camera device does not support a separate gain for even/odd green channels, it will use the `G_even` value, and write `G_odd` equal to `G_even` in the output result metadata. The matrices for color transforms are defined as a 9-entry vector:
    android.colorCorrection.transform = [ I0 I1 I2 I3 I4 I5 I6 I7 I8 ]
which define a transform from input sensor colors, `P_in = [ r g b ]`, to output linear sRGB, `P_out = [ r' g' b' ]`, with colors as follows:
    r' = I0r + I1g + I2b
    g' = I3r + I4g + I5b
    b' = I6r + I7g + I8b
Both the input and output value ranges must match. Overflow/underflow values are clipped to fit within the range.
HAL Implementation Details
HAL must support both FAST and HIGH_QUALITY if color correction control is available on the camera device, but the underlying implementation can be the same for both modes. That is, if the highest quality implementation on the camera device does not slow down capture rate, then FAST and HIGH_QUALITY should generate the same output.
android.colorCorrection.transform | rational x 3 x 3 [public as colorSpaceTransform] [full] 3x3 rational matrix in row-major order | A color transform matrix to use to transform from sensor RGB color space to output linear sRGB color space. | Unitless scale factors |  | 3.2 |
Details
This matrix is either set by the camera device when the request android.colorCorrection.mode is not TRANSFORM_MATRIX, or directly by the application in the request when the android.colorCorrection.mode is TRANSFORM_MATRIX. In the latter case, the camera device may round the matrix to account for precision issues; the final rounded matrix should be reported back in this matrix result metadata. The transform should keep the magnitude of the output color values within `[0, 1.0]` (assuming input color values is within the normalized range `[0, 1.0]`), or clipping may occur. The valid range of each matrix element varies on different devices, but values within [-1.5, 3.0] are guaranteed not to be clipped.
android.colorCorrection.gains | float x 4 [public as rggbChannelVector] [full] A 1D array of floats for 4 color channel gains | Gains applying to Bayer raw color channels for white-balance. | Unitless gain factors |  | 3.2 |
Details
These per-channel gains are either set by the camera device when the request android.colorCorrection.mode is not TRANSFORM_MATRIX, or directly by the application in the request when the android.colorCorrection.mode is TRANSFORM_MATRIX. The gains in the result metadata are the gains actually applied by the camera device to the current frame. The valid range of gains varies on different devices, but gains between [1.0, 3.0] are guaranteed not to be clipped. Even if a given device allows gains below 1.0, this is usually not recommended because this can create color artifacts.
HAL Implementation Details
The 4-channel white-balance gains are defined in the order of `[R G_even G_odd B]`, where `G_even` is the gain for green pixels on even rows of the output, and `G_odd` is the gain for green pixels on the odd rows. If a HAL does not support a separate gain for even/odd green channels, it must use the `G_even` value, and write `G_odd` equal to `G_even` in the output result metadata.
android.colorCorrection.aberrationMode | byte [public] [legacy] OFF (v3.2) No aberration correction is applied. FAST (v3.2) Aberration correction will not slow down capture rate relative to sensor raw output. HIGH_QUALITY (v3.2) Aberration correction operates at improved quality but the capture rate might be reduced (relative to sensor raw output rate) | Mode of operation for the chromatic aberration correction algorithm. |  | android.colorCorrection.availableAberrationModes | 3.2 |
Details
Chromatic (color) aberration is caused by the fact that different wavelengths of light can not focus on the same point after exiting from the lens. This metadata defines the high level control of chromatic aberration correction algorithm, which aims to minimize the chromatic artifacts that may occur along the object boundaries in an image. FAST/HIGH_QUALITY both mean that camera device determined aberration correction will be applied. HIGH_QUALITY mode indicates that the camera device will use the highest-quality aberration correction algorithms, even if it slows down capture rate. FAST means the camera device will not slow down capture rate when applying aberration correction. LEGACY devices will always be in FAST mode.
dynamic
Property Name | Type | Description | Units | Range | Initial HIDL HAL version | Tags
android.colorCorrection.mode | byte [public] [full] TRANSFORM_MATRIX (v3.2) Use the android.colorCorrection.transform matrix and android.colorCorrection.gains to do color conversion. All advanced white balance adjustments (not specified by our white balance pipeline) must be disabled. If AWB is enabled with `android.control.awbMode != OFF`, then TRANSFORM_MATRIX is ignored. The camera device will override this value to either FAST or HIGH_QUALITY. FAST (v3.2) Color correction processing must not slow down capture rate relative to sensor raw output. Advanced white balance adjustments above and beyond the specified white balance pipeline may be applied. If AWB is enabled with `android.control.awbMode != OFF`, then the camera device uses the last frame's AWB values (or defaults if AWB has never been run). HIGH_QUALITY (v3.2) Color correction processing operates at improved quality but the capture rate might be reduced (relative to sensor raw output rate) Advanced white balance adjustments above and beyond the specified white balance pipeline may be applied. If AWB is enabled with `android.control.awbMode != OFF`, then the camera device uses the last frame's AWB values (or defaults if AWB has never been run). | The mode control selects how the image data is converted from the sensor's native color into linear sRGB color. |  |  | 3.2 |
Details
When auto-white balance (AWB) is enabled with android.control.awbMode, this control is overridden by the AWB routine. When AWB is disabled, the application controls how the color mapping is performed. We define the expected processing pipeline below. For consistency across devices, this is always the case with TRANSFORM_MATRIX. When either FAST or HIGH_QUALITY is used, the camera device may do additional processing but android.colorCorrection.gains and android.colorCorrection.transform will still be provided by the camera device (in the results) and be roughly correct. Switching to TRANSFORM_MATRIX and using the data provided from FAST or HIGH_QUALITY will yield a picture with the same white point as what was produced by the camera device in the earlier frame. The expected processing pipeline is as follows: The white balance is encoded by two values, a 4-channel white-balance gain vector (applied in the Bayer domain), and a 3x3 color transform matrix (applied after demosaic). The 4-channel white-balance gains are defined as:
    android.colorCorrection.gains = [ R G_even G_odd B ]
where `G_even` is the gain for green pixels on even rows of the output, and `G_odd` is the gain for green pixels on the odd rows. These may be identical for a given camera device implementation; if the camera device does not support a separate gain for even/odd green channels, it will use the `G_even` value, and write `G_odd` equal to `G_even` in the output result metadata. The matrices for color transforms are defined as a 9-entry vector:
    android.colorCorrection.transform = [ I0 I1 I2 I3 I4 I5 I6 I7 I8 ]
which define a transform from input sensor colors, `P_in = [ r g b ]`, to output linear sRGB, `P_out = [ r' g' b' ]`, with colors as follows:
    r' = I0r + I1g + I2b
    g' = I3r + I4g + I5b
    b' = I6r + I7g + I8b
Both the input and output value ranges must match. Overflow/underflow values are clipped to fit within the range.
HAL Implementation Details
HAL must support both FAST and HIGH_QUALITY if color correction control is available on the camera device, but the underlying implementation can be the same for both modes. That is, if the highest quality implementation on the camera device does not slow down capture rate, then FAST and HIGH_QUALITY should generate the same output.
android.colorCorrection.transform | rational x 3 x 3 [public as colorSpaceTransform] [full] 3x3 rational matrix in row-major order | A color transform matrix to use to transform from sensor RGB color space to output linear sRGB color space. | Unitless scale factors |  | 3.2 |
Details
This matrix is either set by the camera device when the request android.colorCorrection.mode is not TRANSFORM_MATRIX, or directly by the application in the request when the android.colorCorrection.mode is TRANSFORM_MATRIX. In the latter case, the camera device may round the matrix to account for precision issues; the final rounded matrix should be reported back in this matrix result metadata. The transform should keep the magnitude of the output color values within `[0, 1.0]` (assuming input color values is within the normalized range `[0, 1.0]`), or clipping may occur. The valid range of each matrix element varies on different devices, but values within [-1.5, 3.0] are guaranteed not to be clipped.
android.colorCorrection.gains | float x 4 [public as rggbChannelVector] [full] A 1D array of floats for 4 color channel gains | Gains applying to Bayer raw color channels for white-balance. | Unitless gain factors |  | 3.2 |
Details
These per-channel gains are either set by the camera device when the request android.colorCorrection.mode is not TRANSFORM_MATRIX, or directly by the application in the request when the android.colorCorrection.mode is TRANSFORM_MATRIX. The gains in the result metadata are the gains actually applied by the camera device to the current frame. The valid range of gains varies on different devices, but gains between [1.0, 3.0] are guaranteed not to be clipped. Even if a given device allows gains below 1.0, this is usually not recommended because this can create color artifacts.
HAL Implementation Details
The 4-channel white-balance gains are defined in the order of `[R G_even G_odd B]`, where `G_even` is the gain for green pixels on even rows of the output, and `G_odd` is the gain for green pixels on the odd rows. If a HAL does not support a separate gain for even/odd green channels, it must use the `G_even` value, and write `G_odd` equal to `G_even` in the output result metadata.
android.colorCorrection.aberrationMode | byte [public] [legacy] OFF (v3.2) No aberration correction is applied. FAST (v3.2) Aberration correction will not slow down capture rate relative to sensor raw output. HIGH_QUALITY (v3.2) Aberration correction operates at improved quality but the capture rate might be reduced (relative to sensor raw output rate) | Mode of operation for the chromatic aberration correction algorithm. |  | android.colorCorrection.availableAberrationModes | 3.2 |
Details
Chromatic (color) aberration is caused by the fact that different wavelengths of light can not focus on the same point after exiting from the lens. This metadata defines the high level control of chromatic aberration correction algorithm, which aims to minimize the chromatic artifacts that may occur along the object boundaries in an image. FAST/HIGH_QUALITY both mean that camera device determined aberration correction will be applied. HIGH_QUALITY mode indicates that the camera device will use the highest-quality aberration correction algorithms, even if it slows down capture rate. FAST means the camera device will not slow down capture rate when applying aberration correction. LEGACY devices will always be in FAST mode.
static
Property Name | Type | Description | Units | Range | Initial HIDL HAL version | Tags
android.colorCorrection.availableAberrationModes | byte x n [public as enumList] [legacy] list of enums | List of aberration correction modes for android.colorCorrection.aberrationMode that are supported by this camera device. |  | Any value listed in android.colorCorrection.aberrationMode | 3.2 | V1
Details
This key lists the valid modes for android.colorCorrection.aberrationMode. If no aberration correction modes are available for a device, this list will solely include OFF mode. All camera devices will support either OFF or FAST mode. Camera devices that support the MANUAL_POST_PROCESSING capability will always list OFF mode. This includes all FULL level devices. LEGACY devices will always only support FAST mode.
HAL Implementation Details
HAL must support both FAST and HIGH_QUALITY if chromatic aberration control is available on the camera device, but the underlying implementation can be the same for both modes. That is, if the highest quality implementation on the camera device does not slow down capture rate, then FAST and HIGH_QUALITY will generate the same output.
control
controls
Property Name | Type | Description | Units | Range | Initial HIDL HAL version | Tags
android.control.aeAntibandingMode | byte [public] [legacy] OFF (v3.2) The camera device will not adjust exposure duration to avoid banding problems. 50HZ (v3.2) The camera device will adjust exposure duration to avoid banding problems with 50Hz illumination sources. 60HZ (v3.2) The camera device will adjust exposure duration to avoid banding problems with 60Hz illumination sources. AUTO (v3.2) The camera device will automatically adapt its antibanding routine to the current illumination condition. This is the default mode if AUTO is available on given camera device. | The desired setting for the camera device's auto-exposure algorithm's antibanding compensation. |  | android.control.aeAvailableAntibandingModes | 3.2 | BC
Details
Some kinds of lighting fixtures, such as some fluorescent lights, flicker at the rate of the power supply frequency (60Hz or 50Hz, depending on country). While this is typically not noticeable to a person, it can be visible to a camera device. If a camera sets its exposure time to the wrong value, the flicker may become visible in the viewfinder as flicker or in a final captured image, as a set of variable-brightness bands across the image. Therefore, the auto-exposure routines of camera devices include antibanding routines that ensure that the chosen exposure value will not cause such banding. The choice of exposure time depends on the rate of flicker, which the camera device can detect automatically, or the expected rate can be selected by the application using this control. A given camera device may not support all of the possible options for the antibanding mode. The android.control.aeAvailableAntibandingModes key contains the available modes for a given camera device. AUTO mode is the default if it is available on given camera device. When AUTO mode is not available, the default will be either 50HZ or 60HZ, and both 50HZ and 60HZ will be available. If manual exposure control is enabled (by setting android.control.aeMode or android.control.mode to OFF), then this setting has no effect, and the application must ensure it selects exposure times that do not cause banding issues. The android.statistics.sceneFlicker key can assist the application in this.
HAL Implementation Details
For all capture request templates, this field must be set to AUTO if AUTO mode is available. If AUTO is not available, the default must be either 50HZ or 60HZ, and both 50HZ and 60HZ must be available. If manual exposure control is enabled (by setting android.control.aeMode or android.control.mode to OFF), then the exposure values provided by the application must not be adjusted for antibanding.
android.control.aeExposureCompensation | int32 [public] [legacy] | Adjustment to auto-exposure (AE) target image brightness. | Compensation steps | android.control.aeCompensationRange | 3.2 | BC
Details
The adjustment is measured as a count of steps, with the step size defined by android.control.aeCompensationStep and the allowed range by android.control.aeCompensationRange. For example, if the exposure value (EV) step is 0.333, '6' will mean an exposure compensation of +2 EV; -3 will mean an exposure compensation of -1 EV. One EV represents a doubling of image brightness. Note that this control will only be effective if android.control.aeMode `!=` OFF. This control will take effect even when android.control.aeLock `== true`. In the event of exposure compensation value being changed, camera device may take several frames to reach the newly requested exposure target. During that time, android.control.aeState field will be in the SEARCHING state. Once the new exposure target is reached, android.control.aeState will change from SEARCHING to either CONVERGED, LOCKED (if AE lock is enabled), or FLASH_REQUIRED (if the scene is too dark for still capture).
android.control.aeLock | byte [public as boolean] [legacy] OFF (v3.2) Auto-exposure lock is disabled; the AE algorithm is free to update its parameters. ON (v3.2) Auto-exposure lock is enabled; the AE algorithm must not update the exposure and sensitivity parameters while the lock is active. android.control.aeExposureCompensation setting changes will still take effect while auto-exposure is locked. Some rare LEGACY devices may not support this, in which case the value will always be overridden to OFF. | Whether auto-exposure (AE) is currently locked to its latest calculated values. |  |  | 3.2 | BC
Details
When set to `true` (ON), the AE algorithm is locked to its latest parameters, and will not change exposure settings until the lock is set to `false` (OFF). Note that even when AE is locked, the flash may be fired if the android.control.aeMode is ON_AUTO_FLASH / ON_ALWAYS_FLASH / ON_AUTO_FLASH_REDEYE. When android.control.aeExposureCompensation is changed, even if the AE lock is ON, the camera device will still adjust its exposure value. If AE precapture is triggered (see android.control.aePrecaptureTrigger) when AE is already locked, the camera device will not change the exposure time (android.sensor.exposureTime) and sensitivity (android.sensor.sensitivity) parameters. The flash may be fired if the android.control.aeMode is ON_AUTO_FLASH/ON_AUTO_FLASH_REDEYE and the scene is too dark. If the android.control.aeMode is ON_ALWAYS_FLASH, the scene may become overexposed. Similarly, AE precapture trigger CANCEL has no effect when AE is already locked. When an AE precapture sequence is triggered, AE unlock will not be able to unlock the AE if AE is locked by the camera device internally during precapture metering sequence In other words, submitting requests with AE unlock has no effect for an ongoing precapture metering sequence. Otherwise, the precapture metering sequence will never succeed in a sequence of preview requests where AE lock is always set to `false`. Since the camera device has a pipeline of in-flight requests, the settings that get locked do not necessarily correspond to the settings that were present in the latest capture result received from the camera device, since additional captures and AE updates may have occurred even before the result was sent out. If an application is switching between automatic and manual control and wishes to eliminate any flicker during the switch, the following procedure is recommended: Starting in auto-AE mode: Lock AE Wait for the first result to be output that has the AE locked Copy exposure settings from that result into a request, set the request to manual AE Submit the capture request, proceed to run manual AE as desired. See android.control.aeState for AE lock related state transition details.
android.control.aeMode | byte [public] [legacy] OFF (v3.2) The camera device's autoexposure routine is disabled. The application-selected android.sensor.exposureTime, android.sensor.sensitivity and android.sensor.frameDuration are used by the camera device, along with android.flash.* fields, if there's a flash unit for this camera device. Note that auto-white balance (AWB) and auto-focus (AF) behavior is device dependent when AE is in OFF mode. To have consistent behavior across different devices, it is recommended to either set AWB and AF to OFF mode or lock AWB and AF before setting AE to OFF. See android.control.awbMode, android.control.afMode, android.control.awbLock, and android.control.afTrigger for more details. LEGACY devices do not support the OFF mode and will override attempts to use this value to ON. ON (v3.2) The camera device's autoexposure routine is active, with no flash control. The application's values for android.sensor.exposureTime, android.sensor.sensitivity, and android.sensor.frameDuration are ignored. The application has control over the various android.flash.* fields. ON_AUTO_FLASH (v3.2) Like ON, except that the camera device also controls the camera's flash unit, firing it in low-light conditions. The flash may be fired during a precapture sequence (triggered by android.control.aePrecaptureTrigger) and may be fired for captures for which the android.control.captureIntent field is set to STILL_CAPTURE ON_ALWAYS_FLASH (v3.2) Like ON, except that the camera device also controls the camera's flash unit, always firing it for still captures. The flash may be fired during a precapture sequence (triggered by android.control.aePrecaptureTrigger) and will always be fired for captures for which the android.control.captureIntent field is set to STILL_CAPTURE ON_AUTO_FLASH_REDEYE (v3.2) Like ON_AUTO_FLASH, but with automatic red eye reduction. If deemed necessary by the camera device, a red eye reduction flash will fire during the precapture sequence. ON_EXTERNAL_FLASH (v3.3) An external flash has been turned on. It informs the camera device that an external flash has been turned on, and that metering (and continuous focus if active) should be quickly recaculated to account for the external flash. Otherwise, this mode acts like ON. When the external flash is turned off, AE mode should be changed to one of the other available AE modes. If the camera device supports AE external flash mode, android.control.aeState must be FLASH_REQUIRED after the camera device finishes AE scan and it's too dark without flash. | The desired mode for the camera device's auto-exposure routine. |  | android.control.aeAvailableModes | 3.2 | BC
Details
This control is only effective if android.control.mode is AUTO. When set to any of the ON modes, the camera device's auto-exposure routine is enabled, overriding the application's selected exposure time, sensor sensitivity, and frame duration (android.sensor.exposureTime, android.sensor.sensitivity, and android.sensor.frameDuration). If one of the FLASH modes is selected, the camera device's flash unit controls are also overridden. The FLASH modes are only available if the camera device has a flash unit (android.flash.info.available is `true`). If flash TORCH mode is desired, this field must be set to ON or OFF, and android.flash.mode set to TORCH. When set to any of the ON modes, the values chosen by the camera device auto-exposure routine for the overridden fields for a given capture will be available in its CaptureResult.
android.control.aeRegions | int32 x 5 x area_count [public as meteringRectangle] | List of metering areas to use for auto-exposure adjustment. | Pixel coordinates within android.sensor.info.activeArraySize or android.sensor.info.preCorrectionActiveArraySize depending on distortion correction capability and mode | Coordinates must be between `[(0,0), (width, height))` of android.sensor.info.activeArraySize or android.sensor.info.preCorrectionActiveArraySize depending on distortion correction capability and mode | 3.2 | BC
Details
Not available if android.control.maxRegionsAe is 0. Otherwise will always be present. The maximum number of regions supported by the device is determined by the value of android.control.maxRegionsAe. For devices not supporting android.distortionCorrection.mode control, the coordinate system always follows that of android.sensor.info.activeArraySize, with (0,0) being the top-left pixel in the active pixel array, and (android.sensor.info.activeArraySize.width - 1, android.sensor.info.activeArraySize.height - 1) being the bottom-right pixel in the active pixel array. For devices supporting android.distortionCorrection.mode control, the coordinate system depends on the mode being set. When the distortion correction mode is OFF, the coordinate system follows android.sensor.info.preCorrectionActiveArraySize, with `(0, 0)` being the top-left pixel of the pre-correction active array, and (android.sensor.info.preCorrectionActiveArraySize.width - 1, android.sensor.info.preCorrectionActiveArraySize.height - 1) being the bottom-right pixel in the pre-correction active pixel array. When the distortion correction mode is not OFF, the coordinate system follows android.sensor.info.activeArraySize, with `(0, 0)` being the top-left pixel of the active array, and (android.sensor.info.activeArraySize.width - 1, android.sensor.info.activeArraySize.height - 1) being the bottom-right pixel in the active pixel array. The weight must be within `[0, 1000]`, and represents a weight for every pixel in the area. This means that a large metering area with the same weight as a smaller area will have more effect in the metering result. Metering areas can partially overlap and the camera device will add the weights in the overlap region. The weights are relative to weights of other exposure metering regions, so if only one region is used, all non-zero weights will have the same effect. A region with 0 weight is ignored. If all regions have 0 weight, then no specific metering area needs to be used by the camera device. If the metering region is outside the used android.scaler.cropRegion returned in capture result metadata, the camera device will ignore the sections outside the crop region and output only the intersection rectangle as the metering region in the result metadata. If the region is entirely outside the crop region, it will be ignored and not reported in the result metadata. Starting from API level 30, the coordinate system of activeArraySize or preCorrectionActiveArraySize is used to represent post-zoomRatio field of view, not pre-zoom field of view. This means that the same aeRegions values at different android.control.zoomRatio represent different parts of the scene. The aeRegions coordinates are relative to the activeArray/preCorrectionActiveArray representing the zoomed field of view. If android.control.zoomRatio is set to 1.0 (default), the same aeRegions at different android.scaler.cropRegion still represent the same parts of the scene as they do before. See android.control.zoomRatio for details. Whether to use activeArraySize or preCorrectionActiveArraySize still depends on distortion correction mode.
HAL Implementation Details
The HAL level representation of MeteringRectangle[] is a int[5 * area_count]. Every five elements represent a metering region of (xmin, ymin, xmax, ymax, weight). The rectangle is defined to be inclusive on xmin and ymin, but exclusive on xmax and ymax. HAL must always report metering regions in the coordinate system of pre-correction active array.
android.control.aeTargetFpsRange | int32 x 2 [public as rangeInt] [legacy] | Range over which the auto-exposure routine can adjust the capture frame rate to maintain good exposure. | Frames per second (FPS) | Any of the entries in android.control.aeAvailableTargetFpsRanges | 3.2 | BC
Details
Only constrains auto-exposure (AE) algorithm, not manual control of android.sensor.exposureTime and android.sensor.frameDuration.
android.control.aePrecaptureTrigger | byte [public] [limited] IDLE (v3.2) The trigger is idle. START (v3.2) The precapture metering sequence will be started by the camera device. The exact effect of the precapture trigger depends on the current AE mode and state. CANCEL (v3.2) The camera device will cancel any currently active or completed precapture metering sequence, the auto-exposure routine will return to its initial state. | Whether the camera device will trigger a precapture metering sequence when it processes this request. |  |  | 3.2 | BC
Details
This entry is normally set to IDLE, or is not included at all in the request settings. When included and set to START, the camera device will trigger the auto-exposure (AE) precapture metering sequence. When set to CANCEL, the camera device will cancel any active precapture metering trigger, and return to its initial AE state. If a precapture metering sequence is already completed, and the camera device has implicitly locked the AE for subsequent still capture, the CANCEL trigger will unlock the AE and return to its initial AE state. The precapture sequence should be triggered before starting a high-quality still capture for final metering decisions to be made, and for firing pre-capture flash pulses to estimate scene brightness and required final capture flash power, when the flash is enabled. Normally, this entry should be set to START for only a single request, and the application should wait until the sequence completes before starting a new one. When a precapture metering sequence is finished, the camera device may lock the auto-exposure routine internally to be able to accurately expose the subsequent still capture image (`android.control.captureIntent == STILL_CAPTURE`). For this case, the AE may not resume normal scan if no subsequent still capture is submitted. To ensure that the AE routine restarts normal scan, the application should submit a request with `android.control.aeLock == true`, followed by a request with `android.control.aeLock == false`, if the application decides not to submit a still capture request after the precapture sequence completes. Alternatively, for API level 23 or newer devices, the CANCEL can be used to unlock the camera device internally locked AE if the application doesn't submit a still capture request after the AE precapture trigger. Note that, the CANCEL was added in API level 23, and must not be used in devices that have earlier API levels. The exact effect of auto-exposure (AE) precapture trigger depends on the current AE mode and state; see android.control.aeState for AE precapture state transition details. On LEGACY-level devices, the precapture trigger is not supported; capturing a high-resolution JPEG image will automatically trigger a precapture sequence before the high-resolution capture, including potentially firing a pre-capture flash. Using the precapture trigger and the auto-focus trigger android.control.afTrigger simultaneously is allowed. However, since these triggers often require cooperation between the auto-focus and auto-exposure routines (for example, the may need to be enabled for a focus sweep), the camera device may delay acting on a later trigger until the previous trigger has been fully handled. This may lead to longer intervals between the trigger and changes to android.control.aeState indicating the start of the precapture sequence, for example. If both the precapture and the auto-focus trigger are activated on the same request, then the camera device will complete them in the optimal order for that device.
HAL Implementation Details
The HAL must support triggering the AE precapture trigger while an AF trigger is active (and vice versa), or at the same time as the AF trigger. It is acceptable for the HAL to treat these as two consecutive triggers, for example handling the AF trigger and then the AE trigger. Or the HAL may choose to optimize the case with both triggers fired at once, to minimize the latency for converging both focus and exposure/flash usage.
android.control.afMode | byte [public] [legacy] OFF (v3.2) The auto-focus routine does not control the lens; android.lens.focusDistance is controlled by the application. AUTO (v3.2) Basic automatic focus mode. In this mode, the lens does not move unless the autofocus trigger action is called. When that trigger is activated, AF will transition to ACTIVE_SCAN, then to the outcome of the scan (FOCUSED or NOT_FOCUSED). Always supported if lens is not fixed focus. Use android.lens.info.minimumFocusDistance to determine if lens is fixed-focus. Triggering AF_CANCEL resets the lens position to default, and sets the AF state to INACTIVE. MACRO (v3.2) Close-up focusing mode. In this mode, the lens does not move unless the autofocus trigger action is called. When that trigger is activated, AF will transition to ACTIVE_SCAN, then to the outcome of the scan (FOCUSED or NOT_FOCUSED). This mode is optimized for focusing on objects very close to the camera. When that trigger is activated, AF will transition to ACTIVE_SCAN, then to the outcome of the scan (FOCUSED or NOT_FOCUSED). Triggering cancel AF resets the lens position to default, and sets the AF state to INACTIVE. CONTINUOUS_VIDEO (v3.2) In this mode, the AF algorithm modifies the lens position continually to attempt to provide a constantly-in-focus image stream. The focusing behavior should be suitable for good quality video recording; typically this means slower focus movement and no overshoots. When the AF trigger is not involved, the AF algorithm should start in INACTIVE state, and then transition into PASSIVE_SCAN and PASSIVE_FOCUSED states as appropriate. When the AF trigger is activated, the algorithm should immediately transition into AF_FOCUSED or AF_NOT_FOCUSED as appropriate, and lock the lens position until a cancel AF trigger is received. Once cancel is received, the algorithm should transition back to INACTIVE and resume passive scan. Note that this behavior is not identical to CONTINUOUS_PICTURE, since an ongoing PASSIVE_SCAN must immediately be canceled. CONTINUOUS_PICTURE (v3.2) In this mode, the AF algorithm modifies the lens position continually to attempt to provide a constantly-in-focus image stream. The focusing behavior should be suitable for still image capture; typically this means focusing as fast as possible. When the AF trigger is not involved, the AF algorithm should start in INACTIVE state, and then transition into PASSIVE_SCAN and PASSIVE_FOCUSED states as appropriate as it attempts to maintain focus. When the AF trigger is activated, the algorithm should finish its PASSIVE_SCAN if active, and then transition into AF_FOCUSED or AF_NOT_FOCUSED as appropriate, and lock the lens position until a cancel AF trigger is received. When the AF cancel trigger is activated, the algorithm should transition back to INACTIVE and then act as if it has just been started. EDOF (v3.2) Extended depth of field (digital focus) mode. The camera device will produce images with an extended depth of field automatically; no special focusing operations need to be done before taking a picture. AF triggers are ignored, and the AF state will always be INACTIVE. | Whether auto-focus (AF) is currently enabled, and what mode it is set to. |  | android.control.afAvailableModes | 3.2 | BC
Details
Only effective if android.control.mode = AUTO and the lens is not fixed focus (i.e. `android.lens.info.minimumFocusDistance > 0`). Also note that when android.control.aeMode is OFF, the behavior of AF is device dependent. It is recommended to lock AF by using android.control.afTrigger before setting android.control.aeMode to OFF, or set AF mode to OFF when AE is OFF. If the lens is controlled by the camera device auto-focus algorithm, the camera device will report the current AF status in android.control.afState in result metadata.
HAL Implementation Details
When afMode is AUTO or MACRO, the lens must not move until an AF trigger is sent in a request (android.control.afTrigger `==` START). After an AF trigger, the afState will end up with either FOCUSED_LOCKED or NOT_FOCUSED_LOCKED state (see android.control.afState for detailed state transitions), which indicates that the lens is locked and will not move. If camera movement (e.g. tilting camera) causes the lens to move after the lens is locked, the HAL must compensate this movement appropriately such that the same focal plane remains in focus. When afMode is one of the continuous auto focus modes, the HAL is free to start a AF scan whenever it's not locked. When the lens is locked after an AF trigger (see android.control.afState for detailed state transitions), the HAL should maintain the same lock behavior as above. When afMode is OFF, the application controls focus manually. The accuracy of the focus distance control depends on the android.lens.info.focusDistanceCalibration. However, the lens must not move regardless of the camera movement for any focus distance manual control. To put this in concrete terms, if the camera has lens elements which may move based on camera orientation or motion (e.g. due to gravity), then the HAL must drive the lens to remain in a fixed position invariant to the camera's orientation or motion, for example, by using accelerometer measurements in the lens control logic. This is a typical issue that will arise on camera modules with open-loop VCMs.
android.control.afRegions | int32 x 5 x area_count [public as meteringRectangle] | List of metering areas to use for auto-focus. | Pixel coordinates within android.sensor.info.activeArraySize or android.sensor.info.preCorrectionActiveArraySize depending on distortion correction capability and mode | Coordinates must be between `[(0,0), (width, height))` of android.sensor.info.activeArraySize or android.sensor.info.preCorrectionActiveArraySize depending on distortion correction capability and mode | 3.2 | BC
Details
Not available if android.control.maxRegionsAf is 0. Otherwise will always be present. The maximum number of focus areas supported by the device is determined by the value of android.control.maxRegionsAf. For devices not supporting android.distortionCorrection.mode control, the coordinate system always follows that of android.sensor.info.activeArraySize, with (0,0) being the top-left pixel in the active pixel array, and (android.sensor.info.activeArraySize.width - 1, android.sensor.info.activeArraySize.height - 1) being the bottom-right pixel in the active pixel array. For devices supporting android.distortionCorrection.mode control, the coordinate system depends on the mode being set. When the distortion correction mode is OFF, the coordinate system follows android.sensor.info.preCorrectionActiveArraySize, with `(0, 0)` being the top-left pixel of the pre-correction active array, and (android.sensor.info.preCorrectionActiveArraySize.width - 1, android.sensor.info.preCorrectionActiveArraySize.height - 1) being the bottom-right pixel in the pre-correction active pixel array. When the distortion correction mode is not OFF, the coordinate system follows android.sensor.info.activeArraySize, with `(0, 0)` being the top-left pixel of the active array, and (android.sensor.info.activeArraySize.width - 1, android.sensor.info.activeArraySize.height - 1) being the bottom-right pixel in the active pixel array. The weight must be within `[0, 1000]`, and represents a weight for every pixel in the area. This means that a large metering area with the same weight as a smaller area will have more effect in the metering result. Metering areas can partially overlap and the camera device will add the weights in the overlap region. The weights are relative to weights of other metering regions, so if only one region is used, all non-zero weights will have the same effect. A region with 0 weight is ignored. If all regions have 0 weight, then no specific metering area needs to be used by the camera device. The capture result will either be a zero weight region as well, or the region selected by the camera device as the focus area of interest. If the metering region is outside the used android.scaler.cropRegion returned in capture result metadata, the camera device will ignore the sections outside the crop region and output only the intersection rectangle as the metering region in the result metadata. If the region is entirely outside the crop region, it will be ignored and not reported in the result metadata. Starting from API level 30, the coordinate system of activeArraySize or preCorrectionActiveArraySize is used to represent post-zoomRatio field of view, not pre-zoom field of view. This means that the same afRegions values at different android.control.zoomRatio represent different parts of the scene. The afRegions coordinates are relative to the activeArray/preCorrectionActiveArray representing the zoomed field of view. If android.control.zoomRatio is set to 1.0 (default), the same afRegions at different android.scaler.cropRegion still represent the same parts of the scene as they do before. See android.control.zoomRatio for details. Whether to use activeArraySize or preCorrectionActiveArraySize still depends on distortion correction mode.
HAL Implementation Details
The HAL level representation of MeteringRectangle[] is a int[5 * area_count]. Every five elements represent a metering region of (xmin, ymin, xmax, ymax, weight). The rectangle is defined to be inclusive on xmin and ymin, but exclusive on xmax and ymax. HAL must always report metering regions in the coordinate system of pre-correction active array.
android.control.afTrigger | byte [public] [legacy] IDLE (v3.2) The trigger is idle. START (v3.2) Autofocus will trigger now. CANCEL (v3.2) Autofocus will return to its initial state, and cancel any currently active trigger. | Whether the camera device will trigger autofocus for this request. |  |  | 3.2 | BC
Details
This entry is normally set to IDLE, or is not included at all in the request settings. When included and set to START, the camera device will trigger the autofocus algorithm. If autofocus is disabled, this trigger has no effect. When set to CANCEL, the camera device will cancel any active trigger, and return to its initial AF state. Generally, applications should set this entry to START or CANCEL for only a single capture, and then return it to IDLE (or not set at all). Specifying START for multiple captures in a row means restarting the AF operation over and over again. See android.control.afState for what the trigger means for each AF mode. Using the autofocus trigger and the precapture trigger android.control.aePrecaptureTrigger simultaneously is allowed. However, since these triggers often require cooperation between the auto-focus and auto-exposure routines (for example, the may need to be enabled for a focus sweep), the camera device may delay acting on a later trigger until the previous trigger has been fully handled. This may lead to longer intervals between the trigger and changes to android.control.afState, for example.
HAL Implementation Details
The HAL must support triggering the AF trigger while an AE precapture trigger is active (and vice versa), or at the same time as the AE trigger. It is acceptable for the HAL to treat these as two consecutive triggers, for example handling the AF trigger and then the AE trigger. Or the HAL may choose to optimize the case with both triggers fired at once, to minimize the latency for converging both focus and exposure/flash usage.
android.control.awbLock | byte [public as boolean] [legacy] OFF (v3.2) Auto-white balance lock is disabled; the AWB algorithm is free to update its parameters if in AUTO mode. ON (v3.2) Auto-white balance lock is enabled; the AWB algorithm will not update its parameters while the lock is active. | Whether auto-white balance (AWB) is currently locked to its latest calculated values. |  |  | 3.2 | BC
Details
When set to `true` (ON), the AWB algorithm is locked to its latest parameters, and will not change color balance settings until the lock is set to `false` (OFF). Since the camera device has a pipeline of in-flight requests, the settings that get locked do not necessarily correspond to the settings that were present in the latest capture result received from the camera device, since additional captures and AWB updates may have occurred even before the result was sent out. If an application is switching between automatic and manual control and wishes to eliminate any flicker during the switch, the following procedure is recommended: Starting in auto-AWB mode: Lock AWB Wait for the first result to be output that has the AWB locked Copy AWB settings from that result into a request, set the request to manual AWB Submit the capture request, proceed to run manual AWB as desired. Note that AWB lock is only meaningful when android.control.awbMode is in the AUTO mode; in other modes, AWB is already fixed to a specific setting. Some LEGACY devices may not support ON; the value is then overridden to OFF.
android.control.awbMode | byte [public] [legacy] OFF (v3.2) The camera device's auto-white balance routine is disabled. The application-selected color transform matrix (android.colorCorrection.transform) and gains (android.colorCorrection.gains) are used by the camera device for manual white balance control. AUTO (v3.2) The camera device's auto-white balance routine is active. The application's values for android.colorCorrection.transform and android.colorCorrection.gains are ignored. For devices that support the MANUAL_POST_PROCESSING capability, the values used by the camera device for the transform and gains will be available in the capture result for this request. INCANDESCENT (v3.2) The camera device's auto-white balance routine is disabled; the camera device uses incandescent light as the assumed scene illumination for white balance. While the exact white balance transforms are up to the camera device, they will approximately match the CIE standard illuminant A. The application's values for android.colorCorrection.transform and android.colorCorrection.gains are ignored. For devices that support the MANUAL_POST_PROCESSING capability, the values used by the camera device for the transform and gains will be available in the capture result for this request. FLUORESCENT (v3.2) The camera device's auto-white balance routine is disabled; the camera device uses fluorescent light as the assumed scene illumination for white balance. While the exact white balance transforms are up to the camera device, they will approximately match the CIE standard illuminant F2. The application's values for android.colorCorrection.transform and android.colorCorrection.gains are ignored. For devices that support the MANUAL_POST_PROCESSING capability, the values used by the camera device for the transform and gains will be available in the capture result for this request. WARM_FLUORESCENT (v3.2) The camera device's auto-white balance routine is disabled; the camera device uses warm fluorescent light as the assumed scene illumination for white balance. While the exact white balance transforms are up to the camera device, they will approximately match the CIE standard illuminant F4. The application's values for android.colorCorrection.transform and android.colorCorrection.gains are ignored. For devices that support the MANUAL_POST_PROCESSING capability, the values used by the camera device for the transform and gains will be available in the capture result for this request. DAYLIGHT (v3.2) The camera device's auto-white balance routine is disabled; the camera device uses daylight light as the assumed scene illumination for white balance. While the exact white balance transforms are up to the camera device, they will approximately match the CIE standard illuminant D65. The application's values for android.colorCorrection.transform and android.colorCorrection.gains are ignored. For devices that support the MANUAL_POST_PROCESSING capability, the values used by the camera device for the transform and gains will be available in the capture result for this request. CLOUDY_DAYLIGHT (v3.2) The camera device's auto-white balance routine is disabled; the camera device uses cloudy daylight light as the assumed scene illumination for white balance. The application's values for android.colorCorrection.transform and android.colorCorrection.gains are ignored. For devices that support the MANUAL_POST_PROCESSING capability, the values used by the camera device for the transform and gains will be available in the capture result for this request. TWILIGHT (v3.2) The camera device's auto-white balance routine is disabled; the camera device uses twilight light as the assumed scene illumination for white balance. The application's values for android.colorCorrection.transform and android.colorCorrection.gains are ignored. For devices that support the MANUAL_POST_PROCESSING capability, the values used by the camera device for the transform and gains will be available in the capture result for this request. SHADE (v3.2) The camera device's auto-white balance routine is disabled; the camera device uses shade light as the assumed scene illumination for white balance. The application's values for android.colorCorrection.transform and android.colorCorrection.gains are ignored. For devices that support the MANUAL_POST_PROCESSING capability, the values used by the camera device for the transform and gains will be available in the capture result for this request. | Whether auto-white balance (AWB) is currently setting the color transform fields, and what its illumination target is. |  | android.control.awbAvailableModes | 3.2 | BC
Details
This control is only effective if android.control.mode is AUTO. When set to the ON mode, the camera device's auto-white balance routine is enabled, overriding the application's selected android.colorCorrection.transform, android.colorCorrection.gains and android.colorCorrection.mode. Note that when android.control.aeMode is OFF, the behavior of AWB is device dependent. It is recommened to also set AWB mode to OFF or lock AWB by using android.control.awbLock before setting AE mode to OFF. When set to the OFF mode, the camera device's auto-white balance routine is disabled. The application manually controls the white balance by android.colorCorrection.transform, android.colorCorrection.gains and android.colorCorrection.mode. When set to any other modes, the camera device's auto-white balance routine is disabled. The camera device uses each particular illumination target for white balance adjustment. The application's values for android.colorCorrection.transform, android.colorCorrection.gains and android.colorCorrection.mode are ignored.
android.control.awbRegions | int32 x 5 x area_count [public as meteringRectangle] | List of metering areas to use for auto-white-balance illuminant estimation. | Pixel coordinates within android.sensor.info.activeArraySize or android.sensor.info.preCorrectionActiveArraySize depending on distortion correction capability and mode | Coordinates must be between `[(0,0), (width, height))` of android.sensor.info.activeArraySize or android.sensor.info.preCorrectionActiveArraySize depending on distortion correction capability and mode | 3.2 | BC
Details
Not available if android.control.maxRegionsAwb is 0. Otherwise will always be present. The maximum number of regions supported by the device is determined by the value of android.control.maxRegionsAwb. For devices not supporting android.distortionCorrection.mode control, the coordinate system always follows that of android.sensor.info.activeArraySize, with (0,0) being the top-left pixel in the active pixel array, and (android.sensor.info.activeArraySize.width - 1, android.sensor.info.activeArraySize.height - 1) being the bottom-right pixel in the active pixel array. For devices supporting android.distortionCorrection.mode control, the coordinate system depends on the mode being set. When the distortion correction mode is OFF, the coordinate system follows android.sensor.info.preCorrectionActiveArraySize, with `(0, 0)` being the top-left pixel of the pre-correction active array, and (android.sensor.info.preCorrectionActiveArraySize.width - 1, android.sensor.info.preCorrectionActiveArraySize.height - 1) being the bottom-right pixel in the pre-correction active pixel array. When the distortion correction mode is not OFF, the coordinate system follows android.sensor.info.activeArraySize, with `(0, 0)` being the top-left pixel of the active array, and (android.sensor.info.activeArraySize.width - 1, android.sensor.info.activeArraySize.height - 1) being the bottom-right pixel in the active pixel array. The weight must range from 0 to 1000, and represents a weight for every pixel in the area. This means that a large metering area with the same weight as a smaller area will have more effect in the metering result. Metering areas can partially overlap and the camera device will add the weights in the overlap region. The weights are relative to weights of other white balance metering regions, so if only one region is used, all non-zero weights will have the same effect. A region with 0 weight is ignored. If all regions have 0 weight, then no specific metering area needs to be used by the camera device. If the metering region is outside the used android.scaler.cropRegion returned in capture result metadata, the camera device will ignore the sections outside the crop region and output only the intersection rectangle as the metering region in the result metadata. If the region is entirely outside the crop region, it will be ignored and not reported in the result metadata. Starting from API level 30, the coordinate system of activeArraySize or preCorrectionActiveArraySize is used to represent post-zoomRatio field of view, not pre-zoom field of view. This means that the same awbRegions values at different android.control.zoomRatio represent different parts of the scene. The awbRegions coordinates are relative to the activeArray/preCorrectionActiveArray representing the zoomed field of view. If android.control.zoomRatio is set to 1.0 (default), the same awbRegions at different android.scaler.cropRegion still represent the same parts of the scene as they do before. See android.control.zoomRatio for details. Whether to use activeArraySize or preCorrectionActiveArraySize still depends on distortion correction mode.
HAL Implementation Details
The HAL level representation of MeteringRectangle[] is a int[5 * area_count]. Every five elements represent a metering region of (xmin, ymin, xmax, ymax, weight). The rectangle is defined to be inclusive on xmin and ymin, but exclusive on xmax and ymax. HAL must always report metering regions in the coordinate system of pre-correction active array.
android.control.captureIntent | byte [public] [legacy] CUSTOM (v3.2) The goal of this request doesn't fall into the other categories. The camera device will default to preview-like behavior. PREVIEW (v3.2) This request is for a preview-like use case. The precapture trigger may be used to start off a metering w/flash sequence. STILL_CAPTURE (v3.2) This request is for a still capture-type use case. If the flash unit is under automatic control, it may fire as needed. VIDEO_RECORD (v3.2) This request is for a video recording use case. VIDEO_SNAPSHOT (v3.2) This request is for a video snapshot (still image while recording video) use case. The camera device should take the highest-quality image possible (given the other settings) without disrupting the frame rate of video recording. ZERO_SHUTTER_LAG (v3.2) This request is for a ZSL usecase; the application will stream full-resolution images and reprocess one or several later for a final capture. MANUAL (v3.2) This request is for manual capture use case where the applications want to directly control the capture parameters. For example, the application may wish to manually control android.sensor.exposureTime, android.sensor.sensitivity, etc. MOTION_TRACKING (v3.3) This request is for a motion tracking use case, where the application will use camera and inertial sensor data to locate and track objects in the world. The camera device auto-exposure routine will limit the exposure time of the camera to no more than 20 milliseconds, to minimize motion blur. | Information to the camera device 3A (auto-exposure, auto-focus, auto-white balance) routines about the purpose of this capture, to help the camera device to decide optimal 3A strategy. |  |  | 3.2 | BC
Details
This control (except for MANUAL) is only effective if `android.control.mode != OFF` and any 3A routine is active. All intents are supported by all devices, except that: * ZERO_SHUTTER_LAG will be supported if android.request.availableCapabilities contains PRIVATE_REPROCESSING or YUV_REPROCESSING. * MANUAL will be supported if android.request.availableCapabilities contains MANUAL_SENSOR. * MOTION_TRACKING will be supported if android.request.availableCapabilities contains MOTION_TRACKING.
android.control.effectMode | byte [public] [legacy] OFF (v3.2) No color effect will be applied. MONO (v3.2) [optional] A "monocolor" effect where the image is mapped into a single color. This will typically be grayscale. NEGATIVE (v3.2) [optional] A "photo-negative" effect where the image's colors are inverted. SOLARIZE (v3.2) [optional] A "solarisation" effect (Sabattier effect) where the image is wholly or partially reversed in tone. SEPIA (v3.2) [optional] A "sepia" effect where the image is mapped into warm gray, red, and brown tones. POSTERIZE (v3.2) [optional] A "posterization" effect where the image uses discrete regions of tone rather than a continuous gradient of tones. WHITEBOARD (v3.2) [optional] A "whiteboard" effect where the image is typically displayed as regions of white, with black or grey details. BLACKBOARD (v3.2) [optional] A "blackboard" effect where the image is typically displayed as regions of black, with white or grey details. AQUA (v3.2) [optional] An "aqua" effect where a blue hue is added to the image. | A special color effect to apply. |  | android.control.availableEffects | 3.2 | BC
Details
When this mode is set, a color effect will be applied to images produced by the camera device. The interpretation and implementation of these color effects is left to the implementor of the camera device, and should not be depended on to be consistent (or present) across all devices.
android.control.mode | byte [public] [legacy] OFF (v3.2) Full application control of pipeline. All control by the device's metering and focusing (3A) routines is disabled, and no other settings in android.control.* have any effect, except that android.control.captureIntent may be used by the camera device to select post-processing values for processing blocks that do not allow for manual control, or are not exposed by the camera API. However, the camera device's 3A routines may continue to collect statistics and update their internal state so that when control is switched to AUTO mode, good control values can be immediately applied. AUTO (v3.2) Use settings for each individual 3A routine. Manual control of capture parameters is disabled. All controls in android.control.* besides sceneMode take effect. USE_SCENE_MODE (v3.2) [optional] Use a specific scene mode. Enabling this disables control.aeMode, control.awbMode and control.afMode controls; the camera device will ignore those settings while USE_SCENE_MODE is active (except for FACE_PRIORITY scene mode). Other control entries are still active. This setting can only be used if scene mode is supported (i.e. android.control.availableSceneModes contain some modes other than DISABLED). For extended scene modes such as BOKEH, please use USE_EXTENDED_SCENE_MODE instead. OFF_KEEP_STATE (v3.2) [optional] Same as OFF mode, except that this capture will not be used by camera device background auto-exposure, auto-white balance and auto-focus algorithms (3A) to update their statistics. Specifically, the 3A routines are locked to the last values set from a request with AUTO, OFF, or USE_SCENE_MODE, and any statistics or state updates collected from manual captures with OFF_KEEP_STATE will be discarded by the camera device. USE_EXTENDED_SCENE_MODE (v3.5) [optional] Use a specific extended scene mode. When extended scene mode is on, the camera device may override certain control parameters, such as targetFpsRange, AE, AWB, and AF modes, to achieve best power and quality tradeoffs. Only the mandatory stream combinations of LIMITED hardware level are guaranteed. This setting can only be used if extended scene mode is supported (i.e. android.control.availableExtendedSceneModes contains some modes other than DISABLED). | Overall mode of 3A (auto-exposure, auto-white-balance, auto-focus) control routines. |  | android.control.availableModes | 3.2 | BC
Details
This is a top-level 3A control switch. When set to OFF, all 3A control by the camera device is disabled. The application must set the fields for capture parameters itself. When set to AUTO, the individual algorithm controls in android.control.* are in effect, such as android.control.afMode. When set to USE_SCENE_MODE or USE_EXTENDED_SCENE_MODE, the individual controls in android.control.* are mostly disabled, and the camera device implements one of the scene mode or extended scene mode settings (such as ACTION, SUNSET, PARTY, or BOKEH) as it wishes. The camera device scene mode 3A settings are provided by capture results. When set to OFF_KEEP_STATE, it is similar to OFF mode, the only difference is that this frame will not be used by camera device background 3A statistics update, as if this frame is never captured. This mode can be used in the scenario where the application doesn't want a 3A manual control capture to affect the subsequent auto 3A capture results.
android.control.sceneMode | byte [public] [legacy] DISABLED (v3.2) 0 Indicates that no scene modes are set for a given capture request. FACE_PRIORITY (v3.2) If face detection support exists, use face detection data for auto-focus, auto-white balance, and auto-exposure routines. If face detection statistics are disabled (i.e. android.statistics.faceDetectMode is set to OFF), this should still operate correctly (but will not return face detection statistics to the framework). Unlike the other scene modes, android.control.aeMode, android.control.awbMode, and android.control.afMode remain active when FACE_PRIORITY is set. ACTION (v3.2) [optional] Optimized for photos of quickly moving objects. Similar to SPORTS. PORTRAIT (v3.2) [optional] Optimized for still photos of people. LANDSCAPE (v3.2) [optional] Optimized for photos of distant macroscopic objects. NIGHT (v3.2) [optional] Optimized for low-light settings. NIGHT_PORTRAIT (v3.2) [optional] Optimized for still photos of people in low-light settings. THEATRE (v3.2) [optional] Optimized for dim, indoor settings where flash must remain off. BEACH (v3.2) [optional] Optimized for bright, outdoor beach settings. SNOW (v3.2) [optional] Optimized for bright, outdoor settings containing snow. SUNSET (v3.2) [optional] Optimized for scenes of the setting sun. STEADYPHOTO (v3.2) [optional] Optimized to avoid blurry photos due to small amounts of device motion (for example: due to hand shake). FIREWORKS (v3.2) [optional] Optimized for nighttime photos of fireworks. SPORTS (v3.2) [optional] Optimized for photos of quickly moving people. Similar to ACTION. PARTY (v3.2) [optional] Optimized for dim, indoor settings with multiple moving people. CANDLELIGHT (v3.2) [optional] Optimized for dim settings where the main light source is a candle. BARCODE (v3.2) [optional] Optimized for accurately capturing a photo of barcode for use by camera applications that wish to read the barcode value. HIGH_SPEED_VIDEO (v3.2) [deprecated] [optional] This is deprecated, please use CameraDevice#createConstrainedHighSpeedCaptureSession and CameraConstrainedHighSpeedCaptureSession#createHighSpeedRequestList for high speed video recording. Optimized for high speed video recording (frame rate >=60fps) use case. The supported high speed video sizes and fps ranges are specified in android.control.availableHighSpeedVideoConfigurations. To get desired output frame rates, the application is only allowed to select video size and fps range combinations listed in this static metadata. The fps range can be control via android.control.aeTargetFpsRange. In this mode, the camera device will override aeMode, awbMode, and afMode to ON, ON, and CONTINUOUS_VIDEO, respectively. All post-processing block mode controls will be overridden to be FAST. Therefore, no manual control of capture and post-processing parameters is possible. All other controls operate the same as when android.control.mode == AUTO. This means that all other android.control.* fields continue to work, such as android.control.aeTargetFpsRange android.control.aeExposureCompensation android.control.aeLock android.control.awbLock android.control.effectMode android.control.aeRegions android.control.afRegions android.control.awbRegions android.control.afTrigger android.control.aePrecaptureTrigger android.control.zoomRatio Outside of android.control.*, the following controls will work: android.flash.mode (automatic flash for still capture will not work since aeMode is ON) android.lens.opticalStabilizationMode (if it is supported) android.scaler.cropRegion android.statistics.faceDetectMode For high speed recording use case, the actual maximum supported frame rate may be lower than what camera can output, depending on the destination Surfaces for the image data. For example, if the destination surface is from video encoder, the application need check if the video encoder is capable of supporting the high frame rate for a given video size, or it will end up with lower recording frame rate. If the destination surface is from preview window, the preview frame rate will be bounded by the screen refresh rate. The camera device will only support up to 2 output high speed streams (processed non-stalling format defined in android.request.maxNumOutputStreams) in this mode. This control will be effective only if all of below conditions are true: The application created no more than maxNumHighSpeedStreams processed non-stalling format output streams, where maxNumHighSpeedStreams is calculated as min(2, android.request.maxNumOutputStreams[Processed (but not-stalling)]). The stream sizes are selected from the sizes reported by android.control.availableHighSpeedVideoConfigurations. No processed non-stalling or raw streams are configured. When above conditions are NOT satistied, the controls of this mode and android.control.aeTargetFpsRange will be ignored by the camera device, the camera device will fall back to android.control.mode `==` AUTO, and the returned capture result metadata will give the fps range choosen by the camera device. Switching into or out of this mode may trigger some camera ISP/sensor reconfigurations, which may introduce extra latency. It is recommended that the application avoids unnecessary scene mode switch as much as possible. HDR (v3.2) [optional] Turn on a device-specific high dynamic range (HDR) mode. In this scene mode, the camera device captures images that keep a larger range of scene illumination levels visible in the final image. For example, when taking a picture of a object in front of a bright window, both the object and the scene through the window may be visible when using HDR mode, while in normal AUTO mode, one or the other may be poorly exposed. As a tradeoff, HDR mode generally takes much longer to capture a single image, has no user control, and may have other artifacts depending on the HDR method used. Therefore, HDR captures operate at a much slower rate than regular captures. In this mode, on LIMITED or FULL devices, when a request is made with a android.control.captureIntent of STILL_CAPTURE, the camera device will capture an image using a high dynamic range capture technique. On LEGACY devices, captures that target a JPEG-format output will be captured with HDR, and the capture intent is not relevant. The HDR capture may involve the device capturing a burst of images internally and combining them into one, or it may involve the device using specialized high dynamic range capture hardware. In all cases, a single image is produced in response to a capture request submitted while in HDR mode. Since substantial post-processing is generally needed to produce an HDR image, only YUV, PRIVATE, and JPEG outputs are supported for LIMITED/FULL device HDR captures, and only JPEG outputs are supported for LEGACY HDR captures. Using a RAW output for HDR capture is not supported. Some devices may also support always-on HDR, which applies HDR processing at full frame rate. For these devices, intents other than STILL_CAPTURE will also produce an HDR output with no frame rate impact compared to normal operation, though the quality may be lower than for STILL_CAPTURE intents. If SCENE_MODE_HDR is used with unsupported output types or capture intents, the images captured will be as if the SCENE_MODE was not enabled at all. FACE_PRIORITY_LOW_LIGHT (v3.2) [optional] [hidden] Same as FACE_PRIORITY scene mode, except that the camera device will choose higher sensitivity values (android.sensor.sensitivity) under low light conditions. The camera device may be tuned to expose the images in a reduced sensitivity range to produce the best quality images. For example, if the android.sensor.info.sensitivityRange gives range of [100, 1600], the camera device auto-exposure routine tuning process may limit the actual exposure sensitivity range to [100, 1200] to ensure that the noise level isn't exessive in order to preserve the image quality. Under this situation, the image under low light may be under-exposed when the sensor max exposure time (bounded by the android.control.aeTargetFpsRange when android.control.aeMode is one of the ON_* modes) and effective max sensitivity are reached. This scene mode allows the camera device auto-exposure routine to increase the sensitivity up to the max sensitivity specified by android.sensor.info.sensitivityRange when the scene is too dark and the max exposure time is reached. The captured images may be noisier compared with the images captured in normal FACE_PRIORITY mode; therefore, it is recommended that the application only use this scene mode when it is capable of reducing the noise level of the captured images. Unlike the other scene modes, android.control.aeMode, android.control.awbMode, and android.control.afMode remain active when FACE_PRIORITY_LOW_LIGHT is set. DEVICE_CUSTOM_START (v3.2) [optional] [hidden] 100 Scene mode values within the range of `[DEVICE_CUSTOM_START, DEVICE_CUSTOM_END]` are reserved for device specific customized scene modes. DEVICE_CUSTOM_END (v3.2) [optional] [hidden] 127 Scene mode values within the range of `[DEVICE_CUSTOM_START, DEVICE_CUSTOM_END]` are reserved for device specific customized scene modes. | Control for which scene mode is currently active. |  | android.control.availableSceneModes | 3.2 | BC
Details
Scene modes are custom camera modes optimized for a certain set of conditions and capture settings. This is the mode that that is active when `android.control.mode == USE_SCENE_MODE`. Aside from FACE_PRIORITY, these modes will disable android.control.aeMode, android.control.awbMode, and android.control.afMode while in use. The interpretation and implementation of these scene modes is left to the implementor of the camera device. Their behavior will not be consistent across all devices, and any given device may only implement a subset of these modes.
HAL Implementation Details
HAL implementations that include scene modes are expected to provide the per-scene settings to use for android.control.aeMode, android.control.awbMode, and android.control.afMode in android.control.sceneModeOverrides. For HIGH_SPEED_VIDEO mode, if it is included in android.control.availableSceneModes, the HAL must list supported video size and fps range in android.control.availableHighSpeedVideoConfigurations. For a given size, e.g. 1280x720, if the HAL has two different sensor configurations for normal streaming mode and high speed streaming, when this scene mode is set/reset in a sequence of capture requests, the HAL may have to switch between different sensor modes. This mode is deprecated in legacy HAL3.3, to support high speed video recording, please implement android.control.availableHighSpeedVideoConfigurations and CONSTRAINED_HIGH_SPEED_VIDEO capbility defined in android.request.availableCapabilities.
android.control.videoStabilizationMode | byte [public] [legacy] OFF (v3.2) Video stabilization is disabled. ON (v3.2) Video stabilization is enabled. | Whether video stabilization is active. |  |  | 3.2 | BC
Details
Video stabilization automatically warps images from the camera in order to stabilize motion between consecutive frames. If enabled, video stabilization can modify the android.scaler.cropRegion to keep the video stream stabilized. Switching between different video stabilization modes may take several frames to initialize, the camera device will report the current mode in capture result metadata. For example, When "ON" mode is requested, the video stabilization modes in the first several capture results may still be "OFF", and it will become "ON" when the initialization is done. In addition, not all recording sizes or frame rates may be supported for stabilization by a device that reports stabilization support. It is guaranteed that an output targeting a MediaRecorder or MediaCodec will be stabilized if the recording resolution is less than or equal to 1920 x 1080 (width less than or equal to 1920, height less than or equal to 1080), and the recording frame rate is less than or equal to 30fps. At other sizes, the CaptureResult android.control.videoStabilizationMode field will return OFF if the recording output is not stabilized, or if there are no output Surface types that can be stabilized. If a camera device supports both this mode and OIS (android.lens.opticalStabilizationMode), turning both modes on may produce undesirable interaction, so it is recommended not to enable both at the same time.
android.control.postRawSensitivityBoost | int32 [public] | The amount of additional sensitivity boost applied to output images after RAW sensor data is captured. | ISO arithmetic units, the same as android.sensor.sensitivity | android.control.postRawSensitivityBoostRange | 3.2 |
Details
Some camera devices support additional digital sensitivity boosting in the camera processing pipeline after sensor RAW image is captured. Such a boost will be applied to YUV/JPEG format output images but will not have effect on RAW output formats like RAW_SENSOR, RAW10, RAW12 or RAW_OPAQUE. This key will be `null` for devices that do not support any RAW format outputs. For devices that do support RAW format outputs, this key will always present, and if a device does not support post RAW sensitivity boost, it will list `100` in this key. If the camera device cannot apply the exact boost requested, it will reduce the boost to the nearest supported value. The final boost value used will be available in the output capture result. For devices that support post RAW sensitivity boost, the YUV/JPEG output images of such device will have the total sensitivity of `android.sensor.sensitivity * android.control.postRawSensitivityBoost / 100` The sensitivity of RAW format images will always be `android.sensor.sensitivity` This control is only effective if android.control.aeMode or android.control.mode is set to OFF; otherwise the auto-exposure algorithm will override this value.
android.control.enableZsl | byte [public as boolean] FALSE (v3.2) Requests with android.control.captureIntent == STILL_CAPTURE must be captured after previous requests. TRUE (v3.2) Requests with android.control.captureIntent == STILL_CAPTURE may or may not be captured before previous requests. | Allow camera device to enable zero-shutter-lag mode for requests with android.control.captureIntent == STILL_CAPTURE. |  |  | 3.2 |
Details
If enableZsl is `true`, the camera device may enable zero-shutter-lag mode for requests with STILL_CAPTURE capture intent. The camera device may use images captured in the past to produce output images for a zero-shutter-lag request. The result metadata including the android.sensor.timestamp reflects the source frames used to produce output images. Therefore, the contents of the output images and the result metadata may be out of order compared to previous regular requests. enableZsl does not affect requests with other capture intents. For example, when requests are submitted in the following order: Request A: enableZsl is ON, android.control.captureIntent is PREVIEW Request B: enableZsl is ON, android.control.captureIntent is STILL_CAPTURE The output images for request B may have contents captured before the output images for request A, and the result metadata for request B may be older than the result metadata for request A. Note that when enableZsl is `true`, it is not guaranteed to get output images captured in the past for requests with STILL_CAPTURE capture intent. For applications targeting SDK versions O and newer, the value of enableZsl in TEMPLATE_STILL_CAPTURE template may be `true`. The value in other templates is always `false` if present. For applications targeting SDK versions older than O, the value of enableZsl in all capture templates is always `false` if present. For application-operated ZSL, use CAMERA3_TEMPLATE_ZERO_SHUTTER_LAG template.
HAL Implementation Details
It is valid for HAL to produce regular output images for requests with STILL_CAPTURE capture intent.
android.control.extendedSceneMode | byte [public] DISABLED (v3.5) 0 Extended scene mode is disabled. BOKEH_STILL_CAPTURE (v3.5) High quality bokeh mode is enabled for all non-raw streams (including YUV, JPEG, and IMPLEMENTATION_DEFINED) when capture intent is STILL_CAPTURE. Due to the extra image processing, this mode may introduce additional stall to non-raw streams. This mode should be used in high quality still capture use case. BOKEH_CONTINUOUS (v3.5) Bokeh effect must not slow down capture rate relative to sensor raw output, and the effect is applied to all processed streams no larger than the maximum streaming dimension. This mode should be used if performance and power are a priority, such as video recording. VENDOR_START (v3.5) [hidden] 0x40 Vendor defined extended scene modes. These depend on vendor implementation. | Whether extended scene mode is enabled for a particular capture request. |  |  | 3.5 |
Details
With bokeh mode, the camera device may blur out the parts of scene that are not in focus, creating a bokeh (or shallow depth of field) effect for people or objects. When set to BOKEH_STILL_CAPTURE mode with STILL_CAPTURE capture intent, due to the extra processing needed for high quality bokeh effect, the stall may be longer than when capture intent is not STILL_CAPTURE. When set to BOKEH_STILL_CAPTURE mode with PREVIEW capture intent, If the camera device has BURST_CAPTURE capability, the frame rate requirement of BURST_CAPTURE must still be met. All streams not larger than the maximum streaming dimension for BOKEH_STILL_CAPTURE mode (queried via CameraCharacteristics#CONTROL_AVAILABLE_EXTENDED_SCENE_MODE_CAPABILITIES) will have preview bokeh effect applied. When set to BOKEH_CONTINUOUS mode, configured streams dimension should not exceed this mode's maximum streaming dimension in order to have bokeh effect applied. Bokeh effect may not be available for streams larger than the maximum streaming dimension. Switching between different extended scene modes may involve reconfiguration of the camera pipeline, resulting in long latency. The application should check this key against the available session keys queried via CameraCharacteristics#getAvailableSessionKeys. For a logical multi-camera, bokeh may be implemented by stereo vision from sub-cameras with different field of view. As a result, when bokeh mode is enabled, the camera device may override android.scaler.cropRegion or android.control.zoomRatio, and the field of view may be smaller than when bokeh mode is off.
android.control.zoomRatio | float [public] [limited] | The desired zoom ratio |  | android.control.zoomRatioRange | 3.5 |
Details
Instead of using android.scaler.cropRegion for zoom, the application can now choose to use this tag to specify the desired zoom level. By using this control, the application gains a simpler way to control zoom, which can be a combination of optical and digital zoom. For example, a multi-camera system may contain more than one lens with different focal lengths, and the user can use optical zoom by switching between lenses. Using zoomRatio has benefits in the scenarios below: Zooming in from a wide-angle lens to a telephoto lens: A floating-point ratio provides better precision compared to an integer value of android.scaler.cropRegion. Zooming out from a wide lens to an ultrawide lens: zoomRatio supports zoom-out whereas android.scaler.cropRegion doesn't. To illustrate, here are several scenarios of different zoom ratios, crop regions, and output streams, for a hypothetical camera device with an active array of size `(2000,1500)`. Camera Configuration: Active array size: `2000x1500` (3 MP, 4:3 aspect ratio) Output stream #1: `640x480` (VGA, 4:3 aspect ratio) Output stream #2: `1280x720` (720p, 16:9 aspect ratio) Case #1: 4:3 crop region with 2.0x zoom ratio Zoomed field of view: 1/4 of original field of view Crop region: `Rect(0, 0, 2000, 1500) // (left, top, right, bottom)` (post zoom) `640x480` stream source area: `(0, 0, 2000, 1500)` (equal to crop region) `1280x720` stream source area: `(0, 187, 2000, 1312)` (letterboxed) Case #2: 16:9 crop region with 2.0x zoom. Zoomed field of view: 1/4 of original field of view Crop region: `Rect(0, 187, 2000, 1312)` `640x480` stream source area: `(250, 187, 1750, 1312)` (pillarboxed) `1280x720` stream source area: `(0, 187, 2000, 1312)` (equal to crop region) Case #3: 1:1 crop region with 0.5x zoom out to ultrawide lens. Zoomed field of view: 4x of original field of view (switched from wide lens to ultrawide lens) Crop region: `Rect(250, 0, 1750, 1500)` `640x480` stream source area: `(250, 187, 1750, 1312)` (letterboxed) `1280x720` stream source area: `(250, 328, 1750, 1172)` (letterboxed) As seen from the graphs above, the coordinate system of cropRegion now changes to the effective after-zoom field-of-view, and is represented by the rectangle of (0, 0, activeArrayWith, activeArrayHeight). The same applies to AE/AWB/AF regions, and faces. This coordinate system change isn't applicable to RAW capture and its related metadata such as intrinsicCalibration and lensShadingMap. Using the same hypothetical example above, and assuming output stream #1 (640x480) is the viewfinder stream, the application can achieve 2.0x zoom in one of two ways: zoomRatio = 2.0, scaler.cropRegion = (0, 0, 2000, 1500) zoomRatio = 1.0 (default), scaler.cropRegion = (500, 375, 1500, 1125) If the application intends to set aeRegions to be top-left quarter of the viewfinder field-of-view, the android.control.aeRegions should be set to (0, 0, 1000, 750) with zoomRatio set to 2.0. Alternatively, the application can set aeRegions to the equivalent region of (500, 375, 1000, 750) for zoomRatio of 1.0. If the application doesn't explicitly set android.control.zoomRatio, its value defaults to 1.0. One limitation of controlling zoom using zoomRatio is that the android.scaler.cropRegion must only be used for letterboxing or pillarboxing of the sensor active array, and no FREEFORM cropping can be used with android.control.zoomRatio other than 1.0.
HAL Implementation Details
For all capture request templates, this field must be set to 1.0 in order to have consistent field of views between different modes.
static
Property Name | Type | Description | Units | Range | Initial HIDL HAL version | Tags
android.control.aeAvailableAntibandingModes | byte x n [public as enumList] [legacy] list of enums | List of auto-exposure antibanding modes for android.control.aeAntibandingMode that are supported by this camera device. |  | Any value listed in android.control.aeAntibandingMode | 3.2 | BC
Details
Not all of the auto-exposure anti-banding modes may be supported by a given camera device. This field lists the valid anti-banding modes that the application may request for this camera device with the android.control.aeAntibandingMode control.
android.control.aeAvailableModes | byte x n [public as enumList] [legacy] list of enums | List of auto-exposure modes for android.control.aeMode that are supported by this camera device. |  | Any value listed in android.control.aeMode | 3.2 | BC
Details
Not all the auto-exposure modes may be supported by a given camera device, especially if no flash unit is available. This entry lists the valid modes for android.control.aeMode for this camera device. All camera devices support ON, and all camera devices with flash units support ON_AUTO_FLASH and ON_ALWAYS_FLASH. FULL mode camera devices always support OFF mode, which enables application control of camera exposure time, sensitivity, and frame duration. LEGACY mode camera devices never support OFF mode. LIMITED mode devices support OFF if they support the MANUAL_SENSOR capability.
android.control.aeAvailableTargetFpsRanges | int32 x 2 x n [public as rangeInt] [legacy] list of pairs of frame rates | List of frame rate ranges for android.control.aeTargetFpsRange supported by this camera device. | Frames per second (FPS) |  | 3.2 | BC
Details
For devices at the LEGACY level or above: For constant-framerate recording, for each normal CamcorderProfile, that is, a CamcorderProfile that has quality in the range [QUALITY_LOW, QUALITY_2160P], if the profile is supported by the device and has videoFrameRate `x`, this list will always include (`x`,`x`). Also, a camera device must either not support any CamcorderProfile, or support at least one normal CamcorderProfile that has videoFrameRate `x` >= 24. For devices at the LIMITED level or above: For devices that advertise NIR color filter arrangement in android.sensor.info.colorFilterArrangement, this list will always include (`max`, `max`) where `max` = the maximum output frame rate of the maximum YUV_420_888 output size. For devices advertising any color filter arrangement other than NIR, or devices not advertising color filter arrangement, this list will always include (`min`, `max`) and (`max`, `max`) where `min` <= 15 and `max` = the maximum output frame rate of the maximum YUV_420_888 output size.
android.control.aeCompensationRange | int32 x 2 [public as rangeInt] [legacy] | Maximum and minimum exposure compensation values for android.control.aeExposureCompensation, in counts of android.control.aeCompensationStep, that are supported by this camera device. |  | Range [0,0] indicates that exposure compensation is not supported. For LIMITED and FULL devices, range must follow below requirements if exposure compensation is supported (`range != [0, 0]`): `Min.exposure compensation * android.control.aeCompensationStep <= -2 EV` `Max.exposure compensation * android.control.aeCompensationStep >= 2 EV` LEGACY devices may support a smaller range than this. | 3.2 | BC
android.control.aeCompensationStep | rational [public] [legacy] | Smallest step by which the exposure compensation can be changed. | Exposure Value (EV) |  | 3.2 | BC
Details
This is the unit for android.control.aeExposureCompensation. For example, if this key has a value of `1/2`, then a setting of `-2` for android.control.aeExposureCompensation means that the target EV offset for the auto-exposure routine is -1 EV. One unit of EV compensation changes the brightness of the captured image by a factor of two. +1 EV doubles the image brightness, while -1 EV halves the image brightness.
HAL Implementation Details
This must be less than or equal to 1/2.
android.control.afAvailableModes | byte x n [public as enumList] [legacy] List of enums | List of auto-focus (AF) modes for android.control.afMode that are supported by this camera device. |  | Any value listed in android.control.afMode | 3.2 | BC
Details
Not all the auto-focus modes may be supported by a given camera device. This entry lists the valid modes for android.control.afMode for this camera device. All LIMITED and FULL mode camera devices will support OFF mode, and all camera devices with adjustable focuser units (`android.lens.info.minimumFocusDistance > 0`) will support AUTO mode. LEGACY devices will support OFF mode only if they support focusing to infinity (by also setting android.lens.focusDistance to `0.0f`).
android.control.availableEffects | byte x n [public as enumList] [legacy] List of enums (android.control.effectMode). | List of color effects for android.control.effectMode that are supported by this camera device. |  | Any value listed in android.control.effectMode | 3.2 | BC
Details
This list contains the color effect modes that can be applied to images produced by the camera device. Implementations are not expected to be consistent across all devices. If no color effect modes are available for a device, this will only list OFF. A color effect will only be applied if android.control.mode != OFF. OFF is always included in this list. This control has no effect on the operation of other control routines such as auto-exposure, white balance, or focus.
android.control.availableSceneModes | byte x n [public as enumList] [legacy] List of enums (android.control.sceneMode). | List of scene modes for android.control.sceneMode that are supported by this camera device. |  | Any value listed in android.control.sceneMode | 3.2 | BC
Details
This list contains scene modes that can be set for the camera device. Only scene modes that have been fully implemented for the camera device may be included here. Implementations are not expected to be consistent across all devices. If no scene modes are supported by the camera device, this will be set to DISABLED. Otherwise DISABLED will not be listed. FACE_PRIORITY is always listed if face detection is supported (i.e.`android.statistics.info.maxFaceCount > 0`).
android.control.availableVideoStabilizationModes | byte x n [public as enumList] [legacy] List of enums. | List of video stabilization modes for android.control.videoStabilizationMode that are supported by this camera device. |  | Any value listed in android.control.videoStabilizationMode | 3.2 | BC
Details
OFF will always be listed.
android.control.awbAvailableModes | byte x n [public as enumList] [legacy] List of enums | List of auto-white-balance modes for android.control.awbMode that are supported by this camera device. |  | Any value listed in android.control.awbMode | 3.2 | BC
Details
Not all the auto-white-balance modes may be supported by a given camera device. This entry lists the valid modes for android.control.awbMode for this camera device. All camera devices will support ON mode. Camera devices that support the MANUAL_POST_PROCESSING capability will always support OFF mode, which enables application control of white balance, by using android.colorCorrection.transform and android.colorCorrection.gains(android.colorCorrection.mode must be set to TRANSFORM_MATRIX). This includes all FULL mode camera devices.
android.control.maxRegions | int32 x 3 [ndk_public] [legacy] | List of the maximum number of regions that can be used for metering in auto-exposure (AE), auto-white balance (AWB), and auto-focus (AF); this corresponds to the maximum number of elements in android.control.aeRegions, android.control.awbRegions, and android.control.afRegions. |  | Value must be >= 0 for each element. For full-capability devices this value must be >= 1 for AE and AF. The order of the elements is: `(AE, AWB, AF)`. | 3.2 | BC
android.control.maxRegionsAe | int32 [java_public] [synthetic] [legacy] | The maximum number of metering regions that can be used by the auto-exposure (AE) routine. |  | Value will be >= 0. For FULL-capability devices, this value will be >= 1. | 3.2 |
Details
This corresponds to the maximum allowed number of elements in android.control.aeRegions.
HAL Implementation Details
This entry is private to the framework. Fill in maxRegions to have this entry be automatically populated.
android.control.maxRegionsAwb | int32 [java_public] [synthetic] [legacy] | The maximum number of metering regions that can be used by the auto-white balance (AWB) routine. |  | Value will be >= 0. | 3.2 |
Details
This corresponds to the maximum allowed number of elements in android.control.awbRegions.
HAL Implementation Details
This entry is private to the framework. Fill in maxRegions to have this entry be automatically populated.
android.control.maxRegionsAf | int32 [java_public] [synthetic] [legacy] | The maximum number of metering regions that can be used by the auto-focus (AF) routine. |  | Value will be >= 0. For FULL-capability devices, this value will be >= 1. | 3.2 |
Details
This corresponds to the maximum allowed number of elements in android.control.afRegions.
HAL Implementation Details
This entry is private to the framework. Fill in maxRegions to have this entry be automatically populated.
android.control.sceneModeOverrides | byte x 3 x length(availableSceneModes) [system] [limited] | Ordered list of auto-exposure, auto-white balance, and auto-focus settings to use with each available scene mode. |  | For each available scene mode, the list must contain three entries containing the android.control.aeMode, android.control.awbMode, and android.control.afMode values used by the camera device. The entry order is `(aeMode, awbMode, afMode)` where aeMode has the lowest index position. | 3.2 | BC
Details
When a scene mode is enabled, the camera device is expected to override android.control.aeMode, android.control.awbMode, and android.control.afMode with its preferred settings for that scene mode. The order of this list matches that of availableSceneModes, with 3 entries for each mode. The overrides listed for FACE_PRIORITY and FACE_PRIORITY_LOW_LIGHT (if supported) are ignored, since for that mode the application-set android.control.aeMode, android.control.awbMode, and android.control.afMode values are used instead, matching the behavior when android.control.mode is set to AUTO. It is recommended that the FACE_PRIORITY and FACE_PRIORITY_LOW_LIGHT (if supported) overrides should be set to 0. For example, if availableSceneModes contains `(FACE_PRIORITY, ACTION, NIGHT)`, then the camera framework expects sceneModeOverrides to have 9 entries formatted like: `(0, 0, 0, ON_AUTO_FLASH, AUTO, CONTINUOUS_PICTURE, ON_AUTO_FLASH, INCANDESCENT, AUTO)`.
HAL Implementation Details
To maintain backward compatibility, this list will be made available in the static metadata of the camera service. The camera service will use these values to set android.control.aeMode, android.control.awbMode, and android.control.afMode when using a scene mode other than FACE_PRIORITY and FACE_PRIORITY_LOW_LIGHT (if supported).
android.control.availableHighSpeedVideoConfigurations | int32 x 5 x n [hidden as highSpeedVideoConfiguration] [limited] | List of available high speed video size, fps range and max batch size configurations supported by the camera device, in the format of (width, height, fps_min, fps_max, batch_size_max). |  | For each configuration, the fps_max >= 120fps. | 3.2 | V1
Details
When CONSTRAINED_HIGH_SPEED_VIDEO is supported in android.request.availableCapabilities, this metadata will list the supported high speed video size, fps range and max batch size configurations. All the sizes listed in this configuration will be a subset of the sizes reported by StreamConfigurationMap#getOutputSizes for processed non-stalling formats. For the high speed video use case, the application must select the video size and fps range from this metadata to configure the recording and preview streams and setup the recording requests. For example, if the application intends to do high speed recording, it can select the maximum size reported by this metadata to configure output streams. Once the size is selected, application can filter this metadata by selected size and get the supported fps ranges, and use these fps ranges to setup the recording requests. Note that for the use case of multiple output streams, application must select one unique size from this metadata to use (e.g., preview and recording streams must have the same size). Otherwise, the high speed capture session creation will fail. The min and max fps will be multiple times of 30fps. High speed video streaming extends significant performance pressue to camera hardware, to achieve efficient high speed streaming, the camera device may have to aggregate multiple frames together and send to camera device for processing where the request controls are same for all the frames in this batch. Max batch size indicates the max possible number of frames the camera device will group together for this high speed stream configuration. This max batch size will be used to generate a high speed recording request list by CameraConstrainedHighSpeedCaptureSession#createHighSpeedRequestList. The max batch size for each configuration will satisfy below conditions: Each max batch size will be a divisor of its corresponding fps_max / 30. For example, if max_fps is 300, max batch size will only be 1, 2, 5, or 10. The camera device may choose smaller internal batch size for each configuration, but the actual batch size will be a divisor of max batch size. For example, if the max batch size is 8, the actual batch size used by camera device will only be 1, 2, 4, or 8. The max batch size in each configuration entry must be no larger than 32. The camera device doesn't have to support batch mode to achieve high speed video recording, in such case, batch_size_max will be reported as 1 in each configuration entry. This fps ranges in this configuration list can only be used to create requests that are submitted to a high speed camera capture session created by CameraDevice#createConstrainedHighSpeedCaptureSession. The fps ranges reported in this metadata must not be used to setup capture requests for normal capture session, or it will cause request error.
HAL Implementation Details
All the sizes listed in this configuration will be a subset of the sizes reported by android.scaler.availableStreamConfigurations for processed non-stalling output formats. Note that for all high speed video configurations, HAL must be able to support a minimum of two streams, though the application might choose to configure just one stream. The HAL may support multiple sensor modes for high speed outputs, for example, 120fps sensor mode and 120fps recording, 240fps sensor mode for 240fps recording. The application usually starts preview first, then starts recording. To avoid sensor mode switch caused stutter when starting recording as much as possible, the application may want to ensure the same sensor mode is used for preview and recording. Therefore, The HAL must advertise the variable fps range [30, fps_max] for each fixed fps range in this configuration list. For example, if the HAL advertises [120, 120] and [240, 240], the HAL must also advertise [30, 120] and [30, 240] for each configuration. In doing so, if the application intends to do 120fps recording, it can select [30, 120] to start preview, and [120, 120] to start recording. For these variable fps ranges, it's up to the HAL to decide the actual fps values that are suitable for smooth preview streaming. If the HAL sees different max_fps values that fall into different sensor modes in a sequence of requests, the HAL must switch the sensor mode as quick as possible to minimize the mode switch caused stutter.
android.control.aeLockAvailable | byte [public as boolean] [legacy] FALSE (v3.2) TRUE (v3.2) | Whether the camera device supports android.control.aeLock |  |  | 3.2 | BC
Details
Devices with MANUAL_SENSOR capability or BURST_CAPTURE capability will always list `true`. This includes FULL devices.
android.control.awbLockAvailable | byte [public as boolean] [legacy] FALSE (v3.2) TRUE (v3.2) | Whether the camera device supports android.control.awbLock |  |  | 3.2 | BC
Details
Devices with MANUAL_POST_PROCESSING capability or BURST_CAPTURE capability will always list `true`. This includes FULL devices.
android.control.availableModes | byte x n [public as enumList] [legacy] List of enums (android.control.mode). | List of control modes for android.control.mode that are supported by this camera device. |  | Any value listed in android.control.mode | 3.2 |
Details
This list contains control modes that can be set for the camera device. LEGACY mode devices will always support AUTO mode. LIMITED and FULL devices will always support OFF, AUTO modes.
android.control.postRawSensitivityBoostRange | int32 x 2 [public as rangeInt] Range of supported post RAW sensitivitiy boosts | Range of boosts for android.control.postRawSensitivityBoost supported by this camera device. | ISO arithmetic units, the same as android.sensor.sensitivity |  | 3.2 |
Details
Devices support post RAW sensitivity boost will advertise android.control.postRawSensitivityBoost key for controling post RAW sensitivity boost. This key will be `null` for devices that do not support any RAW format outputs. For devices that do support RAW format outputs, this key will always present, and if a device does not support post RAW sensitivity boost, it will list `(100, 100)` in this key.
HAL Implementation Details
This key is added in legacy HAL3.4. For legacy HAL3.3 or earlier devices, camera framework will generate this key as `(100, 100)` if device supports any of RAW output formats. All legacy HAL3.4 and above devices should list this key if device supports any of RAW output formats.
android.control.availableExtendedSceneModeMaxSizes | int32 x 3 x n [ndk_public] [limited] List of extended scene modes and the corresponding max streaming sizes. | The list of extended scene modes for android.control.extendedSceneMode that are supported by this camera device, and each extended scene mode's maximum streaming (non-stall) size with effect. | (mode, width, height) |  | 3.5 |
Details
For DISABLED mode, the camera behaves normally with no extended scene mode enabled. For BOKEH_STILL_CAPTURE mode, the maximum streaming dimension specifies the limit under which bokeh is effective when capture intent is PREVIEW. Note that when capture intent is PREVIEW, the bokeh effect may not be as high in quality compared to STILL_CAPTURE intent in order to maintain reasonable frame rate. The maximum streaming dimension must be one of the YUV_420_888 or PRIVATE resolutions in availableStreamConfigurations, or (0, 0) if preview bokeh is not supported. If the application configures a stream larger than the maximum streaming dimension, bokeh effect may not be applied for this stream for PREVIEW intent. For BOKEH_CONTINUOUS mode, the maximum streaming dimension specifies the limit under which bokeh is effective. This dimension must be one of the YUV_420_888 or PRIVATE resolutions in availableStreamConfigurations, and if the sensor maximum resolution is larger than or equal to 1080p, the maximum streaming dimension must be at least 1080p. If the application configures a stream with larger dimension, the stream may not have bokeh effect applied.
HAL Implementation Details
For available extended scene modes, DISABLED will always be listed. HAL must support at list one non-OFF extended scene mode if extendedSceneMode control is available on the camera device. For DISABLED mode, the maximum streaming resolution must be set to (0, 0).
android.control.availableExtendedSceneModeZoomRatioRanges | float x 2 x n [ndk_public] [limited] Zoom ranges for all supported non-OFF extended scene modes. | The ranges of supported zoom ratio for non-DISABLED android.control.extendedSceneMode. | (minZoom, maxZoom) |  | 3.5 |
Details
When extended scene mode is set, the camera device may have limited range of zoom ratios compared to when extended scene mode is DISABLED. This tag lists the zoom ratio ranges for all supported non-DISABLED extended scene modes, in the same order as in android.control.availableExtended. Range [1.0, 1.0] means that no zoom (optical or digital) is supported.
android.control.availableExtendedSceneModeCapabilities | int32 x n [public as capability] [synthetic] | The list of extended scene modes for android.control.extendedSceneMode that are supported by this camera device, and each extended scene mode's capabilities such as maximum streaming size, and supported zoom ratio ranges. |  |  | 3.5 |
Details
For DISABLED mode, the camera behaves normally with no extended scene mdoe enabled. For BOKEH_STILL_CAPTURE mode, the maximum streaming dimension specifies the limit under which bokeh is effective when capture intent is PREVIEW. Note that when capture intent is PREVIEW, the bokeh effect may not be as high quality compared to STILL_CAPTURE intent in order to maintain reasonable frame rate. The maximum streaming dimension must be one of the YUV_420_888 or PRIVATE resolutions in availableStreamConfigurations, or (0, 0) if preview bokeh is not supported. If the application configures a stream larger than the maximum streaming dimension, bokeh effect may not be applied for this stream for PREVIEW intent. For BOKEH_CONTINUOUS mode, the maximum streaming dimension specifies the limit under which bokeh is effective. This dimension must be one of the YUV_420_888 or PRIVATE resolutions in availableStreamConfigurations, and if the sensor maximum resolution is larger than or equal to 1080p, the maximum streaming dimension must be at least 1080p. If the application configures a stream with larger dimension, the stream may not have bokeh effect applied. When extended scene mode is set, the camera device may have limited range of zoom ratios compared to when the mode is DISABLED. availableExtendedSceneModeCapabilities lists the zoom ranges for all supported extended modes. A range of (1.0, 1.0) means that no zoom (optical or digital) is supported.
android.control.zoomRatioRange | float x 2 [public as rangeFloat] [limited] The range of zoom ratios that this camera device supports. | Minimum and maximum zoom ratios supported by this camera device. | A pair of zoom ratio in floating-points: (minZoom, maxZoom) | maxZoom >= 1.0 >= minZoom | 3.5 |
Details
If the camera device supports zoom-out from 1x zoom, minZoom will be less than 1.0, and setting android.control.zoomRatio to values less than 1.0 increases the camera's field of view.
HAL Implementation Details
When the key is reported, the camera device's android.scaler.availableMaxDigitalZoom must be less than or equal to maxZoom. The camera framework makes sure to always control zoom via android.control.zoomRatio. The android.scaler.cropRegion tag is only used to do horizontal or vertical cropping (but not both) to achieve aspect ratio different than the camera sensor's native aspect ratio. For a logical multi-camera device, this key must either be reported for both the logical camera device and all its physical sub-cameras, or none of them. When the key is not reported, camera framework derives the application-facing zoomRatioRange to be (1, android.scaler.availableMaxDigitalZoom).
dynamic
Property Name | Type | Description | Units | Range | Initial HIDL HAL version | Tags
android.control.aePrecaptureId | int32 [system] [deprecated] | The ID sent with the latest CAMERA2_TRIGGER_PRECAPTURE_METERING call |  | Deprecated. Do not use. | 3.2 |
Details
Must be 0 if no CAMERA2_TRIGGER_PRECAPTURE_METERING trigger received yet by HAL. Always updated even if AE algorithm ignores the trigger
android.control.aeAntibandingMode | byte [public] [legacy] OFF (v3.2) The camera device will not adjust exposure duration to avoid banding problems. 50HZ (v3.2) The camera device will adjust exposure duration to avoid banding problems with 50Hz illumination sources. 60HZ (v3.2) The camera device will adjust exposure duration to avoid banding problems with 60Hz illumination sources. AUTO (v3.2) The camera device will automatically adapt its antibanding routine to the current illumination condition. This is the default mode if AUTO is available on given camera device. | The desired setting for the camera device's auto-exposure algorithm's antibanding compensation. |  | android.control.aeAvailableAntibandingModes | 3.2 | BC
Details
Some kinds of lighting fixtures, such as some fluorescent lights, flicker at the rate of the power supply frequency (60Hz or 50Hz, depending on country). While this is typically not noticeable to a person, it can be visible to a camera device. If a camera sets its exposure time to the wrong value, the flicker may become visible in the viewfinder as flicker or in a final captured image, as a set of variable-brightness bands across the image. Therefore, the auto-exposure routines of camera devices include antibanding routines that ensure that the chosen exposure value will not cause such banding. The choice of exposure time depends on the rate of flicker, which the camera device can detect automatically, or the expected rate can be selected by the application using this control. A given camera device may not support all of the possible options for the antibanding mode. The android.control.aeAvailableAntibandingModes key contains the available modes for a given camera device. AUTO mode is the default if it is available on given camera device. When AUTO mode is not available, the default will be either 50HZ or 60HZ, and both 50HZ and 60HZ will be available. If manual exposure control is enabled (by setting android.control.aeMode or android.control.mode to OFF), then this setting has no effect, and the application must ensure it selects exposure times that do not cause banding issues. The android.statistics.sceneFlicker key can assist the application in this.
HAL Implementation Details
For all capture request templates, this field must be set to AUTO if AUTO mode is available. If AUTO is not available, the default must be either 50HZ or 60HZ, and both 50HZ and 60HZ must be available. If manual exposure control is enabled (by setting android.control.aeMode or android.control.mode to OFF), then the exposure values provided by the application must not be adjusted for antibanding.
android.control.aeExposureCompensation | int32 [public] [legacy] | Adjustment to auto-exposure (AE) target image brightness. | Compensation steps | android.control.aeCompensationRange | 3.2 | BC
Details
The adjustment is measured as a count of steps, with the step size defined by android.control.aeCompensationStep and the allowed range by android.control.aeCompensationRange. For example, if the exposure value (EV) step is 0.333, '6' will mean an exposure compensation of +2 EV; -3 will mean an exposure compensation of -1 EV. One EV represents a doubling of image brightness. Note that this control will only be effective if android.control.aeMode `!=` OFF. This control will take effect even when android.control.aeLock `== true`. In the event of exposure compensation value being changed, camera device may take several frames to reach the newly requested exposure target. During that time, android.control.aeState field will be in the SEARCHING state. Once the new exposure target is reached, android.control.aeState will change from SEARCHING to either CONVERGED, LOCKED (if AE lock is enabled), or FLASH_REQUIRED (if the scene is too dark for still capture).
android.control.aeLock | byte [public as boolean] [legacy] OFF (v3.2) Auto-exposure lock is disabled; the AE algorithm is free to update its parameters. ON (v3.2) Auto-exposure lock is enabled; the AE algorithm must not update the exposure and sensitivity parameters while the lock is active. android.control.aeExposureCompensation setting changes will still take effect while auto-exposure is locked. Some rare LEGACY devices may not support this, in which case the value will always be overridden to OFF. | Whether auto-exposure (AE) is currently locked to its latest calculated values. |  |  | 3.2 | BC
Details
When set to `true` (ON), the AE algorithm is locked to its latest parameters, and will not change exposure settings until the lock is set to `false` (OFF). Note that even when AE is locked, the flash may be fired if the android.control.aeMode is ON_AUTO_FLASH / ON_ALWAYS_FLASH / ON_AUTO_FLASH_REDEYE. When android.control.aeExposureCompensation is changed, even if the AE lock is ON, the camera device will still adjust its exposure value. If AE precapture is triggered (see android.control.aePrecaptureTrigger) when AE is already locked, the camera device will not change the exposure time (android.sensor.exposureTime) and sensitivity (android.sensor.sensitivity) parameters. The flash may be fired if the android.control.aeMode is ON_AUTO_FLASH/ON_AUTO_FLASH_REDEYE and the scene is too dark. If the android.control.aeMode is ON_ALWAYS_FLASH, the scene may become overexposed. Similarly, AE precapture trigger CANCEL has no effect when AE is already locked. When an AE precapture sequence is triggered, AE unlock will not be able to unlock the AE if AE is locked by the camera device internally during precapture metering sequence In other words, submitting requests with AE unlock has no effect for an ongoing precapture metering sequence. Otherwise, the precapture metering sequence will never succeed in a sequence of preview requests where AE lock is always set to `false`. Since the camera device has a pipeline of in-flight requests, the settings that get locked do not necessarily correspond to the settings that were present in the latest capture result received from the camera device, since additional captures and AE updates may have occurred even before the result was sent out. If an application is switching between automatic and manual control and wishes to eliminate any flicker during the switch, the following procedure is recommended: Starting in auto-AE mode: Lock AE Wait for the first result to be output that has the AE locked Copy exposure settings from that result into a request, set the request to manual AE Submit the capture request, proceed to run manual AE as desired. See android.control.aeState for AE lock related state transition details.
android.control.aeMode | byte [public] [legacy] OFF (v3.2) The camera device's autoexposure routine is disabled. The application-selected android.sensor.exposureTime, android.sensor.sensitivity and android.sensor.frameDuration are used by the camera device, along with android.flash.* fields, if there's a flash unit for this camera device. Note that auto-white balance (AWB) and auto-focus (AF) behavior is device dependent when AE is in OFF mode. To have consistent behavior across different devices, it is recommended to either set AWB and AF to OFF mode or lock AWB and AF before setting AE to OFF. See android.control.awbMode, android.control.afMode, android.control.awbLock, and android.control.afTrigger for more details. LEGACY devices do not support the OFF mode and will override attempts to use this value to ON. ON (v3.2) The camera device's autoexposure routine is active, with no flash control. The application's values for android.sensor.exposureTime, android.sensor.sensitivity, and android.sensor.frameDuration are ignored. The application has control over the various android.flash.* fields. ON_AUTO_FLASH (v3.2) Like ON, except that the camera device also controls the camera's flash unit, firing it in low-light conditions. The flash may be fired during a precapture sequence (triggered by android.control.aePrecaptureTrigger) and may be fired for captures for which the android.control.captureIntent field is set to STILL_CAPTURE ON_ALWAYS_FLASH (v3.2) Like ON, except that the camera device also controls the camera's flash unit, always firing it for still captures. The flash may be fired during a precapture sequence (triggered by android.control.aePrecaptureTrigger) and will always be fired for captures for which the android.control.captureIntent field is set to STILL_CAPTURE ON_AUTO_FLASH_REDEYE (v3.2) Like ON_AUTO_FLASH, but with automatic red eye reduction. If deemed necessary by the camera device, a red eye reduction flash will fire during the precapture sequence. ON_EXTERNAL_FLASH (v3.3) An external flash has been turned on. It informs the camera device that an external flash has been turned on, and that metering (and continuous focus if active) should be quickly recaculated to account for the external flash. Otherwise, this mode acts like ON. When the external flash is turned off, AE mode should be changed to one of the other available AE modes. If the camera device supports AE external flash mode, android.control.aeState must be FLASH_REQUIRED after the camera device finishes AE scan and it's too dark without flash. | The desired mode for the camera device's auto-exposure routine. |  | android.control.aeAvailableModes | 3.2 | BC
Details
This control is only effective if android.control.mode is AUTO. When set to any of the ON modes, the camera device's auto-exposure routine is enabled, overriding the application's selected exposure time, sensor sensitivity, and frame duration (android.sensor.exposureTime, android.sensor.sensitivity, and android.sensor.frameDuration). If one of the FLASH modes is selected, the camera device's flash unit controls are also overridden. The FLASH modes are only available if the camera device has a flash unit (android.flash.info.available is `true`). If flash TORCH mode is desired, this field must be set to ON or OFF, and android.flash.mode set to TORCH. When set to any of the ON modes, the values chosen by the camera device auto-exposure routine for the overridden fields for a given capture will be available in its CaptureResult.
android.control.aeRegions | int32 x 5 x area_count [public as meteringRectangle] | List of metering areas to use for auto-exposure adjustment. | Pixel coordinates within android.sensor.info.activeArraySize or android.sensor.info.preCorrectionActiveArraySize depending on distortion correction capability and mode | Coordinates must be between `[(0,0), (width, height))` of android.sensor.info.activeArraySize or android.sensor.info.preCorrectionActiveArraySize depending on distortion correction capability and mode | 3.2 | BC
Details
Not available if android.control.maxRegionsAe is 0. Otherwise will always be present. The maximum number of regions supported by the device is determined by the value of android.control.maxRegionsAe. For devices not supporting android.distortionCorrection.mode control, the coordinate system always follows that of android.sensor.info.activeArraySize, with (0,0) being the top-left pixel in the active pixel array, and (android.sensor.info.activeArraySize.width - 1, android.sensor.info.activeArraySize.height - 1) being the bottom-right pixel in the active pixel array. For devices supporting android.distortionCorrection.mode control, the coordinate system depends on the mode being set. When the distortion correction mode is OFF, the coordinate system follows android.sensor.info.preCorrectionActiveArraySize, with `(0, 0)` being the top-left pixel of the pre-correction active array, and (android.sensor.info.preCorrectionActiveArraySize.width - 1, android.sensor.info.preCorrectionActiveArraySize.height - 1) being the bottom-right pixel in the pre-correction active pixel array. When the distortion correction mode is not OFF, the coordinate system follows android.sensor.info.activeArraySize, with `(0, 0)` being the top-left pixel of the active array, and (android.sensor.info.activeArraySize.width - 1, android.sensor.info.activeArraySize.height - 1) being the bottom-right pixel in the active pixel array. The weight must be within `[0, 1000]`, and represents a weight for every pixel in the area. This means that a large metering area with the same weight as a smaller area will have more effect in the metering result. Metering areas can partially overlap and the camera device will add the weights in the overlap region. The weights are relative to weights of other exposure metering regions, so if only one region is used, all non-zero weights will have the same effect. A region with 0 weight is ignored. If all regions have 0 weight, then no specific metering area needs to be used by the camera device. If the metering region is outside the used android.scaler.cropRegion returned in capture result metadata, the camera device will ignore the sections outside the crop region and output only the intersection rectangle as the metering region in the result metadata. If the region is entirely outside the crop region, it will be ignored and not reported in the result metadata. Starting from API level 30, the coordinate system of activeArraySize or preCorrectionActiveArraySize is used to represent post-zoomRatio field of view, not pre-zoom field of view. This means that the same aeRegions values at different android.control.zoomRatio represent different parts of the scene. The aeRegions coordinates are relative to the activeArray/preCorrectionActiveArray representing the zoomed field of view. If android.control.zoomRatio is set to 1.0 (default), the same aeRegions at different android.scaler.cropRegion still represent the same parts of the scene as they do before. See android.control.zoomRatio for details. Whether to use activeArraySize or preCorrectionActiveArraySize still depends on distortion correction mode.
HAL Implementation Details
The HAL level representation of MeteringRectangle[] is a int[5 * area_count]. Every five elements represent a metering region of (xmin, ymin, xmax, ymax, weight). The rectangle is defined to be inclusive on xmin and ymin, but exclusive on xmax and ymax. HAL must always report metering regions in the coordinate system of pre-correction active array.
android.control.aeTargetFpsRange | int32 x 2 [public as rangeInt] [legacy] | Range over which the auto-exposure routine can adjust the capture frame rate to maintain good exposure. | Frames per second (FPS) | Any of the entries in android.control.aeAvailableTargetFpsRanges | 3.2 | BC
Details
Only constrains auto-exposure (AE) algorithm, not manual control of android.sensor.exposureTime and android.sensor.frameDuration.
android.control.aePrecaptureTrigger | byte [public] [limited] IDLE (v3.2) The trigger is idle. START (v3.2) The precapture metering sequence will be started by the camera device. The exact effect of the precapture trigger depends on the current AE mode and state. CANCEL (v3.2) The camera device will cancel any currently active or completed precapture metering sequence, the auto-exposure routine will return to its initial state. | Whether the camera device will trigger a precapture metering sequence when it processes this request. |  |  | 3.2 | BC
Details
This entry is normally set to IDLE, or is not included at all in the request settings. When included and set to START, the camera device will trigger the auto-exposure (AE) precapture metering sequence. When set to CANCEL, the camera device will cancel any active precapture metering trigger, and return to its initial AE state. If a precapture metering sequence is already completed, and the camera device has implicitly locked the AE for subsequent still capture, the CANCEL trigger will unlock the AE and return to its initial AE state. The precapture sequence should be triggered before starting a high-quality still capture for final metering decisions to be made, and for firing pre-capture flash pulses to estimate scene brightness and required final capture flash power, when the flash is enabled. Normally, this entry should be set to START for only a single request, and the application should wait until the sequence completes before starting a new one. When a precapture metering sequence is finished, the camera device may lock the auto-exposure routine internally to be able to accurately expose the subsequent still capture image (`android.control.captureIntent == STILL_CAPTURE`). For this case, the AE may not resume normal scan if no subsequent still capture is submitted. To ensure that the AE routine restarts normal scan, the application should submit a request with `android.control.aeLock == true`, followed by a request with `android.control.aeLock == false`, if the application decides not to submit a still capture request after the precapture sequence completes. Alternatively, for API level 23 or newer devices, the CANCEL can be used to unlock the camera device internally locked AE if the application doesn't submit a still capture request after the AE precapture trigger. Note that, the CANCEL was added in API level 23, and must not be used in devices that have earlier API levels. The exact effect of auto-exposure (AE) precapture trigger depends on the current AE mode and state; see android.control.aeState for AE precapture state transition details. On LEGACY-level devices, the precapture trigger is not supported; capturing a high-resolution JPEG image will automatically trigger a precapture sequence before the high-resolution capture, including potentially firing a pre-capture flash. Using the precapture trigger and the auto-focus trigger android.control.afTrigger simultaneously is allowed. However, since these triggers often require cooperation between the auto-focus and auto-exposure routines (for example, the may need to be enabled for a focus sweep), the camera device may delay acting on a later trigger until the previous trigger has been fully handled. This may lead to longer intervals between the trigger and changes to android.control.aeState indicating the start of the precapture sequence, for example. If both the precapture and the auto-focus trigger are activated on the same request, then the camera device will complete them in the optimal order for that device.
HAL Implementation Details
The HAL must support triggering the AE precapture trigger while an AF trigger is active (and vice versa), or at the same time as the AF trigger. It is acceptable for the HAL to treat these as two consecutive triggers, for example handling the AF trigger and then the AE trigger. Or the HAL may choose to optimize the case with both triggers fired at once, to minimize the latency for converging both focus and exposure/flash usage.
android.control.aeState | byte [public] [limited] INACTIVE (v3.2) AE is off or recently reset. When a camera device is opened, it starts in this state. This is a transient state, the camera device may skip reporting this state in capture result. SEARCHING (v3.2) AE doesn't yet have a good set of control values for the current scene. This is a transient state, the camera device may skip reporting this state in capture result. CONVERGED (v3.2) AE has a good set of control values for the current scene. LOCKED (v3.2) AE has been locked. FLASH_REQUIRED (v3.2) AE has a good set of control values, but flash needs to be fired for good quality still capture. PRECAPTURE (v3.2) AE has been asked to do a precapture sequence and is currently executing it. Precapture can be triggered through setting android.control.aePrecaptureTrigger to START. Currently active and completed (if it causes camera device internal AE lock) precapture metering sequence can be canceled through setting android.control.aePrecaptureTrigger to CANCEL. Once PRECAPTURE completes, AE will transition to CONVERGED or FLASH_REQUIRED as appropriate. This is a transient state, the camera device may skip reporting this state in capture result. | Current state of the auto-exposure (AE) algorithm. |  |  | 3.2 |
Details
Switching between or enabling AE modes (android.control.aeMode) always resets the AE state to INACTIVE. Similarly, switching between android.control.mode, or android.control.sceneMode if `android.control.mode == USE_SCENE_MODE` resets all the algorithm states to INACTIVE. The camera device can do several state transitions between two results, if it is allowed by the state transition table. For example: INACTIVE may never actually be seen in a result. The state in the result is the state for this image (in sync with this image): if AE state becomes CONVERGED, then the image data associated with this result should be good to use. Below are state transition tables for different AE modes.
State | Transition Cause | New State | Notes
--- | --- | --- | ---
INACTIVE |  | INACTIVE | Camera device auto exposure algorithm is disabled
When android.control.aeMode is AE_MODE_ON*:
State | Transition Cause | New State | Notes
--- | --- | --- | ---
INACTIVE | Camera device initiates AE scan | SEARCHING | Values changing
INACTIVE | android.control.aeLock is ON | LOCKED | Values locked
SEARCHING | Camera device finishes AE scan | CONVERGED | Good values, not changing
SEARCHING | Camera device finishes AE scan | FLASH_REQUIRED | Converged but too dark w/o flash
SEARCHING | android.control.aeLock is ON | LOCKED | Values locked
CONVERGED | Camera device initiates AE scan | SEARCHING | Values changing
CONVERGED | android.control.aeLock is ON | LOCKED | Values locked
FLASH_REQUIRED | Camera device initiates AE scan | SEARCHING | Values changing
FLASH_REQUIRED | android.control.aeLock is ON | LOCKED | Values locked
LOCKED | android.control.aeLock is OFF | SEARCHING | Values not good after unlock
LOCKED | android.control.aeLock is OFF | CONVERGED | Values good after unlock
LOCKED | android.control.aeLock is OFF | FLASH_REQUIRED | Exposure good, but too dark
PRECAPTURE | Sequence done. android.control.aeLock is OFF | CONVERGED | Ready for high-quality capture
PRECAPTURE | Sequence done. android.control.aeLock is ON | LOCKED | Ready for high-quality capture
LOCKED | aeLock is ON and aePrecaptureTrigger is START | LOCKED | Precapture trigger is ignored when AE is already locked
LOCKED | aeLock is ON and aePrecaptureTrigger is CANCEL | LOCKED | Precapture trigger is ignored when AE is already locked
Any state (excluding LOCKED) | android.control.aePrecaptureTrigger is START | PRECAPTURE | Start AE precapture metering sequence
Any state (excluding LOCKED) | android.control.aePrecaptureTrigger is CANCEL | INACTIVE | Currently active precapture metering sequence is canceled
If the camera device supports AE external flash mode (ON_EXTERNAL_FLASH is included in android.control.aeAvailableModes), android.control.aeState must be FLASH_REQUIRED after the camera device finishes AE scan and it's too dark without flash. For the above table, the camera device may skip reporting any state changes that happen without application intervention (i.e. mode switch, trigger, locking). Any state that can be skipped in that manner is called a transient state. For example, for above AE modes (AE_MODE_ON*), in addition to the state transitions listed in above table, it is also legal for the camera device to skip one or more transient states between two results. See below table for examples:
State | Transition Cause | New State | Notes
--- | --- | --- | ---
INACTIVE | Camera device finished AE scan | CONVERGED | Values are already good, transient states are skipped by camera device.
Any state (excluding LOCKED) | android.control.aePrecaptureTrigger is START, sequence done | FLASH_REQUIRED | Converged but too dark w/o flash after a precapture sequence, transient states are skipped by camera device.
Any state (excluding LOCKED) | android.control.aePrecaptureTrigger is START, sequence done | CONVERGED | Converged after a precapture sequence, transient states are skipped by camera device.
Any state (excluding LOCKED) | android.control.aePrecaptureTrigger is CANCEL, converged | FLASH_REQUIRED | Converged but too dark w/o flash after a precapture sequence is canceled, transient states are skipped by camera device.
Any state (excluding LOCKED) | android.control.aePrecaptureTrigger is CANCEL, converged | CONVERGED | Converged after a precapture sequenceis canceled, transient states are skipped by camera device.
CONVERGED | Camera device finished AE scan | FLASH_REQUIRED | Converged but too dark w/o flash after a new scan, transient states are skipped by camera device.
FLASH_REQUIRED | Camera device finished AE scan | CONVERGED | Converged after a new scan, transient states are skipped by camera device.
android.control.afMode | byte [public] [legacy] OFF (v3.2) The auto-focus routine does not control the lens; android.lens.focusDistance is controlled by the application. AUTO (v3.2) Basic automatic focus mode. In this mode, the lens does not move unless the autofocus trigger action is called. When that trigger is activated, AF will transition to ACTIVE_SCAN, then to the outcome of the scan (FOCUSED or NOT_FOCUSED). Always supported if lens is not fixed focus. Use android.lens.info.minimumFocusDistance to determine if lens is fixed-focus. Triggering AF_CANCEL resets the lens position to default, and sets the AF state to INACTIVE. MACRO (v3.2) Close-up focusing mode. In this mode, the lens does not move unless the autofocus trigger action is called. When that trigger is activated, AF will transition to ACTIVE_SCAN, then to the outcome of the scan (FOCUSED or NOT_FOCUSED). This mode is optimized for focusing on objects very close to the camera. When that trigger is activated, AF will transition to ACTIVE_SCAN, then to the outcome of the scan (FOCUSED or NOT_FOCUSED). Triggering cancel AF resets the lens position to default, and sets the AF state to INACTIVE. CONTINUOUS_VIDEO (v3.2) In this mode, the AF algorithm modifies the lens position continually to attempt to provide a constantly-in-focus image stream. The focusing behavior should be suitable for good quality video recording; typically this means slower focus movement and no overshoots. When the AF trigger is not involved, the AF algorithm should start in INACTIVE state, and then transition into PASSIVE_SCAN and PASSIVE_FOCUSED states as appropriate. When the AF trigger is activated, the algorithm should immediately transition into AF_FOCUSED or AF_NOT_FOCUSED as appropriate, and lock the lens position until a cancel AF trigger is received. Once cancel is received, the algorithm should transition back to INACTIVE and resume passive scan. Note that this behavior is not identical to CONTINUOUS_PICTURE, since an ongoing PASSIVE_SCAN must immediately be canceled. CONTINUOUS_PICTURE (v3.2) In this mode, the AF algorithm modifies the lens position continually to attempt to provide a constantly-in-focus image stream. The focusing behavior should be suitable for still image capture; typically this means focusing as fast as possible. When the AF trigger is not involved, the AF algorithm should start in INACTIVE state, and then transition into PASSIVE_SCAN and PASSIVE_FOCUSED states as appropriate as it attempts to maintain focus. When the AF trigger is activated, the algorithm should finish its PASSIVE_SCAN if active, and then transition into AF_FOCUSED or AF_NOT_FOCUSED as appropriate, and lock the lens position until a cancel AF trigger is received. When the AF cancel trigger is activated, the algorithm should transition back to INACTIVE and then act as if it has just been started. EDOF (v3.2) Extended depth of field (digital focus) mode. The camera device will produce images with an extended depth of field automatically; no special focusing operations need to be done before taking a picture. AF triggers are ignored, and the AF state will always be INACTIVE. | Whether auto-focus (AF) is currently enabled, and what mode it is set to. |  | android.control.afAvailableModes | 3.2 | BC
Details
Only effective if android.control.mode = AUTO and the lens is not fixed focus (i.e. `android.lens.info.minimumFocusDistance > 0`). Also note that when android.control.aeMode is OFF, the behavior of AF is device dependent. It is recommended to lock AF by using android.control.afTrigger before setting android.control.aeMode to OFF, or set AF mode to OFF when AE is OFF. If the lens is controlled by the camera device auto-focus algorithm, the camera device will report the current AF status in android.control.afState in result metadata.
HAL Implementation Details
When afMode is AUTO or MACRO, the lens must not move until an AF trigger is sent in a request (android.control.afTrigger `==` START). After an AF trigger, the afState will end up with either FOCUSED_LOCKED or NOT_FOCUSED_LOCKED state (see android.control.afState for detailed state transitions), which indicates that the lens is locked and will not move. If camera movement (e.g. tilting camera) causes the lens to move after the lens is locked, the HAL must compensate this movement appropriately such that the same focal plane remains in focus. When afMode is one of the continuous auto focus modes, the HAL is free to start a AF scan whenever it's not locked. When the lens is locked after an AF trigger (see android.control.afState for detailed state transitions), the HAL should maintain the same lock behavior as above. When afMode is OFF, the application controls focus manually. The accuracy of the focus distance control depends on the android.lens.info.focusDistanceCalibration. However, the lens must not move regardless of the camera movement for any focus distance manual control. To put this in concrete terms, if the camera has lens elements which may move based on camera orientation or motion (e.g. due to gravity), then the HAL must drive the lens to remain in a fixed position invariant to the camera's orientation or motion, for example, by using accelerometer measurements in the lens control logic. This is a typical issue that will arise on camera modules with open-loop VCMs.
android.control.afRegions | int32 x 5 x area_count [public as meteringRectangle] | List of metering areas to use for auto-focus. | Pixel coordinates within android.sensor.info.activeArraySize or android.sensor.info.preCorrectionActiveArraySize depending on distortion correction capability and mode | Coordinates must be between `[(0,0), (width, height))` of android.sensor.info.activeArraySize or android.sensor.info.preCorrectionActiveArraySize depending on distortion correction capability and mode | 3.2 | BC
Details
Not available if android.control.maxRegionsAf is 0. Otherwise will always be present. The maximum number of focus areas supported by the device is determined by the value of android.control.maxRegionsAf. For devices not supporting android.distortionCorrection.mode control, the coordinate system always follows that of android.sensor.info.activeArraySize, with (0,0) being the top-left pixel in the active pixel array, and (android.sensor.info.activeArraySize.width - 1, android.sensor.info.activeArraySize.height - 1) being the bottom-right pixel in the active pixel array. For devices supporting android.distortionCorrection.mode control, the coordinate system depends on the mode being set. When the distortion correction mode is OFF, the coordinate system follows android.sensor.info.preCorrectionActiveArraySize, with `(0, 0)` being the top-left pixel of the pre-correction active array, and (android.sensor.info.preCorrectionActiveArraySize.width - 1, android.sensor.info.preCorrectionActiveArraySize.height - 1) being the bottom-right pixel in the pre-correction active pixel array. When the distortion correction mode is not OFF, the coordinate system follows android.sensor.info.activeArraySize, with `(0, 0)` being the top-left pixel of the active array, and (android.sensor.info.activeArraySize.width - 1, android.sensor.info.activeArraySize.height - 1) being the bottom-right pixel in the active pixel array. The weight must be within `[0, 1000]`, and represents a weight for every pixel in the area. This means that a large metering area with the same weight as a smaller area will have more effect in the metering result. Metering areas can partially overlap and the camera device will add the weights in the overlap region. The weights are relative to weights of other metering regions, so if only one region is used, all non-zero weights will have the same effect. A region with 0 weight is ignored. If all regions have 0 weight, then no specific metering area needs to be used by the camera device. The capture result will either be a zero weight region as well, or the region selected by the camera device as the focus area of interest. If the metering region is outside the used android.scaler.cropRegion returned in capture result metadata, the camera device will ignore the sections outside the crop region and output only the intersection rectangle as the metering region in the result metadata. If the region is entirely outside the crop region, it will be ignored and not reported in the result metadata. Starting from API level 30, the coordinate system of activeArraySize or preCorrectionActiveArraySize is used to represent post-zoomRatio field of view, not pre-zoom field of view. This means that the same afRegions values at different android.control.zoomRatio represent different parts of the scene. The afRegions coordinates are relative to the activeArray/preCorrectionActiveArray representing the zoomed field of view. If android.control.zoomRatio is set to 1.0 (default), the same afRegions at different android.scaler.cropRegion still represent the same parts of the scene as they do before. See android.control.zoomRatio for details. Whether to use activeArraySize or preCorrectionActiveArraySize still depends on distortion correction mode.
HAL Implementation Details
The HAL level representation of MeteringRectangle[] is a int[5 * area_count]. Every five elements represent a metering region of (xmin, ymin, xmax, ymax, weight). The rectangle is defined to be inclusive on xmin and ymin, but exclusive on xmax and ymax. HAL must always report metering regions in the coordinate system of pre-correction active array.
android.control.afTrigger | byte [public] [legacy] IDLE (v3.2) The trigger is idle. START (v3.2) Autofocus will trigger now. CANCEL (v3.2) Autofocus will return to its initial state, and cancel any currently active trigger. | Whether the camera device will trigger autofocus for this request. |  |  | 3.2 | BC
Details
This entry is normally set to IDLE, or is not included at all in the request settings. When included and set to START, the camera device will trigger the autofocus algorithm. If autofocus is disabled, this trigger has no effect. When set to CANCEL, the camera device will cancel any active trigger, and return to its initial AF state. Generally, applications should set this entry to START or CANCEL for only a single capture, and then return it to IDLE (or not set at all). Specifying START for multiple captures in a row means restarting the AF operation over and over again. See android.control.afState for what the trigger means for each AF mode. Using the autofocus trigger and the precapture trigger android.control.aePrecaptureTrigger simultaneously is allowed. However, since these triggers often require cooperation between the auto-focus and auto-exposure routines (for example, the may need to be enabled for a focus sweep), the camera device may delay acting on a later trigger until the previous trigger has been fully handled. This may lead to longer intervals between the trigger and changes to android.control.afState, for example.
HAL Implementation Details
The HAL must support triggering the AF trigger while an AE precapture trigger is active (and vice versa), or at the same time as the AE trigger. It is acceptable for the HAL to treat these as two consecutive triggers, for example handling the AF trigger and then the AE trigger. Or the HAL may choose to optimize the case with both triggers fired at once, to minimize the latency for converging both focus and exposure/flash usage.
android.control.afState | byte [public] [legacy] INACTIVE (v3.2) AF is off or has not yet tried to scan/been asked to scan. When a camera device is opened, it starts in this state. This is a transient state, the camera device may skip reporting this state in capture result. PASSIVE_SCAN (v3.2) AF is currently performing an AF scan initiated the camera device in a continuous autofocus mode. Only used by CONTINUOUS_* AF modes. This is a transient state, the camera device may skip reporting this state in capture result. PASSIVE_FOCUSED (v3.2) AF currently believes it is in focus, but may restart scanning at any time. Only used by CONTINUOUS_* AF modes. This is a transient state, the camera device may skip reporting this state in capture result. ACTIVE_SCAN (v3.2) AF is performing an AF scan because it was triggered by AF trigger. Only used by AUTO or MACRO AF modes. This is a transient state, the camera device may skip reporting this state in capture result. FOCUSED_LOCKED (v3.2) AF believes it is focused correctly and has locked focus. This state is reached only after an explicit START AF trigger has been sent (android.control.afTrigger), when good focus has been obtained. The lens will remain stationary until the AF mode (android.control.afMode) is changed or a new AF trigger is sent to the camera device (android.control.afTrigger). NOT_FOCUSED_LOCKED (v3.2) AF has failed to focus successfully and has locked focus. This state is reached only after an explicit START AF trigger has been sent (android.control.afTrigger), when good focus cannot be obtained. The lens will remain stationary until the AF mode (android.control.afMode) is changed or a new AF trigger is sent to the camera device (android.control.afTrigger). PASSIVE_UNFOCUSED (v3.2) AF finished a passive scan without finding focus, and may restart scanning at any time. Only used by CONTINUOUS_* AF modes. This is a transient state, the camera device may skip reporting this state in capture result. LEGACY camera devices do not support this state. When a passive scan has finished, it will always go to PASSIVE_FOCUSED. | Current state of auto-focus (AF) algorithm. |  |  | 3.2 |
Details
Switching between or enabling AF modes (android.control.afMode) always resets the AF state to INACTIVE. Similarly, switching between android.control.mode, or android.control.sceneMode if `android.control.mode == USE_SCENE_MODE` resets all the algorithm states to INACTIVE. The camera device can do several state transitions between two results, if it is allowed by the state transition table. For example: INACTIVE may never actually be seen in a result. The state in the result is the state for this image (in sync with this image): if AF state becomes FOCUSED, then the image data associated with this result should be sharp. Below are state transition tables for different AF modes. When android.control.afMode is AF_MODE_OFF or AF_MODE_EDOF:
State | Transition Cause | New State | Notes
--- | --- | --- | ---
INACTIVE |  | INACTIVE | Never changes
When android.control.afMode is AF_MODE_AUTO or AF_MODE_MACRO:
State | Transition Cause | New State | Notes
--- | --- | --- | ---
INACTIVE | AF_TRIGGER | ACTIVE_SCAN | Start AF sweep, Lens now moving
ACTIVE_SCAN | AF sweep done | FOCUSED_LOCKED | Focused, Lens now locked
ACTIVE_SCAN | AF sweep done | NOT_FOCUSED_LOCKED | Not focused, Lens now locked
ACTIVE_SCAN | AF_CANCEL | INACTIVE | Cancel/reset AF, Lens now locked
FOCUSED_LOCKED | AF_CANCEL | INACTIVE | Cancel/reset AF
FOCUSED_LOCKED | AF_TRIGGER | ACTIVE_SCAN | Start new sweep, Lens now moving
NOT_FOCUSED_LOCKED | AF_CANCEL | INACTIVE | Cancel/reset AF
NOT_FOCUSED_LOCKED | AF_TRIGGER | ACTIVE_SCAN | Start new sweep, Lens now moving
Any state | Mode change | INACTIVE |
For the above table, the camera device may skip reporting any state changes that happen without application intervention (i.e. mode switch, trigger, locking). Any state that can be skipped in that manner is called a transient state. For example, for these AF modes (AF_MODE_AUTO and AF_MODE_MACRO), in addition to the state transitions listed in above table, it is also legal for the camera device to skip one or more transient states between two results. See below table for examples:
State | Transition Cause | New State | Notes
--- | --- | --- | ---
INACTIVE | AF_TRIGGER | FOCUSED_LOCKED | Focus is already good or good after a scan, lens is now locked.
INACTIVE | AF_TRIGGER | NOT_FOCUSED_LOCKED | Focus failed after a scan, lens is now locked.
FOCUSED_LOCKED | AF_TRIGGER | FOCUSED_LOCKED | Focus is already good or good after a scan, lens is now locked.
NOT_FOCUSED_LOCKED | AF_TRIGGER | FOCUSED_LOCKED | Focus is good after a scan, lens is not locked.
When android.control.afMode is AF_MODE_CONTINUOUS_VIDEO:
State | Transition Cause | New State | Notes
--- | --- | --- | ---
INACTIVE | Camera device initiates new scan | PASSIVE_SCAN | Start AF scan, Lens now moving
INACTIVE | AF_TRIGGER | NOT_FOCUSED_LOCKED | AF state query, Lens now locked
PASSIVE_SCAN | Camera device completes current scan | PASSIVE_FOCUSED | End AF scan, Lens now locked
PASSIVE_SCAN | Camera device fails current scan | PASSIVE_UNFOCUSED | End AF scan, Lens now locked
PASSIVE_SCAN | AF_TRIGGER | FOCUSED_LOCKED | Immediate transition, if focus is good. Lens now locked
PASSIVE_SCAN | AF_TRIGGER | NOT_FOCUSED_LOCKED | Immediate transition, if focus is bad. Lens now locked
PASSIVE_SCAN | AF_CANCEL | INACTIVE | Reset lens position, Lens now locked
PASSIVE_FOCUSED | Camera device initiates new scan | PASSIVE_SCAN | Start AF scan, Lens now moving
PASSIVE_UNFOCUSED | Camera device initiates new scan | PASSIVE_SCAN | Start AF scan, Lens now moving
PASSIVE_FOCUSED | AF_TRIGGER | FOCUSED_LOCKED | Immediate transition, lens now locked
PASSIVE_UNFOCUSED | AF_TRIGGER | NOT_FOCUSED_LOCKED | Immediate transition, lens now locked
FOCUSED_LOCKED | AF_TRIGGER | FOCUSED_LOCKED | No effect
FOCUSED_LOCKED | AF_CANCEL | INACTIVE | Restart AF scan
NOT_FOCUSED_LOCKED | AF_TRIGGER | NOT_FOCUSED_LOCKED | No effect
NOT_FOCUSED_LOCKED | AF_CANCEL | INACTIVE | Restart AF scan
When android.control.afMode is AF_MODE_CONTINUOUS_PICTURE:
State | Transition Cause | New State | Notes
--- | --- | --- | ---
INACTIVE | Camera device initiates new scan | PASSIVE_SCAN | Start AF scan, Lens now moving
INACTIVE | AF_TRIGGER | NOT_FOCUSED_LOCKED | AF state query, Lens now locked
PASSIVE_SCAN | Camera device completes current scan | PASSIVE_FOCUSED | End AF scan, Lens now locked
PASSIVE_SCAN | Camera device fails current scan | PASSIVE_UNFOCUSED | End AF scan, Lens now locked
PASSIVE_SCAN | AF_TRIGGER | FOCUSED_LOCKED | Eventual transition once the focus is good. Lens now locked
PASSIVE_SCAN | AF_TRIGGER | NOT_FOCUSED_LOCKED | Eventual transition if cannot find focus. Lens now locked
PASSIVE_SCAN | AF_CANCEL | INACTIVE | Reset lens position, Lens now locked
PASSIVE_FOCUSED | Camera device initiates new scan | PASSIVE_SCAN | Start AF scan, Lens now moving
PASSIVE_UNFOCUSED | Camera device initiates new scan | PASSIVE_SCAN | Start AF scan, Lens now moving
PASSIVE_FOCUSED | AF_TRIGGER | FOCUSED_LOCKED | Immediate trans. Lens now locked
PASSIVE_UNFOCUSED | AF_TRIGGER | NOT_FOCUSED_LOCKED | Immediate trans. Lens now locked
FOCUSED_LOCKED | AF_TRIGGER | FOCUSED_LOCKED | No effect
FOCUSED_LOCKED | AF_CANCEL | INACTIVE | Restart AF scan
NOT_FOCUSED_LOCKED | AF_TRIGGER | NOT_FOCUSED_LOCKED | No effect
NOT_FOCUSED_LOCKED | AF_CANCEL | INACTIVE | Restart AF scan
When switch between AF_MODE_CONTINUOUS_* (CAF modes) and AF_MODE_AUTO/AF_MODE_MACRO (AUTO modes), the initial INACTIVE or PASSIVE_SCAN states may be skipped by the camera device. When a trigger is included in a mode switch request, the trigger will be evaluated in the context of the new mode in the request. See below table for examples:
State | Transition Cause | New State | Notes
--- | --- | --- | ---
any state | CAF-->AUTO mode switch | INACTIVE | Mode switch without trigger, initial state must be INACTIVE
any state | CAF-->AUTO mode switch with AF_TRIGGER | trigger-reachable states from INACTIVE | Mode switch with trigger, INACTIVE is skipped
any state | AUTO-->CAF mode switch | passively reachable states from INACTIVE | Mode switch without trigger, passive transient state is skipped
android.control.afTriggerId | int32 [system] [deprecated] | The ID sent with the latest CAMERA2_TRIGGER_AUTOFOCUS call |  | Deprecated. Do not use. | 3.2 |
Details
Must be 0 if no CAMERA2_TRIGGER_AUTOFOCUS trigger received yet by HAL. Always updated even if AF algorithm ignores the trigger
android.control.awbLock | byte [public as boolean] [legacy] OFF (v3.2) Auto-white balance lock is disabled; the AWB algorithm is free to update its parameters if in AUTO mode. ON (v3.2) Auto-white balance lock is enabled; the AWB algorithm will not update its parameters while the lock is active. | Whether auto-white balance (AWB) is currently locked to its latest calculated values. |  |  | 3.2 | BC
Details
When set to `true` (ON), the AWB algorithm is locked to its latest parameters, and will not change color balance settings until the lock is set to `false` (OFF). Since the camera device has a pipeline of in-flight requests, the settings that get locked do not necessarily correspond to the settings that were present in the latest capture result received from the camera device, since additional captures and AWB updates may have occurred even before the result was sent out. If an application is switching between automatic and manual control and wishes to eliminate any flicker during the switch, the following procedure is recommended: Starting in auto-AWB mode: Lock AWB Wait for the first result to be output that has the AWB locked Copy AWB settings from that result into a request, set the request to manual AWB Submit the capture request, proceed to run manual AWB as desired. Note that AWB lock is only meaningful when android.control.awbMode is in the AUTO mode; in other modes, AWB is already fixed to a specific setting. Some LEGACY devices may not support ON; the value is then overridden to OFF.
android.control.awbMode | byte [public] [legacy] OFF (v3.2) The camera device's auto-white balance routine is disabled. The application-selected color transform matrix (android.colorCorrection.transform) and gains (android.colorCorrection.gains) are used by the camera device for manual white balance control. AUTO (v3.2) The camera device's auto-white balance routine is active. The application's values for android.colorCorrection.transform and android.colorCorrection.gains are ignored. For devices that support the MANUAL_POST_PROCESSING capability, the values used by the camera device for the transform and gains will be available in the capture result for this request. INCANDESCENT (v3.2) The camera device's auto-white balance routine is disabled; the camera device uses incandescent light as the assumed scene illumination for white balance. While the exact white balance transforms are up to the camera device, they will approximately match the CIE standard illuminant A. The application's values for android.colorCorrection.transform and android.colorCorrection.gains are ignored. For devices that support the MANUAL_POST_PROCESSING capability, the values used by the camera device for the transform and gains will be available in the capture result for this request. FLUORESCENT (v3.2) The camera device's auto-white balance routine is disabled; the camera device uses fluorescent light as the assumed scene illumination for white balance. While the exact white balance transforms are up to the camera device, they will approximately match the CIE standard illuminant F2. The application's values for android.colorCorrection.transform and android.colorCorrection.gains are ignored. For devices that support the MANUAL_POST_PROCESSING capability, the values used by the camera device for the transform and gains will be available in the capture result for this request. WARM_FLUORESCENT (v3.2) The camera device's auto-white balance routine is disabled; the camera device uses warm fluorescent light as the assumed scene illumination for white balance. While the exact white balance transforms are up to the camera device, they will approximately match the CIE standard illuminant F4. The application's values for android.colorCorrection.transform and android.colorCorrection.gains are ignored. For devices that support the MANUAL_POST_PROCESSING capability, the values used by the camera device for the transform and gains will be available in the capture result for this request. DAYLIGHT (v3.2) The camera device's auto-white balance routine is disabled; the camera device uses daylight light as the assumed scene illumination for white balance. While the exact white balance transforms are up to the camera device, they will approximately match the CIE standard illuminant D65. The application's values for android.colorCorrection.transform and android.colorCorrection.gains are ignored. For devices that support the MANUAL_POST_PROCESSING capability, the values used by the camera device for the transform and gains will be available in the capture result for this request. CLOUDY_DAYLIGHT (v3.2) The camera device's auto-white balance routine is disabled; the camera device uses cloudy daylight light as the assumed scene illumination for white balance. The application's values for android.colorCorrection.transform and android.colorCorrection.gains are ignored. For devices that support the MANUAL_POST_PROCESSING capability, the values used by the camera device for the transform and gains will be available in the capture result for this request. TWILIGHT (v3.2) The camera device's auto-white balance routine is disabled; the camera device uses twilight light as the assumed scene illumination for white balance. The application's values for android.colorCorrection.transform and android.colorCorrection.gains are ignored. For devices that support the MANUAL_POST_PROCESSING capability, the values used by the camera device for the transform and gains will be available in the capture result for this request. SHADE (v3.2) The camera device's auto-white balance routine is disabled; the camera device uses shade light as the assumed scene illumination for white balance. The application's values for android.colorCorrection.transform and android.colorCorrection.gains are ignored. For devices that support the MANUAL_POST_PROCESSING capability, the values used by the camera device for the transform and gains will be available in the capture result for this request. | Whether auto-white balance (AWB) is currently setting the color transform fields, and what its illumination target is. |  | android.control.awbAvailableModes | 3.2 | BC
Details
This control is only effective if android.control.mode is AUTO. When set to the ON mode, the camera device's auto-white balance routine is enabled, overriding the application's selected android.colorCorrection.transform, android.colorCorrection.gains and android.colorCorrection.mode. Note that when android.control.aeMode is OFF, the behavior of AWB is device dependent. It is recommened to also set AWB mode to OFF or lock AWB by using android.control.awbLock before setting AE mode to OFF. When set to the OFF mode, the camera device's auto-white balance routine is disabled. The application manually controls the white balance by android.colorCorrection.transform, android.colorCorrection.gains and android.colorCorrection.mode. When set to any other modes, the camera device's auto-white balance routine is disabled. The camera device uses each particular illumination target for white balance adjustment. The application's values for android.colorCorrection.transform, android.colorCorrection.gains and android.colorCorrection.mode are ignored.
android.control.awbRegions | int32 x 5 x area_count [public as meteringRectangle] | List of metering areas to use for auto-white-balance illuminant estimation. | Pixel coordinates within android.sensor.info.activeArraySize or android.sensor.info.preCorrectionActiveArraySize depending on distortion correction capability and mode | Coordinates must be between `[(0,0), (width, height))` of android.sensor.info.activeArraySize or android.sensor.info.preCorrectionActiveArraySize depending on distortion correction capability and mode | 3.2 | BC
Details
Not available if android.control.maxRegionsAwb is 0. Otherwise will always be present. The maximum number of regions supported by the device is determined by the value of android.control.maxRegionsAwb. For devices not supporting android.distortionCorrection.mode control, the coordinate system always follows that of android.sensor.info.activeArraySize, with (0,0) being the top-left pixel in the active pixel array, and (android.sensor.info.activeArraySize.width - 1, android.sensor.info.activeArraySize.height - 1) being the bottom-right pixel in the active pixel array. For devices supporting android.distortionCorrection.mode control, the coordinate system depends on the mode being set. When the distortion correction mode is OFF, the coordinate system follows android.sensor.info.preCorrectionActiveArraySize, with `(0, 0)` being the top-left pixel of the pre-correction active array, and (android.sensor.info.preCorrectionActiveArraySize.width - 1, android.sensor.info.preCorrectionActiveArraySize.height - 1) being the bottom-right pixel in the pre-correction active pixel array. When the distortion correction mode is not OFF, the coordinate system follows android.sensor.info.activeArraySize, with `(0, 0)` being the top-left pixel of the active array, and (android.sensor.info.activeArraySize.width - 1, android.sensor.info.activeArraySize.height - 1) being the bottom-right pixel in the active pixel array. The weight must range from 0 to 1000, and represents a weight for every pixel in the area. This means that a large metering area with the same weight as a smaller area will have more effect in the metering result. Metering areas can partially overlap and the camera device will add the weights in the overlap region. The weights are relative to weights of other white balance metering regions, so if only one region is used, all non-zero weights will have the same effect. A region with 0 weight is ignored. If all regions have 0 weight, then no specific metering area needs to be used by the camera device. If the metering region is outside the used android.scaler.cropRegion returned in capture result metadata, the camera device will ignore the sections outside the crop region and output only the intersection rectangle as the metering region in the result metadata. If the region is entirely outside the crop region, it will be ignored and not reported in the result metadata. Starting from API level 30, the coordinate system of activeArraySize or preCorrectionActiveArraySize is used to represent post-zoomRatio field of view, not pre-zoom field of view. This means that the same awbRegions values at different android.control.zoomRatio represent different parts of the scene. The awbRegions coordinates are relative to the activeArray/preCorrectionActiveArray representing the zoomed field of view. If android.control.zoomRatio is set to 1.0 (default), the same awbRegions at different android.scaler.cropRegion still represent the same parts of the scene as they do before. See android.control.zoomRatio for details. Whether to use activeArraySize or preCorrectionActiveArraySize still depends on distortion correction mode.
HAL Implementation Details
The HAL level representation of MeteringRectangle[] is a int[5 * area_count]. Every five elements represent a metering region of (xmin, ymin, xmax, ymax, weight). The rectangle is defined to be inclusive on xmin and ymin, but exclusive on xmax and ymax. HAL must always report metering regions in the coordinate system of pre-correction active array.
android.control.captureIntent | byte [public] [legacy] CUSTOM (v3.2) The goal of this request doesn't fall into the other categories. The camera device will default to preview-like behavior. PREVIEW (v3.2) This request is for a preview-like use case. The precapture trigger may be used to start off a metering w/flash sequence. STILL_CAPTURE (v3.2) This request is for a still capture-type use case. If the flash unit is under automatic control, it may fire as needed. VIDEO_RECORD (v3.2) This request is for a video recording use case. VIDEO_SNAPSHOT (v3.2) This request is for a video snapshot (still image while recording video) use case. The camera device should take the highest-quality image possible (given the other settings) without disrupting the frame rate of video recording. ZERO_SHUTTER_LAG (v3.2) This request is for a ZSL usecase; the application will stream full-resolution images and reprocess one or several later for a final capture. MANUAL (v3.2) This request is for manual capture use case where the applications want to directly control the capture parameters. For example, the application may wish to manually control android.sensor.exposureTime, android.sensor.sensitivity, etc. MOTION_TRACKING (v3.3) This request is for a motion tracking use case, where the application will use camera and inertial sensor data to locate and track objects in the world. The camera device auto-exposure routine will limit the exposure time of the camera to no more than 20 milliseconds, to minimize motion blur. | Information to the camera device 3A (auto-exposure, auto-focus, auto-white balance) routines about the purpose of this capture, to help the camera device to decide optimal 3A strategy. |  |  | 3.2 | BC
Details
This control (except for MANUAL) is only effective if `android.control.mode != OFF` and any 3A routine is active. All intents are supported by all devices, except that: * ZERO_SHUTTER_LAG will be supported if android.request.availableCapabilities contains PRIVATE_REPROCESSING or YUV_REPROCESSING. * MANUAL will be supported if android.request.availableCapabilities contains MANUAL_SENSOR. * MOTION_TRACKING will be supported if android.request.availableCapabilities contains MOTION_TRACKING.
android.control.awbState | byte [public] [limited] INACTIVE (v3.2) AWB is not in auto mode, or has not yet started metering. When a camera device is opened, it starts in this state. This is a transient state, the camera device may skip reporting this state in capture result. SEARCHING (v3.2) AWB doesn't yet have a good set of control values for the current scene. This is a transient state, the camera device may skip reporting this state in capture result. CONVERGED (v3.2) AWB has a good set of control values for the current scene. LOCKED (v3.2) AWB has been locked. | Current state of auto-white balance (AWB) algorithm. |  |  | 3.2 |
Details
Switching between or enabling AWB modes (android.control.awbMode) always resets the AWB state to INACTIVE. Similarly, switching between android.control.mode, or android.control.sceneMode if `android.control.mode == USE_SCENE_MODE` resets all the algorithm states to INACTIVE. The camera device can do several state transitions between two results, if it is allowed by the state transition table. So INACTIVE may never actually be seen in a result. The state in the result is the state for this image (in sync with this image): if AWB state becomes CONVERGED, then the image data associated with this result should be good to use. Below are state transition tables for different AWB modes. When `android.control.awbMode != AWB_MODE_AUTO`:
State | Transition Cause | New State | Notes
--- | --- | --- | ---
INACTIVE |  | INACTIVE | Camera device auto white balance algorithm is disabled
When android.control.awbMode is AWB_MODE_AUTO:
State | Transition Cause | New State | Notes
--- | --- | --- | ---
INACTIVE | Camera device initiates AWB scan | SEARCHING | Values changing
INACTIVE | android.control.awbLock is ON | LOCKED | Values locked
SEARCHING | Camera device finishes AWB scan | CONVERGED | Good values, not changing
SEARCHING | android.control.awbLock is ON | LOCKED | Values locked
CONVERGED | Camera device initiates AWB scan | SEARCHING | Values changing
CONVERGED | android.control.awbLock is ON | LOCKED | Values locked
LOCKED | android.control.awbLock is OFF | SEARCHING | Values not good after unlock
For the above table, the camera device may skip reporting any state changes that happen without application intervention (i.e. mode switch, trigger, locking). Any state that can be skipped in that manner is called a transient state. For example, for this AWB mode (AWB_MODE_AUTO), in addition to the state transitions listed in above table, it is also legal for the camera device to skip one or more transient states between two results. See below table for examples:
State | Transition Cause | New State | Notes
--- | --- | --- | ---
INACTIVE | Camera device finished AWB scan | CONVERGED | Values are already good, transient states are skipped by camera device.
LOCKED | android.control.awbLock is OFF | CONVERGED | Values good after unlock, transient states are skipped by camera device.
android.control.effectMode | byte [public] [legacy] OFF (v3.2) No color effect will be applied. MONO (v3.2) [optional] A "monocolor" effect where the image is mapped into a single color. This will typically be grayscale. NEGATIVE (v3.2) [optional] A "photo-negative" effect where the image's colors are inverted. SOLARIZE (v3.2) [optional] A "solarisation" effect (Sabattier effect) where the image is wholly or partially reversed in tone. SEPIA (v3.2) [optional] A "sepia" effect where the image is mapped into warm gray, red, and brown tones. POSTERIZE (v3.2) [optional] A "posterization" effect where the image uses discrete regions of tone rather than a continuous gradient of tones. WHITEBOARD (v3.2) [optional] A "whiteboard" effect where the image is typically displayed as regions of white, with black or grey details. BLACKBOARD (v3.2) [optional] A "blackboard" effect where the image is typically displayed as regions of black, with white or grey details. AQUA (v3.2) [optional] An "aqua" effect where a blue hue is added to the image. | A special color effect to apply. |  | android.control.availableEffects | 3.2 | BC
Details
When this mode is set, a color effect will be applied to images produced by the camera device. The interpretation and implementation of these color effects is left to the implementor of the camera device, and should not be depended on to be consistent (or present) across all devices.
android.control.mode | byte [public] [legacy] OFF (v3.2) Full application control of pipeline. All control by the device's metering and focusing (3A) routines is disabled, and no other settings in android.control.* have any effect, except that android.control.captureIntent may be used by the camera device to select post-processing values for processing blocks that do not allow for manual control, or are not exposed by the camera API. However, the camera device's 3A routines may continue to collect statistics and update their internal state so that when control is switched to AUTO mode, good control values can be immediately applied. AUTO (v3.2) Use settings for each individual 3A routine. Manual control of capture parameters is disabled. All controls in android.control.* besides sceneMode take effect. USE_SCENE_MODE (v3.2) [optional] Use a specific scene mode. Enabling this disables control.aeMode, control.awbMode and control.afMode controls; the camera device will ignore those settings while USE_SCENE_MODE is active (except for FACE_PRIORITY scene mode). Other control entries are still active. This setting can only be used if scene mode is supported (i.e. android.control.availableSceneModes contain some modes other than DISABLED). For extended scene modes such as BOKEH, please use USE_EXTENDED_SCENE_MODE instead. OFF_KEEP_STATE (v3.2) [optional] Same as OFF mode, except that this capture will not be used by camera device background auto-exposure, auto-white balance and auto-focus algorithms (3A) to update their statistics. Specifically, the 3A routines are locked to the last values set from a request with AUTO, OFF, or USE_SCENE_MODE, and any statistics or state updates collected from manual captures with OFF_KEEP_STATE will be discarded by the camera device. USE_EXTENDED_SCENE_MODE (v3.5) [optional] Use a specific extended scene mode. When extended scene mode is on, the camera device may override certain control parameters, such as targetFpsRange, AE, AWB, and AF modes, to achieve best power and quality tradeoffs. Only the mandatory stream combinations of LIMITED hardware level are guaranteed. This setting can only be used if extended scene mode is supported (i.e. android.control.availableExtendedSceneModes contains some modes other than DISABLED). | Overall mode of 3A (auto-exposure, auto-white-balance, auto-focus) control routines. |  | android.control.availableModes | 3.2 | BC
Details
This is a top-level 3A control switch. When set to OFF, all 3A control by the camera device is disabled. The application must set the fields for capture parameters itself. When set to AUTO, the individual algorithm controls in android.control.* are in effect, such as android.control.afMode. When set to USE_SCENE_MODE or USE_EXTENDED_SCENE_MODE, the individual controls in android.control.* are mostly disabled, and the camera device implements one of the scene mode or extended scene mode settings (such as ACTION, SUNSET, PARTY, or BOKEH) as it wishes. The camera device scene mode 3A settings are provided by capture results. When set to OFF_KEEP_STATE, it is similar to OFF mode, the only difference is that this frame will not be used by camera device background 3A statistics update, as if this frame is never captured. This mode can be used in the scenario where the application doesn't want a 3A manual control capture to affect the subsequent auto 3A capture results.
android.control.sceneMode | byte [public] [legacy] DISABLED (v3.2) 0 Indicates that no scene modes are set for a given capture request. FACE_PRIORITY (v3.2) If face detection support exists, use face detection data for auto-focus, auto-white balance, and auto-exposure routines. If face detection statistics are disabled (i.e. android.statistics.faceDetectMode is set to OFF), this should still operate correctly (but will not return face detection statistics to the framework). Unlike the other scene modes, android.control.aeMode, android.control.awbMode, and android.control.afMode remain active when FACE_PRIORITY is set. ACTION (v3.2) [optional] Optimized for photos of quickly moving objects. Similar to SPORTS. PORTRAIT (v3.2) [optional] Optimized for still photos of people. LANDSCAPE (v3.2) [optional] Optimized for photos of distant macroscopic objects. NIGHT (v3.2) [optional] Optimized for low-light settings. NIGHT_PORTRAIT (v3.2) [optional] Optimized for still photos of people in low-light settings. THEATRE (v3.2) [optional] Optimized for dim, indoor settings where flash must remain off. BEACH (v3.2) [optional] Optimized for bright, outdoor beach settings. SNOW (v3.2) [optional] Optimized for bright, outdoor settings containing snow. SUNSET (v3.2) [optional] Optimized for scenes of the setting sun. STEADYPHOTO (v3.2) [optional] Optimized to avoid blurry photos due to small amounts of device motion (for example: due to hand shake). FIREWORKS (v3.2) [optional] Optimized for nighttime photos of fireworks. SPORTS (v3.2) [optional] Optimized for photos of quickly moving people. Similar to ACTION. PARTY (v3.2) [optional] Optimized for dim, indoor settings with multiple moving people. CANDLELIGHT (v3.2) [optional] Optimized for dim settings where the main light source is a candle. BARCODE (v3.2) [optional] Optimized for accurately capturing a photo of barcode for use by camera applications that wish to read the barcode value. HIGH_SPEED_VIDEO (v3.2) [deprecated] [optional] This is deprecated, please use CameraDevice#createConstrainedHighSpeedCaptureSession and CameraConstrainedHighSpeedCaptureSession#createHighSpeedRequestList for high speed video recording. Optimized for high speed video recording (frame rate >=60fps) use case. The supported high speed video sizes and fps ranges are specified in android.control.availableHighSpeedVideoConfigurations. To get desired output frame rates, the application is only allowed to select video size and fps range combinations listed in this static metadata. The fps range can be control via android.control.aeTargetFpsRange. In this mode, the camera device will override aeMode, awbMode, and afMode to ON, ON, and CONTINUOUS_VIDEO, respectively. All post-processing block mode controls will be overridden to be FAST. Therefore, no manual control of capture and post-processing parameters is possible. All other controls operate the same as when android.control.mode == AUTO. This means that all other android.control.* fields continue to work, such as android.control.aeTargetFpsRange android.control.aeExposureCompensation android.control.aeLock android.control.awbLock android.control.effectMode android.control.aeRegions android.control.afRegions android.control.awbRegions android.control.afTrigger android.control.aePrecaptureTrigger android.control.zoomRatio Outside of android.control.*, the following controls will work: android.flash.mode (automatic flash for still capture will not work since aeMode is ON) android.lens.opticalStabilizationMode (if it is supported) android.scaler.cropRegion android.statistics.faceDetectMode For high speed recording use case, the actual maximum supported frame rate may be lower than what camera can output, depending on the destination Surfaces for the image data. For example, if the destination surface is from video encoder, the application need check if the video encoder is capable of supporting the high frame rate for a given video size, or it will end up with lower recording frame rate. If the destination surface is from preview window, the preview frame rate will be bounded by the screen refresh rate. The camera device will only support up to 2 output high speed streams (processed non-stalling format defined in android.request.maxNumOutputStreams) in this mode. This control will be effective only if all of below conditions are true: The application created no more than maxNumHighSpeedStreams processed non-stalling format output streams, where maxNumHighSpeedStreams is calculated as min(2, android.request.maxNumOutputStreams[Processed (but not-stalling)]). The stream sizes are selected from the sizes reported by android.control.availableHighSpeedVideoConfigurations. No processed non-stalling or raw streams are configured. When above conditions are NOT satistied, the controls of this mode and android.control.aeTargetFpsRange will be ignored by the camera device, the camera device will fall back to android.control.mode `==` AUTO, and the returned capture result metadata will give the fps range choosen by the camera device. Switching into or out of this mode may trigger some camera ISP/sensor reconfigurations, which may introduce extra latency. It is recommended that the application avoids unnecessary scene mode switch as much as possible. HDR (v3.2) [optional] Turn on a device-specific high dynamic range (HDR) mode. In this scene mode, the camera device captures images that keep a larger range of scene illumination levels visible in the final image. For example, when taking a picture of a object in front of a bright window, both the object and the scene through the window may be visible when using HDR mode, while in normal AUTO mode, one or the other may be poorly exposed. As a tradeoff, HDR mode generally takes much longer to capture a single image, has no user control, and may have other artifacts depending on the HDR method used. Therefore, HDR captures operate at a much slower rate than regular captures. In this mode, on LIMITED or FULL devices, when a request is made with a android.control.captureIntent of STILL_CAPTURE, the camera device will capture an image using a high dynamic range capture technique. On LEGACY devices, captures that target a JPEG-format output will be captured with HDR, and the capture intent is not relevant. The HDR capture may involve the device capturing a burst of images internally and combining them into one, or it may involve the device using specialized high dynamic range capture hardware. In all cases, a single image is produced in response to a capture request submitted while in HDR mode. Since substantial post-processing is generally needed to produce an HDR image, only YUV, PRIVATE, and JPEG outputs are supported for LIMITED/FULL device HDR captures, and only JPEG outputs are supported for LEGACY HDR captures. Using a RAW output for HDR capture is not supported. Some devices may also support always-on HDR, which applies HDR processing at full frame rate. For these devices, intents other than STILL_CAPTURE will also produce an HDR output with no frame rate impact compared to normal operation, though the quality may be lower than for STILL_CAPTURE intents. If SCENE_MODE_HDR is used with unsupported output types or capture intents, the images captured will be as if the SCENE_MODE was not enabled at all. FACE_PRIORITY_LOW_LIGHT (v3.2) [optional] [hidden] Same as FACE_PRIORITY scene mode, except that the camera device will choose higher sensitivity values (android.sensor.sensitivity) under low light conditions. The camera device may be tuned to expose the images in a reduced sensitivity range to produce the best quality images. For example, if the android.sensor.info.sensitivityRange gives range of [100, 1600], the camera device auto-exposure routine tuning process may limit the actual exposure sensitivity range to [100, 1200] to ensure that the noise level isn't exessive in order to preserve the image quality. Under this situation, the image under low light may be under-exposed when the sensor max exposure time (bounded by the android.control.aeTargetFpsRange when android.control.aeMode is one of the ON_* modes) and effective max sensitivity are reached. This scene mode allows the camera device auto-exposure routine to increase the sensitivity up to the max sensitivity specified by android.sensor.info.sensitivityRange when the scene is too dark and the max exposure time is reached. The captured images may be noisier compared with the images captured in normal FACE_PRIORITY mode; therefore, it is recommended that the application only use this scene mode when it is capable of reducing the noise level of the captured images. Unlike the other scene modes, android.control.aeMode, android.control.awbMode, and android.control.afMode remain active when FACE_PRIORITY_LOW_LIGHT is set. DEVICE_CUSTOM_START (v3.2) [optional] [hidden] 100 Scene mode values within the range of `[DEVICE_CUSTOM_START, DEVICE_CUSTOM_END]` are reserved for device specific customized scene modes. DEVICE_CUSTOM_END (v3.2) [optional] [hidden] 127 Scene mode values within the range of `[DEVICE_CUSTOM_START, DEVICE_CUSTOM_END]` are reserved for device specific customized scene modes. | Control for which scene mode is currently active. |  | android.control.availableSceneModes | 3.2 | BC
Details
Scene modes are custom camera modes optimized for a certain set of conditions and capture settings. This is the mode that that is active when `android.control.mode == USE_SCENE_MODE`. Aside from FACE_PRIORITY, these modes will disable android.control.aeMode, android.control.awbMode, and android.control.afMode while in use. The interpretation and implementation of these scene modes is left to the implementor of the camera device. Their behavior will not be consistent across all devices, and any given device may only implement a subset of these modes.
HAL Implementation Details
HAL implementations that include scene modes are expected to provide the per-scene settings to use for android.control.aeMode, android.control.awbMode, and android.control.afMode in android.control.sceneModeOverrides. For HIGH_SPEED_VIDEO mode, if it is included in android.control.availableSceneModes, the HAL must list supported video size and fps range in android.control.availableHighSpeedVideoConfigurations. For a given size, e.g. 1280x720, if the HAL has two different sensor configurations for normal streaming mode and high speed streaming, when this scene mode is set/reset in a sequence of capture requests, the HAL may have to switch between different sensor modes. This mode is deprecated in legacy HAL3.3, to support high speed video recording, please implement android.control.availableHighSpeedVideoConfigurations and CONSTRAINED_HIGH_SPEED_VIDEO capbility defined in android.request.availableCapabilities.
android.control.videoStabilizationMode | byte [public] [legacy] OFF (v3.2) Video stabilization is disabled. ON (v3.2) Video stabilization is enabled. | Whether video stabilization is active. |  |  | 3.2 | BC
Details
Video stabilization automatically warps images from the camera in order to stabilize motion between consecutive frames. If enabled, video stabilization can modify the android.scaler.cropRegion to keep the video stream stabilized. Switching between different video stabilization modes may take several frames to initialize, the camera device will report the current mode in capture result metadata. For example, When "ON" mode is requested, the video stabilization modes in the first several capture results may still be "OFF", and it will become "ON" when the initialization is done. In addition, not all recording sizes or frame rates may be supported for stabilization by a device that reports stabilization support. It is guaranteed that an output targeting a MediaRecorder or MediaCodec will be stabilized if the recording resolution is less than or equal to 1920 x 1080 (width less than or equal to 1920, height less than or equal to 1080), and the recording frame rate is less than or equal to 30fps. At other sizes, the CaptureResult android.control.videoStabilizationMode field will return OFF if the recording output is not stabilized, or if there are no output Surface types that can be stabilized. If a camera device supports both this mode and OIS (android.lens.opticalStabilizationMode), turning both modes on may produce undesirable interaction, so it is recommended not to enable both at the same time.
android.control.postRawSensitivityBoost | int32 [public] | The amount of additional sensitivity boost applied to output images after RAW sensor data is captured. | ISO arithmetic units, the same as android.sensor.sensitivity | android.control.postRawSensitivityBoostRange | 3.2 |
Details
Some camera devices support additional digital sensitivity boosting in the camera processing pipeline after sensor RAW image is captured. Such a boost will be applied to YUV/JPEG format output images but will not have effect on RAW output formats like RAW_SENSOR, RAW10, RAW12 or RAW_OPAQUE. This key will be `null` for devices that do not support any RAW format outputs. For devices that do support RAW format outputs, this key will always present, and if a device does not support post RAW sensitivity boost, it will list `100` in this key. If the camera device cannot apply the exact boost requested, it will reduce the boost to the nearest supported value. The final boost value used will be available in the output capture result. For devices that support post RAW sensitivity boost, the YUV/JPEG output images of such device will have the total sensitivity of `android.sensor.sensitivity * android.control.postRawSensitivityBoost / 100` The sensitivity of RAW format images will always be `android.sensor.sensitivity` This control is only effective if android.control.aeMode or android.control.mode is set to OFF; otherwise the auto-exposure algorithm will override this value.
android.control.enableZsl | byte [public as boolean] FALSE (v3.2) Requests with android.control.captureIntent == STILL_CAPTURE must be captured after previous requests. TRUE (v3.2) Requests with android.control.captureIntent == STILL_CAPTURE may or may not be captured before previous requests. | Allow camera device to enable zero-shutter-lag mode for requests with android.control.captureIntent == STILL_CAPTURE. |  |  | 3.2 |
Details
If enableZsl is `true`, the camera device may enable zero-shutter-lag mode for requests with STILL_CAPTURE capture intent. The camera device may use images captured in the past to produce output images for a zero-shutter-lag request. The result metadata including the android.sensor.timestamp reflects the source frames used to produce output images. Therefore, the contents of the output images and the result metadata may be out of order compared to previous regular requests. enableZsl does not affect requests with other capture intents. For example, when requests are submitted in the following order: Request A: enableZsl is ON, android.control.captureIntent is PREVIEW Request B: enableZsl is ON, android.control.captureIntent is STILL_CAPTURE The output images for request B may have contents captured before the output images for request A, and the result metadata for request B may be older than the result metadata for request A. Note that when enableZsl is `true`, it is not guaranteed to get output images captured in the past for requests with STILL_CAPTURE capture intent. For applications targeting SDK versions O and newer, the value of enableZsl in TEMPLATE_STILL_CAPTURE template may be `true`. The value in other templates is always `false` if present. For applications targeting SDK versions older than O, the value of enableZsl in all capture templates is always `false` if present. For application-operated ZSL, use CAMERA3_TEMPLATE_ZERO_SHUTTER_LAG template.
HAL Implementation Details
It is valid for HAL to produce regular output images for requests with STILL_CAPTURE capture intent.
android.control.afSceneChange | byte [public] NOT_DETECTED (v3.3) Scene change is not detected within the AF region(s). DETECTED (v3.3) Scene change is detected within the AF region(s). | Whether a significant scene change is detected within the currently-set AF region(s). |  |  | 3.3 |
Details
When the camera focus routine detects a change in the scene it is looking at, such as a large shift in camera viewpoint, significant motion in the scene, or a significant illumination change, this value will be set to DETECTED for a single capture result. Otherwise the value will be NOT_DETECTED. The threshold for detection is similar to what would trigger a new passive focus scan to begin in CONTINUOUS autofocus modes. This key will be available if the camera device advertises this key via CameraCharacteristics#getAvailableCaptureResultKeys.
android.control.extendedSceneMode | byte [public] DISABLED (v3.5) 0 Extended scene mode is disabled. BOKEH_STILL_CAPTURE (v3.5) High quality bokeh mode is enabled for all non-raw streams (including YUV, JPEG, and IMPLEMENTATION_DEFINED) when capture intent is STILL_CAPTURE. Due to the extra image processing, this mode may introduce additional stall to non-raw streams. This mode should be used in high quality still capture use case. BOKEH_CONTINUOUS (v3.5) Bokeh effect must not slow down capture rate relative to sensor raw output, and the effect is applied to all processed streams no larger than the maximum streaming dimension. This mode should be used if performance and power are a priority, such as video recording. VENDOR_START (v3.5) [hidden] 0x40 Vendor defined extended scene modes. These depend on vendor implementation. | Whether extended scene mode is enabled for a particular capture request. |  |  | 3.5 |
Details
With bokeh mode, the camera device may blur out the parts of scene that are not in focus, creating a bokeh (or shallow depth of field) effect for people or objects. When set to BOKEH_STILL_CAPTURE mode with STILL_CAPTURE capture intent, due to the extra processing needed for high quality bokeh effect, the stall may be longer than when capture intent is not STILL_CAPTURE. When set to BOKEH_STILL_CAPTURE mode with PREVIEW capture intent, If the camera device has BURST_CAPTURE capability, the frame rate requirement of BURST_CAPTURE must still be met. All streams not larger than the maximum streaming dimension for BOKEH_STILL_CAPTURE mode (queried via CameraCharacteristics#CONTROL_AVAILABLE_EXTENDED_SCENE_MODE_CAPABILITIES) will have preview bokeh effect applied. When set to BOKEH_CONTINUOUS mode, configured streams dimension should not exceed this mode's maximum streaming dimension in order to have bokeh effect applied. Bokeh effect may not be available for streams larger than the maximum streaming dimension. Switching between different extended scene modes may involve reconfiguration of the camera pipeline, resulting in long latency. The application should check this key against the available session keys queried via CameraCharacteristics#getAvailableSessionKeys. For a logical multi-camera, bokeh may be implemented by stereo vision from sub-cameras with different field of view. As a result, when bokeh mode is enabled, the camera device may override android.scaler.cropRegion or android.control.zoomRatio, and the field of view may be smaller than when bokeh mode is off.
android.control.zoomRatio | float [public] [limited] | The desired zoom ratio |  | android.control.zoomRatioRange | 3.5 |
Details
Instead of using android.scaler.cropRegion for zoom, the application can now choose to use this tag to specify the desired zoom level. By using this control, the application gains a simpler way to control zoom, which can be a combination of optical and digital zoom. For example, a multi-camera system may contain more than one lens with different focal lengths, and the user can use optical zoom by switching between lenses. Using zoomRatio has benefits in the scenarios below: Zooming in from a wide-angle lens to a telephoto lens: A floating-point ratio provides better precision compared to an integer value of android.scaler.cropRegion. Zooming out from a wide lens to an ultrawide lens: zoomRatio supports zoom-out whereas android.scaler.cropRegion doesn't. To illustrate, here are several scenarios of different zoom ratios, crop regions, and output streams, for a hypothetical camera device with an active array of size `(2000,1500)`. Camera Configuration: Active array size: `2000x1500` (3 MP, 4:3 aspect ratio) Output stream #1: `640x480` (VGA, 4:3 aspect ratio) Output stream #2: `1280x720` (720p, 16:9 aspect ratio) Case #1: 4:3 crop region with 2.0x zoom ratio Zoomed field of view: 1/4 of original field of view Crop region: `Rect(0, 0, 2000, 1500) // (left, top, right, bottom)` (post zoom) `640x480` stream source area: `(0, 0, 2000, 1500)` (equal to crop region) `1280x720` stream source area: `(0, 187, 2000, 1312)` (letterboxed) Case #2: 16:9 crop region with 2.0x zoom. Zoomed field of view: 1/4 of original field of view Crop region: `Rect(0, 187, 2000, 1312)` `640x480` stream source area: `(250, 187, 1750, 1312)` (pillarboxed) `1280x720` stream source area: `(0, 187, 2000, 1312)` (equal to crop region) Case #3: 1:1 crop region with 0.5x zoom out to ultrawide lens. Zoomed field of view: 4x of original field of view (switched from wide lens to ultrawide lens) Crop region: `Rect(250, 0, 1750, 1500)` `640x480` stream source area: `(250, 187, 1750, 1312)` (letterboxed) `1280x720` stream source area: `(250, 328, 1750, 1172)` (letterboxed) As seen from the graphs above, the coordinate system of cropRegion now changes to the effective after-zoom field-of-view, and is represented by the rectangle of (0, 0, activeArrayWith, activeArrayHeight). The same applies to AE/AWB/AF regions, and faces. This coordinate system change isn't applicable to RAW capture and its related metadata such as intrinsicCalibration and lensShadingMap. Using the same hypothetical example above, and assuming output stream #1 (640x480) is the viewfinder stream, the application can achieve 2.0x zoom in one of two ways: zoomRatio = 2.0, scaler.cropRegion = (0, 0, 2000, 1500) zoomRatio = 1.0 (default), scaler.cropRegion = (500, 375, 1500, 1125) If the application intends to set aeRegions to be top-left quarter of the viewfinder field-of-view, the android.control.aeRegions should be set to (0, 0, 1000, 750) with zoomRatio set to 2.0. Alternatively, the application can set aeRegions to the equivalent region of (500, 375, 1000, 750) for zoomRatio of 1.0. If the application doesn't explicitly set android.control.zoomRatio, its value defaults to 1.0. One limitation of controlling zoom using zoomRatio is that the android.scaler.cropRegion must only be used for letterboxing or pillarboxing of the sensor active array, and no FREEFORM cropping can be used with android.control.zoomRatio other than 1.0.
HAL Implementation Details
For all capture request templates, this field must be set to 1.0 in order to have consistent field of views between different modes.
demosaic
controls
Property Name | Type | Description | Units | Range | Initial HIDL HAL version | Tags
android.demosaic.mode | byte [system] FAST (v3.2) Minimal or no slowdown of frame rate compared to Bayer RAW output. HIGH_QUALITY (v3.2) Improved processing quality but the frame rate might be slowed down relative to raw output. | Controls the quality of the demosaicing processing. |  |  | 3.2 | FUTURE
edge
controls
Property Name | Type | Description | Units | Range | Initial HIDL HAL version | Tags
android.edge.mode | byte [public] [full] OFF (v3.2) No edge enhancement is applied. FAST (v3.2) Apply edge enhancement at a quality level that does not slow down frame rate relative to sensor output. It may be the same as OFF if edge enhancement will slow down frame rate relative to sensor. HIGH_QUALITY (v3.2) Apply high-quality edge enhancement, at a cost of possibly reduced output frame rate. ZERO_SHUTTER_LAG (v3.2) [optional] Edge enhancement is applied at different levels for different output streams, based on resolution. Streams at maximum recording resolution (see CameraDevice#createCaptureSession) or below have edge enhancement applied, while higher-resolution streams have no edge enhancement applied. The level of edge enhancement for low-resolution streams is tuned so that frame rate is not impacted, and the quality is equal to or better than FAST (since it is only applied to lower-resolution outputs, quality may improve from FAST). This mode is intended to be used by applications operating in a zero-shutter-lag mode with YUV or PRIVATE reprocessing, where the application continuously captures high-resolution intermediate buffers into a circular buffer, from which a final image is produced via reprocessing when a user takes a picture. For such a use case, the high-resolution buffers must not have edge enhancement applied to maximize efficiency of preview and to avoid double-applying enhancement when reprocessed, while low-resolution buffers (used for recording or preview, generally) need edge enhancement applied for reasonable preview quality. This mode is guaranteed to be supported by devices that support either the YUV_REPROCESSING or PRIVATE_REPROCESSING capabilities (android.request.availableCapabilities lists either of those capabilities) and it will be the default mode for CAMERA3_TEMPLATE_ZERO_SHUTTER_LAG template. | Operation mode for edge enhancement. |  | android.edge.availableEdgeModes | 3.2 | V1 REPROC
Details
Edge enhancement improves sharpness and details in the captured image. OFF means no enhancement will be applied by the camera device. FAST/HIGH_QUALITY both mean camera device determined enhancement will be applied. HIGH_QUALITY mode indicates that the camera device will use the highest-quality enhancement algorithms, even if it slows down capture rate. FAST means the camera device will not slow down capture rate when applying edge enhancement. FAST may be the same as OFF if edge enhancement will slow down capture rate. Every output stream will have a similar amount of enhancement applied. ZERO_SHUTTER_LAG is meant to be used by applications that maintain a continuous circular buffer of high-resolution images during preview and reprocess image(s) from that buffer into a final capture when triggered by the user. In this mode, the camera device applies edge enhancement to low-resolution streams (below maximum recording resolution) to maximize preview quality, but does not apply edge enhancement to high-resolution streams, since those will be reprocessed later if necessary. For YUV_REPROCESSING, these FAST/HIGH_QUALITY modes both mean that the camera device will apply FAST/HIGH_QUALITY YUV-domain edge enhancement, respectively. The camera device may adjust its internal edge enhancement parameters for best image quality based on the android.reprocess.effectiveExposureFactor, if it is set.
HAL Implementation Details
For YUV_REPROCESSING The HAL can use android.reprocess.effectiveExposureFactor to adjust the internal edge enhancement reduction parameters appropriately to get the best quality images.
android.edge.strength | byte [system] | Control the amount of edge enhancement applied to the images | 1-10; 10 is maximum sharpening |  | 3.2 | FUTURE
static
Property Name | Type | Description | Units | Range | Initial HIDL HAL version | Tags
android.edge.availableEdgeModes | byte x n [public as enumList] [full] list of enums | List of edge enhancement modes for android.edge.mode that are supported by this camera device. |  | Any value listed in android.edge.mode | 3.2 | V1 REPROC
Details
Full-capability camera devices must always support OFF; camera devices that support YUV_REPROCESSING or PRIVATE_REPROCESSING will list ZERO_SHUTTER_LAG; all devices will list FAST.
HAL Implementation Details
HAL must support both FAST and HIGH_QUALITY if edge enhancement control is available on the camera device, but the underlying implementation can be the same for both modes. That is, if the highest quality implementation on the camera device does not slow down capture rate, then FAST and HIGH_QUALITY will generate the same output.
dynamic
Property Name | Type | Description | Units | Range | Initial HIDL HAL version | Tags
android.edge.mode | byte [public] [full] OFF (v3.2) No edge enhancement is applied. FAST (v3.2) Apply edge enhancement at a quality level that does not slow down frame rate relative to sensor output. It may be the same as OFF if edge enhancement will slow down frame rate relative to sensor. HIGH_QUALITY (v3.2) Apply high-quality edge enhancement, at a cost of possibly reduced output frame rate. ZERO_SHUTTER_LAG (v3.2) [optional] Edge enhancement is applied at different levels for different output streams, based on resolution. Streams at maximum recording resolution (see CameraDevice#createCaptureSession) or below have edge enhancement applied, while higher-resolution streams have no edge enhancement applied. The level of edge enhancement for low-resolution streams is tuned so that frame rate is not impacted, and the quality is equal to or better than FAST (since it is only applied to lower-resolution outputs, quality may improve from FAST). This mode is intended to be used by applications operating in a zero-shutter-lag mode with YUV or PRIVATE reprocessing, where the application continuously captures high-resolution intermediate buffers into a circular buffer, from which a final image is produced via reprocessing when a user takes a picture. For such a use case, the high-resolution buffers must not have edge enhancement applied to maximize efficiency of preview and to avoid double-applying enhancement when reprocessed, while low-resolution buffers (used for recording or preview, generally) need edge enhancement applied for reasonable preview quality. This mode is guaranteed to be supported by devices that support either the YUV_REPROCESSING or PRIVATE_REPROCESSING capabilities (android.request.availableCapabilities lists either of those capabilities) and it will be the default mode for CAMERA3_TEMPLATE_ZERO_SHUTTER_LAG template. | Operation mode for edge enhancement. |  | android.edge.availableEdgeModes | 3.2 | V1 REPROC
Details
Edge enhancement improves sharpness and details in the captured image. OFF means no enhancement will be applied by the camera device. FAST/HIGH_QUALITY both mean camera device determined enhancement will be applied. HIGH_QUALITY mode indicates that the camera device will use the highest-quality enhancement algorithms, even if it slows down capture rate. FAST means the camera device will not slow down capture rate when applying edge enhancement. FAST may be the same as OFF if edge enhancement will slow down capture rate. Every output stream will have a similar amount of enhancement applied. ZERO_SHUTTER_LAG is meant to be used by applications that maintain a continuous circular buffer of high-resolution images during preview and reprocess image(s) from that buffer into a final capture when triggered by the user. In this mode, the camera device applies edge enhancement to low-resolution streams (below maximum recording resolution) to maximize preview quality, but does not apply edge enhancement to high-resolution streams, since those will be reprocessed later if necessary. For YUV_REPROCESSING, these FAST/HIGH_QUALITY modes both mean that the camera device will apply FAST/HIGH_QUALITY YUV-domain edge enhancement, respectively. The camera device may adjust its internal edge enhancement parameters for best image quality based on the android.reprocess.effectiveExposureFactor, if it is set.
HAL Implementation Details
For YUV_REPROCESSING The HAL can use android.reprocess.effectiveExposureFactor to adjust the internal edge enhancement reduction parameters appropriately to get the best quality images.
flash
controls
Property Name | Type | Description | Units | Range | Initial HIDL HAL version | Tags
android.flash.firingPower | byte [system] | Power for flash firing/torch | 10 is max power; 0 is no flash. Linear | 0 - 10 | 3.2 | FUTURE
Details
Power for snapshot may use a different scale than for torch mode. Only one entry for torch mode will be used
android.flash.firingTime | int64 [system] | Firing time of flash relative to start of exposure | nanoseconds | 0-(exposure time-flash duration) | 3.2 | FUTURE
Details
Clamped to (0, exposure time - flash duration).
android.flash.mode | byte [public] [legacy] OFF (v3.2) Do not fire the flash for this capture. SINGLE (v3.2) If the flash is available and charged, fire flash for this capture. TORCH (v3.2) Transition flash to continuously on. | The desired mode for for the camera device's flash control. |  |  | 3.2 | BC
Details
This control is only effective when flash unit is available (`android.flash.info.available == true`). When this control is used, the android.control.aeMode must be set to ON or OFF. Otherwise, the camera device auto-exposure related flash control (ON_AUTO_FLASH, ON_ALWAYS_FLASH, or ON_AUTO_FLASH_REDEYE) will override this control. When set to OFF, the camera device will not fire flash for this capture. When set to SINGLE, the camera device will fire flash regardless of the camera device's auto-exposure routine's result. When used in still capture case, this control should be used along with auto-exposure (AE) precapture metering sequence (android.control.aePrecaptureTrigger), otherwise, the image may be incorrectly exposed. When set to TORCH, the flash will be on continuously. This mode can be used for use cases such as preview, auto-focus assist, still capture, or video recording. The flash status will be reported by android.flash.state in the capture result metadata.
static
Property Name | Type | Description | Units | Range | Initial HIDL HAL version | Tags
android.flash.info.available | byte [public as boolean] [legacy] FALSE (v3.2) TRUE (v3.2) | Whether this camera device has a flash unit. |  |  | 3.2 | BC
Details
Will be `false` if no flash is available. If there is no flash unit, none of the flash controls do anything.
android.flash.info.chargeDuration | int64 [system] | Time taken before flash can fire again | nanoseconds | 0-1e9 | 3.2 | FUTURE
Details
1 second too long/too short for recharge? Should this be power-dependent?
android.flash.colorTemperature | byte [system] | The x,y whitepoint of the flash | pair of floats | 0-1 for both | 3.2 | FUTURE
android.flash.maxEnergy | byte [system] | Max energy output of the flash for a full power single flash | lumen-seconds | >= 0 | 3.2 | FUTURE
dynamic
Property Name | Type | Description | Units | Range | Initial HIDL HAL version | Tags
android.flash.firingPower | byte [system] | Power for flash firing/torch | 10 is max power; 0 is no flash. Linear | 0 - 10 | 3.2 | FUTURE
Details
Power for snapshot may use a different scale than for torch mode. Only one entry for torch mode will be used
android.flash.firingTime | int64 [system] | Firing time of flash relative to start of exposure | nanoseconds | 0-(exposure time-flash duration) | 3.2 | FUTURE
Details
Clamped to (0, exposure time - flash duration).
android.flash.mode | byte [public] [legacy] OFF (v3.2) Do not fire the flash for this capture. SINGLE (v3.2) If the flash is available and charged, fire flash for this capture. TORCH (v3.2) Transition flash to continuously on. | The desired mode for for the camera device's flash control. |  |  | 3.2 | BC
Details
This control is only effective when flash unit is available (`android.flash.info.available == true`). When this control is used, the android.control.aeMode must be set to ON or OFF. Otherwise, the camera device auto-exposure related flash control (ON_AUTO_FLASH, ON_ALWAYS_FLASH, or ON_AUTO_FLASH_REDEYE) will override this control. When set to OFF, the camera device will not fire flash for this capture. When set to SINGLE, the camera device will fire flash regardless of the camera device's auto-exposure routine's result. When used in still capture case, this control should be used along with auto-exposure (AE) precapture metering sequence (android.control.aePrecaptureTrigger), otherwise, the image may be incorrectly exposed. When set to TORCH, the flash will be on continuously. This mode can be used for use cases such as preview, auto-focus assist, still capture, or video recording. The flash status will be reported by android.flash.state in the capture result metadata.
android.flash.state | byte [public] [limited] UNAVAILABLE (v3.2) No flash on camera. CHARGING (v3.2) Flash is charging and cannot be fired. READY (v3.2) Flash is ready to fire. FIRED (v3.2) Flash fired for this capture. PARTIAL (v3.2) Flash partially illuminated this frame. This is usually due to the next or previous frame having the flash fire, and the flash spilling into this capture due to hardware limitations. | Current state of the flash unit. |  |  | 3.2 |
Details
When the camera device doesn't have flash unit (i.e. `android.flash.info.available == false`), this state will always be UNAVAILABLE. Other states indicate the current flash status. In certain conditions, this will be available on LEGACY devices: Flash-less cameras always return UNAVAILABLE. Using android.control.aeMode `==` ON_ALWAYS_FLASH will always return FIRED. Using android.flash.mode `==` TORCH will always return FIRED. In all other conditions the state will not be available on LEGACY devices (i.e. it will be `null`).
hotPixel
controls
Property Name | Type | Description | Units | Range | Initial HIDL HAL version | Tags
android.hotPixel.mode | byte [public] OFF (v3.2) No hot pixel correction is applied. The frame rate must not be reduced relative to sensor raw output for this option. The hotpixel map may be returned in android.statistics.hotPixelMap. FAST (v3.2) Hot pixel correction is applied, without reducing frame rate relative to sensor raw output. The hotpixel map may be returned in android.statistics.hotPixelMap. HIGH_QUALITY (v3.2) High-quality hot pixel correction is applied, at a cost of possibly reduced frame rate relative to sensor raw output. The hotpixel map may be returned in android.statistics.hotPixelMap. | Operational mode for hot pixel correction. |  | android.hotPixel.availableHotPixelModes | 3.2 | V1 RAW
Details
Hotpixel correction interpolates out, or otherwise removes, pixels that do not accurately measure the incoming light (i.e. pixels that are stuck at an arbitrary value or are oversensitive).
static
Property Name | Type | Description | Units | Range | Initial HIDL HAL version | Tags
android.hotPixel.availableHotPixelModes | byte x n [public as enumList] list of enums | List of hot pixel correction modes for android.hotPixel.mode that are supported by this camera device. |  | Any value listed in android.hotPixel.mode | 3.2 | V1 RAW
Details
FULL mode camera devices will always support FAST.
HAL Implementation Details
To avoid performance issues, there will be significantly fewer hot pixels than actual pixels on the camera sensor. HAL must support both FAST and HIGH_QUALITY if hot pixel correction control is available on the camera device, but the underlying implementation can be the same for both modes. That is, if the highest quality implementation on the camera device does not slow down capture rate, then FAST and HIGH_QUALITY will generate the same output.
dynamic
Property Name | Type | Description | Units | Range | Initial HIDL HAL version | Tags
android.hotPixel.mode | byte [public] OFF (v3.2) No hot pixel correction is applied. The frame rate must not be reduced relative to sensor raw output for this option. The hotpixel map may be returned in android.statistics.hotPixelMap. FAST (v3.2) Hot pixel correction is applied, without reducing frame rate relative to sensor raw output. The hotpixel map may be returned in android.statistics.hotPixelMap. HIGH_QUALITY (v3.2) High-quality hot pixel correction is applied, at a cost of possibly reduced frame rate relative to sensor raw output. The hotpixel map may be returned in android.statistics.hotPixelMap. | Operational mode for hot pixel correction. |  | android.hotPixel.availableHotPixelModes | 3.2 | V1 RAW
Details
Hotpixel correction interpolates out, or otherwise removes, pixels that do not accurately measure the incoming light (i.e. pixels that are stuck at an arbitrary value or are oversensitive).
jpeg
controls
Property Name | Type | Description | Units | Range | Initial HIDL HAL version | Tags
android.jpeg.gpsLocation | byte [java_public as location] [synthetic] [legacy] | A location object to use when generating image GPS metadata. |  |  | 3.2 |
Details
Setting a location object in a request will include the GPS coordinates of the location into any JPEG images captured based on the request. These coordinates can then be viewed by anyone who receives the JPEG image. This tag is also used for HEIC image capture.
android.jpeg.gpsCoordinates | double x 3 [ndk_public] [legacy] latitude, longitude, altitude. First two in degrees, the third in meters | GPS coordinates to include in output JPEG EXIF. |  | (-180 - 180], [-90,90], [-inf, inf] | 3.2 | BC
Details
This tag is also used for HEIC image capture.
android.jpeg.gpsProcessingMethod | byte [ndk_public as string] [legacy] | 32 characters describing GPS algorithm to include in EXIF. | UTF-8 null-terminated string |  | 3.2 | BC
Details
This tag is also used for HEIC image capture.
android.jpeg.gpsTimestamp | int64 [ndk_public] [legacy] | Time GPS fix was made to include in EXIF. | UTC in seconds since January 1, 1970 |  | 3.2 | BC
Details
This tag is also used for HEIC image capture.
android.jpeg.orientation | int32 [public] [legacy] | The orientation for a JPEG image. | Degrees in multiples of 90 | 0, 90, 180, 270 | 3.2 | BC
Details
The clockwise rotation angle in degrees, relative to the orientation to the camera, that the JPEG picture needs to be rotated by, to be viewed upright. Camera devices may either encode this value into the JPEG EXIF header, or rotate the image data to match this orientation. When the image data is rotated, the thumbnail data will also be rotated. Note that this orientation is relative to the orientation of the camera sensor, given by android.sensor.orientation. To translate from the device orientation given by the Android sensor APIs for camera sensors which are not EXTERNAL, the following sample code may be used:
    private int getJpegOrientation(CameraCharacteristics c, int deviceOrientation) {
        if (deviceOrientation == android.view.OrientationEventListener.ORIENTATION_UNKNOWN) return 0;
        int sensorOrientation = c.get(CameraCharacteristics.SENSOR_ORIENTATION);

        // Round device orientation to a multiple of 90
        deviceOrientation = (deviceOrientation + 45) / 90 * 90;

        // Reverse device orientation for front-facing cameras
        boolean facingFront = c.get(CameraCharacteristics.LENS_FACING) == CameraCharacteristics.LENS_FACING_FRONT;
        if (facingFront) deviceOrientation = -deviceOrientation;

        // Calculate desired JPEG orientation relative to camera orientation to make
        // the image upright relative to the device orientation
        int jpegOrientation = (sensorOrientation + deviceOrientation + 360) % 360;

        return jpegOrientation;
    }
For EXTERNAL cameras the sensor orientation will always be set to 0 and the facing will also be set to EXTERNAL. The above code is not relevant in such case. This tag is also used to describe the orientation of the HEIC image capture, in which case the rotation is reflected by EXIF orientation flag, and not by rotating the image data itself.
android.jpeg.quality | byte [public] [legacy] | Compression quality of the final JPEG image. |  | 1-100; larger is higher quality | 3.2 | BC
Details
85-95 is typical usage range. This tag is also used to describe the quality of the HEIC image capture.
android.jpeg.thumbnailQuality | byte [public] [legacy] | Compression quality of JPEG thumbnail. |  | 1-100; larger is higher quality | 3.2 | BC
Details
This tag is also used to describe the quality of the HEIC image capture.
android.jpeg.thumbnailSize | int32 x 2 [public as size] [legacy] | Resolution of embedded JPEG thumbnail. |  | android.jpeg.availableThumbnailSizes | 3.2 | BC
Details
When set to (0, 0) value, the JPEG EXIF will not contain thumbnail, but the captured JPEG will still be a valid image. For best results, when issuing a request for a JPEG image, the thumbnail size selected should have the same aspect ratio as the main JPEG output. If the thumbnail image aspect ratio differs from the JPEG primary image aspect ratio, the camera device creates the thumbnail by cropping it from the primary image. For example, if the primary image has 4:3 aspect ratio, the thumbnail image has 16:9 aspect ratio, the primary image will be cropped vertically (letterbox) to generate the thumbnail image. The thumbnail image will always have a smaller Field Of View (FOV) than the primary image when aspect ratios differ. When an android.jpeg.orientation of non-zero degree is requested, the camera device will handle thumbnail rotation in one of the following ways: Set the EXIF orientation flag and keep jpeg and thumbnail image data unrotated. Rotate the jpeg and thumbnail image data and not set EXIF orientation flag. In this case, LIMITED or FULL hardware level devices will report rotated thumnail size in capture result, so the width and height will be interchanged if 90 or 270 degree orientation is requested. LEGACY device will always report unrotated thumbnail size. The tag is also used as thumbnail size for HEIC image format capture, in which case the the thumbnail rotation is reflected by EXIF orientation flag, and not by rotating the thumbnail data itself.
HAL Implementation Details
The HAL must not squeeze or stretch the downscaled primary image to generate thumbnail. The cropping must be done on the primary jpeg image rather than the sensor pre-correction active array. The stream cropping rule specified by "S5. Cropping" in camera3.h doesn't apply to the thumbnail image cropping.
static
Property Name | Type | Description | Units | Range | Initial HIDL HAL version | Tags
android.jpeg.availableThumbnailSizes | int32 x 2 x n [public as size] [legacy] | List of JPEG thumbnail sizes for android.jpeg.thumbnailSize supported by this camera device. |  |  | 3.2 | BC
Details
This list will include at least one non-zero resolution, plus `(0,0)` for indicating no thumbnail should be generated. Below condiditions will be satisfied for this size list: The sizes will be sorted by increasing pixel area (width x height). If several resolutions have the same area, they will be sorted by increasing width. The aspect ratio of the largest thumbnail size will be same as the aspect ratio of largest JPEG output size in android.scaler.availableStreamConfigurations. The largest size is defined as the size that has the largest pixel area in a given size list. Each output JPEG size in android.scaler.availableStreamConfigurations will have at least one corresponding size that has the same aspect ratio in availableThumbnailSizes, and vice versa. All non-`(0, 0)` sizes will have non-zero widths and heights. This list is also used as supported thumbnail sizes for HEIC image format capture.
android.jpeg.maxSize | int32 [system] | Maximum size in bytes for the compressed JPEG buffer |  | Must be large enough to fit any JPEG produced by the camera | 3.2 |
Details
This is used for sizing the gralloc buffers for JPEG
dynamic
Property Name | Type | Description | Units | Range | Initial HIDL HAL version | Tags
android.jpeg.gpsLocation | byte [java_public as location] [synthetic] [legacy] | A location object to use when generating image GPS metadata. |  |  | 3.2 |
Details
Setting a location object in a request will include the GPS coordinates of the location into any JPEG images captured based on the request. These coordinates can then be viewed by anyone who receives the JPEG image. This tag is also used for HEIC image capture.
android.jpeg.gpsCoordinates | double x 3 [ndk_public] [legacy] latitude, longitude, altitude. First two in degrees, the third in meters | GPS coordinates to include in output JPEG EXIF. |  | (-180 - 180], [-90,90], [-inf, inf] | 3.2 | BC
Details
This tag is also used for HEIC image capture.
android.jpeg.gpsProcessingMethod | byte [ndk_public as string] [legacy] | 32 characters describing GPS algorithm to include in EXIF. | UTF-8 null-terminated string |  | 3.2 | BC
Details
This tag is also used for HEIC image capture.
android.jpeg.gpsTimestamp | int64 [ndk_public] [legacy] | Time GPS fix was made to include in EXIF. | UTC in seconds since January 1, 1970 |  | 3.2 | BC
Details
This tag is also used for HEIC image capture.
android.jpeg.orientation | int32 [public] [legacy] | The orientation for a JPEG image. | Degrees in multiples of 90 | 0, 90, 180, 270 | 3.2 | BC
Details
The clockwise rotation angle in degrees, relative to the orientation to the camera, that the JPEG picture needs to be rotated by, to be viewed upright. Camera devices may either encode this value into the JPEG EXIF header, or rotate the image data to match this orientation. When the image data is rotated, the thumbnail data will also be rotated. Note that this orientation is relative to the orientation of the camera sensor, given by android.sensor.orientation. To translate from the device orientation given by the Android sensor APIs for camera sensors which are not EXTERNAL, the following sample code may be used:
    private int getJpegOrientation(CameraCharacteristics c, int deviceOrientation) {
        if (deviceOrientation == android.view.OrientationEventListener.ORIENTATION_UNKNOWN) return 0;
        int sensorOrientation = c.get(CameraCharacteristics.SENSOR_ORIENTATION);

        // Round device orientation to a multiple of 90
        deviceOrientation = (deviceOrientation + 45) / 90 * 90;

        // Reverse device orientation for front-facing cameras
        boolean facingFront = c.get(CameraCharacteristics.LENS_FACING) == CameraCharacteristics.LENS_FACING_FRONT;
        if (facingFront) deviceOrientation = -deviceOrientation;

        // Calculate desired JPEG orientation relative to camera orientation to make
        // the image upright relative to the device orientation
        int jpegOrientation = (sensorOrientation + deviceOrientation + 360) % 360;

        return jpegOrientation;
    }
For EXTERNAL cameras the sensor orientation will always be set to 0 and the facing will also be set to EXTERNAL. The above code is not relevant in such case. This tag is also used to describe the orientation of the HEIC image capture, in which case the rotation is reflected by EXIF orientation flag, and not by rotating the image data itself.
android.jpeg.quality | byte [public] [legacy] | Compression quality of the final JPEG image. |  | 1-100; larger is higher quality | 3.2 | BC
Details
85-95 is typical usage range. This tag is also used to describe the quality of the HEIC image capture.
android.jpeg.size | int32 [system] | The size of the compressed JPEG image, in bytes |  | >= 0 | 3.2 | FUTURE
Details
If no JPEG output is produced for the request, this must be 0. Otherwise, this describes the real size of the compressed JPEG image placed in the output stream. More specifically, if android.jpeg.maxSize = 1000000, and a specific capture has android.jpeg.size = 500000, then the output buffer from the JPEG stream will be 1000000 bytes, of which the first 500000 make up the real data.
android.jpeg.thumbnailQuality | byte [public] [legacy] | Compression quality of JPEG thumbnail. |  | 1-100; larger is higher quality | 3.2 | BC
Details
This tag is also used to describe the quality of the HEIC image capture.
android.jpeg.thumbnailSize | int32 x 2 [public as size] [legacy] | Resolution of embedded JPEG thumbnail. |  | android.jpeg.availableThumbnailSizes | 3.2 | BC
Details
When set to (0, 0) value, the JPEG EXIF will not contain thumbnail, but the captured JPEG will still be a valid image. For best results, when issuing a request for a JPEG image, the thumbnail size selected should have the same aspect ratio as the main JPEG output. If the thumbnail image aspect ratio differs from the JPEG primary image aspect ratio, the camera device creates the thumbnail by cropping it from the primary image. For example, if the primary image has 4:3 aspect ratio, the thumbnail image has 16:9 aspect ratio, the primary image will be cropped vertically (letterbox) to generate the thumbnail image. The thumbnail image will always have a smaller Field Of View (FOV) than the primary image when aspect ratios differ. When an android.jpeg.orientation of non-zero degree is requested, the camera device will handle thumbnail rotation in one of the following ways: Set the EXIF orientation flag and keep jpeg and thumbnail image data unrotated. Rotate the jpeg and thumbnail image data and not set EXIF orientation flag. In this case, LIMITED or FULL hardware level devices will report rotated thumnail size in capture result, so the width and height will be interchanged if 90 or 270 degree orientation is requested. LEGACY device will always report unrotated thumbnail size. The tag is also used as thumbnail size for HEIC image format capture, in which case the the thumbnail rotation is reflected by EXIF orientation flag, and not by rotating the thumbnail data itself.
HAL Implementation Details
The HAL must not squeeze or stretch the downscaled primary image to generate thumbnail. The cropping must be done on the primary jpeg image rather than the sensor pre-correction active array. The stream cropping rule specified by "S5. Cropping" in camera3.h doesn't apply to the thumbnail image cropping.
lens
controls
Property Name | Type | Description | Units | Range | Initial HIDL HAL version | Tags
android.lens.aperture | float [public] [full] | The desired lens aperture size, as a ratio of lens focal length to the effective aperture diameter. | The f-number (f/N) | android.lens.info.availableApertures | 3.2 | V1
Details
Setting this value is only supported on the camera devices that have a variable aperture lens. When this is supported and android.control.aeMode is OFF, this can be set along with android.sensor.exposureTime, android.sensor.sensitivity, and android.sensor.frameDuration to achieve manual exposure control. The requested aperture value may take several frames to reach the requested value; the camera device will report the current (intermediate) aperture size in capture result metadata while the aperture is changing. While the aperture is still changing, android.lens.state will be set to MOVING. When this is supported and android.control.aeMode is one of the ON modes, this will be overridden by the camera device auto-exposure algorithm, the overridden values are then provided back to the user in the corresponding result.
android.lens.filterDensity | float [public] [full] | The desired setting for the lens neutral density filter(s). | Exposure Value (EV) | android.lens.info.availableFilterDensities | 3.2 | V1
Details
This control will not be supported on most camera devices. Lens filters are typically used to lower the amount of light the sensor is exposed to (measured in steps of EV). As used here, an EV step is the standard logarithmic representation, which are non-negative, and inversely proportional to the amount of light hitting the sensor. For example, setting this to 0 would result in no reduction of the incoming light, and setting this to 2 would mean that the filter is set to reduce incoming light by two stops (allowing 1/4 of the prior amount of light to the sensor). It may take several frames before the lens filter density changes to the requested value. While the filter density is still changing, android.lens.state will be set to MOVING.
android.lens.focalLength | float [public] [legacy] | The desired lens focal length; used for optical zoom. | Millimeters | android.lens.info.availableFocalLengths | 3.2 | V1
Details
This setting controls the physical focal length of the camera device's lens. Changing the focal length changes the field of view of the camera device, and is usually used for optical zoom. Like android.lens.focusDistance and android.lens.aperture, this setting won't be applied instantaneously, and it may take several frames before the lens can change to the requested focal length. While the focal length is still changing, android.lens.state will be set to MOVING. Optical zoom via this control will not be supported on most devices. Starting from API level 30, the camera device may combine optical and digital zoom through the android.control.zoomRatio control.
HAL Implementation Details
For a logical camera device supporting both optical and digital zoom, if focalLength and cropRegion change in the same request, the camera device must make sure that the new focalLength and cropRegion take effect in the same frame. This is to make sure that there is no visible field-of-view jump during zoom. For example, if cropRegion is applied immediately, but focalLength takes more than 1 frame to take effect, the camera device will delay the cropRegion so that it's synchronized with focalLength. Starting from API level 30, it's strongly recommended for HAL to implement the combination of optical and digital zoom using the new android.control.zoomRatio API, in lieu of using android.lens.focalLength and android.scaler.cropRegion.
android.lens.focusDistance | float [public] [full] | Desired distance to plane of sharpest focus, measured from frontmost surface of the lens. | See android.lens.info.focusDistanceCalibration for details | >= 0 | 3.2 | BC V1
Details
This control can be used for setting manual focus, on devices that support the MANUAL_SENSOR capability and have a variable-focus lens (see android.lens.info.minimumFocusDistance). A value of `0.0f` means infinity focus. The value set will be clamped to `[0.0f, android.lens.info.minimumFocusDistance]`. Like android.lens.focalLength, this setting won't be applied instantaneously, and it may take several frames before the lens can move to the requested focus distance. While the lens is still moving, android.lens.state will be set to MOVING. LEGACY devices support at most setting this to `0.0f` for infinity focus.
android.lens.opticalStabilizationMode | byte [public] [limited] OFF (v3.2) Optical stabilization is unavailable. ON (v3.2) [optional] Optical stabilization is enabled. | Sets whether the camera device uses optical image stabilization (OIS) when capturing images. |  | android.lens.info.availableOpticalStabilization | 3.2 | V1
Details
OIS is used to compensate for motion blur due to small movements of the camera during capture. Unlike digital image stabilization (android.control.videoStabilizationMode), OIS makes use of mechanical elements to stabilize the camera sensor, and thus allows for longer exposure times before camera shake becomes apparent. Switching between different optical stabilization modes may take several frames to initialize, the camera device will report the current mode in capture result metadata. For example, When "ON" mode is requested, the optical stabilization modes in the first several capture results may still be "OFF", and it will become "ON" when the initialization is done. If a camera device supports both OIS and digital image stabilization (android.control.videoStabilizationMode), turning both modes on may produce undesirable interaction, so it is recommended not to enable both at the same time. Not all devices will support OIS; see android.lens.info.availableOpticalStabilization for available controls.
static
Property Name | Type | Description | Units | Range | Initial HIDL HAL version | Tags
android.lens.info.availableApertures | float x n [public] [full] | List of aperture size values for android.lens.aperture that are supported by this camera device. | The aperture f-number |  | 3.2 | V1
Details
If the camera device doesn't support a variable lens aperture, this list will contain only one value, which is the fixed aperture size. If the camera device supports a variable aperture, the aperture values in this list will be sorted in ascending order.
android.lens.info.availableFilterDensities | float x n [public] [full] | List of neutral density filter values for android.lens.filterDensity that are supported by this camera device. | Exposure value (EV) | Values are >= 0 | 3.2 | V1
Details
If a neutral density filter is not supported by this camera device, this list will contain only 0. Otherwise, this list will include every filter density supported by the camera device, in ascending order.
android.lens.info.availableFocalLengths | float x n [public] [legacy] The list of available focal lengths | List of focal lengths for android.lens.focalLength that are supported by this camera device. | Millimeters | Values are > 0 | 3.2 | BC V1
Details
If optical zoom is not supported, this list will only contain a single value corresponding to the fixed focal length of the device. Otherwise, this list will include every focal length supported by the camera device, in ascending order.
android.lens.info.availableOpticalStabilization | byte x n [public as enumList] [limited] list of enums | List of optical image stabilization (OIS) modes for android.lens.opticalStabilizationMode that are supported by this camera device. |  | Any value listed in android.lens.opticalStabilizationMode | 3.2 | V1
Details
If OIS is not supported by a given camera device, this list will contain only OFF.
android.lens.info.hyperfocalDistance | float [public] [limited] | Hyperfocal distance for this lens. | See android.lens.info.focusDistanceCalibration for details | If lens is fixed focus, >= 0. If lens has focuser unit, the value is within `(0.0f, android.lens.info.minimumFocusDistance]` | 3.2 |
Details
If the lens is not fixed focus, the camera device will report this field when android.lens.info.focusDistanceCalibration is APPROXIMATE or CALIBRATED.
android.lens.info.minimumFocusDistance | float [public] [limited] | Shortest distance from frontmost surface of the lens that can be brought into sharp focus. | See android.lens.info.focusDistanceCalibration for details | >= 0 | 3.2 | V1
Details
If the lens is fixed-focus, this will be 0.
HAL Implementation Details
Mandatory for FULL devices; LIMITED devices must always set this value to 0 for fixed-focus; and may omit the minimum focus distance otherwise. This field is also mandatory for all devices advertising the MANUAL_SENSOR capability.
android.lens.info.shadingMapSize | int32 x 2 [ndk_public as size] [full] width and height (N, M) of lens shading map provided by the camera device. | Dimensions of lens shading map. |  | Both values >= 1 | 3.2 | V1
Details
The map should be on the order of 30-40 rows and columns, and must be smaller than 64x64.
android.lens.info.focusDistanceCalibration | byte [public] [limited] UNCALIBRATED (v3.2) The lens focus distance is not accurate, and the units used for android.lens.focusDistance do not correspond to any physical units. Setting the lens to the same focus distance on separate occasions may result in a different real focus distance, depending on factors such as the orientation of the device, the age of the focusing mechanism, and the device temperature. The focus distance value will still be in the range of `[0, android.lens.info.minimumFocusDistance]`, where 0 represents the farthest focus. APPROXIMATE (v3.2) The lens focus distance is measured in diopters. However, setting the lens to the same focus distance on separate occasions may result in a different real focus distance, depending on factors such as the orientation of the device, the age of the focusing mechanism, and the device temperature. CALIBRATED (v3.2) The lens focus distance is measured in diopters, and is calibrated. The lens mechanism is calibrated so that setting the same focus distance is repeatable on multiple occasions with good accuracy, and the focus distance corresponds to the real physical distance to the plane of best focus. | The lens focus distance calibration quality. |  |  | 3.2 | V1
Details
The lens focus distance calibration quality determines the reliability of focus related metadata entries, i.e. android.lens.focusDistance, android.lens.focusRange, android.lens.info.hyperfocalDistance, and android.lens.info.minimumFocusDistance. APPROXIMATE and CALIBRATED devices report the focus metadata in units of diopters (1/meter), so `0.0f` represents focusing at infinity, and increasing positive numbers represent focusing closer and closer to the camera device. The focus distance control also uses diopters on these devices. UNCALIBRATED devices do not use units that are directly comparable to any real physical measurement, but `0.0f` still represents farthest focus, and android.lens.info.minimumFocusDistance represents the nearest focus the device can achieve.
HAL Implementation Details
For devices advertise APPROXIMATE quality or higher, diopters 0 (infinity focus) must work. When autofocus is disabled (android.control.afMode == OFF) and the lens focus distance is set to 0 diopters (android.lens.focusDistance == 0), the lens will move to focus at infinity and is stably focused at infinity even if the device tilts. It may take the lens some time to move; during the move the lens state should be MOVING and the output diopter value should be changing toward 0.
android.lens.facing | byte [public] [legacy] FRONT (v3.2) The camera device faces the same direction as the device's screen. BACK (v3.2) The camera device faces the opposite direction as the device's screen. EXTERNAL (v3.2) The camera device is an external camera, and has no fixed facing relative to the device's screen. | Direction the camera faces relative to device screen. |  |  | 3.2 |
android.lens.poseRotation | float x 4 [public] | The orientation of the camera relative to the sensor coordinate system. | Quaternion coefficients |  | 3.2 | DEPTH
Details
The four coefficients that describe the quaternion rotation from the Android sensor coordinate system to a camera-aligned coordinate system where the X-axis is aligned with the long side of the image sensor, the Y-axis is aligned with the short side of the image sensor, and the Z-axis is aligned with the optical axis of the sensor. To convert from the quaternion coefficients `(x,y,z,w)` to the axis of rotation `(a_x, a_y, a_z)` and rotation amount `theta`, the following formulas can be used:
     theta = 2 * acos(w)
    a_x = x / sin(theta/2)
    a_y = y / sin(theta/2)
    a_z = z / sin(theta/2)
To create a 3x3 rotation matrix that applies the rotation defined by this quaternion, the following matrix can be used:
    R = [ 1 - 2y^2 - 2z^2,       2xy - 2zw,       2xz + 2yw,
               2xy + 2zw, 1 - 2x^2 - 2z^2,       2yz - 2xw,
               2xz - 2yw,       2yz + 2xw, 1 - 2x^2 - 2y^2 ]
This matrix can then be used to apply the rotation to a column vector point with `p' = Rp` where `p` is in the device sensor coordinate system, and `p'` is in the camera-oriented coordinate system. If android.lens.poseReference is UNDEFINED, the quaternion rotation cannot be accurately represented by the camera device, and will be represented by default values matching its default facing.
android.lens.poseTranslation | float x 3 [public] | Position of the camera optical center. | Meters |  | 3.2 | DEPTH
Details
The position of the camera device's lens optical center, as a three-dimensional vector `(x,y,z)`. Prior to Android P, or when android.lens.poseReference is PRIMARY_CAMERA, this position is relative to the optical center of the largest camera device facing in the same direction as this camera, in the Android sensor coordinate axes. Note that only the axis definitions are shared with the sensor coordinate system, but not the origin. If this device is the largest or only camera device with a given facing, then this position will be `(0, 0, 0)`; a camera device with a lens optical center located 3 cm from the main sensor along the +X axis (to the right from the user's perspective) will report `(0.03, 0, 0)`. Note that this means that, for many computer vision applications, the position needs to be negated to convert it to a translation from the camera to the origin. To transform a pixel coordinates between two cameras facing the same direction, first the source camera android.lens.distortion must be corrected for. Then the source camera android.lens.intrinsicCalibration needs to be applied, followed by the android.lens.poseRotation of the source camera, the translation of the source camera relative to the destination camera, the android.lens.poseRotation of the destination camera, and finally the inverse of android.lens.intrinsicCalibration of the destination camera. This obtains a radial-distortion-free coordinate in the destination camera pixel coordinates. To compare this against a real image from the destination camera, the destination camera image then needs to be corrected for radial distortion before comparison or sampling. When android.lens.poseReference is GYROSCOPE, then this position is relative to the center of the primary gyroscope on the device. The axis definitions are the same as with PRIMARY_CAMERA. When android.lens.poseReference is UNDEFINED, this position cannot be accurately represented by the camera device, and will be represented as `(0, 0, 0)`.
android.lens.intrinsicCalibration | float x 5 [public] | The parameters for this camera device's intrinsic calibration. | Pixels in the android.sensor.info.preCorrectionActiveArraySize coordinate system. |  | 3.2 | DEPTH
Details
The five calibration parameters that describe the transform from camera-centric 3D coordinates to sensor pixel coordinates:
    [f_x, f_y, c_x, c_y, s]
Where `f_x` and `f_y` are the horizontal and vertical focal lengths, `[c_x, c_y]` is the position of the optical axis, and `s` is a skew parameter for the sensor plane not being aligned with the lens plane. These are typically used within a transformation matrix K:
    K = [ f_x,   s, c_x,
           0, f_y, c_y,
           0    0,   1 ]
which can then be combined with the camera pose rotation `R` and translation `t` (android.lens.poseRotation and android.lens.poseTranslation, respectively) to calculate the complete transform from world coordinates to pixel coordinates:
    P = [ K 0   * [ R -Rt
         0 1 ]      0 1 ]
(Note the negation of poseTranslation when mapping from camera to world coordinates, and multiplication by the rotation). With `p_w` being a point in the world coordinate system and `p_s` being a point in the camera active pixel array coordinate system, and with the mapping including the homogeneous division by z:
     p_h = (x_h, y_h, z_h) = P p_w
    p_s = p_h / z_h
so `[x_s, y_s]` is the pixel coordinates of the world point, `z_s = 1`, and `w_s` is a measurement of disparity (depth) in pixel coordinates. Note that the coordinate system for this transform is the android.sensor.info.preCorrectionActiveArraySize system, where `(0,0)` is the top-left of the preCorrectionActiveArraySize rectangle. Once the pose and intrinsic calibration transforms have been applied to a world point, then the android.lens.distortion transform needs to be applied, and the result adjusted to be in the android.sensor.info.activeArraySize coordinate system (where `(0, 0)` is the top-left of the activeArraySize rectangle), to determine the final pixel coordinate of the world point for processed (non-RAW) output buffers. For camera devices, the center of pixel `(x,y)` is located at coordinate `(x + 0.5, y + 0.5)`. So on a device with a precorrection active array of size `(10,10)`, the valid pixel indices go from `(0,0)-(9,9)`, and an perfectly-built camera would have an optical center at the exact center of the pixel grid, at coordinates `(5.0, 5.0)`, which is the top-left corner of pixel `(5,5)`.
android.lens.radialDistortion | float x 6 [public] [deprecated] | The correction coefficients to correct for this camera device's radial and tangential lens distortion. | Unitless coefficients. | Deprecated. Do not use. | 3.2 | DEPTH
Details
Four radial distortion coefficients `[kappa_0, kappa_1, kappa_2, kappa_3]` and two tangential distortion coefficients `[kappa_4, kappa_5]` that can be used to correct the lens's geometric distortion with the mapping equations:
     x_c = x_i * ( kappa_0 + kappa_1 * r^2 + kappa_2 * r^4 + kappa_3 * r^6 ) +
           kappa_4 * (2 * x_i * y_i) + kappa_5 * ( r^2 + 2 * x_i^2 )
     y_c = y_i * ( kappa_0 + kappa_1 * r^2 + kappa_2 * r^4 + kappa_3 * r^6 ) +
           kappa_5 * (2 * x_i * y_i) + kappa_4 * ( r^2 + 2 * y_i^2 )
Here, `[x_c, y_c]` are the coordinates to sample in the input image that correspond to the pixel values in the corrected image at the coordinate `[x_i, y_i]`:
     correctedImage(x_i, y_i) = sample_at(x_c, y_c, inputImage)
The pixel coordinates are defined in a normalized coordinate system related to the android.lens.intrinsicCalibration calibration fields. Both `[x_i, y_i]` and `[x_c, y_c]` have `(0,0)` at the lens optical center `[c_x, c_y]`. The maximum magnitudes of both x and y coordinates are normalized to be 1 at the edge further from the optical center, so the range for both dimensions is `-1 <= x <= 1`. Finally, `r` represents the radial distance from the optical center, `r^2 = x_i^2 + y_i^2`, and its magnitude is therefore no larger than `|r| <= sqrt(2)`. The distortion model used is the Brown-Conrady model.
android.lens.poseReference | byte [public] PRIMARY_CAMERA (v3.3) The value of android.lens.poseTranslation is relative to the optical center of the largest camera device facing the same direction as this camera. This is the default value for API levels before Android P. GYROSCOPE (v3.3) The value of android.lens.poseTranslation is relative to the position of the primary gyroscope of this Android device. UNDEFINED (v3.5) The camera device cannot represent the values of android.lens.poseTranslation and android.lens.poseRotation accurately enough. One such example is a camera device on the cover of a foldable phone: in order to measure the pose translation and rotation, some kind of hinge position sensor would be needed. The value of android.lens.poseTranslation must be all zeros, and android.lens.poseRotation must be values matching its default facing. | The origin for android.lens.poseTranslation, and the accuracy of android.lens.poseTranslation and android.lens.poseRotation. |  |  | 3.3 |
Details
Different calibration methods and use cases can produce better or worse results depending on the selected coordinate origin.
android.lens.distortion | float x 5 [public] | The correction coefficients to correct for this camera device's radial and tangential lens distortion. Replaces the deprecated android.lens.radialDistortion field, which was inconsistently defined. | Unitless coefficients. |  | 3.3 | DEPTH
Details
Three radial distortion coefficients `[kappa_1, kappa_2, kappa_3]` and two tangential distortion coefficients `[kappa_4, kappa_5]` that can be used to correct the lens's geometric distortion with the mapping equations:
     x_c = x_i * ( 1 + kappa_1 * r^2 + kappa_2 * r^4 + kappa_3 * r^6 ) +
           kappa_4 * (2 * x_i * y_i) + kappa_5 * ( r^2 + 2 * x_i^2 )
     y_c = y_i * ( 1 + kappa_1 * r^2 + kappa_2 * r^4 + kappa_3 * r^6 ) +
           kappa_5 * (2 * x_i * y_i) + kappa_4 * ( r^2 + 2 * y_i^2 )
Here, `[x_c, y_c]` are the coordinates to sample in the input image that correspond to the pixel values in the corrected image at the coordinate `[x_i, y_i]`:
     correctedImage(x_i, y_i) = sample_at(x_c, y_c, inputImage)
The pixel coordinates are defined in a coordinate system related to the android.lens.intrinsicCalibration calibration fields; see that entry for details of the mapping stages. Both `[x_i, y_i]` and `[x_c, y_c]` have `(0,0)` at the lens optical center `[c_x, c_y]`, and the range of the coordinates depends on the focal length terms of the intrinsic calibration. Finally, `r` represents the radial distance from the optical center, `r^2 = x_i^2 + y_i^2`. The distortion model used is the Brown-Conrady model.
dynamic
Property Name | Type | Description | Units | Range | Initial HIDL HAL version | Tags
android.lens.aperture | float [public] [full] | The desired lens aperture size, as a ratio of lens focal length to the effective aperture diameter. | The f-number (f/N) | android.lens.info.availableApertures | 3.2 | V1
Details
Setting this value is only supported on the camera devices that have a variable aperture lens. When this is supported and android.control.aeMode is OFF, this can be set along with android.sensor.exposureTime, android.sensor.sensitivity, and android.sensor.frameDuration to achieve manual exposure control. The requested aperture value may take several frames to reach the requested value; the camera device will report the current (intermediate) aperture size in capture result metadata while the aperture is changing. While the aperture is still changing, android.lens.state will be set to MOVING. When this is supported and android.control.aeMode is one of the ON modes, this will be overridden by the camera device auto-exposure algorithm, the overridden values are then provided back to the user in the corresponding result.
android.lens.filterDensity | float [public] [full] | The desired setting for the lens neutral density filter(s). | Exposure Value (EV) | android.lens.info.availableFilterDensities | 3.2 | V1
Details
This control will not be supported on most camera devices. Lens filters are typically used to lower the amount of light the sensor is exposed to (measured in steps of EV). As used here, an EV step is the standard logarithmic representation, which are non-negative, and inversely proportional to the amount of light hitting the sensor. For example, setting this to 0 would result in no reduction of the incoming light, and setting this to 2 would mean that the filter is set to reduce incoming light by two stops (allowing 1/4 of the prior amount of light to the sensor). It may take several frames before the lens filter density changes to the requested value. While the filter density is still changing, android.lens.state will be set to MOVING.
android.lens.focalLength | float [public] [legacy] | The desired lens focal length; used for optical zoom. | Millimeters | android.lens.info.availableFocalLengths | 3.2 | BC
Details
This setting controls the physical focal length of the camera device's lens. Changing the focal length changes the field of view of the camera device, and is usually used for optical zoom. Like android.lens.focusDistance and android.lens.aperture, this setting won't be applied instantaneously, and it may take several frames before the lens can change to the requested focal length. While the focal length is still changing, android.lens.state will be set to MOVING. Optical zoom via this control will not be supported on most devices. Starting from API level 30, the camera device may combine optical and digital zoom through the android.control.zoomRatio control.
HAL Implementation Details
For a logical camera device supporting both optical and digital zoom, if focalLength and cropRegion change in the same request, the camera device must make sure that the new focalLength and cropRegion take effect in the same frame. This is to make sure that there is no visible field-of-view jump during zoom. For example, if cropRegion is applied immediately, but focalLength takes more than 1 frame to take effect, the camera device will delay the cropRegion so that it's synchronized with focalLength. Starting from API level 30, it's strongly recommended for HAL to implement the combination of optical and digital zoom using the new android.control.zoomRatio API, in lieu of using android.lens.focalLength and android.scaler.cropRegion.
android.lens.focusDistance | float [public] [full] | Desired distance to plane of sharpest focus, measured from frontmost surface of the lens. | See android.lens.info.focusDistanceCalibration for details | >= 0 | 3.2 | BC
Details
Should be zero for fixed-focus cameras
android.lens.focusRange | float x 2 [public as pairFloatFloat] [limited] Range of scene distances that are in focus | The range of scene distances that are in sharp focus (depth of field). | A pair of focus distances in diopters: (near, far); see android.lens.info.focusDistanceCalibration for details. | >=0 | 3.2 | BC
Details
If variable focus not supported, can still report fixed depth of field range
android.lens.opticalStabilizationMode | byte [public] [limited] OFF (v3.2) Optical stabilization is unavailable. ON (v3.2) [optional] Optical stabilization is enabled. | Sets whether the camera device uses optical image stabilization (OIS) when capturing images. |  | android.lens.info.availableOpticalStabilization | 3.2 | V1
Details
OIS is used to compensate for motion blur due to small movements of the camera during capture. Unlike digital image stabilization (android.control.videoStabilizationMode), OIS makes use of mechanical elements to stabilize the camera sensor, and thus allows for longer exposure times before camera shake becomes apparent. Switching between different optical stabilization modes may take several frames to initialize, the camera device will report the current mode in capture result metadata. For example, When "ON" mode is requested, the optical stabilization modes in the first several capture results may still be "OFF", and it will become "ON" when the initialization is done. If a camera device supports both OIS and digital image stabilization (android.control.videoStabilizationMode), turning both modes on may produce undesirable interaction, so it is recommended not to enable both at the same time. Not all devices will support OIS; see android.lens.info.availableOpticalStabilization for available controls.
android.lens.state | byte [public] [limited] STATIONARY (v3.2) The lens parameters (android.lens.focalLength, android.lens.focusDistance, android.lens.filterDensity and android.lens.aperture) are not changing. MOVING (v3.2) One or several of the lens parameters (android.lens.focalLength, android.lens.focusDistance, android.lens.filterDensity or android.lens.aperture) is currently changing. | Current lens status. |  |  | 3.2 | V1
Details
For lens parameters android.lens.focalLength, android.lens.focusDistance, android.lens.filterDensity and android.lens.aperture, when changes are requested, they may take several frames to reach the requested values. This state indicates the current status of the lens parameters. When the state is STATIONARY, the lens parameters are not changing. This could be either because the parameters are all fixed, or because the lens has had enough time to reach the most recently-requested values. If all these lens parameters are not changable for a camera device, as listed below: Fixed focus (`android.lens.info.minimumFocusDistance == 0`), which means android.lens.focusDistance parameter will always be 0. Fixed focal length (android.lens.info.availableFocalLengths contains single value), which means the optical zoom is not supported. No ND filter (android.lens.info.availableFilterDensities contains only 0). Fixed aperture (android.lens.info.availableApertures contains single value). Then this state will always be STATIONARY. When the state is MOVING, it indicates that at least one of the lens parameters is changing.
android.lens.poseRotation | float x 4 [public] | The orientation of the camera relative to the sensor coordinate system. | Quaternion coefficients |  | 3.2 | DEPTH
Details
The four coefficients that describe the quaternion rotation from the Android sensor coordinate system to a camera-aligned coordinate system where the X-axis is aligned with the long side of the image sensor, the Y-axis is aligned with the short side of the image sensor, and the Z-axis is aligned with the optical axis of the sensor. To convert from the quaternion coefficients `(x,y,z,w)` to the axis of rotation `(a_x, a_y, a_z)` and rotation amount `theta`, the following formulas can be used:
     theta = 2 * acos(w)
    a_x = x / sin(theta/2)
    a_y = y / sin(theta/2)
    a_z = z / sin(theta/2)
To create a 3x3 rotation matrix that applies the rotation defined by this quaternion, the following matrix can be used:
    R = [ 1 - 2y^2 - 2z^2,       2xy - 2zw,       2xz + 2yw,
               2xy + 2zw, 1 - 2x^2 - 2z^2,       2yz - 2xw,
               2xz - 2yw,       2yz + 2xw, 1 - 2x^2 - 2y^2 ]
This matrix can then be used to apply the rotation to a column vector point with `p' = Rp` where `p` is in the device sensor coordinate system, and `p'` is in the camera-oriented coordinate system. If android.lens.poseReference is UNDEFINED, the quaternion rotation cannot be accurately represented by the camera device, and will be represented by default values matching its default facing.
android.lens.poseTranslation | float x 3 [public] | Position of the camera optical center. | Meters |  | 3.2 | DEPTH
Details
The position of the camera device's lens optical center, as a three-dimensional vector `(x,y,z)`. Prior to Android P, or when android.lens.poseReference is PRIMARY_CAMERA, this position is relative to the optical center of the largest camera device facing in the same direction as this camera, in the Android sensor coordinate axes. Note that only the axis definitions are shared with the sensor coordinate system, but not the origin. If this device is the largest or only camera device with a given facing, then this position will be `(0, 0, 0)`; a camera device with a lens optical center located 3 cm from the main sensor along the +X axis (to the right from the user's perspective) will report `(0.03, 0, 0)`. Note that this means that, for many computer vision applications, the position needs to be negated to convert it to a translation from the camera to the origin. To transform a pixel coordinates between two cameras facing the same direction, first the source camera android.lens.distortion must be corrected for. Then the source camera android.lens.intrinsicCalibration needs to be applied, followed by the android.lens.poseRotation of the source camera, the translation of the source camera relative to the destination camera, the android.lens.poseRotation of the destination camera, and finally the inverse of android.lens.intrinsicCalibration of the destination camera. This obtains a radial-distortion-free coordinate in the destination camera pixel coordinates. To compare this against a real image from the destination camera, the destination camera image then needs to be corrected for radial distortion before comparison or sampling. When android.lens.poseReference is GYROSCOPE, then this position is relative to the center of the primary gyroscope on the device. The axis definitions are the same as with PRIMARY_CAMERA. When android.lens.poseReference is UNDEFINED, this position cannot be accurately represented by the camera device, and will be represented as `(0, 0, 0)`.
android.lens.intrinsicCalibration | float x 5 [public] | The parameters for this camera device's intrinsic calibration. | Pixels in the android.sensor.info.preCorrectionActiveArraySize coordinate system. |  | 3.2 | DEPTH
Details
The five calibration parameters that describe the transform from camera-centric 3D coordinates to sensor pixel coordinates:
    [f_x, f_y, c_x, c_y, s]
Where `f_x` and `f_y` are the horizontal and vertical focal lengths, `[c_x, c_y]` is the position of the optical axis, and `s` is a skew parameter for the sensor plane not being aligned with the lens plane. These are typically used within a transformation matrix K:
    K = [ f_x,   s, c_x,
           0, f_y, c_y,
           0    0,   1 ]
which can then be combined with the camera pose rotation `R` and translation `t` (android.lens.poseRotation and android.lens.poseTranslation, respectively) to calculate the complete transform from world coordinates to pixel coordinates:
    P = [ K 0   * [ R -Rt
         0 1 ]      0 1 ]
(Note the negation of poseTranslation when mapping from camera to world coordinates, and multiplication by the rotation). With `p_w` being a point in the world coordinate system and `p_s` being a point in the camera active pixel array coordinate system, and with the mapping including the homogeneous division by z:
     p_h = (x_h, y_h, z_h) = P p_w
    p_s = p_h / z_h
so `[x_s, y_s]` is the pixel coordinates of the world point, `z_s = 1`, and `w_s` is a measurement of disparity (depth) in pixel coordinates. Note that the coordinate system for this transform is the android.sensor.info.preCorrectionActiveArraySize system, where `(0,0)` is the top-left of the preCorrectionActiveArraySize rectangle. Once the pose and intrinsic calibration transforms have been applied to a world point, then the android.lens.distortion transform needs to be applied, and the result adjusted to be in the android.sensor.info.activeArraySize coordinate system (where `(0, 0)` is the top-left of the activeArraySize rectangle), to determine the final pixel coordinate of the world point for processed (non-RAW) output buffers. For camera devices, the center of pixel `(x,y)` is located at coordinate `(x + 0.5, y + 0.5)`. So on a device with a precorrection active array of size `(10,10)`, the valid pixel indices go from `(0,0)-(9,9)`, and an perfectly-built camera would have an optical center at the exact center of the pixel grid, at coordinates `(5.0, 5.0)`, which is the top-left corner of pixel `(5,5)`.
android.lens.radialDistortion | float x 6 [public] [deprecated] | The correction coefficients to correct for this camera device's radial and tangential lens distortion. | Unitless coefficients. | Deprecated. Do not use. | 3.2 | DEPTH
Details
Four radial distortion coefficients `[kappa_0, kappa_1, kappa_2, kappa_3]` and two tangential distortion coefficients `[kappa_4, kappa_5]` that can be used to correct the lens's geometric distortion with the mapping equations:
     x_c = x_i * ( kappa_0 + kappa_1 * r^2 + kappa_2 * r^4 + kappa_3 * r^6 ) +
           kappa_4 * (2 * x_i * y_i) + kappa_5 * ( r^2 + 2 * x_i^2 )
     y_c = y_i * ( kappa_0 + kappa_1 * r^2 + kappa_2 * r^4 + kappa_3 * r^6 ) +
           kappa_5 * (2 * x_i * y_i) + kappa_4 * ( r^2 + 2 * y_i^2 )
Here, `[x_c, y_c]` are the coordinates to sample in the input image that correspond to the pixel values in the corrected image at the coordinate `[x_i, y_i]`:
     correctedImage(x_i, y_i) = sample_at(x_c, y_c, inputImage)
The pixel coordinates are defined in a normalized coordinate system related to the android.lens.intrinsicCalibration calibration fields. Both `[x_i, y_i]` and `[x_c, y_c]` have `(0,0)` at the lens optical center `[c_x, c_y]`. The maximum magnitudes of both x and y coordinates are normalized to be 1 at the edge further from the optical center, so the range for both dimensions is `-1 <= x <= 1`. Finally, `r` represents the radial distance from the optical center, `r^2 = x_i^2 + y_i^2`, and its magnitude is therefore no larger than `|r| <= sqrt(2)`. The distortion model used is the Brown-Conrady model.
android.lens.distortion | float x 5 [public] | The correction coefficients to correct for this camera device's radial and tangential lens distortion. Replaces the deprecated android.lens.radialDistortion field, which was inconsistently defined. | Unitless coefficients. |  | 3.3 | DEPTH
Details
Three radial distortion coefficients `[kappa_1, kappa_2, kappa_3]` and two tangential distortion coefficients `[kappa_4, kappa_5]` that can be used to correct the lens's geometric distortion with the mapping equations:
     x_c = x_i * ( 1 + kappa_1 * r^2 + kappa_2 * r^4 + kappa_3 * r^6 ) +
           kappa_4 * (2 * x_i * y_i) + kappa_5 * ( r^2 + 2 * x_i^2 )
     y_c = y_i * ( 1 + kappa_1 * r^2 + kappa_2 * r^4 + kappa_3 * r^6 ) +
           kappa_5 * (2 * x_i * y_i) + kappa_4 * ( r^2 + 2 * y_i^2 )
Here, `[x_c, y_c]` are the coordinates to sample in the input image that correspond to the pixel values in the corrected image at the coordinate `[x_i, y_i]`:
     correctedImage(x_i, y_i) = sample_at(x_c, y_c, inputImage)
The pixel coordinates are defined in a coordinate system related to the android.lens.intrinsicCalibration calibration fields; see that entry for details of the mapping stages. Both `[x_i, y_i]` and `[x_c, y_c]` have `(0,0)` at the lens optical center `[c_x, c_y]`, and the range of the coordinates depends on the focal length terms of the intrinsic calibration. Finally, `r` represents the radial distance from the optical center, `r^2 = x_i^2 + y_i^2`. The distortion model used is the Brown-Conrady model.
noiseReduction
controls
Property Name | Type | Description | Units | Range | Initial HIDL HAL version | Tags
android.noiseReduction.mode | byte [public] [full] OFF (v3.2) No noise reduction is applied. FAST (v3.2) Noise reduction is applied without reducing frame rate relative to sensor output. It may be the same as OFF if noise reduction will reduce frame rate relative to sensor. HIGH_QUALITY (v3.2) High-quality noise reduction is applied, at the cost of possibly reduced frame rate relative to sensor output. MINIMAL (v3.2) [optional] MINIMAL noise reduction is applied without reducing frame rate relative to sensor output. ZERO_SHUTTER_LAG (v3.2) [optional] Noise reduction is applied at different levels for different output streams, based on resolution. Streams at maximum recording resolution (see CameraDevice#createCaptureSession) or below have noise reduction applied, while higher-resolution streams have MINIMAL (if supported) or no noise reduction applied (if MINIMAL is not supported.) The degree of noise reduction for low-resolution streams is tuned so that frame rate is not impacted, and the quality is equal to or better than FAST (since it is only applied to lower-resolution outputs, quality may improve from FAST). This mode is intended to be used by applications operating in a zero-shutter-lag mode with YUV or PRIVATE reprocessing, where the application continuously captures high-resolution intermediate buffers into a circular buffer, from which a final image is produced via reprocessing when a user takes a picture. For such a use case, the high-resolution buffers must not have noise reduction applied to maximize efficiency of preview and to avoid over-applying noise filtering when reprocessing, while low-resolution buffers (used for recording or preview, generally) need noise reduction applied for reasonable preview quality. This mode is guaranteed to be supported by devices that support either the YUV_REPROCESSING or PRIVATE_REPROCESSING capabilities (android.request.availableCapabilities lists either of those capabilities) and it will be the default mode for CAMERA3_TEMPLATE_ZERO_SHUTTER_LAG template. | Mode of operation for the noise reduction algorithm. |  | android.noiseReduction.availableNoiseReductionModes | 3.2 | V1 REPROC
Details
The noise reduction algorithm attempts to improve image quality by removing excessive noise added by the capture process, especially in dark conditions. OFF means no noise reduction will be applied by the camera device, for both raw and YUV domain. MINIMAL means that only sensor raw domain basic noise reduction is enabled ,to remove demosaicing or other processing artifacts. For YUV_REPROCESSING, MINIMAL is same as OFF. This mode is optional, may not be support by all devices. The application should check android.noiseReduction.availableNoiseReductionModes before using it. FAST/HIGH_QUALITY both mean camera device determined noise filtering will be applied. HIGH_QUALITY mode indicates that the camera device will use the highest-quality noise filtering algorithms, even if it slows down capture rate. FAST means the camera device will not slow down capture rate when applying noise filtering. FAST may be the same as MINIMAL if MINIMAL is listed, or the same as OFF if any noise filtering will slow down capture rate. Every output stream will have a similar amount of enhancement applied. ZERO_SHUTTER_LAG is meant to be used by applications that maintain a continuous circular buffer of high-resolution images during preview and reprocess image(s) from that buffer into a final capture when triggered by the user. In this mode, the camera device applies noise reduction to low-resolution streams (below maximum recording resolution) to maximize preview quality, but does not apply noise reduction to high-resolution streams, since those will be reprocessed later if necessary. For YUV_REPROCESSING, these FAST/HIGH_QUALITY modes both mean that the camera device will apply FAST/HIGH_QUALITY YUV domain noise reduction, respectively. The camera device may adjust the noise reduction parameters for best image quality based on the android.reprocess.effectiveExposureFactor if it is set.
HAL Implementation Details
For YUV_REPROCESSING The HAL can use android.reprocess.effectiveExposureFactor to adjust the internal noise reduction parameters appropriately to get the best quality images.
android.noiseReduction.strength | byte [system] | Control the amount of noise reduction applied to the images | 1-10; 10 is max noise reduction | 1 - 10 | 3.2 | FUTURE
static
Property Name | Type | Description | Units | Range | Initial HIDL HAL version | Tags
android.noiseReduction.availableNoiseReductionModes | byte x n [public as enumList] [limited] list of enums | List of noise reduction modes for android.noiseReduction.mode that are supported by this camera device. |  | Any value listed in android.noiseReduction.mode | 3.2 | V1 REPROC
Details
Full-capability camera devices will always support OFF and FAST. Camera devices that support YUV_REPROCESSING or PRIVATE_REPROCESSING will support ZERO_SHUTTER_LAG. Legacy-capability camera devices will only support FAST mode.
HAL Implementation Details
HAL must support both FAST and HIGH_QUALITY if noise reduction control is available on the camera device, but the underlying implementation can be the same for both modes. That is, if the highest quality implementation on the camera device does not slow down capture rate, then FAST and HIGH_QUALITY will generate the same output.
dynamic
Property Name | Type | Description | Units | Range | Initial HIDL HAL version | Tags
android.noiseReduction.mode | byte [public] [full] OFF (v3.2) No noise reduction is applied. FAST (v3.2) Noise reduction is applied without reducing frame rate relative to sensor output. It may be the same as OFF if noise reduction will reduce frame rate relative to sensor. HIGH_QUALITY (v3.2) High-quality noise reduction is applied, at the cost of possibly reduced frame rate relative to sensor output. MINIMAL (v3.2) [optional] MINIMAL noise reduction is applied without reducing frame rate relative to sensor output. ZERO_SHUTTER_LAG (v3.2) [optional] Noise reduction is applied at different levels for different output streams, based on resolution. Streams at maximum recording resolution (see CameraDevice#createCaptureSession) or below have noise reduction applied, while higher-resolution streams have MINIMAL (if supported) or no noise reduction applied (if MINIMAL is not supported.) The degree of noise reduction for low-resolution streams is tuned so that frame rate is not impacted, and the quality is equal to or better than FAST (since it is only applied to lower-resolution outputs, quality may improve from FAST). This mode is intended to be used by applications operating in a zero-shutter-lag mode with YUV or PRIVATE reprocessing, where the application continuously captures high-resolution intermediate buffers into a circular buffer, from which a final image is produced via reprocessing when a user takes a picture. For such a use case, the high-resolution buffers must not have noise reduction applied to maximize efficiency of preview and to avoid over-applying noise filtering when reprocessing, while low-resolution buffers (used for recording or preview, generally) need noise reduction applied for reasonable preview quality. This mode is guaranteed to be supported by devices that support either the YUV_REPROCESSING or PRIVATE_REPROCESSING capabilities (android.request.availableCapabilities lists either of those capabilities) and it will be the default mode for CAMERA3_TEMPLATE_ZERO_SHUTTER_LAG template. | Mode of operation for the noise reduction algorithm. |  | android.noiseReduction.availableNoiseReductionModes | 3.2 | V1 REPROC
Details
The noise reduction algorithm attempts to improve image quality by removing excessive noise added by the capture process, especially in dark conditions. OFF means no noise reduction will be applied by the camera device, for both raw and YUV domain. MINIMAL means that only sensor raw domain basic noise reduction is enabled ,to remove demosaicing or other processing artifacts. For YUV_REPROCESSING, MINIMAL is same as OFF. This mode is optional, may not be support by all devices. The application should check android.noiseReduction.availableNoiseReductionModes before using it. FAST/HIGH_QUALITY both mean camera device determined noise filtering will be applied. HIGH_QUALITY mode indicates that the camera device will use the highest-quality noise filtering algorithms, even if it slows down capture rate. FAST means the camera device will not slow down capture rate when applying noise filtering. FAST may be the same as MINIMAL if MINIMAL is listed, or the same as OFF if any noise filtering will slow down capture rate. Every output stream will have a similar amount of enhancement applied. ZERO_SHUTTER_LAG is meant to be used by applications that maintain a continuous circular buffer of high-resolution images during preview and reprocess image(s) from that buffer into a final capture when triggered by the user. In this mode, the camera device applies noise reduction to low-resolution streams (below maximum recording resolution) to maximize preview quality, but does not apply noise reduction to high-resolution streams, since those will be reprocessed later if necessary. For YUV_REPROCESSING, these FAST/HIGH_QUALITY modes both mean that the camera device will apply FAST/HIGH_QUALITY YUV domain noise reduction, respectively. The camera device may adjust the noise reduction parameters for best image quality based on the android.reprocess.effectiveExposureFactor if it is set.
HAL Implementation Details
For YUV_REPROCESSING The HAL can use android.reprocess.effectiveExposureFactor to adjust the internal noise reduction parameters appropriately to get the best quality images.
quirks
static
Property Name | Type | Description | Units | Range | Initial HIDL HAL version | Tags
android.quirks.meteringCropRegion | byte [system] [deprecated] | If set to 1, the camera service does not scale 'normalized' coordinates with respect to the crop region. This applies to metering input (a{e,f,wb}Region and output (face rectangles). |  | Deprecated. Do not use. | 3.2 |
Details
Normalized coordinates refer to those in the (-1000,1000) range mentioned in the android.hardware.Camera API. HAL implementations should instead always use and emit sensor array-relative coordinates for all region data. Does not need to be listed in static metadata. Support will be removed in future versions of camera service.
android.quirks.triggerAfWithAuto | byte [system] [deprecated] | If set to 1, then the camera service always switches to FOCUS_MODE_AUTO before issuing a AF trigger. |  | Deprecated. Do not use. | 3.2 |
Details
HAL implementations should implement AF trigger modes for AUTO, MACRO, CONTINUOUS_FOCUS, and CONTINUOUS_PICTURE modes instead of using this flag. Does not need to be listed in static metadata. Support will be removed in future versions of camera service
android.quirks.useZslFormat | byte [system] [deprecated] | If set to 1, the camera service uses CAMERA2_PIXEL_FORMAT_ZSL instead of HAL_PIXEL_FORMAT_IMPLEMENTATION_DEFINED for the zero shutter lag stream |  | Deprecated. Do not use. | 3.2 |
Details
HAL implementations should use gralloc usage flags to determine that a stream will be used for zero-shutter-lag, instead of relying on an explicit format setting. Does not need to be listed in static metadata. Support will be removed in future versions of camera service.
android.quirks.usePartialResult | byte [hidden] [deprecated] | If set to 1, the HAL will always split result metadata for a single capture into multiple buffers, returned using multiple process_capture_result calls. |  | Deprecated. Do not use. | 3.2 |
Details
Does not need to be listed in static metadata. Support for partial results will be reworked in future versions of camera service. This quirk will stop working at that point; DO NOT USE without careful consideration of future support.
HAL Implementation Details
Refer to `camera3_capture_result::partial_result` for information on how to implement partial results.
dynamic
Property Name | Type | Description | Units | Range | Initial HIDL HAL version | Tags
android.quirks.partialResult | byte [hidden as boolean] [deprecated] FINAL (v3.2) The last or only metadata result buffer for this capture. PARTIAL (v3.2) A partial buffer of result metadata for this capture. More result buffers for this capture will be sent by the camera device, the last of which will be marked FINAL. | Whether a result given to the framework is the final one for the capture, or only a partial that contains a subset of the full set of dynamic metadata values. |  | Deprecated. Do not use. Optional. Default value is FINAL. | 3.2 |
Details
The entries in the result metadata buffers for a single capture may not overlap, except for this entry. The FINAL buffers must retain FIFO ordering relative to the requests that generate them, so the FINAL buffer for frame 3 must always be sent to the framework after the FINAL buffer for frame 2, and before the FINAL buffer for frame 4. PARTIAL buffers may be returned in any order relative to other frames, but all PARTIAL buffers for a given capture must arrive before the FINAL buffer for that capture. This entry may only be used by the camera device if quirks.usePartialResult is set to 1.
HAL Implementation Details
Refer to `camera3_capture_result::partial_result` for information on how to implement partial results.
request
controls
Property Name | Type | Description | Units | Range | Initial HIDL HAL version | Tags
android.request.frameCount | int32 [system] [deprecated] | A frame counter set by the framework. Must be maintained unchanged in output frame. This value monotonically increases with every new result (that is, each new result has a unique frameCount value). | incrementing integer | Deprecated. Do not use. Any int. | 3.2 |
android.request.id | int32 [hidden] | An application-specified ID for the current request. Must be maintained unchanged in output frame | arbitrary integer assigned by application | Any int | 3.2 | V1
android.request.inputStreams | int32 x n [system] [deprecated] | List which camera reprocess stream is used for the source of reprocessing data. | List of camera reprocess stream IDs | Deprecated. Do not use. Typically, only one entry allowed, must be a valid reprocess stream ID. | 3.2 | HAL2
Details
Only meaningful when android.request.type == REPROCESS. Ignored otherwise
android.request.metadataMode | byte [system] NONE (v3.2) No metadata should be produced on output, except for application-bound buffer data. If no application-bound streams exist, no frame should be placed in the output frame queue. If such streams exist, a frame should be placed on the output queue with null metadata but with the necessary output buffer information. Timestamp information should still be included with any output stream buffers FULL (v3.2) All metadata should be produced. Statistics will only be produced if they are separately enabled | How much metadata to produce on output |  |  | 3.2 | FUTURE
android.request.outputStreams | int32 x n [system] [deprecated] | Lists which camera output streams image data from this capture must be sent to | List of camera stream IDs | Deprecated. Do not use. List must only include streams that have been created | 3.2 | HAL2
Details
If no output streams are listed, then the image data should simply be discarded. The image data must still be captured for metadata and statistics production, and the lens and flash must operate as requested.
android.request.type | byte [system] [deprecated] CAPTURE (v3.2) Capture a new image from the imaging hardware, and process it according to the settings REPROCESS (v3.2) Process previously captured data; the android.request.inputStreams parameter determines the source reprocessing stream. TODO: Mark dynamic metadata needed for reprocessing with [RP] | The type of the request; either CAPTURE or REPROCESS. For legacy HAL3, this tag is redundant. |  | Deprecated. Do not use. | 3.2 | HAL2
static
Property Name | Type | Description | Units | Range | Initial HIDL HAL version | Tags
android.request.maxNumOutputStreams | int32 x 3 [ndk_public] [legacy] | The maximum numbers of different types of output streams that can be configured and used simultaneously by a camera device. |  | For processed (and stalling) format streams, >= 1. For Raw format (either stalling or non-stalling) streams, >= 0. For processed (but not stalling) format streams, >= 3 for FULL mode devices (`android.info.supportedHardwareLevel == FULL`); >= 2 for LIMITED mode devices (`android.info.supportedHardwareLevel == LIMITED`). | 3.2 | BC
Details
This is a 3 element tuple that contains the max number of output simultaneous streams for raw sensor, processed (but not stalling), and processed (and stalling) formats respectively. For example, assuming that JPEG is typically a processed and stalling stream, if max raw sensor format output stream number is 1, max YUV streams number is 3, and max JPEG stream number is 2, then this tuple should be `(1, 3, 2)`. This lists the upper bound of the number of output streams supported by the camera device. Using more streams simultaneously may require more hardware and CPU resources that will consume more power. The image format for an output stream can be any supported format provided by android.scaler.availableStreamConfigurations. The formats defined in android.scaler.availableStreamConfigurations can be catergorized into the 3 stream types as below: Processed (but stalling): any non-RAW format with a stallDurations > 0. Typically JPEG format. Raw formats: RAW_SENSOR, RAW10, or RAW12. Processed (but not-stalling): any non-RAW format without a stall duration. Typically YUV_420_888, NV21, YV12, or Y8 .
android.request.maxNumOutputRaw | int32 [java_public] [synthetic] [legacy] | The maximum numbers of different types of output streams that can be configured and used simultaneously by a camera device for any `RAW` formats. |  | >= 0 | 3.2 |
Details
This value contains the max number of output simultaneous streams from the raw sensor. This lists the upper bound of the number of output streams supported by the camera device. Using more streams simultaneously may require more hardware and CPU resources that will consume more power. The image format for this kind of an output stream can be any `RAW` and supported format provided by android.scaler.streamConfigurationMap. In particular, a `RAW` format is typically one of: RAW_SENSOR RAW10 RAW12 LEGACY mode devices (android.info.supportedHardwareLevel `==` LEGACY) never support raw streams.
android.request.maxNumOutputProc | int32 [java_public] [synthetic] [legacy] | The maximum numbers of different types of output streams that can be configured and used simultaneously by a camera device for any processed (but not-stalling) formats. |  | >= 3 for FULL mode devices (`android.info.supportedHardwareLevel == FULL`); >= 2 for LIMITED mode devices (`android.info.supportedHardwareLevel == LIMITED`). | 3.2 |
Details
This value contains the max number of output simultaneous streams for any processed (but not-stalling) formats. This lists the upper bound of the number of output streams supported by the camera device. Using more streams simultaneously may require more hardware and CPU resources that will consume more power. The image format for this kind of an output stream can be any non-`RAW` and supported format provided by android.scaler.streamConfigurationMap. Processed (but not-stalling) is defined as any non-RAW format without a stall duration. Typically: YUV_420_888 NV21 YV12 Implementation-defined formats, i.e. StreamConfigurationMap#isOutputSupportedFor(Class) Y8 For full guarantees, query StreamConfigurationMap#getOutputStallDuration with a processed format -- it will return 0 for a non-stalling stream. LEGACY devices will support at least 2 processing/non-stalling streams.
android.request.maxNumOutputProcStalling | int32 [java_public] [synthetic] [legacy] | The maximum numbers of different types of output streams that can be configured and used simultaneously by a camera device for any processed (and stalling) formats. |  | >= 1 | 3.2 |
Details
This value contains the max number of output simultaneous streams for any processed (but not-stalling) formats. This lists the upper bound of the number of output streams supported by the camera device. Using more streams simultaneously may require more hardware and CPU resources that will consume more power. The image format for this kind of an output stream can be any non-`RAW` and supported format provided by android.scaler.streamConfigurationMap. A processed and stalling format is defined as any non-RAW format with a stallDurations > 0. Typically only the JPEG format is a stalling format. For full guarantees, query StreamConfigurationMap#getOutputStallDuration with a processed format -- it will return a non-0 value for a stalling stream. LEGACY devices will support up to 1 processing/stalling stream.
android.request.maxNumReprocessStreams | int32 x 1 [system] [deprecated] | How many reprocessing streams of any type can be allocated at the same time. |  | Deprecated. Do not use. >= 0 | 3.2 | HAL2
Details
Only used by HAL2.x. When set to 0, it means no reprocess stream is supported.
android.request.maxNumInputStreams | int32 [java_public] [full] | The maximum numbers of any type of input streams that can be configured and used simultaneously by a camera device. |  | 0 or 1. | 3.2 | REPROC
Details
When set to 0, it means no input stream is supported. The image format for a input stream can be any supported format returned by StreamConfigurationMap#getInputFormats. When using an input stream, there must be at least one output stream configured to to receive the reprocessed images. When an input stream and some output streams are used in a reprocessing request, only the input buffer will be used to produce these output stream buffers, and a new sensor image will not be captured. For example, for Zero Shutter Lag (ZSL) still capture use case, the input stream image format will be PRIVATE, the associated output stream image format should be JPEG.
HAL Implementation Details
For the reprocessing flow and controls, see hardware/libhardware/include/hardware/camera3.h Section 10 for more details.
android.request.pipelineMaxDepth | byte [public] [legacy] | Specifies the number of maximum pipeline stages a frame has to go through from when it's exposed to when it's available to the framework. |  |  | 3.2 |
Details
A typical minimum value for this is 2 (one stage to expose, one stage to readout) from the sensor. The ISP then usually adds its own stages to do custom HW processing. Further stages may be added by SW processing. Depending on what settings are used (e.g. YUV, JPEG) and what processing is enabled (e.g. face detection), the actual pipeline depth (specified by android.request.pipelineDepth) may be less than the max pipeline depth. A pipeline depth of X stages is equivalent to a pipeline latency of X frame intervals. This value will normally be 8 or less, however, for high speed capture session, the max pipeline depth will be up to 8 x size of high speed capture request list.
HAL Implementation Details
This value should be 4 or less, expect for the high speed recording session, where the max batch sizes may be larger than 1.
android.request.partialResultCount | int32 [public] | Defines how many sub-components a result will be composed of. |  | >= 1 | 3.2 |
Details
In order to combat the pipeline latency, partial results may be delivered to the application layer from the camera device as soon as they are available. Optional; defaults to 1. A value of 1 means that partial results are not supported, and only the final TotalCaptureResult will be produced by the camera device. A typical use case for this might be: after requesting an auto-focus (AF) lock the new AF state might be available 50% of the way through the pipeline. The camera device could then immediately dispatch this state via a partial result to the application, and the rest of the metadata via later partial results.
- android.request.availableCapabilities | byte x n [public] [legacy] BACKWARD_COMPATIBLE (v3.2) The minimal set of capabilities that every camera device (regardless of android.info.supportedHardwareLevel) supports. This capability is listed by all normal devices, and indicates that the camera device has a feature set that's comparable to the baseline requirements for the older android.hardware.Camera API. Devices with the DEPTH_OUTPUT capability might not list this capability, indicating that they support only depth measurement, not standard color output. MANUAL_SENSOR (v3.2) [optional] The camera device can be manually controlled (3A algorithms such as auto-exposure, and auto-focus can be bypassed). The camera device supports basic manual control of the sensor image acquisition related stages. This means the following controls are guaranteed to be supported: Manual frame duration control android.sensor.frameDuration android.sensor.info.maxFrameDuration Manual exposure control android.sensor.exposureTime android.sensor.info.exposureTimeRange Manual sensitivity control android.sensor.sensitivity android.sensor.info.sensitivityRange Manual lens control (if the lens is adjustable) android.lens.* Manual flash control (if a flash unit is present) android.flash.* Manual black level locking android.blackLevel.lock Auto exposure lock android.control.aeLock If any of the above 3A algorithms are enabled, then the camera device will accurately report the values applied by 3A in the result. A given camera device may also support additional manual sensor controls, but this capability only covers the above list of controls. If this is supported, android.scaler.streamConfigurationMap will additionally return a min frame duration that is greater than zero for each supported size-format combination. For camera devices with LOGICAL_MULTI_CAMERA capability, when the underlying active physical camera switches, exposureTime, sensitivity, and lens properties may change even if AE/AF is locked. However, the overall auto exposure and auto focus experience for users will be consistent. Refer to LOGICAL_MULTI_CAMERA capability for details. MANUAL_POST_PROCESSING (v3.2) [optional] The camera device post-processing stages can be manually controlled. The camera device supports basic manual control of the image post-processing stages. This means the following controls are guaranteed to be supported: Manual tonemap control android.tonemap.curve android.tonemap.mode android.tonemap.maxCurvePoints android.tonemap.gamma android.tonemap.presetCurve Manual white balance control android.colorCorrection.transform android.colorCorrection.gains Manual lens shading map control android.shading.mode android.statistics.lensShadingMapMode android.statistics.lensShadingMap android.lens.info.shadingMapSize Manual aberration correction control (if aberration correction is supported) android.colorCorrection.aberrationMode android.colorCorrection.availableAberrationModes Auto white balance lock android.control.awbLock If auto white balance is enabled, then the camera device will accurately report the values applied by AWB in the result. A given camera device may also support additional post-processing controls, but this capability only covers the above list of controls. For camera devices with LOGICAL_MULTI_CAMERA capability, when underlying active physical camera switches, tonemap, white balance, and shading map may change even if awb is locked. However, the overall post-processing experience for users will be consistent. Refer to LOGICAL_MULTI_CAMERA capability for details. RAW (v3.2) [optional] The camera device supports outputting RAW buffers and metadata for interpreting them. Devices supporting the RAW capability allow both for saving DNG files, and for direct application processing of raw sensor images. RAW_SENSOR is supported as an output format. The maximum available resolution for RAW_SENSOR streams will match either the value in android.sensor.info.pixelArraySize or android.sensor.info.preCorrectionActiveArraySize. All DNG-related optional metadata entries are provided by the camera device. PRIVATE_REPROCESSING (v3.2) [optional] The camera device supports the Zero Shutter Lag reprocessing use case. One input stream is supported, that is, `android.request.maxNumInputStreams == 1`. ImageFormat#PRIVATE is supported as an output/input format, that is, ImageFormat#PRIVATE is included in the lists of formats returned by StreamConfigurationMap#getInputFormats and StreamConfigurationMap#getOutputFormats. StreamConfigurationMap#getValidOutputFormatsForInput returns non empty int[] for each supported input format returned by StreamConfigurationMap#getInputFormats. Each size returned by getInputSizes(ImageFormat.PRIVATE) is also included in getOutputSizes(ImageFormat.PRIVATE) Using ImageFormat#PRIVATE does not cause a frame rate drop relative to the sensor's maximum capture rate (at that resolution). ImageFormat#PRIVATE will be reprocessable into both ImageFormat#YUV_420_888 and ImageFormat#JPEG formats. For a MONOCHROME camera supporting Y8 format, ImageFormat#PRIVATE will be reprocessable into ImageFormat#Y8. The maximum available resolution for PRIVATE streams (both input/output) will match the maximum available resolution of JPEG streams. Static metadata android.reprocess.maxCaptureStall. Only below controls are effective for reprocessing requests and will be present in capture results, other controls in reprocess requests will be ignored by the camera device. android.jpeg.* android.noiseReduction.mode android.edge.mode android.noiseReduction.availableNoiseReductionModes and android.edge.availableEdgeModes will both list ZERO_SHUTTER_LAG as a supported mode. READ_SENSOR_SETTINGS (v3.2) [optional] The camera device supports accurately reporting the sensor settings for many of the sensor controls while the built-in 3A algorithm is running. This allows reporting of sensor settings even when these settings cannot be manually changed. The values reported for the following controls are guaranteed to be available in the CaptureResult, including when 3A is enabled: Exposure control android.sensor.exposureTime Sensitivity control android.sensor.sensitivity Lens controls (if the lens is adjustable) android.lens.focusDistance android.lens.aperture This capability is a subset of the MANUAL_SENSOR control capability, and will always be included if the MANUAL_SENSOR capability is available. BURST_CAPTURE (v3.2) [optional] The camera device supports capturing high-resolution images at >= 20 frames per second, in at least the uncompressed YUV format, when post-processing settings are set to FAST. Additionally, all image resolutions less than 24 megapixels can be captured at >= 10 frames per second. Here, 'high resolution' means at least 8 megapixels, or the maximum resolution of the device, whichever is smaller. YUV_REPROCESSING (v3.2) [optional] The camera device supports the YUV_420_888 reprocessing use case, similar as PRIVATE_REPROCESSING, This capability requires the camera device to support the following: One input stream is supported, that is, `android.request.maxNumInputStreams == 1`. ImageFormat#YUV_420_888 is supported as an output/input format, that is, YUV_420_888 is included in the lists of formats returned by StreamConfigurationMap#getInputFormats and StreamConfigurationMap#getOutputFormats. StreamConfigurationMap#getValidOutputFormatsForInput returns non-empty int[] for each supported input format returned by StreamConfigurationMap#getInputFormats. Each size returned by getInputSizes(YUV_420_888) is also included in getOutputSizes(YUV_420_888) Using ImageFormat#YUV_420_888 does not cause a frame rate drop relative to the sensor's maximum capture rate (at that resolution). ImageFormat#YUV_420_888 will be reprocessable into both ImageFormat#YUV_420_888 and ImageFormat#JPEG formats. The maximum available resolution for ImageFormat#YUV_420_888 streams (both input/output) will match the maximum available resolution of ImageFormat#JPEG streams. For a MONOCHROME camera with Y8 format support, all the requirements mentioned above for YUV_420_888 apply for Y8 format as well. Static metadata android.reprocess.maxCaptureStall. Only the below controls are effective for reprocessing requests and will be present in capture results. The reprocess requests are from the original capture results that are associated with the intermediate ImageFormat#YUV_420_888 output buffers. All other controls in the reprocess requests will be ignored by the camera device. android.jpeg.* android.noiseReduction.mode android.edge.mode android.reprocess.effectiveExposureFactor android.noiseReduction.availableNoiseReductionModes and android.edge.availableEdgeModes will both list ZERO_SHUTTER_LAG as a supported mode. DEPTH_OUTPUT (v3.2) [optional] The camera device can produce depth measurements from its field of view. This capability requires the camera device to support the following: ImageFormat#DEPTH16 is supported as an output format. ImageFormat#DEPTH_POINT_CLOUD is optionally supported as an output format. This camera device, and all camera devices with the same android.lens.facing, will list the following calibration metadata entries in both CameraCharacteristics and CaptureResult: android.lens.poseTranslation android.lens.poseRotation android.lens.intrinsicCalibration android.lens.distortion The android.depth.depthIsExclusive entry is listed by this device. As of Android P, the android.lens.poseReference entry is listed by this device. A LIMITED camera with only the DEPTH_OUTPUT capability does not have to support normal YUV_420_888, Y8, JPEG, and PRIV-format outputs. It only has to support the DEPTH16 format. Generally, depth output operates at a slower frame rate than standard color capture, so the DEPTH16 and DEPTH_POINT_CLOUD formats will commonly have a stall duration that should be accounted for (see StreamConfigurationMap#getOutputStallDuration). On a device that supports both depth and color-based output, to enable smooth preview, using a repeating burst is recommended, where a depth-output target is only included once every N frames, where N is the ratio between preview output rate and depth output rate, including depth stall time. CONSTRAINED_HIGH_SPEED_VIDEO (v3.2) [optional] The device supports constrained high speed video recording (frame rate >=120fps) use case. The camera device will support high speed capture session created by CameraDevice#createConstrainedHighSpeedCaptureSession, which only accepts high speed request lists created by CameraConstrainedHighSpeedCaptureSession#createHighSpeedRequestList. A camera device can still support high speed video streaming by advertising the high speed FPS ranges in android.control.aeAvailableTargetFpsRanges. For this case, all normal capture request per frame control and synchronization requirements will apply to the high speed fps ranges, the same as all other fps ranges. This capability describes the capability of a specialized operating mode with many limitations (see below), which is only targeted at high speed video recording. The supported high speed video sizes and fps ranges are specified in StreamConfigurationMap#getHighSpeedVideoFpsRanges. To get desired output frame rates, the application is only allowed to select video size and FPS range combinations provided by StreamConfigurationMap#getHighSpeedVideoSizes. The fps range can be controlled via android.control.aeTargetFpsRange. In this capability, the camera device will override aeMode, awbMode, and afMode to ON, AUTO, and CONTINUOUS_VIDEO, respectively. All post-processing block mode controls will be overridden to be FAST. Therefore, no manual control of capture and post-processing parameters is possible. All other controls operate the same as when android.control.mode == AUTO. This means that all other android.control.* fields continue to work, such as android.control.aeTargetFpsRange android.control.aeExposureCompensation android.control.aeLock android.control.awbLock android.control.effectMode android.control.aeRegions android.control.afRegions android.control.awbRegions android.control.afTrigger android.control.aePrecaptureTrigger android.control.zoomRatio Outside of android.control.*, the following controls will work: android.flash.mode (TORCH mode only, automatic flash for still capture will not work since aeMode is ON) android.lens.opticalStabilizationMode (if it is supported) android.scaler.cropRegion android.statistics.faceDetectMode (if it is supported) For high speed recording use case, the actual maximum supported frame rate may be lower than what camera can output, depending on the destination Surfaces for the image data. For example, if the destination surface is from video encoder, the application need check if the video encoder is capable of supporting the high frame rate for a given video size, or it will end up with lower recording frame rate. If the destination surface is from preview window, the actual preview frame rate will be bounded by the screen refresh rate. The camera device will only support up to 2 high speed simultaneous output surfaces (preview and recording surfaces) in this mode. Above controls will be effective only if all of below conditions are true: The application creates a camera capture session with no more than 2 surfaces via CameraDevice#createConstrainedHighSpeedCaptureSession. The targeted surfaces must be preview surface (either from SurfaceView or SurfaceTexture) or recording surface(either from MediaRecorder#getSurface or MediaCodec#createInputSurface). The stream sizes are selected from the sizes reported by StreamConfigurationMap#getHighSpeedVideoSizes. The FPS ranges are selected from StreamConfigurationMap#getHighSpeedVideoFpsRanges. When above conditions are NOT satistied, CameraDevice#createConstrainedHighSpeedCaptureSession will fail. Switching to a FPS range that has different maximum FPS may trigger some camera device reconfigurations, which may introduce extra latency. It is recommended that the application avoids unnecessary maximum target FPS changes as much as possible during high speed streaming. MOTION_TRACKING (v3.3) [optional] The camera device supports the MOTION_TRACKING value for android.control.captureIntent, which limits maximum exposure time to 20 ms. This limits the motion blur of capture images, resulting in better image tracking results for use cases such as image stabilization or augmented reality. LOGICAL_MULTI_CAMERA (v3.3) [optional] The camera device is a logical camera backed by two or more physical cameras. In API level 28, the physical cameras must also be exposed to the application via CameraManager#getCameraIdList. Starting from API level 29: Some or all physical cameras may not be independently exposed to the application, in which case the physical camera IDs will not be available in CameraManager#getCameraIdList. But the application can still query the physical cameras' characteristics by calling CameraManager#getCameraCharacteristics. If a physical camera is hidden from camera ID list, the mandatory stream combinations for that physical camera must be supported through the logical camera using physical streams. One exception is that in API level 30, a physical camera may become unavailable via AvailabilityCallback#onPhysicalCameraUnavailable callback. Combinations of logical and physical streams, or physical streams from different physical cameras are not guaranteed. However, if the camera device supports CameraDevice#isSessionConfigurationSupported, application must be able to query whether a stream combination involving physical streams is supported by calling CameraDevice#isSessionConfigurationSupported. Camera application shouldn't assume that there are at most 1 rear camera and 1 front camera in the system. For an application that switches between front and back cameras, the recommendation is to switch between the first rear camera and the first front camera in the list of supported camera devices. This capability requires the camera device to support the following: The IDs of underlying physical cameras are returned via CameraCharacteristics#getPhysicalCameraIds. This camera device must list static metadata android.logicalMultiCamera.sensorSyncType in CameraCharacteristics. The underlying physical cameras' static metadata must list the following entries, so that the application can correlate pixels from the physical streams: android.lens.poseReference android.lens.poseRotation android.lens.poseTranslation android.lens.intrinsicCalibration android.lens.distortion The SENSOR_INFO_TIMESTAMP_SOURCE of the logical device and physical devices must be the same. The logical camera must be LIMITED or higher device. A logical camera device's dynamic metadata may contain android.logicalMultiCamera.activePhysicalId to notify the application of the current active physical camera Id. An active physical camera is the physical camera from which the logical camera's main image data outputs (YUV or RAW) and metadata come from. In addition, this serves as an indication which physical camera is used to output to a RAW stream, or in case only physical cameras support RAW, which physical RAW stream the application should request. Logical camera's static metadata tags below describe the default active physical camera. An active physical camera is default if it's used when application directly uses requests built from a template. All templates will default to the same active physical camera. android.sensor.info.sensitivityRange android.sensor.info.colorFilterArrangement android.sensor.info.exposureTimeRange android.sensor.info.maxFrameDuration android.sensor.info.physicalSize android.sensor.info.whiteLevel android.sensor.info.lensShadingApplied android.sensor.referenceIlluminant1 android.sensor.referenceIlluminant2 android.sensor.calibrationTransform1 android.sensor.calibrationTransform2 android.sensor.colorTransform1 android.sensor.colorTransform2 android.sensor.forwardMatrix1 android.sensor.forwardMatrix2 android.sensor.blackLevelPattern android.sensor.maxAnalogSensitivity android.sensor.opticalBlackRegions android.sensor.availableTestPatternModes android.lens.info.hyperfocalDistance android.lens.info.minimumFocusDistance android.lens.info.focusDistanceCalibration android.lens.poseRotation android.lens.poseTranslation android.lens.intrinsicCalibration android.lens.poseReference android.lens.distortion The field of view of non-RAW physical streams must not be smaller than that of the non-RAW logical streams, or the maximum field-of-view of the physical camera, whichever is smaller. The application should check the physical capture result metadata for how the physical streams are cropped or zoomed. More specifically, given the physical camera result metadata, the effective horizontal field-of-view of the physical camera is:
      fov = 2 * atan2(cropW * sensorW / (2 * zoomRatio * activeArrayW), focalLength)
where the equation parameters are the physical camera's crop region width, physical sensor width, zoom ratio, active array width, and focal length respectively. Typically the physical stream of active physical camera has the same field-of-view as the logical streams. However, the same may not be true for physical streams from non-active physical cameras. For example, if the logical camera has a wide-ultrawide configuration where the wide lens is the default, when the crop region is set to the logical camera's active array size, (and the zoom ratio set to 1.0 starting from Android 11), a physical stream for the ultrawide camera may prefer outputing images with larger field-of-view than that of the wide camera for better stereo matching margin or more robust motion tracking. At the same time, the physical non-RAW streams' field of view must not be smaller than the requested crop region and zoom ratio, as long as it's within the physical lens' capability. For example, for a logical camera with wide-tele lens configuration where the wide lens is the default, if the logical camera's crop region is set to maximum size, and zoom ratio set to 1.0, the physical stream for the tele lens will be configured to its maximum size crop region (no zoom). Deprecated: Prior to Android 11, the field of view of all non-RAW physical streams cannot be larger than that of non-RAW logical streams. If the logical camera has a wide-ultrawide lens configuration where the wide lens is the default, when the logical camera's crop region is set to maximum size, the FOV of the physical streams for the ultrawide lens will be the same as the logical stream, by making the crop region smaller than its active array size to compensate for the smaller focal length. Even if the underlying physical cameras have different RAW characteristics (such as size or CFA pattern), a logical camera can still advertise RAW capability. In this case, when the application configures a RAW stream, the camera device will make sure the active physical camera will remain active to ensure consistent RAW output behavior, and not switch to other physical cameras. The capture request and result metadata tags required for backward compatible camera functionalities will be solely based on the logical camera capabiltity. On the other hand, the use of manual capture controls (sensor or post-processing) with a logical camera may result in unexpected behavior when the HAL decides to switch between physical cameras with different characteristics under the hood. For example, when the application manually sets exposure time and sensitivity while zooming in, the brightness of the camera images may suddenly change because HAL switches from one physical camera to the other. MONOCHROME (v3.3) [optional] The camera device is a monochrome camera that doesn't contain a color filter array, and for YUV_420_888 stream, the pixel values on U and V planes are all 128. A MONOCHROME camera must support the guaranteed stream combinations required for its device level and capabilities. Additionally, if the monochrome camera device supports Y8 format, all mandatory stream combination requirements related to YUV_420_888 apply to Y8 as well. There are no mandatory stream combination requirements with regard to Y8 for Bayer camera devices. Starting from Android Q, the SENSOR_INFO_COLOR_FILTER_ARRANGEMENT of a MONOCHROME camera will be either MONO or NIR. SECURE_IMAGE_DATA (v3.4) [optional] The camera device is capable of writing image data into a region of memory inaccessible to Android userspace or the Android kernel, and only accessible to trusted execution environments (TEE). SYSTEM_CAMERA (v3.5) [optional] The camera device is only accessible by Android's system components and privileged applications. Processes need to have the android.permission.SYSTEM_CAMERA in addition to android.permission.CAMERA in order to connect to this camera device. OFFLINE_PROCESSING (v3.5) [optional] The camera device supports the OFFLINE_PROCESSING use case. With OFFLINE_PROCESSING capability, the application can switch an ongoing capture session to offline mode by calling the CameraCaptureSession#switchToOffline method and specify streams to be kept in offline mode. The camera will then stop currently active repeating requests, prepare for some requests to go into offline mode, and return an offline session object. After the switchToOffline call returns, the original capture session is in closed state as if the CameraCaptureSession#close method has been called. In the offline mode, all inflight requests will continue to be processed in the background, and the application can immediately close the camera or create a new capture session without losing those requests' output images and capture results. While the camera device is processing offline requests, it might not be able to support all stream configurations it can support without offline requests. When that happens, the createCaptureSession method call will fail. The following stream configurations are guaranteed to work without hitting the resource busy exception: One ongoing offline session: target one output surface of YUV or JPEG format, any resolution. The active camera capture session: One preview surface (SurfaceView or SurfaceTexture) up to 1920 width One YUV ImageReader surface up to 1920 width One Jpeg ImageReader, any resolution: the camera device is allowed to slow down JPEG output speed by 50% if there is any ongoing offline session. If the device supports PRIVATE_REPROCESSING, one pair of ImageWriter/ImageReader surfaces of private format, with the same resolution that is larger or equal to the JPEG ImageReader resolution above. Alternatively, the active camera session above can be replaced by an legacy Camera with the following parameter settings: Preview size up to 1920 width Preview callback size up to 1920 width Video size up to 1920 width Picture size, any resolution: the camera device is allowed to slow down JPEG output speed by 50% if there is any ongoing offline session. | List of capabilities that this camera device advertises as fully supporting. |  |  | 3.2 |
Details
A capability is a contract that the camera device makes in order to be able to satisfy one or more use cases. Listing a capability guarantees that the whole set of features required to support a common use will all be available. Using a subset of the functionality provided by an unsupported capability may be possible on a specific camera device implementation; to do this query each of android.request.availableRequestKeys, android.request.availableResultKeys, android.request.availableCharacteristicsKeys. The following capabilities are guaranteed to be available on android.info.supportedHardwareLevel `==` FULL devices: MANUAL_SENSOR MANUAL_POST_PROCESSING Other capabilities may be available on either FULL or LIMITED devices, but the application should query this key to be sure.
HAL Implementation Details
Additional constraint details per-capability will be available in the Compatibility Test Suite. Minimum baseline requirements required for the BACKWARD_COMPATIBLE capability are not explicitly listed. Instead refer to "BC" tags and the camera CTS tests in the android.hardware.camera2.cts package. Listed controls that can be either request or result (e.g. android.sensor.exposureTime) must be available both in the request and the result in order to be considered to be capability-compliant. For example, if the HAL claims to support MANUAL control, then exposure time must be configurable via the request and the actual exposure applied must be available via the result. If MANUAL_SENSOR is omitted, the HAL may choose to omit the android.scaler.availableMinFrameDurations static property entirely. For PRIVATE_REPROCESSING and YUV_REPROCESSING capabilities, see hardware/libhardware/include/hardware/camera3.h Section 10 for more information. Devices that support the MANUAL_SENSOR capability must support the CAMERA3_TEMPLATE_MANUAL template defined in camera3.h. Devices that support the PRIVATE_REPROCESSING capability or the YUV_REPROCESSING capability must support the CAMERA3_TEMPLATE_ZERO_SHUTTER_LAG template defined in camera3.h. For DEPTH_OUTPUT, the depth-format keys android.depth.availableDepthStreamConfigurations, android.depth.availableDepthMinFrameDurations, android.depth.availableDepthStallDurations must be available, in addition to the other keys explicitly mentioned in the DEPTH_OUTPUT enum notes. The entry android.depth.maxDepthSamples must be available if the DEPTH_POINT_CLOUD format is supported (HAL pixel format BLOB, dataspace DEPTH). For a camera device with LOGICAL_MULTI_CAMERA capability, it should operate in the same way as a physical camera device based on its hardware level and capabilities. It's recommended that its feature set is superset of that of individual physical cameras. In camera1 API, to maintain application compatibility, for each camera facing, there may be one or more {logical_camera_id, physical_camera_1_id, physical_camera_2_id, ...} combinations, where logical_camera_id is composed of physical_camera_N_id, camera framework will only advertise one camera id (within the combinations for the particular facing) that is frontmost in the HAL published camera id list. For example, if HAL advertises 6 back facing camera IDs (ID0 to ID5), among which ID4 and ID5 are logical cameras backed by ID0+ID1 and ID2+ID3 respectively. In this case, only ID0 will be available for camera1 API to use. Camera HAL is strongly recommended to advertise camera devices with best feature, power, performance, and latency tradeoffs at the front of the camera id list. Camera HAL may switch between physical cameras depending on focalLength, cropRegion, or zoomRatio. If physical cameras have different sizes, HAL must maintain a single logical camera activeArraySize/pixelArraySize/preCorrectionActiveArraySize, and must do proper mapping between logical camera and underlying physical cameras for all related metadata tags, such as crop region, zoomRatio, 3A regions, and intrinsicCalibration. Starting from HIDL ICameraDevice version 3.5, camera HAL must support isStreamCombinationSupported for application to query whether a particular logical and physical streams combination are supported. A MONOCHROME camera device must also advertise BACKWARD_COMPATIBLE capability, and must not advertise MANUAL_POST_PROCESSING capability. To maintain backward compatibility, the camera device must support all BACKWARD_COMPATIBLE required keys. The android.control.awbAvailableModes key only contains AUTO, and android.control.awbState are either CONVERGED or LOCKED depending on android.control.awbLock. android.colorCorrection.mode, android.colorCorrection.transform, and android.colorCorrection.gains must not be in available request and result keys. As a result, the camera device cannot be a FULL device. However, the HAL can still advertise other individual capabilites. If the device supports tonemap control, only android.tonemap.curveRed is used. CurveGreen and curveBlue are no-ops. In Android API level 28, a MONOCHROME camera device must not have RAW capability. From API level 29, a camera is allowed to have both MONOCHROME and RAW capabilities. To support the legacy API to ICameraDevice 3.x shim layer, devices advertising OFFLINE_PROCESSING capability must also support configuring an input stream of the same size as the picture size if: The device supports PRIVATE_REPROCESSING capability The device's maximal JPEG resolution can reach 30 FPS min frame duration The device does not support HAL based ZSL (android.control.enableZsl) For devices which support SYSTEM_CAMERA and LOGICAL_MULTI_CAMERA capabilities: Hidden physical camera ids[1] must not be be shared[2] between public camera devices and camera devices advertising SYSTEM_CAMERA capability. [1] - Camera device ids which are advertised in the ANDROID_LOGICAL_MULTI_CAMERA_PHYSICAL_IDS list, and not available through ICameraProvider.getCameraIdList(). [2] - The ANDROID_LOGICAL_MULTI_CAMERA_PHYSICAL_IDS lists, must not have common camera ids.
android.request.availableRequestKeys | int32 x n [ndk_public] [legacy] | A list of all keys that the camera device has available to use with CaptureRequest. |  |  | 3.2 |
Details
Attempting to set a key into a CaptureRequest that is not listed here will result in an invalid request and will be rejected by the camera device. This field can be used to query the feature set of a camera device at a more granular level than capabilities. This is especially important for optional keys that are not listed under any capability in android.request.availableCapabilities.
HAL Implementation Details
Vendor tags can be listed here. Vendor tag metadata should also use the extensions C api (refer to camera3.h for more details). Setting/getting vendor tags will be checked against the metadata vendor extensions API and not against this field. The HAL must not consume any request tags that are not listed either here or in the vendor tag list. The public camera2 API will always make the vendor tags visible via CameraCharacteristics#getAvailableCaptureRequestKeys.
android.request.availableResultKeys | int32 x n [ndk_public] [legacy] | A list of all keys that the camera device has available to use with CaptureResult. |  |  | 3.2 |
Details
Attempting to get a key from a CaptureResult that is not listed here will always return a `null` value. Getting a key from a CaptureResult that is listed here will generally never return a `null` value. The following keys may return `null` unless they are enabled: android.statistics.lensShadingMap (non-null iff android.statistics.lensShadingMapMode == ON) (Those sometimes-null keys will nevertheless be listed here if they are available.) This field can be used to query the feature set of a camera device at a more granular level than capabilities. This is especially important for optional keys that are not listed under any capability in android.request.availableCapabilities.
HAL Implementation Details
Tags listed here must always have an entry in the result metadata, even if that size is 0 elements. Only array-type tags (e.g. lists, matrices, strings) are allowed to have 0 elements. Vendor tags can be listed here. Vendor tag metadata should also use the extensions C api (refer to camera3.h for more details). Setting/getting vendor tags will be checked against the metadata vendor extensions API and not against this field. The HAL must not produce any result tags that are not listed either here or in the vendor tag list. The public camera2 API will always make the vendor tags visible via CameraCharacteristics#getAvailableCaptureResultKeys.
android.request.availableCharacteristicsKeys | int32 x n [ndk_public] [legacy] | A list of all keys that the camera device has available to use with CameraCharacteristics. |  |  | 3.2 |
Details
This entry follows the same rules as android.request.availableResultKeys (except that it applies for CameraCharacteristics instead of CaptureResult). See above for more details.
HAL Implementation Details
Keys listed here must always have an entry in the static info metadata, even if that size is 0 elements. Only array-type tags (e.g. lists, matrices, strings) are allowed to have 0 elements. Vendor tags can listed here. Vendor tag metadata should also use the extensions C api (refer to camera3.h for more details). Setting/getting vendor tags will be checked against the metadata vendor extensions API and not against this field. The HAL must not have any tags in its static info that are not listed either here or in the vendor tag list. The public camera2 API will always make the vendor tags visible via CameraCharacteristics#getKeys.
android.request.availableSessionKeys | int32 x n [ndk_public] [legacy] | A subset of the available request keys that the camera device can pass as part of the capture session initialization. |  |  | 3.3 |
Details
This is a subset of android.request.availableRequestKeys which contains a list of keys that are difficult to apply per-frame and can result in unexpected delays when modified during the capture session lifetime. Typical examples include parameters that require a time-consuming hardware re-configuration or internal camera pipeline change. For performance reasons we advise clients to pass their initial values as part of SessionConfiguration#setSessionParameters. Once the camera capture session is enabled it is also recommended to avoid changing them from their initial values set in SessionConfiguration#setSessionParameters. Control over session parameters can still be exerted in capture requests but clients should be aware and expect delays during their application. An example usage scenario could look like this: The camera client starts by quering the session parameter key list via CameraCharacteristics#getAvailableSessionKeys. Before triggering the capture session create sequence, a capture request must be built via CameraDevice#createCaptureRequest using an appropriate template matching the particular use case. The client should go over the list of session parameters and check whether some of the keys listed matches with the parameters that they intend to modify as part of the first capture request. If there is no such match, the capture request can be passed unmodified to SessionConfiguration#setSessionParameters. If matches do exist, the client should update the respective values and pass the request to SessionConfiguration#setSessionParameters. After the capture session initialization completes the session parameter key list can continue to serve as reference when posting or updating further requests. As mentioned above further changes to session parameters should ideally be avoided, if updates are necessary however clients could expect a delay/glitch during the parameter switch.
HAL Implementation Details
If android.control.aeTargetFpsRange is part of the session parameters and constrained high speed mode is enabled, then only modifications of the maximum framerate value will be monitored by the framework and can trigger camera re-configuration. For more information about framerate ranges during constrained high speed sessions see CameraDevice#createConstrainedHighSpeedCaptureSession. Vendor tags can be listed here. Vendor tag metadata should also use the extensions C api (refer to android.hardware.camera.device.V3_4.StreamConfiguration.sessionParams for more details). Setting/getting vendor tags will be checked against the metadata vendor extensions API and not against this field. The HAL must not consume any request tags in the session parameters that are not listed either here or in the vendor tag list. The public camera2 API will always make the vendor tags visible via CameraCharacteristics#getAvailableSessionKeys.
android.request.availablePhysicalCameraRequestKeys | int32 x n [ndk_public] [limited] | A subset of the available request keys that can be overridden for physical devices backing a logical multi-camera. |  |  | 3.3 |
Details
This is a subset of android.request.availableRequestKeys which contains a list of keys that can be overridden using Builder#setPhysicalCameraKey. The respective value of such request key can be obtained by calling Builder#getPhysicalCameraKey. Capture requests that contain individual physical device requests must be built via Set).
HAL Implementation Details
Vendor tags can be listed here. Vendor tag metadata should also use the extensions C api (refer to android.hardware.camera.device.V3_4.CaptureRequest.physicalCameraSettings for more details). Setting/getting vendor tags will be checked against the metadata vendor extensions API and not against this field. The HAL must not consume any request tags in the session parameters that are not listed either here or in the vendor tag list. There should be no overlap between this set of keys and the available session keys CameraCharacteristics#getAvailableSessionKeys along with any other controls that can have impact on the dual-camera sync. The public camera2 API will always make the vendor tags visible via CameraCharacteristics#getAvailablePhysicalCameraRequestKeys.
android.request.characteristicKeysNeedingPermission | int32 x n [hidden] [legacy] | A list of camera characteristics keys that are only available in case the camera client has camera permission. |  |  | 3.4 |
Details
The entry contains a subset of CameraCharacteristics#getKeys that require camera clients to acquire the permission#CAMERA permission before calling CameraManager#getCameraCharacteristics. If the permission is not held by the camera client, then the values of the repsective properties will not be present in CameraCharacteristics.
HAL Implementation Details
Do not set this property directly, camera service will overwrite any previous values.
dynamic
Property Name | Type | Description | Units | Range | Initial HIDL HAL version | Tags
android.request.frameCount | int32 [hidden] [deprecated] | A frame counter set by the framework. This value monotonically increases with every new result (that is, each new result has a unique frameCount value). | count of frames | Deprecated. Do not use. > 0 | 3.2 |
Details
Reset on release()
android.request.id | int32 [hidden] | An application-specified ID for the current request. Must be maintained unchanged in output frame | arbitrary integer assigned by application | Any int | 3.2 | V1
android.request.metadataMode | byte [system] NONE (v3.2) No metadata should be produced on output, except for application-bound buffer data. If no application-bound streams exist, no frame should be placed in the output frame queue. If such streams exist, a frame should be placed on the output queue with null metadata but with the necessary output buffer information. Timestamp information should still be included with any output stream buffers FULL (v3.2) All metadata should be produced. Statistics will only be produced if they are separately enabled | How much metadata to produce on output |  |  | 3.2 | FUTURE
android.request.outputStreams | int32 x n [system] [deprecated] | Lists which camera output streams image data from this capture must be sent to | List of camera stream IDs | Deprecated. Do not use. List must only include streams that have been created | 3.2 | HAL2
Details
If no output streams are listed, then the image data should simply be discarded. The image data must still be captured for metadata and statistics production, and the lens and flash must operate as requested.
android.request.pipelineDepth | byte [public] [legacy] | Specifies the number of pipeline stages the frame went through from when it was exposed to when the final completed result was available to the framework. |  | <= android.request.pipelineMaxDepth | 3.2 |
Details
Depending on what settings are used in the request, and what streams are configured, the data may undergo less processing, and some pipeline stages skipped. See android.request.pipelineMaxDepth for more details.
HAL Implementation Details
This value must always represent the accurate count of how many pipeline stages were actually used.
scaler
controls
Property Name | Type | Description | Units | Range | Initial HIDL HAL version | Tags
android.scaler.cropRegion | int32 x 4 [public as rectangle] [legacy] | The desired region of the sensor to read out for this capture. | Pixel coordinates relative to android.sensor.info.activeArraySize or android.sensor.info.preCorrectionActiveArraySize depending on distortion correction capability and mode |  | 3.2 | BC
Details
This control can be used to implement digital zoom. For devices not supporting android.distortionCorrection.mode control, the coordinate system always follows that of android.sensor.info.activeArraySize, with `(0, 0)` being the top-left pixel of the active array. For devices supporting android.distortionCorrection.mode control, the coordinate system depends on the mode being set. When the distortion correction mode is OFF, the coordinate system follows android.sensor.info.preCorrectionActiveArraySize, with `(0, 0)` being the top-left pixel of the pre-correction active array. When the distortion correction mode is not OFF, the coordinate system follows android.sensor.info.activeArraySize, with `(0, 0)` being the top-left pixel of the active array. Output streams use this rectangle to produce their output, cropping to a smaller region if necessary to maintain the stream's aspect ratio, then scaling the sensor input to match the output's configured resolution. The crop region is applied after the RAW to other color space (e.g. YUV) conversion. Since raw streams (e.g. RAW16) don't have the conversion stage, they are not croppable. The crop region will be ignored by raw streams. For non-raw streams, any additional per-stream cropping will be done to maximize the final pixel area of the stream. For example, if the crop region is set to a 4:3 aspect ratio, then 4:3 streams will use the exact crop region. 16:9 streams will further crop vertically (letterbox). Conversely, if the crop region is set to a 16:9, then 4:3 outputs will crop horizontally (pillarbox), and 16:9 streams will match exactly. These additional crops will be centered within the crop region. To illustrate, here are several scenarios of different crop regions and output streams, for a hypothetical camera device with an active array of size `(2000,1500)`. Note that several of these examples use non-centered crop regions for ease of illustration; such regions are only supported on devices with FREEFORM capability (android.scaler.croppingType `== FREEFORM`), but this does not affect the way the crop rules work otherwise. Camera Configuration: Active array size: `2000x1500` (3 MP, 4:3 aspect ratio) Output stream #1: `640x480` (VGA, 4:3 aspect ratio) Output stream #2: `1280x720` (720p, 16:9 aspect ratio) Case #1: 4:3 crop region with 2x digital zoom Crop region: `Rect(500, 375, 1500, 1125) // (left, top, right, bottom)` `640x480` stream source area: `(500, 375, 1500, 1125)` (equal to crop region) `1280x720` stream source area: `(500, 469, 1500, 1031)` (letterboxed) Case #2: 16:9 crop region with ~1.5x digital zoom. Crop region: `Rect(500, 375, 1833, 1125)` `640x480` stream source area: `(666, 375, 1666, 1125)` (pillarboxed) `1280x720` stream source area: `(500, 375, 1833, 1125)` (equal to crop region) Case #3: 1:1 crop region with ~2.6x digital zoom. Crop region: `Rect(500, 375, 1250, 1125)` `640x480` stream source area: `(500, 469, 1250, 1031)` (letterboxed) `1280x720` stream source area: `(500, 543, 1250, 957)` (letterboxed) Case #4: Replace `640x480` stream with `1024x1024` stream, with 4:3 crop region: Crop region: `Rect(500, 375, 1500, 1125)` `1024x1024` stream source area: `(625, 375, 1375, 1125)` (pillarboxed) `1280x720` stream source area: `(500, 469, 1500, 1031)` (letterboxed) Note that in this case, neither of the two outputs is a subset of the other, with each containing image data the other doesn't have. If the coordinate system is android.sensor.info.activeArraySize, the width and height of the crop region cannot be set to be smaller than `floor( activeArraySize.width / android.scaler.availableMaxDigitalZoom )` and `floor( activeArraySize.height / android.scaler.availableMaxDigitalZoom )`, respectively. If the coordinate system is android.sensor.info.preCorrectionActiveArraySize, the width and height of the crop region cannot be set to be smaller than `floor( preCorrectionActiveArraySize.width / android.scaler.availableMaxDigitalZoom )` and `floor( preCorrectionActiveArraySize.height / android.scaler.availableMaxDigitalZoom )`, respectively. The camera device may adjust the crop region to account for rounding and other hardware requirements; the final crop region used will be included in the output capture result. The camera sensor output aspect ratio depends on factors such as output stream combination and android.control.aeTargetFpsRange, and shouldn't be adjusted by using this control. And the camera device will treat different camera sensor output sizes (potentially with in-sensor crop) as the same crop of android.sensor.info.activeArraySize. As a result, the application shouldn't assume the maximum crop region always maps to the same aspect ratio or field of view for the sensor output. Starting from API level 30, it's strongly recommended to use android.control.zoomRatio to take advantage of better support for zoom with logical multi-camera. The benefits include better precision with optical-digital zoom combination, and ability to do zoom-out from 1.0x. When using android.control.zoomRatio for zoom, the crop region in the capture request should be left as the default activeArray size. The coordinate system is post-zoom, meaning that the activeArraySize or preCorrectionActiveArraySize covers the camera device's field of view "after" zoom. See android.control.zoomRatio for details.
HAL Implementation Details
The output streams must maintain square pixels at all times, no matter what the relative aspect ratios of the crop region and the stream are. Negative values for corner are allowed for raw output if full pixel array is larger than active pixel array. Width and height may be rounded to nearest larger supportable width, especially for raw output, where only a few fixed scales may be possible. For a set of output streams configured, if the sensor output is cropped to a smaller size than pre-correction active array size, the HAL need follow below cropping rules: The HAL need to handle the cropRegion as if the sensor crop size is the effective pre-correction active array size. More specifically, the HAL must transform the request cropRegion from android.sensor.info.preCorrectionActiveArraySize to the sensor cropped pixel area size in this way: If android.control.zoomRatio is set to value x, scale the requested cropRegion with 1.0/x in relation to its center as the origin. For example, say the requested cropRegion is (crX, crY, crWidth, crHeight), override it with `crX' = crX + crWidth * (1.0 - 1.0 / x) / 2`, `crY' = crY + crHeight * (1.0 - 1.0 / x) / 2`, `crWidth' = crWidth / x`, and `crHeight' = crHeight / x`. Translate the requested cropRegion w.r.t., the left top corner of the sensor cropped pixel area by (tx, ty), where `ty = sensorCrop.top * (sensorCrop.height / preCorrectionActiveArraySize.height)` and `tx = sensorCrop.left * (sensorCrop.width / preCorrectionActiveArraySize.width)`. The (sensorCrop.top, sensorCrop.left) is the coordinate based off the android.sensor.info.activeArraySize. Scale the width and height of requested cropRegion with scaling factor of sensorCrop.width/preCorrectionActiveArraySize.width and sensorCrop.height/preCorrectionActiveArraySize.height respectively. Once this new cropRegion is calculated, the HAL must use this region to crop the image with regard to the sensor crop size (effective pre-correction active array size). The HAL still need follow the general cropping rule for this new cropRegion and effective pre-correction active array size. The HAL must report the cropRegion with regard to android.sensor.info.preCorrectionActiveArraySize. The HAL need convert the new cropRegion generated above w.r.t., full pre-correction active array size. The reported cropRegion may be slightly different with the requested cropRegion since the HAL may adjust the crop region to account for rounding, conversion error, or other hardware limitations. If android.control.zoomRatio is supported by the HAL, the HAL must report the zoom ratio via android.control.zoomRatio, and change the coordinate system such that android.sensor.info.preCorrectionActiveArraySize or android.sensor.info.activeArraySize(depending on whether android.distortionCorrection.mode is supported) is used to represent the camera field-of-view after zoom. see android.control.zoomRatio for details. HAL2.x uses only (x, y, width)
android.scaler.rotateAndCrop | byte [hidden] NONE (v3.5) No rotate and crop is applied. Processed outputs are in the sensor orientation. 90 (v3.5) Processed images are rotated by 90 degrees clockwise, and then cropped to the original aspect ratio. 180 (v3.5) Processed images are rotated by 180 degrees. Since the aspect ratio does not change, no cropping is performed. 270 (v3.5) Processed images are rotated by 270 degrees clockwise, and then cropped to the original aspect ratio. AUTO (v3.5) The camera API automatically selects the best concrete value for rotate-and-crop based on the application's support for resizability and the current multi-window mode. If the application does not support resizing but the display mode for its main Activity is not in a typical orientation, the camera API will set `ROTATE_AND_CROP_90` or some other supported rotation value, depending on device configuration, to ensure preview and captured images are correctly shown to the user. Otherwise, `ROTATE_AND_CROP_NONE` will be selected. When a value other than NONE is selected, several metadata fields will also be parsed differently to ensure that coordinates are correctly handled for features like drawing face detection boxes or passing in tap-to-focus coordinates. The camera API will convert positions in the active array coordinate system to/from the cropped-and-rotated coordinate system to make the operation transparent for applications. No coordinate mapping will be done when the application selects a non-AUTO mode. | Whether a rotation-and-crop operation is applied to processed outputs from the camera. |  | android.scaler.availableRotateAndCropModes | 3.5 |
Details
This control is primarily intended to help camera applications with no support for multi-window modes to work correctly on devices where multi-window scenarios are unavoidable, such as foldables or other devices with variable display geometry or more free-form window placement (such as laptops, which often place portrait-orientation apps in landscape with pillarboxing). If supported, the default value is `ROTATE_AND_CROP_AUTO`, which allows the camera API to enable backwards-compatibility support for applications that do not support resizing / multi-window modes, when the device is in fact in a multi-window mode (such as inset portrait on laptops, or on a foldable device in some fold states). In addition, `ROTATE_AND_CROP_NONE` and `ROTATE_AND_CROP_90` will always be available if this control is supported by the device. If not supported, devices API level 30 or higher will always list only `ROTATE_AND_CROP_NONE`. When `CROP_AUTO` is in use, and the camera API activates backward-compatibility mode, several metadata fields will also be parsed differently to ensure that coordinates are correctly handled for features like drawing face detection boxes or passing in tap-to-focus coordinates. The camera API will convert positions in the active array coordinate system to/from the cropped-and-rotated coordinate system to make the operation transparent for applications. The following controls are affected: android.control.aeRegions android.control.afRegions android.control.awbRegions android.statistics.faces Capture results will contain the actual value selected by the API; `ROTATE_AND_CROP_AUTO` will never be seen in a capture result. Applications can also select their preferred cropping mode, either to opt out of the backwards-compatibility treatment, or to use the cropping feature themselves as needed. In this case, no coordinate translation will be done automatically, and all controls will continue to use the normal active array coordinates. Cropping and rotating is done after the application of digital zoom (via either android.scaler.cropRegion or android.control.zoomRatio), but before each individual output is further cropped and scaled. It only affects processed outputs such as YUV, PRIVATE, and JPEG. It has no effect on RAW outputs. When `CROP_90` or `CROP_270` are selected, there is a significant loss to the field of view. For example, with a 4:3 aspect ratio output of 1600x1200, `CROP_90` will still produce 1600x1200 output, but these buffers are cropped from a vertical 3:4 slice at the center of the 4:3 area, then rotated to be 4:3, and then upscaled to 1600x1200. Only 56.25% of the original FOV is still visible. In general, for an aspect ratio of `w:h`, the crop and rotate operation leaves `(h/w)^2` of the field of view visible. For 16:9, this is ~31.6%. As a visual example, the figure below shows the effect of `ROTATE_AND_CROP_90` on the outputs for the following parameters: Sensor active array: `2000x1500` Crop region: top-left: `(500, 375)`, size: `(1000, 750)` (4:3 aspect ratio) Output streams: YUV `640x480` and YUV `1280x720` `ROTATE_AND_CROP_90` With these settings, the regions of the active array covered by the output streams are: 640x480 stream crop: top-left: `(219, 375)`, size: `(562, 750)` 1280x720 stream crop: top-left: `(289, 375)`, size: `(422, 750)` Since the buffers are rotated, the buffers as seen by the application are: 640x480 stream: top-left: `(781, 375)` on active array, size: `(640, 480)`, downscaled 1.17x from sensor pixels 1280x720 stream: top-left: `(711, 375)` on active array, size: `(1280, 720)`, upscaled 1.71x from sensor pixels
HAL Implementation Details
Not ready for use in Android 11. ROTATE_AND_CROP_AUTO will never be sent to the HAL, though it must be set as the default value in all the capture request templates by the HAL. The camera service will translate AUTO to a specific rotation value based on the current application's multi-window state and its support of resizability. The HAL also does not need to consider coordinate transforms for ROTATE_AND_CROP - all capture request and result fields should be kept in the active array coordinate frame. Any translation required to implement ROTATE_AND_CROP_AUTO will be handled by the camera service.
static
Property Name | Type | Description | Units | Range | Initial HIDL HAL version | Tags
android.scaler.availableFormats | int32 x n [hidden as imageFormat] [deprecated] RAW16 (v3.2) [optional] 0x20 RAW16 is a standard, cross-platform format for raw image buffers with 16-bit pixels. Buffers of this format are typically expected to have a Color Filter Array (CFA) layout, which is given in android.sensor.info.colorFilterArrangement. Sensors with CFAs that are not representable by a format in android.sensor.info.colorFilterArrangement should not use this format. Buffers of this format will also follow the constraints given for RAW_OPAQUE buffers, but with relaxed performance constraints. This format is intended to give users access to the full contents of the buffers coming directly from the image sensor prior to any cropping or scaling operations, and all coordinate systems for metadata used for this format are relative to the size of the active region of the image sensor before any geometric distortion correction has been applied (i.e. android.sensor.info.preCorrectionActiveArraySize). Supported dimensions for this format are limited to the full dimensions of the sensor (e.g. either android.sensor.info.pixelArraySize or android.sensor.info.preCorrectionActiveArraySize will be the only supported output size). See android.scaler.availableInputOutputFormatsMap for the full set of performance guarantees. RAW_OPAQUE (v3.2) [optional] 0x24 RAW_OPAQUE (or RAW_PRIVATE as referred in public API) is a format for raw image buffers coming from an image sensor. The actual structure of buffers of this format is platform-specific, but must follow several constraints: No image post-processing operations may have been applied to buffers of this type. These buffers contain raw image data coming directly from the image sensor. If a buffer of this format is passed to the camera device for reprocessing, the resulting images will be identical to the images produced if the buffer had come directly from the sensor and was processed with the same settings. The intended use for this format is to allow access to the native raw format buffers coming directly from the camera sensor without any additional conversions or decrease in framerate. See android.scaler.availableInputOutputFormatsMap for the full set of performance guarantees. YV12 (v3.2) [optional] 0x32315659 YCrCb 4:2:0 Planar YCrCb_420_SP (v3.2) [optional] 0x11 NV21 IMPLEMENTATION_DEFINED (v3.2) 0x22 System internal format, not application-accessible YCbCr_420_888 (v3.2) 0x23 Flexible YUV420 Format BLOB (v3.2) 0x21 JPEG format RAW10 (v3.4) 0x25 RAW10 RAW12 (v3.4) 0x26 RAW12 Y8 (v3.4) 0x20203859 Y8 | The list of image formats that are supported by this camera device for output streams. |  | Deprecated. Do not use. | 3.2 | BC
Details
All camera devices will support JPEG and YUV_420_888 formats. When set to YUV_420_888, application can access the YUV420 data directly.
HAL Implementation Details
These format values are from HAL_PIXEL_FORMAT_* in system/core/include/system/graphics.h. When IMPLEMENTATION_DEFINED is used, the platform gralloc module will select a format based on the usage flags provided by the camera HAL device and the other endpoint of the stream. It is usually used by preview and recording streams, where the application doesn't need access the image data. YCbCr_420_888 format must be supported by the HAL. When an image stream needs CPU/application direct access, this format will be used. For a MONOCHROME camera device, the pixel value of Cb and Cr planes is 128. The BLOB format must be supported by the HAL. This is used for the JPEG stream. A RAW_OPAQUE buffer should contain only pixel data. It is strongly recommended that any information used by the camera device when processing images is fully expressed by the result metadata for that image buffer.
android.scaler.availableJpegMinDurations | int64 x n [hidden] [deprecated] | The minimum frame duration that is supported for each resolution in android.scaler.availableJpegSizes. | Nanoseconds | Deprecated. Do not use. TODO: Remove property. | 3.2 | BC
Details
This corresponds to the minimum steady-state frame duration when only that JPEG stream is active and captured in a burst, with all processing (typically in android.*.mode) set to FAST. When multiple streams are configured, the minimum frame duration will be >= max(individual stream min durations)
android.scaler.availableJpegSizes | int32 x n x 2 [hidden as size] [deprecated] | The JPEG resolutions that are supported by this camera device. |  | Deprecated. Do not use. TODO: Remove property. | 3.2 | BC
Details
The resolutions are listed as `(width, height)` pairs. All camera devices will support sensor maximum resolution (defined by android.sensor.info.activeArraySize).
HAL Implementation Details
The HAL must include sensor maximum resolution (defined by android.sensor.info.activeArraySize), and should include half/quarter of sensor maximum resolution.
android.scaler.availableMaxDigitalZoom | float [public] [legacy] | The maximum ratio between both active area width and crop region width, and active area height and crop region height, for android.scaler.cropRegion. | Zoom scale factor | >=1 | 3.2 | BC
Details
This represents the maximum amount of zooming possible by the camera device, or equivalently, the minimum cropping window size. Crop regions that have a width or height that is smaller than this ratio allows will be rounded up to the minimum allowed size by the camera device. Starting from API level 30, when using android.control.zoomRatio to zoom in or out, the application must use android.control.zoomRatioRange to query both the minimum and maximum zoom ratio.
HAL Implementation Details
If the HAL supports android.control.zoomRatio, this value must be equal to the maximum supported zoomRatio specified in android.control.zoomRatioRange.
android.scaler.availableProcessedMinDurations | int64 x n [hidden] [deprecated] | For each available processed output size (defined in android.scaler.availableProcessedSizes), this property lists the minimum supportable frame duration for that size. | Nanoseconds | Deprecated. Do not use. | 3.2 | BC
Details
This should correspond to the frame duration when only that processed stream is active, with all processing (typically in android.*.mode) set to FAST. When multiple streams are configured, the minimum frame duration will be >= max(individual stream min durations).
android.scaler.availableProcessedSizes | int32 x n x 2 [hidden as size] [deprecated] | The resolutions available for use with processed output streams, such as YV12, NV12, and platform opaque YUV/RGB streams to the GPU or video encoders. |  | Deprecated. Do not use. | 3.2 | BC
Details
The resolutions are listed as `(width, height)` pairs. For a given use case, the actual maximum supported resolution may be lower than what is listed here, depending on the destination Surface for the image data. For example, for recording video, the video encoder chosen may have a maximum size limit (e.g. 1080p) smaller than what the camera (e.g. maximum resolution is 3264x2448) can provide. Please reference the documentation for the image data destination to check if it limits the maximum size for image data.
HAL Implementation Details
For FULL capability devices (`android.info.supportedHardwareLevel == FULL`), the HAL must include all JPEG sizes listed in android.scaler.availableJpegSizes and each below resolution if it is smaller than or equal to the sensor maximum resolution (if they are not listed in JPEG sizes already): 240p (320 x 240) 480p (640 x 480) 720p (1280 x 720) 1080p (1920 x 1080) For LIMITED capability devices (`android.info.supportedHardwareLevel == LIMITED`), the HAL only has to list up to the maximum video size supported by the devices.
android.scaler.availableRawMinDurations | int64 x n [system] [deprecated] | For each available raw output size (defined in android.scaler.availableRawSizes), this property lists the minimum supportable frame duration for that size. | Nanoseconds | Deprecated. Do not use. | 3.2 | BC
Details
Should correspond to the frame duration when only the raw stream is active. When multiple streams are configured, the minimum frame duration will be >= max(individual stream min durations)
android.scaler.availableRawSizes | int32 x n x 2 [system as size] [deprecated] | The resolutions available for use with raw sensor output streams, listed as width, height |  | Deprecated. Do not use. | 3.2 |
android.scaler.availableInputOutputFormatsMap | int32 [hidden as reprocessFormatsMap] | The mapping of image formats that are supported by this camera device for input streams, to their corresponding output formats. |  |  | 3.2 | REPROC
Details
All camera devices with at least 1 android.request.maxNumInputStreams will have at least one available input format. The camera device will support the following map of formats, if its dependent capability (android.request.availableCapabilities) is supported:
Input Format | Output Format | Capability
--- | --- | ---
ImageFormat#PRIVATE | ImageFormat#JPEG | PRIVATE_REPROCESSING
ImageFormat#PRIVATE | ImageFormat#YUV_420_888 | PRIVATE_REPROCESSING
ImageFormat#YUV_420_888 | ImageFormat#JPEG | YUV_REPROCESSING
ImageFormat#YUV_420_888 | ImageFormat#YUV_420_888 | YUV_REPROCESSING
PRIVATE refers to a device-internal format that is not directly application-visible. A PRIVATE input surface can be acquired by ImageReader#newInstance with ImageFormat#PRIVATE as the format. For a PRIVATE_REPROCESSING-capable camera device, using the PRIVATE format as either input or output will never hurt maximum frame rate (i.e. getOutputStallDuration(ImageFormat.PRIVATE, size) is always 0), Attempting to configure an input stream with output streams not listed as available in this map is not valid. Additionally, if the camera device is MONOCHROME with Y8 support, it will also support the following map of formats if its dependent capability (android.request.availableCapabilities) is supported:
Input Format | Output Format | Capability
--- | --- | ---
ImageFormat#PRIVATE | ImageFormat#Y8 | PRIVATE_REPROCESSING
ImageFormat#Y8 | ImageFormat#JPEG | YUV_REPROCESSING
ImageFormat#Y8 | ImageFormat#Y8 | YUV_REPROCESSING
HAL Implementation Details
For the formats, see `system/core/include/system/graphics.h` for a definition of the image format enumerations. The PRIVATE format refers to the HAL_PIXEL_FORMAT_IMPLEMENTATION_DEFINED format. The HAL could determine the actual format by using the gralloc usage flags. For ZSL use case in particular, the HAL could choose appropriate format (partially processed YUV or RAW based format) by checking the format and GRALLOC_USAGE_HW_CAMERA_ZSL. See camera3.h for more details. This value is encoded as a variable-size array-of-arrays. The inner array always contains `[format, length, ...]` where `...` has `length` elements. An inner array is followed by another inner array if the total metadata entry size hasn't yet been exceeded. A code sample to read/write this encoding (with a device that supports reprocessing IMPLEMENTATION_DEFINED to YUV_420_888, and JPEG, and reprocessing YUV_420_888 to YUV_420_888 and JPEG):
    // reading
    int32_t* contents = &entry.i32[0];
    for (size_t i = 0; i < entry.count; ) {
        int32_t format = contents[i++];
        int32_t length = contents[i++];
        int32_t output_formats[length];
        memcpy(&output_formats[0], &contents[i],
               length * sizeof(int32_t));
        i += length;
    }

    // writing (static example, PRIVATE_REPROCESSING + YUV_REPROCESSING)
    int32_t[] contents = {
      IMPLEMENTATION_DEFINED, 2, YUV_420_888, BLOB,
      YUV_420_888, 2, YUV_420_888, BLOB,
    };
    update_camera_metadata_entry(metadata, index, &contents[0],
          sizeof(contents)/sizeof(contents[0]), &updated_entry);
If the HAL claims to support any of the capabilities listed in the above details, then it must also support all the input-output combinations listed for that capability. It can optionally support additional formats if it so chooses.
android.scaler.availableStreamConfigurations | int32 x n x 4 [ndk_public as streamConfiguration] [legacy] OUTPUT (v3.2) INPUT (v3.2) | The available stream configurations that this camera device supports (i.e. format, width, height, output/input stream). |  |  | 3.2 |
Details
The configurations are listed as `(format, width, height, input?)` tuples. For a given use case, the actual maximum supported resolution may be lower than what is listed here, depending on the destination Surface for the image data. For example, for recording video, the video encoder chosen may have a maximum size limit (e.g. 1080p) smaller than what the camera (e.g. maximum resolution is 3264x2448) can provide. Please reference the documentation for the image data destination to check if it limits the maximum size for image data. Not all output formats may be supported in a configuration with an input stream of a particular format. For more details, see android.scaler.availableInputOutputFormatsMap. The following table describes the minimum required output stream configurations based on the hardware level (android.info.supportedHardwareLevel):
Format | Size | Hardware Level | Notes
--- | --- | --- | ---
JPEG | android.sensor.info.activeArraySize | Any |
JPEG | 1920x1080 (1080p) | Any | if 1080p <= activeArraySize
JPEG | 1280x720 (720) | Any | if 720p <= activeArraySize
JPEG | 640x480 (480p) | Any | if 480p <= activeArraySize
JPEG | 320x240 (240p) | Any | if 240p <= activeArraySize
YUV_420_888 | all output sizes available for JPEG | FULL |
YUV_420_888 | all output sizes available for JPEG, up to the maximum video size | LIMITED |
IMPLEMENTATION_DEFINED | same as YUV_420_888 | Any |
Refer to android.request.availableCapabilities for additional mandatory stream configurations on a per-capability basis. Exception on 176x144 (QCIF) resolution: camera devices usually have a fixed capability for downscaling from larger resolution to smaller, and the QCIF resolution sometimes is not fully supported due to this limitation on devices with high-resolution image sensors. Therefore, trying to configure a QCIF resolution stream together with any other stream larger than 1920x1080 resolution (either width or height) might not be supported, and capture session creation will fail if it is not.
HAL Implementation Details
It is recommended (but not mandatory) to also include half/quarter of sensor maximum resolution for JPEG formats (regardless of hardware level). (The following is a rewording of the above required table): For JPEG format, the sizes may be restricted by below conditions: The HAL may choose the aspect ratio of each Jpeg size to be one of well known ones (e.g. 4:3, 16:9, 3:2 etc.). If the sensor maximum resolution (defined by android.sensor.info.activeArraySize) has an aspect ratio other than these, it does not have to be included in the supported JPEG sizes. Some hardware JPEG encoders may have pixel boundary alignment requirements, such as the dimensions being a multiple of 16. Therefore, the maximum JPEG size may be smaller than sensor maximum resolution. However, the largest JPEG size must be as close as possible to the sensor maximum resolution given above constraints. It is required that after aspect ratio adjustments, additional size reduction due to other issues must be less than 3% in area. For example, if the sensor maximum resolution is 3280x2464, if the maximum JPEG size has aspect ratio 4:3, the JPEG encoder alignment requirement is 16, the maximum JPEG size will be 3264x2448. For FULL capability devices (`android.info.supportedHardwareLevel == FULL`), the HAL must include all YUV_420_888 sizes that have JPEG sizes listed here as output streams. It must also include each below resolution if it is smaller than or equal to the sensor maximum resolution (for both YUV_420_888 and JPEG formats), as output streams: 240p (320 x 240) 480p (640 x 480) 720p (1280 x 720) 1080p (1920 x 1080) For LIMITED capability devices (`android.info.supportedHardwareLevel == LIMITED`), the HAL only has to list up to the maximum video size supported by the device. Regardless of hardware level, every output resolution available for YUV_420_888 must also be available for IMPLEMENTATION_DEFINED. This supercedes the following fields, which are now deprecated: availableFormats available[Processed,Raw,Jpeg]Sizes
android.scaler.availableMinFrameDurations | int64 x 4 x n [ndk_public as streamConfigurationDuration] [legacy] | This lists the minimum frame duration for each format/size combination. | (format, width, height, ns) x n |  | 3.2 | V1
Details
This should correspond to the frame duration when only that stream is active, with all processing (typically in android.*.mode) set to either OFF or FAST. When multiple streams are used in a request, the minimum frame duration will be max(individual stream min durations). The minimum frame duration of a stream (of a particular format, size) is the same regardless of whether the stream is input or output. See android.sensor.frameDuration and android.scaler.availableStallDurations for more details about calculating the max frame rate.
android.scaler.availableStallDurations | int64 x 4 x n [ndk_public as streamConfigurationDuration] [legacy] | This lists the maximum stall duration for each output format/size combination. | (format, width, height, ns) x n |  | 3.2 | V1
Details
A stall duration is how much extra time would get added to the normal minimum frame duration for a repeating request that has streams with non-zero stall. For example, consider JPEG captures which have the following characteristics: JPEG streams act like processed YUV streams in requests for which they are not included; in requests in which they are directly referenced, they act as JPEG streams. This is because supporting a JPEG stream requires the underlying YUV data to always be ready for use by a JPEG encoder, but the encoder will only be used (and impact frame duration) on requests that actually reference a JPEG stream. The JPEG processor can run concurrently to the rest of the camera pipeline, but cannot process more than 1 capture at a time. In other words, using a repeating YUV request would result in a steady frame rate (let's say it's 30 FPS). If a single JPEG request is submitted periodically, the frame rate will stay at 30 FPS (as long as we wait for the previous JPEG to return each time). If we try to submit a repeating YUV + JPEG request, then the frame rate will drop from 30 FPS. In general, submitting a new request with a non-0 stall time stream will not cause a frame rate drop unless there are still outstanding buffers for that stream from previous requests. Submitting a repeating request with streams (call this `S`) is the same as setting the minimum frame duration from the normal minimum frame duration corresponding to `S`, added with the maximum stall duration for `S`. If interleaving requests with and without a stall duration, a request will stall by the maximum of the remaining times for each can-stall stream with outstanding buffers. This means that a stalling request will not have an exposure start until the stall has completed. This should correspond to the stall duration when only that stream is active, with all processing (typically in android.*.mode) set to FAST or OFF. Setting any of the processing modes to HIGH_QUALITY effectively results in an indeterminate stall duration for all streams in a request (the regular stall calculation rules are ignored). The following formats may always have a stall duration: ImageFormat#JPEG ImageFormat#RAW_SENSOR The following formats will never have a stall duration: ImageFormat#YUV_420_888 ImageFormat#RAW10 ImageFormat#RAW12 ImageFormat#Y8 All other formats may or may not have an allowed stall duration on a per-capability basis; refer to android.request.availableCapabilities for more details. See android.sensor.frameDuration for more information about calculating the max frame rate (absent stalls).
HAL Implementation Details
If possible, it is recommended that all non-JPEG formats (such as RAW16) should not have a stall duration. RAW10, RAW12, RAW_OPAQUE and IMPLEMENTATION_DEFINED must not have stall durations.
android.scaler.streamConfigurationMap | int32 [java_public as streamConfigurationMap] [synthetic] [legacy] | The available stream configurations that this camera device supports; also includes the minimum frame durations and the stall durations for each format/size combination. |  |  | 3.2 |
Details
All camera devices will support sensor maximum resolution (defined by android.sensor.info.activeArraySize) for the JPEG format. For a given use case, the actual maximum supported resolution may be lower than what is listed here, depending on the destination Surface for the image data. For example, for recording video, the video encoder chosen may have a maximum size limit (e.g. 1080p) smaller than what the camera (e.g. maximum resolution is 3264x2448) can provide. Please reference the documentation for the image data destination to check if it limits the maximum size for image data. The following table describes the minimum required output stream configurations based on the hardware level (android.info.supportedHardwareLevel):
Format | Size | Hardware Level | Notes
--- | --- | --- | ---
ImageFormat#JPEG | android.sensor.info.activeArraySize (*1) | Any |
ImageFormat#JPEG | 1920x1080 (1080p) | Any | if 1080p <= activeArraySize
ImageFormat#JPEG | 1280x720 (720p) | Any | if 720p <= activeArraySize
ImageFormat#JPEG | 640x480 (480p) | Any | if 480p <= activeArraySize
ImageFormat#JPEG | 320x240 (240p) | Any | if 240p <= activeArraySize
ImageFormat#YUV_420_888 | all output sizes available for JPEG | FULL |
ImageFormat#YUV_420_888 | all output sizes available for JPEG, up to the maximum video size | LIMITED |
ImageFormat#PRIVATE | same as YUV_420_888 | Any |
Refer to android.request.availableCapabilities and CameraDevice#createCaptureSession for additional mandatory stream configurations on a per-capability basis. *1: For JPEG format, the sizes may be restricted by below conditions: The HAL may choose the aspect ratio of each Jpeg size to be one of well known ones (e.g. 4:3, 16:9, 3:2 etc.). If the sensor maximum resolution (defined by android.sensor.info.activeArraySize) has an aspect ratio other than these, it does not have to be included in the supported JPEG sizes. Some hardware JPEG encoders may have pixel boundary alignment requirements, such as the dimensions being a multiple of 16. Therefore, the maximum JPEG size may be smaller than sensor maximum resolution. However, the largest JPEG size will be as close as possible to the sensor maximum resolution given above constraints. It is required that after aspect ratio adjustments, additional size reduction due to other issues must be less than 3% in area. For example, if the sensor maximum resolution is 3280x2464, if the maximum JPEG size has aspect ratio 4:3, and the JPEG encoder alignment requirement is 16, the maximum JPEG size will be 3264x2448. Exception on 176x144 (QCIF) resolution: camera devices usually have a fixed capability on downscaling from larger resolution to smaller ones, and the QCIF resolution can sometimes not be fully supported due to this limitation on devices with high-resolution image sensors. Therefore, trying to configure a QCIF resolution stream together with any other stream larger than 1920x1080 resolution (either width or height) might not be supported, and capture session creation will fail if it is not.
HAL Implementation Details
Do not set this property directly (it is synthetic and will not be available at the HAL layer); set the android.scaler.availableStreamConfigurations instead. Not all output formats may be supported in a configuration with an input stream of a particular format. For more details, see android.scaler.availableInputOutputFormatsMap. It is recommended (but not mandatory) to also include half/quarter of sensor maximum resolution for JPEG formats (regardless of hardware level). (The following is a rewording of the above required table): The HAL must include sensor maximum resolution (defined by android.sensor.info.activeArraySize). For FULL capability devices (`android.info.supportedHardwareLevel == FULL`), the HAL must include all YUV_420_888 sizes that have JPEG sizes listed here as output streams. It must also include each below resolution if it is smaller than or equal to the sensor maximum resolution (for both YUV_420_888 and JPEG formats), as output streams: 240p (320 x 240) 480p (640 x 480) 720p (1280 x 720) 1080p (1920 x 1080) For LIMITED capability devices (`android.info.supportedHardwareLevel == LIMITED`), the HAL only has to list up to the maximum video size supported by the device. Regardless of hardware level, every output resolution available for YUV_420_888 must also be available for IMPLEMENTATION_DEFINED. This supercedes the following fields, which are now deprecated: availableFormats available[Processed,Raw,Jpeg]Sizes
android.scaler.croppingType | byte [public] [legacy] CENTER_ONLY (v3.2) The camera device only supports centered crop regions. FREEFORM (v3.2) The camera device supports arbitrarily chosen crop regions. | The crop type that this camera device supports. |  |  | 3.2 |
Details
When passing a non-centered crop region (android.scaler.cropRegion) to a camera device that only supports CENTER_ONLY cropping, the camera device will move the crop region to the center of the sensor active array (android.sensor.info.activeArraySize) and keep the crop region width and height unchanged. The camera device will return the final used crop region in metadata result android.scaler.cropRegion. Camera devices that support FREEFORM cropping will support any crop region that is inside of the active array. The camera device will apply the same crop region and return the final used crop region in capture result metadata android.scaler.cropRegion. Starting from API level 30, If the camera device supports FREEFORM cropping, in order to do FREEFORM cropping, the application must set android.control.zoomRatio to 1.0, and use android.scaler.cropRegion for zoom. To do CENTER_ONLY zoom, the application has below 2 options: Set android.control.zoomRatio to 1.0; adjust zoom by android.scaler.cropRegion. Adjust zoom by android.control.zoomRatio; use android.scaler.cropRegion to crop the field of view vertically (letterboxing) or horizontally (pillarboxing), but not windowboxing. Setting android.control.zoomRatio to values different than 1.0 and android.scaler.cropRegion to be windowboxing at the same time is undefined behavior. LEGACY capability devices will only support CENTER_ONLY cropping.
HAL Implementation Details
If the HAL supports android.control.zoomRatio, this tag must be set to CENTER_ONLY.
android.scaler.availableRecommendedStreamConfigurations | int32 x n x 5 [ndk_public as recommendedStreamConfiguration] PREVIEW (v3.4) 0x0 Preview must only include non-stalling processed stream configurations with output formats like ImageFormat#YUV_420_888, ImageFormat#PRIVATE, etc. RECORD (v3.4) 0x1 Video record must include stream configurations that match the advertised supported media profiles CamcorderProfile with IMPLEMENTATION_DEFINED format. VIDEO_SNAPSHOT (v3.4) 0x2 Video snapshot must include stream configurations at least as big as the maximum RECORD resolutions and only with JPEG output format. Additionally the configurations shouldn't cause preview glitches and also be able to run at 30 fps. SNAPSHOT (v3.4) 0x3 Recommended snapshot stream configurations must include at least one with size close to android.sensor.info.activeArraySize and JPEG output format. Taking into account restrictions on aspect ratio, alignment etc. the area of the maximum suggested size shouldn’t be less than 97% of the sensor array size area. ZSL (v3.4) 0x4 If supported, recommended input stream configurations must only be advertised with ZSL along with other processed and/or stalling output formats. RAW (v3.4) 0x5 If supported, recommended raw stream configurations must only include RAW based output formats. LOW_LATENCY_SNAPSHOT (v3.4) 0x6 If supported, the recommended low latency stream configurations must have end-to-end latency that does not exceed 200 ms. under standard operating conditions (reasonable light levels, not loaded system) and using template TEMPLATE_STILL_CAPTURE. This is primarily for listing configurations for the JPEG output format however other supported output formats can be added as well. PUBLIC_END (v3.4) 0x7 VENDOR_START (v3.4) 0x18 Vendor defined use cases. These depend on the vendor implementation. | Recommended stream configurations for common client use cases. |  |  | 3.4 |
Details
Optional subset of the android.scaler.availableStreamConfigurations that contains similar tuples listed as (i.e. width, height, format, output/input stream, usecase bit field). Camera devices will be able to suggest particular stream configurations which are power and performance efficient for specific use cases. For more information about retrieving the suggestions see CameraCharacteristics#getRecommendedStreamConfigurationMap.
HAL Implementation Details
There are some requirements that need to be considered regarding the usecases and the suggested configurations: If android.scaler.availableRecommendedStreamConfigurations is set, then recommended stream configurations must be present for all mandatory usecases PREVIEW, SNAPSHOT, RECORD, VIDEO_SNAPSHOT. ZSL and RAW are required depending on device capabilities see android.request.availableCapabilities. Non-existing usecases and non-vendor usecases within the range (RAW : VENDOR_START] are prohibited as well as stream configurations not present in the exhaustive android.scaler.availableStreamConfigurations list. For example, in case the camera device supports only 4K and 1080p and both resolutions are recommended for the mandatory usecases except preview which can run efficiently only on 1080p. The array may look like this: [3840, 2160, HAL_PIXEL_FORMAT_IMPLEMENTATION_DEFINED, ANDROID_SCALER_AVAILABLE_STREAM_CONFIGURATIONS_OUTPUT, (1<< ANDROID_SCALER_AVAILABLE_RECOMMENDED_STREAM_CONFIGURATIONS_RECORD | 1<< ANDROID_SCALER_AVAILABLE_RECOMMENDED_STREAM_CONFIGURATIONS_SNAPSHOT | 1<< ANDROID_SCALER_AVAILABLE_RECOMMENDED_STREAM_CONFIGURATIONS_VIDEO_SNAPSHOT), 1920, 1080, HAL_PIXEL_FORMAT_IMPLEMENTATION_DEFINED, ANDROID_SCALER_AVAILABLE_STREAM_CONFIGURATIONS_OUTPUT, (1<< ANDROID_SCALER_AVAILABLE_RECOMMENDED_STREAM_CONFIGURATIONS_PREVIEW | 1<< ANDROID_SCALER_AVAILABLE_RECOMMENDED_STREAM_CONFIGURATIONS_RECORD | 1<< ANDROID_SCALER_AVAILABLE_RECOMMENDED_STREAM_CONFIGURATIONS_SNAPSHOT | 1<< ANDROID_SCALER_AVAILABLE_RECOMMENDED_STREAM_CONFIGURATIONS_VIDEO_SNAPSHOT)]
android.scaler.availableRecommendedInputOutputFormatsMap | int32 [ndk_public as reprocessFormatsMap] | Recommended mappings of image formats that are supported by this camera device for input streams, to their corresponding output formats. |  |  | 3.4 | REPROC
Details
This is a recommended subset of the complete list of mappings found in android.scaler.availableInputOutputFormatsMap. The same requirements apply here as well. The list however doesn't need to contain all available and supported mappings. Instead of this developers must list only recommended and efficient entries. If set, the information will be available in the ZERO_SHUTTER_LAG recommended stream configuration see CameraCharacteristics#getRecommendedStreamConfigurationMap.
HAL Implementation Details
For a code sample of the required data encoding please check android.scaler.availableInputOutputFormatsMap.
android.scaler.mandatoryStreamCombinations | int32 x n [java_public as mandatoryStreamCombination] [synthetic] [limited] | An array of mandatory stream combinations generated according to the camera device CameraCharacteristics#INFO_SUPPORTED_HARDWARE_LEVEL and CameraCharacteristics#REQUEST_AVAILABLE_CAPABILITIES. This is an app-readable conversion of the mandatory stream combination tables. |  |  | 3.2 |
Details
The array of combinations is generated according to the documented guideline based on specific device level and capabilities. Clients can use the array as a quick reference to find an appropriate camera stream combination. As per documentation, the stream combinations with given PREVIEW, RECORD and MAXIMUM resolutions and anything smaller from the list given by StreamConfigurationMap#getOutputSizes are guaranteed to work. For a physical camera not independently exposed in CameraManager#getCameraIdList, the mandatory stream combinations for that physical camera Id are also generated, so that the application can configure them as physical streams via the logical camera. The mandatory stream combination array will be {@code null} in case the device is not backward compatible.
HAL Implementation Details
Do not set this property directly (it is synthetic and will not be available at the HAL layer).
android.scaler.mandatoryConcurrentStreamCombinations | int32 x n [java_public as mandatoryStreamCombination] [synthetic] | An array of mandatory concurrent stream combinations. This is an app-readable conversion of the concurrent mandatory stream combination tables. |  |  | 3.2 |
Details
The array of combinations is generated according to the documented guideline for each device which has its Id present in the set returned by CameraManager#getConcurrentCameraIds. Clients can use the array as a quick reference to find an appropriate camera stream combination. The mandatory stream combination array will be {@code null} in case the device is not a part of at least one set of combinations returned by CameraManager#getConcurrentCameraIds.
HAL Implementation Details
Do not set this property directly (it is synthetic and will not be available at the HAL layer).
android.scaler.availableRotateAndCropModes | byte x n [hidden as enumList] list of enums | List of rotate-and-crop modes for android.scaler.rotateAndCrop that are supported by this camera device. |  | Any value listed in android.scaler.rotateAndCrop | 3.5 |
Details
This entry lists the valid modes for android.scaler.rotateAndCrop for this camera device. Starting at some future API level, all devices will list at least `ROTATE_AND_CROP_NONE`. Devices with support for rotate-and-crop will additionally list at least `ROTATE_AND_CROP_AUTO` and `ROTATE_AND_CROP_90`.
dynamic
Property Name | Type | Description | Units | Range | Initial HIDL HAL version | Tags
android.scaler.cropRegion | int32 x 4 [public as rectangle] [legacy] | The desired region of the sensor to read out for this capture. | Pixel coordinates relative to android.sensor.info.activeArraySize or android.sensor.info.preCorrectionActiveArraySize depending on distortion correction capability and mode |  | 3.2 | BC
Details
This control can be used to implement digital zoom. For devices not supporting android.distortionCorrection.mode control, the coordinate system always follows that of android.sensor.info.activeArraySize, with `(0, 0)` being the top-left pixel of the active array. For devices supporting android.distortionCorrection.mode control, the coordinate system depends on the mode being set. When the distortion correction mode is OFF, the coordinate system follows android.sensor.info.preCorrectionActiveArraySize, with `(0, 0)` being the top-left pixel of the pre-correction active array. When the distortion correction mode is not OFF, the coordinate system follows android.sensor.info.activeArraySize, with `(0, 0)` being the top-left pixel of the active array. Output streams use this rectangle to produce their output, cropping to a smaller region if necessary to maintain the stream's aspect ratio, then scaling the sensor input to match the output's configured resolution. The crop region is applied after the RAW to other color space (e.g. YUV) conversion. Since raw streams (e.g. RAW16) don't have the conversion stage, they are not croppable. The crop region will be ignored by raw streams. For non-raw streams, any additional per-stream cropping will be done to maximize the final pixel area of the stream. For example, if the crop region is set to a 4:3 aspect ratio, then 4:3 streams will use the exact crop region. 16:9 streams will further crop vertically (letterbox). Conversely, if the crop region is set to a 16:9, then 4:3 outputs will crop horizontally (pillarbox), and 16:9 streams will match exactly. These additional crops will be centered within the crop region. To illustrate, here are several scenarios of different crop regions and output streams, for a hypothetical camera device with an active array of size `(2000,1500)`. Note that several of these examples use non-centered crop regions for ease of illustration; such regions are only supported on devices with FREEFORM capability (android.scaler.croppingType `== FREEFORM`), but this does not affect the way the crop rules work otherwise. Camera Configuration: Active array size: `2000x1500` (3 MP, 4:3 aspect ratio) Output stream #1: `640x480` (VGA, 4:3 aspect ratio) Output stream #2: `1280x720` (720p, 16:9 aspect ratio) Case #1: 4:3 crop region with 2x digital zoom Crop region: `Rect(500, 375, 1500, 1125) // (left, top, right, bottom)` `640x480` stream source area: `(500, 375, 1500, 1125)` (equal to crop region) `1280x720` stream source area: `(500, 469, 1500, 1031)` (letterboxed) Case #2: 16:9 crop region with ~1.5x digital zoom. Crop region: `Rect(500, 375, 1833, 1125)` `640x480` stream source area: `(666, 375, 1666, 1125)` (pillarboxed) `1280x720` stream source area: `(500, 375, 1833, 1125)` (equal to crop region) Case #3: 1:1 crop region with ~2.6x digital zoom. Crop region: `Rect(500, 375, 1250, 1125)` `640x480` stream source area: `(500, 469, 1250, 1031)` (letterboxed) `1280x720` stream source area: `(500, 543, 1250, 957)` (letterboxed) Case #4: Replace `640x480` stream with `1024x1024` stream, with 4:3 crop region: Crop region: `Rect(500, 375, 1500, 1125)` `1024x1024` stream source area: `(625, 375, 1375, 1125)` (pillarboxed) `1280x720` stream source area: `(500, 469, 1500, 1031)` (letterboxed) Note that in this case, neither of the two outputs is a subset of the other, with each containing image data the other doesn't have. If the coordinate system is android.sensor.info.activeArraySize, the width and height of the crop region cannot be set to be smaller than `floor( activeArraySize.width / android.scaler.availableMaxDigitalZoom )` and `floor( activeArraySize.height / android.scaler.availableMaxDigitalZoom )`, respectively. If the coordinate system is android.sensor.info.preCorrectionActiveArraySize, the width and height of the crop region cannot be set to be smaller than `floor( preCorrectionActiveArraySize.width / android.scaler.availableMaxDigitalZoom )` and `floor( preCorrectionActiveArraySize.height / android.scaler.availableMaxDigitalZoom )`, respectively. The camera device may adjust the crop region to account for rounding and other hardware requirements; the final crop region used will be included in the output capture result. The camera sensor output aspect ratio depends on factors such as output stream combination and android.control.aeTargetFpsRange, and shouldn't be adjusted by using this control. And the camera device will treat different camera sensor output sizes (potentially with in-sensor crop) as the same crop of android.sensor.info.activeArraySize. As a result, the application shouldn't assume the maximum crop region always maps to the same aspect ratio or field of view for the sensor output. Starting from API level 30, it's strongly recommended to use android.control.zoomRatio to take advantage of better support for zoom with logical multi-camera. The benefits include better precision with optical-digital zoom combination, and ability to do zoom-out from 1.0x. When using android.control.zoomRatio for zoom, the crop region in the capture request should be left as the default activeArray size. The coordinate system is post-zoom, meaning that the activeArraySize or preCorrectionActiveArraySize covers the camera device's field of view "after" zoom. See android.control.zoomRatio for details.
HAL Implementation Details
The output streams must maintain square pixels at all times, no matter what the relative aspect ratios of the crop region and the stream are. Negative values for corner are allowed for raw output if full pixel array is larger than active pixel array. Width and height may be rounded to nearest larger supportable width, especially for raw output, where only a few fixed scales may be possible. For a set of output streams configured, if the sensor output is cropped to a smaller size than pre-correction active array size, the HAL need follow below cropping rules: The HAL need to handle the cropRegion as if the sensor crop size is the effective pre-correction active array size. More specifically, the HAL must transform the request cropRegion from android.sensor.info.preCorrectionActiveArraySize to the sensor cropped pixel area size in this way: If android.control.zoomRatio is set to value x, scale the requested cropRegion with 1.0/x in relation to its center as the origin. For example, say the requested cropRegion is (crX, crY, crWidth, crHeight), override it with `crX' = crX + crWidth * (1.0 - 1.0 / x) / 2`, `crY' = crY + crHeight * (1.0 - 1.0 / x) / 2`, `crWidth' = crWidth / x`, and `crHeight' = crHeight / x`. Translate the requested cropRegion w.r.t., the left top corner of the sensor cropped pixel area by (tx, ty), where `ty = sensorCrop.top * (sensorCrop.height / preCorrectionActiveArraySize.height)` and `tx = sensorCrop.left * (sensorCrop.width / preCorrectionActiveArraySize.width)`. The (sensorCrop.top, sensorCrop.left) is the coordinate based off the android.sensor.info.activeArraySize. Scale the width and height of requested cropRegion with scaling factor of sensorCrop.width/preCorrectionActiveArraySize.width and sensorCrop.height/preCorrectionActiveArraySize.height respectively. Once this new cropRegion is calculated, the HAL must use this region to crop the image with regard to the sensor crop size (effective pre-correction active array size). The HAL still need follow the general cropping rule for this new cropRegion and effective pre-correction active array size. The HAL must report the cropRegion with regard to android.sensor.info.preCorrectionActiveArraySize. The HAL need convert the new cropRegion generated above w.r.t., full pre-correction active array size. The reported cropRegion may be slightly different with the requested cropRegion since the HAL may adjust the crop region to account for rounding, conversion error, or other hardware limitations. If android.control.zoomRatio is supported by the HAL, the HAL must report the zoom ratio via android.control.zoomRatio, and change the coordinate system such that android.sensor.info.preCorrectionActiveArraySize or android.sensor.info.activeArraySize(depending on whether android.distortionCorrection.mode is supported) is used to represent the camera field-of-view after zoom. see android.control.zoomRatio for details. HAL2.x uses only (x, y, width)
android.scaler.rotateAndCrop | byte [hidden] NONE (v3.5) No rotate and crop is applied. Processed outputs are in the sensor orientation. 90 (v3.5) Processed images are rotated by 90 degrees clockwise, and then cropped to the original aspect ratio. 180 (v3.5) Processed images are rotated by 180 degrees. Since the aspect ratio does not change, no cropping is performed. 270 (v3.5) Processed images are rotated by 270 degrees clockwise, and then cropped to the original aspect ratio. AUTO (v3.5) The camera API automatically selects the best concrete value for rotate-and-crop based on the application's support for resizability and the current multi-window mode. If the application does not support resizing but the display mode for its main Activity is not in a typical orientation, the camera API will set `ROTATE_AND_CROP_90` or some other supported rotation value, depending on device configuration, to ensure preview and captured images are correctly shown to the user. Otherwise, `ROTATE_AND_CROP_NONE` will be selected. When a value other than NONE is selected, several metadata fields will also be parsed differently to ensure that coordinates are correctly handled for features like drawing face detection boxes or passing in tap-to-focus coordinates. The camera API will convert positions in the active array coordinate system to/from the cropped-and-rotated coordinate system to make the operation transparent for applications. No coordinate mapping will be done when the application selects a non-AUTO mode. | Whether a rotation-and-crop operation is applied to processed outputs from the camera. |  | android.scaler.availableRotateAndCropModes | 3.5 |
Details
This control is primarily intended to help camera applications with no support for multi-window modes to work correctly on devices where multi-window scenarios are unavoidable, such as foldables or other devices with variable display geometry or more free-form window placement (such as laptops, which often place portrait-orientation apps in landscape with pillarboxing). If supported, the default value is `ROTATE_AND_CROP_AUTO`, which allows the camera API to enable backwards-compatibility support for applications that do not support resizing / multi-window modes, when the device is in fact in a multi-window mode (such as inset portrait on laptops, or on a foldable device in some fold states). In addition, `ROTATE_AND_CROP_NONE` and `ROTATE_AND_CROP_90` will always be available if this control is supported by the device. If not supported, devices API level 30 or higher will always list only `ROTATE_AND_CROP_NONE`. When `CROP_AUTO` is in use, and the camera API activates backward-compatibility mode, several metadata fields will also be parsed differently to ensure that coordinates are correctly handled for features like drawing face detection boxes or passing in tap-to-focus coordinates. The camera API will convert positions in the active array coordinate system to/from the cropped-and-rotated coordinate system to make the operation transparent for applications. The following controls are affected: android.control.aeRegions android.control.afRegions android.control.awbRegions android.statistics.faces Capture results will contain the actual value selected by the API; `ROTATE_AND_CROP_AUTO` will never be seen in a capture result. Applications can also select their preferred cropping mode, either to opt out of the backwards-compatibility treatment, or to use the cropping feature themselves as needed. In this case, no coordinate translation will be done automatically, and all controls will continue to use the normal active array coordinates. Cropping and rotating is done after the application of digital zoom (via either android.scaler.cropRegion or android.control.zoomRatio), but before each individual output is further cropped and scaled. It only affects processed outputs such as YUV, PRIVATE, and JPEG. It has no effect on RAW outputs. When `CROP_90` or `CROP_270` are selected, there is a significant loss to the field of view. For example, with a 4:3 aspect ratio output of 1600x1200, `CROP_90` will still produce 1600x1200 output, but these buffers are cropped from a vertical 3:4 slice at the center of the 4:3 area, then rotated to be 4:3, and then upscaled to 1600x1200. Only 56.25% of the original FOV is still visible. In general, for an aspect ratio of `w:h`, the crop and rotate operation leaves `(h/w)^2` of the field of view visible. For 16:9, this is ~31.6%. As a visual example, the figure below shows the effect of `ROTATE_AND_CROP_90` on the outputs for the following parameters: Sensor active array: `2000x1500` Crop region: top-left: `(500, 375)`, size: `(1000, 750)` (4:3 aspect ratio) Output streams: YUV `640x480` and YUV `1280x720` `ROTATE_AND_CROP_90` With these settings, the regions of the active array covered by the output streams are: 640x480 stream crop: top-left: `(219, 375)`, size: `(562, 750)` 1280x720 stream crop: top-left: `(289, 375)`, size: `(422, 750)` Since the buffers are rotated, the buffers as seen by the application are: 640x480 stream: top-left: `(781, 375)` on active array, size: `(640, 480)`, downscaled 1.17x from sensor pixels 1280x720 stream: top-left: `(711, 375)` on active array, size: `(1280, 720)`, upscaled 1.71x from sensor pixels
HAL Implementation Details
Not ready for use in Android 11. ROTATE_AND_CROP_AUTO will never be sent to the HAL, though it must be set as the default value in all the capture request templates by the HAL. The camera service will translate AUTO to a specific rotation value based on the current application's multi-window state and its support of resizability. The HAL also does not need to consider coordinate transforms for ROTATE_AND_CROP - all capture request and result fields should be kept in the active array coordinate frame. Any translation required to implement ROTATE_AND_CROP_AUTO will be handled by the camera service.
sensor
controls
Property Name | Type | Description | Units | Range | Initial HIDL HAL version | Tags
android.sensor.exposureTime | int64 [public] [full] | Duration each pixel is exposed to light. | Nanoseconds | android.sensor.info.exposureTimeRange | 3.2 | V1
Details
If the sensor can't expose this exact duration, it will shorten the duration exposed to the nearest possible value (rather than expose longer). The final exposure time used will be available in the output capture result. This control is only effective if android.control.aeMode or android.control.mode is set to OFF; otherwise the auto-exposure algorithm will override this value.
android.sensor.frameDuration | int64 [public] [full] | Duration from start of frame exposure to start of next frame exposure. | Nanoseconds | See android.sensor.info.maxFrameDuration, StreamConfigurationMap. The duration is capped to `max(duration, exposureTime + overhead)`. | 3.2 | V1
Details
The maximum frame rate that can be supported by a camera subsystem is a function of many factors: Requested resolutions of output image streams Availability of binning / skipping modes on the imager The bandwidth of the imager interface The bandwidth of the various ISP processing blocks Since these factors can vary greatly between different ISPs and sensors, the camera abstraction tries to represent the bandwidth restrictions with as simple a model as possible. The model presented has the following characteristics: The image sensor is always configured to output the smallest resolution possible given the application's requested output stream sizes. The smallest resolution is defined as being at least as large as the largest requested output stream size; the camera pipeline must never digitally upsample sensor data when the crop region covers the whole sensor. In general, this means that if only small output stream resolutions are configured, the sensor can provide a higher frame rate. Since any request may use any or all the currently configured output streams, the sensor and ISP must be configured to support scaling a single capture to all the streams at the same time. This means the camera pipeline must be ready to produce the largest requested output size without any delay. Therefore, the overall frame rate of a given configured stream set is governed only by the largest requested stream resolution. Using more than one output stream in a request does not affect the frame duration. Certain format-streams may need to do additional background processing before data is consumed/produced by that stream. These processors can run concurrently to the rest of the camera pipeline, but cannot process more than 1 capture at a time. The necessary information for the application, given the model above, is provided via StreamConfigurationMap#getOutputMinFrameDuration. These are used to determine the maximum frame rate / minimum frame duration that is possible for a given stream configuration. Specifically, the application can use the following rules to determine the minimum frame duration it can request from the camera device: Let the set of currently configured input/output streams be called `S`. Find the minimum frame durations for each stream in `S`, by looking it up in StreamConfigurationMap#getOutputMinFrameDuration (with its respective size/format). Let this set of frame durations be called `F`. For any given request `R`, the minimum frame duration allowed for `R` is the maximum out of all values in `F`. Let the streams used in `R` be called `S_r`. If none of the streams in `S_r` have a stall time (listed in StreamConfigurationMap#getOutputStallDuration using its respective size/format), then the frame duration in `F` determines the steady state frame rate that the application will get if it uses `R` as a repeating request. Let this special kind of request be called `Rsimple`. A repeating request `Rsimple` can be occasionally interleaved by a single capture of a new request `Rstall` (which has at least one in-use stream with a non-0 stall time) and if `Rstall` has the same minimum frame duration this will not cause a frame rate loss if all buffers from the previous `Rstall` have already been delivered. For more details about stalling, see StreamConfigurationMap#getOutputStallDuration. This control is only effective if android.control.aeMode or android.control.mode is set to OFF; otherwise the auto-exposure algorithm will override this value.
HAL Implementation Details
For more details about stalling, see android.scaler.availableStallDurations.
android.sensor.sensitivity | int32 [public] [full] | The amount of gain applied to sensor data before processing. | ISO arithmetic units | android.sensor.info.sensitivityRange | 3.2 | V1
Details
The sensitivity is the standard ISO sensitivity value, as defined in ISO 12232:2006. The sensitivity must be within android.sensor.info.sensitivityRange, and if if it less than android.sensor.maxAnalogSensitivity, the camera device is guaranteed to use only analog amplification for applying the gain. If the camera device cannot apply the exact sensitivity requested, it will reduce the gain to the nearest supported value. The final sensitivity used will be available in the output capture result. This control is only effective if android.control.aeMode or android.control.mode is set to OFF; otherwise the auto-exposure algorithm will override this value. Note that for devices supporting postRawSensitivityBoost, the total sensitivity applied to the final processed image is the combination of android.sensor.sensitivity and android.control.postRawSensitivityBoost. In case the application uses the sensor sensitivity from last capture result of an auto request for a manual request, in order to achieve the same brightness in the output image, the application should also set postRawSensitivityBoost.
HAL Implementation Details
ISO 12232:2006 REI method is acceptable.
android.sensor.testPatternData | int32 x 4 [public] | A pixel `[R, G_even, G_odd, B]` that supplies the test pattern when android.sensor.testPatternMode is SOLID_COLOR. |  |  | 3.2 |
Details
Each color channel is treated as an unsigned 32-bit integer. The camera device then uses the most significant X bits that correspond to how many bits are in its Bayer raw sensor output. For example, a sensor with RAW10 Bayer output would use the 10 most significant bits from each color channel.
HAL Implementation Details
- android.sensor.testPatternMode | int32 [public] OFF (v3.2) No test pattern mode is used, and the camera device returns captures from the image sensor. This is the default if the key is not set. SOLID_COLOR (v3.2) Each pixel in `[R, G_even, G_odd, B]` is replaced by its respective color channel provided in android.sensor.testPatternData. For example:
      android.testPatternData = [0, 0xFFFFFFFF, 0xFFFFFFFF, 0]
  All green pixels are 100% green. All red/blue pixels are black.
      android.testPatternData = [0xFFFFFFFF, 0, 0xFFFFFFFF, 0]
- All red pixels are 100% red. Only the odd green pixels are 100% green. All blue pixels are 100% black. COLOR_BARS (v3.2) All pixel data is replaced with an 8-bar color pattern. The vertical bars (left-to-right) are as follows: 100% white yellow cyan green magenta red blue black In general the image would look like the following:
      W Y C G M R B K
      W Y C G M R B K
      W Y C G M R B K
      W Y C G M R B K
      W Y C G M R B K
      . . . . . . . .
      . . . . . . . .
      . . . . . . . .

      (B = Blue, K = Black)
Each bar should take up 1/8 of the sensor pixel array width. When this is not possible, the bar size should be rounded down to the nearest integer and the pattern can repeat on the right side. Each bar's height must always take up the full sensor pixel array height. Each pixel in this test pattern must be set to either 0% intensity or 100% intensity. COLOR_BARS_FADE_TO_GRAY (v3.2) The test pattern is similar to COLOR_BARS, except that each bar should start at its specified color at the top, and fade to gray at the bottom. Furthermore each bar is further subdivided into a left and right half. The left half should have a smooth gradient, and the right half should have a quantized gradient. In particular, the right half's should consist of blocks of the same color for 1/16th active sensor pixel array width. The least significant bits in the quantized gradient should be copied from the most significant bits of the smooth gradient. The height of each bar should always be a multiple of 128. When this is not the case, the pattern should repeat at the bottom of the image. PN9 (v3.2) All pixel data is replaced by a pseudo-random sequence generated from a PN9 512-bit sequence (typically implemented in hardware with a linear feedback shift register). The generator should be reset at the beginning of each frame, and thus each subsequent raw frame with this test pattern should be exactly the same as the last. CUSTOM1 (v3.2) 256 The first custom test pattern. All custom patterns that are available only on this camera device are at least this numeric value. All of the custom test patterns will be static (that is the raw image must not vary from frame to frame). | When enabled, the sensor sends a test pattern instead of doing a real exposure from the camera. |  | android.sensor.availableTestPatternModes | 3.2 |
Details
When a test pattern is enabled, all manual sensor controls specified by android.sensor.* will be ignored. All other controls should work as normal. For example, if manual flash is enabled, flash firing should still occur (and that the test pattern remain unmodified, since the flash would not actually affect it). Defaults to OFF.
HAL Implementation Details
All test patterns are specified in the Bayer domain. The HAL may choose to substitute test patterns from the sensor with test patterns from on-device memory. In that case, it should be indistinguishable to the ISP whether the data came from the sensor interconnect bus (such as CSI2) or memory.
static
Property Name | Type | Description | Units | Range | Initial HIDL HAL version | Tags
android.sensor.info.activeArraySize | int32 x 4 [public as rectangle] [legacy] Four ints defining the active pixel rectangle | The area of the image sensor which corresponds to active pixels after any geometric distortion correction has been applied. | Pixel coordinates on the image sensor |  | 3.2 | RAW
Details
This is the rectangle representing the size of the active region of the sensor (i.e. the region that actually receives light from the scene) after any geometric correction has been applied, and should be treated as the maximum size in pixels of any of the image output formats aside from the raw formats. This rectangle is defined relative to the full pixel array; (0,0) is the top-left of the full pixel array, and the size of the full pixel array is given by android.sensor.info.pixelArraySize. The coordinate system for most other keys that list pixel coordinates, including android.scaler.cropRegion, is defined relative to the active array rectangle given in this field, with `(0, 0)` being the top-left of this rectangle. The active array may be smaller than the full pixel array, since the full array may include black calibration pixels or other inactive regions. For devices that do not support android.distortionCorrection.mode control, the active array must be the same as android.sensor.info.preCorrectionActiveArraySize. For devices that support android.distortionCorrection.mode control, the active array must be enclosed by android.sensor.info.preCorrectionActiveArraySize. The difference between pre-correction active array and active array accounts for scaling or cropping caused by lens geometric distortion correction. In general, application should always refer to active array size for controls like metering regions or crop region. Two exceptions are when the application is dealing with RAW image buffers (RAW_SENSOR, RAW10, RAW12 etc), or when application explicitly set android.distortionCorrection.mode to OFF. In these cases, application should refer to android.sensor.info.preCorrectionActiveArraySize.
HAL Implementation Details
This array contains `(xmin, ymin, width, height)`. The `(xmin, ymin)` must be >= `(0,0)`. The `(width, height)` must be <= `android.sensor.info.pixelArraySize`.
android.sensor.info.sensitivityRange | int32 x 2 [public as rangeInt] [full] Range of supported sensitivities | Range of sensitivities for android.sensor.sensitivity supported by this camera device. |  | Min <= 100, Max >= 800 | 3.2 | BC V1
Details
The values are the standard ISO sensitivity values, as defined in ISO 12232:2006.
android.sensor.info.colorFilterArrangement | byte [public] [full] RGGB (v3.2) GRBG (v3.2) GBRG (v3.2) BGGR (v3.2) RGB (v3.2) Sensor is not Bayer; output has 3 16-bit values for each pixel, instead of just 1 16-bit value per pixel. MONO (v3.4) Sensor doesn't have any Bayer color filter. Such sensor captures visible light in monochrome. The exact weighting and wavelengths captured is not specified, but generally only includes the visible frequencies. This value implies a MONOCHROME camera. NIR (v3.4) Sensor has a near infrared filter capturing light with wavelength between roughly 750nm and 1400nm, and the same filter covers the whole sensor array. This value implies a MONOCHROME camera. | The arrangement of color filters on sensor; represents the colors in the top-left 2x2 section of the sensor, in reading order, for a Bayer camera, or the light spectrum it captures for MONOCHROME camera. |  |  | 3.2 | RAW
HAL Implementation Details
Starting from Android Q, the colorFilterArrangement for a MONOCHROME camera must be single color patterns, such as MONO or NIR.
android.sensor.info.exposureTimeRange | int64 x 2 [public as rangeLong] [full] nanoseconds | The range of image exposure times for android.sensor.exposureTime supported by this camera device. | Nanoseconds | The minimum exposure time will be less than 100 us. For FULL capability devices (android.info.supportedHardwareLevel == FULL), the maximum exposure time will be greater than 100ms. | 3.2 | V1
HAL Implementation Details
For FULL capability devices (android.info.supportedHardwareLevel == FULL), The maximum of the range SHOULD be at least 1 second (1e9), MUST be at least 100ms.
android.sensor.info.maxFrameDuration | int64 [public] [full] | The maximum possible frame duration (minimum frame rate) for android.sensor.frameDuration that is supported this camera device. | Nanoseconds | For FULL capability devices (android.info.supportedHardwareLevel == FULL), at least 100ms. | 3.2 | V1
Details
Attempting to use frame durations beyond the maximum will result in the frame duration being clipped to the maximum. See that control for a full definition of frame durations. Refer to StreamConfigurationMap#getOutputMinFrameDuration for the minimum frame duration values.
HAL Implementation Details
For FULL capability devices (android.info.supportedHardwareLevel == FULL), The maximum of the range SHOULD be at least 1 second (1e9), MUST be at least 100ms (100e6). android.sensor.info.maxFrameDuration must be greater or equal to the android.sensor.info.exposureTimeRange max value (since exposure time overrides frame duration). Available minimum frame durations for JPEG must be no greater than that of the YUV_420_888/IMPLEMENTATION_DEFINED minimum frame durations (for that respective size). Since JPEG processing is considered offline and can take longer than a single uncompressed capture, refer to android.scaler.availableStallDurations for details about encoding this scenario.
android.sensor.info.physicalSize | float x 2 [public as sizeF] [legacy] width x height | The physical dimensions of the full pixel array. | Millimeters |  | 3.2 | V1 BC
Details
This is the physical size of the sensor pixel array defined by android.sensor.info.pixelArraySize.
HAL Implementation Details
Needed for FOV calculation for old API
android.sensor.info.pixelArraySize | int32 x 2 [public as size] [legacy] | Dimensions of the full pixel array, possibly including black calibration pixels. | Pixels |  | 3.2 | RAW BC
Details
The pixel count of the full pixel array of the image sensor, which covers android.sensor.info.physicalSize area. This represents the full pixel dimensions of the raw buffers produced by this sensor. If a camera device supports raw sensor formats, either this or android.sensor.info.preCorrectionActiveArraySize is the maximum dimensions for the raw output formats listed in StreamConfigurationMap (this depends on whether or not the image sensor returns buffers containing pixels that are not part of the active array region for blacklevel calibration or other purposes). Some parts of the full pixel array may not receive light from the scene, or be otherwise inactive. The android.sensor.info.preCorrectionActiveArraySize key defines the rectangle of active pixels that will be included in processed image formats.
android.sensor.info.whiteLevel | int32 [public] | Maximum raw value output by sensor. |  | > 255 (8-bit output) | 3.2 | RAW
Details
This specifies the fully-saturated encoding level for the raw sample values from the sensor. This is typically caused by the sensor becoming highly non-linear or clipping. The minimum for each channel is specified by the offset in the android.sensor.blackLevelPattern key. The white level is typically determined either by sensor bit depth (8-14 bits is expected), or by the point where the sensor response becomes too non-linear to be useful. The default value for this is maximum representable value for a 16-bit raw sample (2^16 - 1). The white level values of captured images may vary for different capture settings (e.g., android.sensor.sensitivity). This key represents a coarse approximation for such case. It is recommended to use android.sensor.dynamicWhiteLevel for captures when supported by the camera device, which provides more accurate white level values.
HAL Implementation Details
The full bit depth of the sensor must be available in the raw data, so the value for linear sensors should not be significantly lower than maximum raw value supported, i.e. 2^(sensor bits per pixel).
android.sensor.info.timestampSource | byte [public] [legacy] UNKNOWN (v3.2) Timestamps from android.sensor.timestamp are in nanoseconds and monotonic, but can not be compared to timestamps from other subsystems (e.g. accelerometer, gyro etc.), or other instances of the same or different camera devices in the same system with accuracy. However, the timestamps are roughly in the same timebase as SystemClock#uptimeMillis. The accuracy is sufficient for tasks like A/V synchronization for video recording, at least, and the timestamps can be directly used together with timestamps from the audio subsystem for that task. Timestamps between streams and results for a single camera instance are comparable, and the timestamps for all buffers and the result metadata generated by a single capture are identical. REALTIME (v3.2) Timestamps from android.sensor.timestamp are in the same timebase as SystemClock#elapsedRealtimeNanos, and they can be compared to other timestamps using that base. When buffers from a REALTIME device are passed directly to a video encoder from the camera, automatic compensation is done to account for differing timebases of the audio and camera subsystems. If the application is receiving buffers and then later sending them to a video encoder or other application where they are compared with audio subsystem timestamps or similar, this compensation is not present. In those cases, applications need to adjust the timestamps themselves. Since SystemClock#elapsedRealtimeNanos and SystemClock#uptimeMillis only diverge while the device is asleep, an offset between the two sources can be measured once per active session and applied to timestamps for sufficient accuracy for A/V sync. | The time base source for sensor capture start timestamps. |  |  | 3.2 | V1
Details
The timestamps provided for captures are always in nanoseconds and monotonic, but may not based on a time source that can be compared to other system time sources. This characteristic defines the source for the timestamps, and therefore whether they can be compared against other system time sources/timestamps.
HAL Implementation Details
For camera devices implement UNKNOWN, the camera framework expects that the timestamp source to be SYSTEM_TIME_MONOTONIC. For camera devices implement REALTIME, the camera framework expects that the timestamp source to be SYSTEM_TIME_BOOTTIME. See system/core/include/utils/Timers.h for the definition of SYSTEM_TIME_MONOTONIC and SYSTEM_TIME_BOOTTIME. Note that HAL must follow above expectation; otherwise video recording might suffer unexpected behavior. Also, camera devices which implement REALTIME must pass the ITS sensor fusion test which tests the alignment between camera timestamps and gyro sensor timestamps.
android.sensor.info.lensShadingApplied | byte [public as boolean] FALSE (v3.2) TRUE (v3.2) | Whether the RAW images output from this camera device are subject to lens shading correction. |  |  | 3.2 |
Details
If TRUE, all images produced by the camera device in the RAW image formats will have lens shading correction already applied to it. If FALSE, the images will not be adjusted for lens shading correction. See android.request.maxNumOutputRaw for a list of RAW image formats. This key will be `null` for all devices do not report this information. Devices with RAW capability will always report this information in this key.
android.sensor.info.preCorrectionActiveArraySize | int32 x 4 [public as rectangle] [legacy] Four ints defining the active pixel rectangle | The area of the image sensor which corresponds to active pixels prior to the application of any geometric distortion correction. | Pixel coordinates on the image sensor |  | 3.2 | RAW
Details
This is the rectangle representing the size of the active region of the sensor (i.e. the region that actually receives light from the scene) before any geometric correction has been applied, and should be treated as the active region rectangle for any of the raw formats. All metadata associated with raw processing (e.g. the lens shading correction map, and radial distortion fields) treats the top, left of this rectangle as the origin, (0,0). The size of this region determines the maximum field of view and the maximum number of pixels that an image from this sensor can contain, prior to the application of geometric distortion correction. The effective maximum pixel dimensions of a post-distortion-corrected image is given by the android.sensor.info.activeArraySize field, and the effective maximum field of view for a post-distortion-corrected image can be calculated by applying the geometric distortion correction fields to this rectangle, and cropping to the rectangle given in android.sensor.info.activeArraySize. E.g. to calculate position of a pixel, (x,y), in a processed YUV output image with the dimensions in android.sensor.info.activeArraySize given the position of a pixel, (x', y'), in the raw pixel array with dimensions give in android.sensor.info.pixelArraySize: Choose a pixel (x', y') within the active array region of the raw buffer given in android.sensor.info.preCorrectionActiveArraySize, otherwise this pixel is considered to be outside of the FOV, and will not be shown in the processed output image. Apply geometric distortion correction to get the post-distortion pixel coordinate, (x_i, y_i). When applying geometric correction metadata, note that metadata for raw buffers is defined relative to the top, left of the android.sensor.info.preCorrectionActiveArraySize rectangle. If the resulting corrected pixel coordinate is within the region given in android.sensor.info.activeArraySize, then the position of this pixel in the processed output image buffer is `(x_i - activeArray.left, y_i - activeArray.top)`, when the top, left coordinate of that buffer is treated as (0, 0). Thus, for pixel x',y' = (25, 25) on a sensor where android.sensor.info.pixelArraySize is (100,100), android.sensor.info.preCorrectionActiveArraySize is (10, 10, 100, 100), android.sensor.info.activeArraySize is (20, 20, 80, 80), and the geometric distortion correction doesn't change the pixel coordinate, the resulting pixel selected in pixel coordinates would be x,y = (25, 25) relative to the top,left of the raw buffer with dimensions given in android.sensor.info.pixelArraySize, and would be (5, 5) relative to the top,left of post-processed YUV output buffer with dimensions given in android.sensor.info.activeArraySize. The currently supported fields that correct for geometric distortion are: android.lens.distortion. If the camera device doesn't support geometric distortion correction, or all of the geometric distortion fields are no-ops, this rectangle will be the same as the post-distortion-corrected rectangle given in android.sensor.info.activeArraySize. This rectangle is defined relative to the full pixel array; (0,0) is the top-left of the full pixel array, and the size of the full pixel array is given by android.sensor.info.pixelArraySize. The pre-correction active array may be smaller than the full pixel array, since the full array may include black calibration pixels or other inactive regions.
HAL Implementation Details
This array contains `(xmin, ymin, width, height)`. The `(xmin, ymin)` must be >= `(0,0)`. The `(width, height)` must be <= `android.sensor.info.pixelArraySize`. If omitted by the HAL implementation, the camera framework will assume that this is the same as the post-correction active array region given in android.sensor.info.activeArraySize.
android.sensor.referenceIlluminant1 | byte [public] DAYLIGHT (v3.2) 1 FLUORESCENT (v3.2) 2 TUNGSTEN (v3.2) 3 Incandescent light FLASH (v3.2) 4 FINE_WEATHER (v3.2) 9 CLOUDY_WEATHER (v3.2) 10 SHADE (v3.2) 11 DAYLIGHT_FLUORESCENT (v3.2) 12 D 5700 - 7100K DAY_WHITE_FLUORESCENT (v3.2) 13 N 4600 - 5400K COOL_WHITE_FLUORESCENT (v3.2) 14 W 3900 - 4500K WHITE_FLUORESCENT (v3.2) 15 WW 3200 - 3700K STANDARD_A (v3.2) 17 STANDARD_B (v3.2) 18 STANDARD_C (v3.2) 19 D55 (v3.2) 20 D65 (v3.2) 21 D75 (v3.2) 22 D50 (v3.2) 23 ISO_STUDIO_TUNGSTEN (v3.2) 24 | The standard reference illuminant used as the scene light source when calculating the android.sensor.colorTransform1, android.sensor.calibrationTransform1, and android.sensor.forwardMatrix1 matrices. |  |  | 3.2 | RAW
Details
The values in this key correspond to the values defined for the EXIF LightSource tag. These illuminants are standard light sources that are often used calibrating camera devices. If this key is present, then android.sensor.colorTransform1, android.sensor.calibrationTransform1, and android.sensor.forwardMatrix1 will also be present. Some devices may choose to provide a second set of calibration information for improved quality, including android.sensor.referenceIlluminant2 and its corresponding matrices. Starting from Android Q, this key will not be present for a MONOCHROME camera, even if the camera device has RAW capability.
HAL Implementation Details
The first reference illuminant (android.sensor.referenceIlluminant1) and corresponding matrices must be present to support the RAW capability and DNG output. When producing raw images with a color profile that has only been calibrated against a single light source, it is valid to omit android.sensor.referenceIlluminant2 along with the android.sensor.colorTransform2, android.sensor.calibrationTransform2, and android.sensor.forwardMatrix2 matrices. If only android.sensor.referenceIlluminant1 is included, it should be chosen so that it is representative of typical scene lighting. In general, D50 or DAYLIGHT will be chosen for this case. If both android.sensor.referenceIlluminant1 and android.sensor.referenceIlluminant2 are included, they should be chosen to represent the typical range of scene lighting conditions. In general, low color temperature illuminant such as Standard-A will be chosen for the first reference illuminant and a higher color temperature illuminant such as D65 will be chosen for the second reference illuminant.
android.sensor.referenceIlluminant2 | byte [public] | The standard reference illuminant used as the scene light source when calculating the android.sensor.colorTransform2, android.sensor.calibrationTransform2, and android.sensor.forwardMatrix2 matrices. |  | Any value listed in android.sensor.referenceIlluminant1 | 3.2 | RAW
Details
See android.sensor.referenceIlluminant1 for more details. If this key is present, then android.sensor.colorTransform2, android.sensor.calibrationTransform2, and android.sensor.forwardMatrix2 will also be present. Starting from Android Q, this key will not be present for a MONOCHROME camera, even if the camera device has RAW capability.
android.sensor.calibrationTransform1 | rational x 3 x 3 [public as colorSpaceTransform] 3x3 matrix in row-major-order | A per-device calibration transform matrix that maps from the reference sensor colorspace to the actual device sensor colorspace. |  |  | 3.2 | RAW
Details
This matrix is used to correct for per-device variations in the sensor colorspace, and is used for processing raw buffer data. The matrix is expressed as a 3x3 matrix in row-major-order, and contains a per-device calibration transform that maps colors from reference sensor color space (i.e. the "golden module" colorspace) into this camera device's native sensor color space under the first reference illuminant (android.sensor.referenceIlluminant1). Starting from Android Q, this key will not be present for a MONOCHROME camera, even if the camera device has RAW capability.
android.sensor.calibrationTransform2 | rational x 3 x 3 [public as colorSpaceTransform] 3x3 matrix in row-major-order | A per-device calibration transform matrix that maps from the reference sensor colorspace to the actual device sensor colorspace (this is the colorspace of the raw buffer data). |  |  | 3.2 | RAW
Details
This matrix is used to correct for per-device variations in the sensor colorspace, and is used for processing raw buffer data. The matrix is expressed as a 3x3 matrix in row-major-order, and contains a per-device calibration transform that maps colors from reference sensor color space (i.e. the "golden module" colorspace) into this camera device's native sensor color space under the second reference illuminant (android.sensor.referenceIlluminant2). This matrix will only be present if the second reference illuminant is present. Starting from Android Q, this key will not be present for a MONOCHROME camera, even if the camera device has RAW capability.
android.sensor.colorTransform1 | rational x 3 x 3 [public as colorSpaceTransform] 3x3 matrix in row-major-order | A matrix that transforms color values from CIE XYZ color space to reference sensor color space. |  |  | 3.2 | RAW
Details
This matrix is used to convert from the standard CIE XYZ color space to the reference sensor colorspace, and is used when processing raw buffer data. The matrix is expressed as a 3x3 matrix in row-major-order, and contains a color transform matrix that maps colors from the CIE XYZ color space to the reference sensor color space (i.e. the "golden module" colorspace) under the first reference illuminant (android.sensor.referenceIlluminant1). The white points chosen in both the reference sensor color space and the CIE XYZ colorspace when calculating this transform will match the standard white point for the first reference illuminant (i.e. no chromatic adaptation will be applied by this transform). Starting from Android Q, this key will not be present for a MONOCHROME camera, even if the camera device has RAW capability.
android.sensor.colorTransform2 | rational x 3 x 3 [public as colorSpaceTransform] 3x3 matrix in row-major-order | A matrix that transforms color values from CIE XYZ color space to reference sensor color space. |  |  | 3.2 | RAW
Details
This matrix is used to convert from the standard CIE XYZ color space to the reference sensor colorspace, and is used when processing raw buffer data. The matrix is expressed as a 3x3 matrix in row-major-order, and contains a color transform matrix that maps colors from the CIE XYZ color space to the reference sensor color space (i.e. the "golden module" colorspace) under the second reference illuminant (android.sensor.referenceIlluminant2). The white points chosen in both the reference sensor color space and the CIE XYZ colorspace when calculating this transform will match the standard white point for the second reference illuminant (i.e. no chromatic adaptation will be applied by this transform). This matrix will only be present if the second reference illuminant is present. Starting from Android Q, this key will not be present for a MONOCHROME camera, even if the camera device has RAW capability.
android.sensor.forwardMatrix1 | rational x 3 x 3 [public as colorSpaceTransform] 3x3 matrix in row-major-order | A matrix that transforms white balanced camera colors from the reference sensor colorspace to the CIE XYZ colorspace with a D50 whitepoint. |  |  | 3.2 | RAW
Details
This matrix is used to convert to the standard CIE XYZ colorspace, and is used when processing raw buffer data. This matrix is expressed as a 3x3 matrix in row-major-order, and contains a color transform matrix that maps white balanced colors from the reference sensor color space to the CIE XYZ color space with a D50 white point. Under the first reference illuminant (android.sensor.referenceIlluminant1) this matrix is chosen so that the standard white point for this reference illuminant in the reference sensor colorspace is mapped to D50 in the CIE XYZ colorspace. Starting from Android Q, this key will not be present for a MONOCHROME camera, even if the camera device has RAW capability.
android.sensor.forwardMatrix2 | rational x 3 x 3 [public as colorSpaceTransform] 3x3 matrix in row-major-order | A matrix that transforms white balanced camera colors from the reference sensor colorspace to the CIE XYZ colorspace with a D50 whitepoint. |  |  | 3.2 | RAW
Details
This matrix is used to convert to the standard CIE XYZ colorspace, and is used when processing raw buffer data. This matrix is expressed as a 3x3 matrix in row-major-order, and contains a color transform matrix that maps white balanced colors from the reference sensor color space to the CIE XYZ color space with a D50 white point. Under the second reference illuminant (android.sensor.referenceIlluminant2) this matrix is chosen so that the standard white point for this reference illuminant in the reference sensor colorspace is mapped to D50 in the CIE XYZ colorspace. This matrix will only be present if the second reference illuminant is present. Starting from Android Q, this key will not be present for a MONOCHROME camera, even if the camera device has RAW capability.
android.sensor.baseGainFactor | rational [system] | Gain factor from electrons to raw units when ISO=100 |  |  | 3.2 | FUTURE
android.sensor.blackLevelPattern | int32 x 4 [public as blackLevelPattern] 2x2 raw count block | A fixed black level offset for each of the color filter arrangement (CFA) mosaic channels. |  | >= 0 for each. | 3.2 | RAW
Details
This key specifies the zero light value for each of the CFA mosaic channels in the camera sensor. The maximal value output by the sensor is represented by the value in android.sensor.info.whiteLevel. The values are given in the same order as channels listed for the CFA layout key (see android.sensor.info.colorFilterArrangement), i.e. the nth value given corresponds to the black level offset for the nth color channel listed in the CFA. The black level values of captured images may vary for different capture settings (e.g., android.sensor.sensitivity). This key represents a coarse approximation for such case. It is recommended to use android.sensor.dynamicBlackLevel or use pixels from android.sensor.opticalBlackRegions directly for captures when supported by the camera device, which provides more accurate black level values. For raw capture in particular, it is recommended to use pixels from android.sensor.opticalBlackRegions to calculate black level values for each frame. For a MONOCHROME camera device, all of the 2x2 channels must have the same values.
HAL Implementation Details
The values are given in row-column scan order, with the first value corresponding to the element of the CFA in row=0, column=0.
android.sensor.maxAnalogSensitivity | int32 [public] [full] | Maximum sensitivity that is implemented purely through analog gain. |  |  | 3.2 | V1 FULL
Details
For android.sensor.sensitivity values less than or equal to this, all applied gain must be analog. For values above this, the gain applied can be a mix of analog and digital.
android.sensor.orientation | int32 [public] [legacy] | Clockwise angle through which the output image needs to be rotated to be upright on the device screen in its native orientation. | Degrees of clockwise rotation; always a multiple of 90 | 0, 90, 180, 270 | 3.2 | BC
Details
Also defines the direction of rolling shutter readout, which is from top to bottom in the sensor's coordinate system.
android.sensor.profileHueSatMapDimensions | int32 x 3 [system] Number of samples for hue, saturation, and value | The number of input samples for each dimension of android.sensor.profileHueSatMap. |  | Hue >= 1, Saturation >= 2, Value >= 1 | 3.2 | RAW
Details
The number of input samples for the hue, saturation, and value dimension of android.sensor.profileHueSatMap. The order of the dimensions given is hue, saturation, value; where hue is the 0th element.
android.sensor.availableTestPatternModes | int32 x n [public] list of enums | List of sensor test pattern modes for android.sensor.testPatternMode supported by this camera device. |  | Any value listed in android.sensor.testPatternMode | 3.2 |
Details
Defaults to OFF, and always includes OFF if defined.
HAL Implementation Details
All custom modes must be >= CUSTOM1.
android.sensor.opticalBlackRegions | int32 x 4 x num_regions [public as rectangle] | List of disjoint rectangles indicating the sensor optically shielded black pixel regions. |  |  | 3.2 |
Details
In most camera sensors, the active array is surrounded by some optically shielded pixel areas. By blocking light, these pixels provides a reliable black reference for black level compensation in active array region. This key provides a list of disjoint rectangles specifying the regions of optically shielded (with metal shield) black pixel regions if the camera device is capable of reading out these black pixels in the output raw images. In comparison to the fixed black level values reported by android.sensor.blackLevelPattern, this key may provide a more accurate way for the application to calculate black level of each captured raw images. When this key is reported, the android.sensor.dynamicBlackLevel and android.sensor.dynamicWhiteLevel will also be reported.
HAL Implementation Details
This array contains (xmin, ymin, width, height). The (xmin, ymin) must be >= (0,0) and <= android.sensor.info.pixelArraySize. The (width, height) must be <= android.sensor.info.pixelArraySize. Each region must be outside the region reported by android.sensor.info.preCorrectionActiveArraySize. The HAL must report minimal number of disjoint regions for the optically shielded back pixel regions. For example, if a region can be covered by one rectangle, the HAL must not split this region into multiple rectangles.
android.sensor.opaqueRawSize | int32 x n x 3 [system] | Size in bytes for all the listed opaque RAW buffer sizes |  | Must be large enough to fit the opaque RAW of corresponding size produced by the camera | 3.2 |
Details
This configurations are listed as `(width, height, size_in_bytes)` tuples. This is used for sizing the gralloc buffers for opaque RAW buffers. All RAW_OPAQUE output stream configuration listed in android.scaler.availableStreamConfigurations will have a corresponding tuple in this key.
HAL Implementation Details
This key is added in legacy HAL3.4. For legacy HAL3.4 or above: devices advertising RAW_OPAQUE format output must list this key. For legacy HAL3.3 or earlier devices: if RAW_OPAQUE ouput is advertised, camera framework will derive this key by assuming each pixel takes two bytes and no padding bytes between rows.
dynamic
Property Name | Type | Description | Units | Range | Initial HIDL HAL version | Tags
android.sensor.exposureTime | int64 [public] [full] | Duration each pixel is exposed to light. | Nanoseconds | android.sensor.info.exposureTimeRange | 3.2 | V1
Details
If the sensor can't expose this exact duration, it will shorten the duration exposed to the nearest possible value (rather than expose longer). The final exposure time used will be available in the output capture result. This control is only effective if android.control.aeMode or android.control.mode is set to OFF; otherwise the auto-exposure algorithm will override this value.
android.sensor.frameDuration | int64 [public] [full] | Duration from start of frame exposure to start of next frame exposure. | Nanoseconds | See android.sensor.info.maxFrameDuration, StreamConfigurationMap. The duration is capped to `max(duration, exposureTime + overhead)`. | 3.2 | V1
Details
The maximum frame rate that can be supported by a camera subsystem is a function of many factors: Requested resolutions of output image streams Availability of binning / skipping modes on the imager The bandwidth of the imager interface The bandwidth of the various ISP processing blocks Since these factors can vary greatly between different ISPs and sensors, the camera abstraction tries to represent the bandwidth restrictions with as simple a model as possible. The model presented has the following characteristics: The image sensor is always configured to output the smallest resolution possible given the application's requested output stream sizes. The smallest resolution is defined as being at least as large as the largest requested output stream size; the camera pipeline must never digitally upsample sensor data when the crop region covers the whole sensor. In general, this means that if only small output stream resolutions are configured, the sensor can provide a higher frame rate. Since any request may use any or all the currently configured output streams, the sensor and ISP must be configured to support scaling a single capture to all the streams at the same time. This means the camera pipeline must be ready to produce the largest requested output size without any delay. Therefore, the overall frame rate of a given configured stream set is governed only by the largest requested stream resolution. Using more than one output stream in a request does not affect the frame duration. Certain format-streams may need to do additional background processing before data is consumed/produced by that stream. These processors can run concurrently to the rest of the camera pipeline, but cannot process more than 1 capture at a time. The necessary information for the application, given the model above, is provided via StreamConfigurationMap#getOutputMinFrameDuration. These are used to determine the maximum frame rate / minimum frame duration that is possible for a given stream configuration. Specifically, the application can use the following rules to determine the minimum frame duration it can request from the camera device: Let the set of currently configured input/output streams be called `S`. Find the minimum frame durations for each stream in `S`, by looking it up in StreamConfigurationMap#getOutputMinFrameDuration (with its respective size/format). Let this set of frame durations be called `F`. For any given request `R`, the minimum frame duration allowed for `R` is the maximum out of all values in `F`. Let the streams used in `R` be called `S_r`. If none of the streams in `S_r` have a stall time (listed in StreamConfigurationMap#getOutputStallDuration using its respective size/format), then the frame duration in `F` determines the steady state frame rate that the application will get if it uses `R` as a repeating request. Let this special kind of request be called `Rsimple`. A repeating request `Rsimple` can be occasionally interleaved by a single capture of a new request `Rstall` (which has at least one in-use stream with a non-0 stall time) and if `Rstall` has the same minimum frame duration this will not cause a frame rate loss if all buffers from the previous `Rstall` have already been delivered. For more details about stalling, see StreamConfigurationMap#getOutputStallDuration. This control is only effective if android.control.aeMode or android.control.mode is set to OFF; otherwise the auto-exposure algorithm will override this value.
HAL Implementation Details
For more details about stalling, see android.scaler.availableStallDurations.
android.sensor.sensitivity | int32 [public] [full] | The amount of gain applied to sensor data before processing. | ISO arithmetic units | android.sensor.info.sensitivityRange | 3.2 | V1
Details
The sensitivity is the standard ISO sensitivity value, as defined in ISO 12232:2006. The sensitivity must be within android.sensor.info.sensitivityRange, and if if it less than android.sensor.maxAnalogSensitivity, the camera device is guaranteed to use only analog amplification for applying the gain. If the camera device cannot apply the exact sensitivity requested, it will reduce the gain to the nearest supported value. The final sensitivity used will be available in the output capture result. This control is only effective if android.control.aeMode or android.control.mode is set to OFF; otherwise the auto-exposure algorithm will override this value. Note that for devices supporting postRawSensitivityBoost, the total sensitivity applied to the final processed image is the combination of android.sensor.sensitivity and android.control.postRawSensitivityBoost. In case the application uses the sensor sensitivity from last capture result of an auto request for a manual request, in order to achieve the same brightness in the output image, the application should also set postRawSensitivityBoost.
HAL Implementation Details
ISO 12232:2006 REI method is acceptable.
android.sensor.timestamp | int64 [public] [legacy] | Time at start of exposure of first row of the image sensor active array, in nanoseconds. | Nanoseconds | > 0 | 3.2 | BC
Details
The timestamps are also included in all image buffers produced for the same capture, and will be identical on all the outputs. When android.sensor.info.timestampSource `==` UNKNOWN, the timestamps measure time since an unspecified starting point, and are monotonically increasing. They can be compared with the timestamps for other captures from the same camera device, but are not guaranteed to be comparable to any other time source. When android.sensor.info.timestampSource `==` REALTIME, the timestamps measure time in the same timebase as SystemClock#elapsedRealtimeNanos, and they can be compared to other timestamps from other subsystems that are using that base. For reprocessing, the timestamp will match the start of exposure of the input image, i.e. the timestamp in the TotalCaptureResult that was used to create the reprocess capture request.
HAL Implementation Details
All timestamps must be in reference to the kernel's CLOCK_BOOTTIME monotonic clock, which properly accounts for time spent asleep. This allows for synchronization with sensors that continue to operate while the system is otherwise asleep. If android.sensor.info.timestampSource `==` REALTIME, The timestamp must be synchronized with the timestamps from other sensor subsystems that are using the same timebase. For reprocessing, the input image's start of exposure can be looked up with android.sensor.timestamp from the metadata included in the capture request.
android.sensor.temperature | float [system] | The temperature of the sensor, sampled at the time exposure began for this frame. The thermal diode being queried should be inside the sensor PCB, or somewhere close to it. | Celsius | Optional. This value is missing if no temperature is available. | 3.2 | FUTURE
android.sensor.neutralColorPoint | rational x 3 [public] | The estimated camera neutral color in the native sensor colorspace at the time of capture. |  |  | 3.2 | RAW
Details
This value gives the neutral color point encoded as an RGB value in the native sensor color space. The neutral color point indicates the currently estimated white point of the scene illumination. It can be used to interpolate between the provided color transforms when processing raw sensor data. The order of the values is R, G, B; where R is in the lowest index. Starting from Android Q, this key will not be present for a MONOCHROME camera, even if the camera device has RAW capability.
android.sensor.noiseProfile | double x 2 x CFA Channels [public as pairDoubleDouble] Pairs of noise model coefficients | Noise model coefficients for each CFA mosaic channel. |  |  | 3.2 | RAW
Details
This key contains two noise model coefficients for each CFA channel corresponding to the sensor amplification (S) and sensor readout noise (O). These are given as pairs of coefficients for each channel in the same order as channels listed for the CFA layout key (see android.sensor.info.colorFilterArrangement). This is represented as an array of Pair<Double, Double>, where the first member of the Pair at index n is the S coefficient and the second member is the O coefficient for the nth color channel in the CFA. These coefficients are used in a two parameter noise model to describe the amount of noise present in the image for each CFA channel. The noise model used here is: N(x) = sqrt(Sx + O) Where x represents the recorded signal of a CFA channel normalized to the range [0, 1], and S and O are the noise model coeffiecients for that channel. A more detailed description of the noise model can be found in the Adobe DNG specification for the NoiseProfile tag. For a MONOCHROME camera, there is only one color channel. So the noise model coefficients will only contain one S and one O.
HAL Implementation Details
For a CFA layout of RGGB, the list of coefficients would be given as an array of doubles S0,O0,S1,O1,..., where S0 and O0 are the coefficients for the red channel, S1 and O1 are the coefficients for the first green channel, etc.
android.sensor.profileHueSatMap | float x hue_samples x saturation_samples x value_samples x 3 [system] Mapping for hue, saturation, and value | A mapping containing a hue shift, saturation scale, and value scale for each pixel. | The hue shift is given in degrees; saturation and value scale factors are unitless and are between 0 and 1 inclusive |  | 3.2 | RAW
Details
hue_samples, saturation_samples, and value_samples are given in android.sensor.profileHueSatMapDimensions. Each entry of this map contains three floats corresponding to the hue shift, saturation scale, and value scale, respectively; where the hue shift has the lowest index. The map entries are stored in the key in nested loop order, with the value divisions in the outer loop, the hue divisions in the middle loop, and the saturation divisions in the inner loop. All zero input saturation entries are required to have a value scale factor of 1.0.
android.sensor.profileToneCurve | float x samples x 2 [system] Samples defining a spline for a tone-mapping curve | A list of x,y samples defining a tone-mapping curve for gamma adjustment. |  | Each sample has an input range of `[0, 1]` and an output range of `[0, 1]`. The first sample is required to be `(0, 0)`, and the last sample is required to be `(1, 1)`. | 3.2 | RAW
Details
This key contains a default tone curve that can be applied while processing the image as a starting point for user adjustments. The curve is specified as a list of value pairs in linear gamma. The curve is interpolated using a cubic spline.
android.sensor.greenSplit | float [public] | The worst-case divergence between Bayer green channels. |  | >= 0 | 3.2 | RAW
Details
This value is an estimate of the worst case split between the Bayer green channels in the red and blue rows in the sensor color filter array. The green split is calculated as follows: A 5x5 pixel (or larger) window W within the active sensor array is chosen. The term 'pixel' here is taken to mean a group of 4 Bayer mosaic channels (R, Gr, Gb, B). The location and size of the window chosen is implementation defined, and should be chosen to provide a green split estimate that is both representative of the entire image for this camera sensor, and can be calculated quickly. The arithmetic mean of the green channels from the red rows (mean_Gr) within W is computed. The arithmetic mean of the green channels from the blue rows (mean_Gb) within W is computed. The maximum ratio R of the two means is computed as follows: `R = max((mean_Gr + 1)/(mean_Gb + 1), (mean_Gb + 1)/(mean_Gr + 1))` The ratio R is the green split divergence reported for this property, which represents how much the green channels differ in the mosaic pattern. This value is typically used to determine the treatment of the green mosaic channels when demosaicing. The green split value can be roughly interpreted as follows: R < 1.03 is a negligible split (<3% divergence). 1.20 <= R >= 1.03 will require some software correction to avoid demosaic errors (3-20% divergence). R > 1.20 will require strong software correction to produce a usuable image (>20% divergence). Starting from Android Q, this key will not be present for a MONOCHROME camera, even if the camera device has RAW capability.
HAL Implementation Details
The green split given may be a static value based on prior characterization of the camera sensor using the green split calculation method given here over a large, representative, sample set of images. Other methods of calculation that produce equivalent results, and can be interpreted in the same manner, may be used.
android.sensor.testPatternData | int32 x 4 [public] | A pixel `[R, G_even, G_odd, B]` that supplies the test pattern when android.sensor.testPatternMode is SOLID_COLOR. |  |  | 3.2 |
Details
Each color channel is treated as an unsigned 32-bit integer. The camera device then uses the most significant X bits that correspond to how many bits are in its Bayer raw sensor output. For example, a sensor with RAW10 Bayer output would use the 10 most significant bits from each color channel.
HAL Implementation Details
- android.sensor.testPatternMode | int32 [public] OFF (v3.2) No test pattern mode is used, and the camera device returns captures from the image sensor. This is the default if the key is not set. SOLID_COLOR (v3.2) Each pixel in `[R, G_even, G_odd, B]` is replaced by its respective color channel provided in android.sensor.testPatternData. For example:
      android.testPatternData = [0, 0xFFFFFFFF, 0xFFFFFFFF, 0]
  All green pixels are 100% green. All red/blue pixels are black.
      android.testPatternData = [0xFFFFFFFF, 0, 0xFFFFFFFF, 0]
- All red pixels are 100% red. Only the odd green pixels are 100% green. All blue pixels are 100% black. COLOR_BARS (v3.2) All pixel data is replaced with an 8-bar color pattern. The vertical bars (left-to-right) are as follows: 100% white yellow cyan green magenta red blue black In general the image would look like the following:
      W Y C G M R B K
      W Y C G M R B K
      W Y C G M R B K
      W Y C G M R B K
      W Y C G M R B K
      . . . . . . . .
      . . . . . . . .
      . . . . . . . .

      (B = Blue, K = Black)
Each bar should take up 1/8 of the sensor pixel array width. When this is not possible, the bar size should be rounded down to the nearest integer and the pattern can repeat on the right side. Each bar's height must always take up the full sensor pixel array height. Each pixel in this test pattern must be set to either 0% intensity or 100% intensity. COLOR_BARS_FADE_TO_GRAY (v3.2) The test pattern is similar to COLOR_BARS, except that each bar should start at its specified color at the top, and fade to gray at the bottom. Furthermore each bar is further subdivided into a left and right half. The left half should have a smooth gradient, and the right half should have a quantized gradient. In particular, the right half's should consist of blocks of the same color for 1/16th active sensor pixel array width. The least significant bits in the quantized gradient should be copied from the most significant bits of the smooth gradient. The height of each bar should always be a multiple of 128. When this is not the case, the pattern should repeat at the bottom of the image. PN9 (v3.2) All pixel data is replaced by a pseudo-random sequence generated from a PN9 512-bit sequence (typically implemented in hardware with a linear feedback shift register). The generator should be reset at the beginning of each frame, and thus each subsequent raw frame with this test pattern should be exactly the same as the last. CUSTOM1 (v3.2) 256 The first custom test pattern. All custom patterns that are available only on this camera device are at least this numeric value. All of the custom test patterns will be static (that is the raw image must not vary from frame to frame). | When enabled, the sensor sends a test pattern instead of doing a real exposure from the camera. |  | android.sensor.availableTestPatternModes | 3.2 |
Details
When a test pattern is enabled, all manual sensor controls specified by android.sensor.* will be ignored. All other controls should work as normal. For example, if manual flash is enabled, flash firing should still occur (and that the test pattern remain unmodified, since the flash would not actually affect it). Defaults to OFF.
HAL Implementation Details
All test patterns are specified in the Bayer domain. The HAL may choose to substitute test patterns from the sensor with test patterns from on-device memory. In that case, it should be indistinguishable to the ISP whether the data came from the sensor interconnect bus (such as CSI2) or memory.
android.sensor.rollingShutterSkew | int64 [public] [limited] | Duration between the start of exposure for the first row of the image sensor, and the start of exposure for one past the last row of the image sensor. | Nanoseconds | >= 0 and < StreamConfigurationMap#getOutputMinFrameDuration. | 3.2 | V1
Details
This is the exposure time skew between the first and `(last+1)` row exposure start times. The first row and the last row are the first and last rows inside of the android.sensor.info.activeArraySize. For typical camera sensors that use rolling shutters, this is also equivalent to the frame readout time. If the image sensor is operating in a binned or cropped mode due to the current output target resolutions, it's possible this skew is reported to be larger than the exposure time, for example, since it is based on the full array even if a partial array is read out. Be sure to scale the number to cover the section of the sensor actually being used for the outputs you care about. So if your output covers N rows of the active array of height H, scale this value by N/H to get the total skew for that viewport. Note: Prior to Android 11, this field was described as measuring duration from first to last row of the image sensor, which is not equal to the frame readout time for a rolling shutter sensor. Implementations generally reported the latter value, so to resolve the inconsistency, the description has been updated to range from (first, last+1) row exposure start, instead.
HAL Implementation Details
The HAL must report `0` if the sensor is using global shutter, where all pixels begin exposure at the same time.
android.sensor.dynamicBlackLevel | float x 4 [public] 2x2 raw count block | A per-frame dynamic black level offset for each of the color filter arrangement (CFA) mosaic channels. |  | >= 0 for each. | 3.2 | RAW
Details
Camera sensor black levels may vary dramatically for different capture settings (e.g. android.sensor.sensitivity). The fixed black level reported by android.sensor.blackLevelPattern may be too inaccurate to represent the actual value on a per-frame basis. The camera device internal pipeline relies on reliable black level values to process the raw images appropriately. To get the best image quality, the camera device may choose to estimate the per frame black level values either based on optically shielded black regions (android.sensor.opticalBlackRegions) or its internal model. This key reports the camera device estimated per-frame zero light value for each of the CFA mosaic channels in the camera sensor. The android.sensor.blackLevelPattern may only represent a coarse approximation of the actual black level values. This value is the black level used in camera device internal image processing pipeline and generally more accurate than the fixed black level values. However, since they are estimated values by the camera device, they may not be as accurate as the black level values calculated from the optical black pixels reported by android.sensor.opticalBlackRegions. The values are given in the same order as channels listed for the CFA layout key (see android.sensor.info.colorFilterArrangement), i.e. the nth value given corresponds to the black level offset for the nth color channel listed in the CFA. For a MONOCHROME camera, all of the 2x2 channels must have the same values. This key will be available if android.sensor.opticalBlackRegions is available or the camera device advertises this key via CameraCharacteristics#getAvailableCaptureResultKeys.
HAL Implementation Details
The values are given in row-column scan order, with the first value corresponding to the element of the CFA in row=0, column=0.
android.sensor.dynamicWhiteLevel | int32 [public] | Maximum raw value output by sensor for this frame. |  | >= 0 | 3.2 | RAW
Details
Since the android.sensor.blackLevelPattern may change for different capture settings (e.g., android.sensor.sensitivity), the white level will change accordingly. This key is similar to android.sensor.info.whiteLevel, but specifies the camera device estimated white level for each frame. This key will be available if android.sensor.opticalBlackRegions is available or the camera device advertises this key via CameraCharacteristics#getAvailableCaptureRequestKeys.
HAL Implementation Details
The full bit depth of the sensor must be available in the raw data, so the value for linear sensors should not be significantly lower than maximum raw value supported, i.e. 2^(sensor bits per pixel).
shading
controls
Property Name | Type | Description | Units | Range | Initial HIDL HAL version | Tags
android.shading.mode | byte [public] [full] OFF (v3.2) No lens shading correction is applied. FAST (v3.2) Apply lens shading corrections, without slowing frame rate relative to sensor raw output HIGH_QUALITY (v3.2) Apply high-quality lens shading correction, at the cost of possibly reduced frame rate. | Quality of lens shading correction applied to the image data. |  | android.shading.availableModes | 3.2 |
Details
When set to OFF mode, no lens shading correction will be applied by the camera device, and an identity lens shading map data will be provided if `android.statistics.lensShadingMapMode == ON`. For example, for lens shading map with size of `[ 4, 3 ]`, the output android.statistics.lensShadingCorrectionMap for this case will be an identity map shown below:
    [ 1.0, 1.0, 1.0, 1.0,  1.0, 1.0, 1.0, 1.0,
     1.0, 1.0, 1.0, 1.0,  1.0, 1.0, 1.0, 1.0,
     1.0, 1.0, 1.0, 1.0,  1.0, 1.0, 1.0, 1.0,
     1.0, 1.0, 1.0, 1.0,  1.0, 1.0, 1.0, 1.0,
     1.0, 1.0, 1.0, 1.0,  1.0, 1.0, 1.0, 1.0,
     1.0, 1.0, 1.0, 1.0,  1.0, 1.0, 1.0, 1.0 ]
When set to other modes, lens shading correction will be applied by the camera device. Applications can request lens shading map data by setting android.statistics.lensShadingMapMode to ON, and then the camera device will provide lens shading map data in android.statistics.lensShadingCorrectionMap; the returned shading map data will be the one applied by the camera device for this capture request. The shading map data may depend on the auto-exposure (AE) and AWB statistics, therefore the reliability of the map data may be affected by the AE and AWB algorithms. When AE and AWB are in AUTO modes(android.control.aeMode `!=` OFF and android.control.awbMode `!=` OFF), to get best results, it is recommended that the applications wait for the AE and AWB to be converged before using the returned shading map data.
android.shading.strength | byte [system] | Control the amount of shading correction applied to the images | unitless: 1-10; 10 is full shading compensation |  | 3.2 | FUTURE
dynamic
Property Name | Type | Description | Units | Range | Initial HIDL HAL version | Tags
android.shading.mode | byte [public] [full] OFF (v3.2) No lens shading correction is applied. FAST (v3.2) Apply lens shading corrections, without slowing frame rate relative to sensor raw output HIGH_QUALITY (v3.2) Apply high-quality lens shading correction, at the cost of possibly reduced frame rate. | Quality of lens shading correction applied to the image data. |  | android.shading.availableModes | 3.2 |
Details
When set to OFF mode, no lens shading correction will be applied by the camera device, and an identity lens shading map data will be provided if `android.statistics.lensShadingMapMode == ON`. For example, for lens shading map with size of `[ 4, 3 ]`, the output android.statistics.lensShadingCorrectionMap for this case will be an identity map shown below:
    [ 1.0, 1.0, 1.0, 1.0,  1.0, 1.0, 1.0, 1.0,
     1.0, 1.0, 1.0, 1.0,  1.0, 1.0, 1.0, 1.0,
     1.0, 1.0, 1.0, 1.0,  1.0, 1.0, 1.0, 1.0,
     1.0, 1.0, 1.0, 1.0,  1.0, 1.0, 1.0, 1.0,
     1.0, 1.0, 1.0, 1.0,  1.0, 1.0, 1.0, 1.0,
     1.0, 1.0, 1.0, 1.0,  1.0, 1.0, 1.0, 1.0 ]
When set to other modes, lens shading correction will be applied by the camera device. Applications can request lens shading map data by setting android.statistics.lensShadingMapMode to ON, and then the camera device will provide lens shading map data in android.statistics.lensShadingCorrectionMap; the returned shading map data will be the one applied by the camera device for this capture request. The shading map data may depend on the auto-exposure (AE) and AWB statistics, therefore the reliability of the map data may be affected by the AE and AWB algorithms. When AE and AWB are in AUTO modes(android.control.aeMode `!=` OFF and android.control.awbMode `!=` OFF), to get best results, it is recommended that the applications wait for the AE and AWB to be converged before using the returned shading map data.
static
Property Name | Type | Description | Units | Range | Initial HIDL HAL version | Tags
android.shading.availableModes | byte x n [public as enumList] [legacy] List of enums (android.shading.mode). | List of lens shading modes for android.shading.mode that are supported by this camera device. |  | Any value listed in android.shading.mode | 3.2 |
Details
This list contains lens shading modes that can be set for the camera device. Camera devices that support the MANUAL_POST_PROCESSING capability will always list OFF and FAST mode. This includes all FULL level devices. LEGACY devices will always only support FAST mode.
HAL Implementation Details
HAL must support both FAST and HIGH_QUALITY if lens shading correction control is available on the camera device, but the underlying implementation can be the same for both modes. That is, if the highest quality implementation on the camera device does not slow down capture rate, then FAST and HIGH_QUALITY will generate the same output.
statistics
controls
Property Name | Type | Description | Units | Range | Initial HIDL HAL version | Tags
android.statistics.faceDetectMode | byte [public] [legacy] OFF (v3.2) Do not include face detection statistics in capture results. SIMPLE (v3.2) [optional] Return face rectangle and confidence values only. FULL (v3.2) [optional] Return all face metadata. In this mode, face rectangles, scores, landmarks, and face IDs are all valid. | Operating mode for the face detector unit. |  | android.statistics.info.availableFaceDetectModes | 3.2 | BC
Details
Whether face detection is enabled, and whether it should output just the basic fields or the full set of fields.
HAL Implementation Details
SIMPLE mode must fill in android.statistics.faceRectangles and android.statistics.faceScores. FULL mode must also fill in android.statistics.faceIds, and android.statistics.faceLandmarks.
android.statistics.histogramMode | byte [system as boolean] OFF (v3.2) ON (v3.2) | Operating mode for histogram generation |  |  | 3.2 | FUTURE
android.statistics.sharpnessMapMode | byte [system as boolean] OFF (v3.2) ON (v3.2) | Operating mode for sharpness map generation |  |  | 3.2 | FUTURE
android.statistics.hotPixelMapMode | byte [public as boolean] OFF (v3.2) Hot pixel map production is disabled. ON (v3.2) Hot pixel map production is enabled. | Operating mode for hot pixel map generation. |  | android.statistics.info.availableHotPixelMapModes | 3.2 | V1 RAW
Details
If set to `true`, a hot pixel map is returned in android.statistics.hotPixelMap. If set to `false`, no hot pixel map will be returned.
android.statistics.lensShadingMapMode | byte [public] [full] OFF (v3.2) Do not include a lens shading map in the capture result. ON (v3.2) Include a lens shading map in the capture result. | Whether the camera device will output the lens shading map in output result metadata. |  | android.statistics.info.availableLensShadingMapModes | 3.2 | RAW
Details
When set to ON, android.statistics.lensShadingMap will be provided in the output result metadata. ON is always supported on devices with the RAW capability.
android.statistics.oisDataMode | byte [public] OFF (v3.3) Do not include OIS data in the capture result. ON (v3.3) Include OIS data in the capture result. | A control for selecting whether optical stabilization (OIS) position information is included in output result metadata. |  | android.statistics.info.availableOisDataModes | 3.3 |
Details
Since optical image stabilization generally involves motion much faster than the duration of individualq image exposure, multiple OIS samples can be included for a single capture result. For example, if the OIS reporting operates at 200 Hz, a typical camera operating at 30fps may have 6-7 OIS samples per capture result. This information can be combined with the rolling shutter skew to account for lens motion during image exposure in post-processing algorithms.
static
Property Name | Type | Description | Units | Range | Initial HIDL HAL version | Tags
android.statistics.info.availableFaceDetectModes | byte x n [public as enumList] [legacy] List of enums from android.statistics.faceDetectMode | List of face detection modes for android.statistics.faceDetectMode that are supported by this camera device. |  | Any value listed in android.statistics.faceDetectMode | 3.2 |
Details
OFF is always supported.
android.statistics.info.histogramBucketCount | int32 [system] | Number of histogram buckets supported |  | >= 64 | 3.2 | FUTURE
android.statistics.info.maxFaceCount | int32 [public] [legacy] | The maximum number of simultaneously detectable faces. |  | 0 for cameras without available face detection; otherwise: `>=4` for LIMITED or FULL hwlevel devices or `>0` for LEGACY devices. | 3.2 | BC
android.statistics.info.maxHistogramCount | int32 [system] | Maximum value possible for a histogram bucket |  |  | 3.2 | FUTURE
android.statistics.info.maxSharpnessMapValue | int32 [system] | Maximum value possible for a sharpness map region. |  |  | 3.2 | FUTURE
android.statistics.info.sharpnessMapSize | int32 x 2 [system as size] width x height | Dimensions of the sharpness map |  | Must be at least 32 x 32 | 3.2 | FUTURE
android.statistics.info.availableHotPixelMapModes | byte x n [public as boolean] list of enums | List of hot pixel map output modes for android.statistics.hotPixelMapMode that are supported by this camera device. |  | Any value listed in android.statistics.hotPixelMapMode | 3.2 | V1 RAW
Details
If no hotpixel map output is available for this camera device, this will contain only `false`. ON is always supported on devices with the RAW capability.
android.statistics.info.availableLensShadingMapModes | byte x n [public as enumList] list of enums | List of lens shading map output modes for android.statistics.lensShadingMapMode that are supported by this camera device. |  | Any value listed in android.statistics.lensShadingMapMode | 3.2 |
Details
If no lens shading map output is available for this camera device, this key will contain only OFF. ON is always supported on devices with the RAW capability. LEGACY mode devices will always only support OFF.
android.statistics.info.availableOisDataModes | byte x n [public as enumList] list of enums | List of OIS data output modes for android.statistics.oisDataMode that are supported by this camera device. |  | Any value listed in android.statistics.oisDataMode | 3.3 |
Details
If no OIS data output is available for this camera device, this key will contain only OFF.
dynamic
Property Name | Type | Description | Units | Range | Initial HIDL HAL version | Tags
android.statistics.faceDetectMode | byte [public] [legacy] OFF (v3.2) Do not include face detection statistics in capture results. SIMPLE (v3.2) [optional] Return face rectangle and confidence values only. FULL (v3.2) [optional] Return all face metadata. In this mode, face rectangles, scores, landmarks, and face IDs are all valid. | Operating mode for the face detector unit. |  | android.statistics.info.availableFaceDetectModes | 3.2 | BC
Details
Whether face detection is enabled, and whether it should output just the basic fields or the full set of fields.
HAL Implementation Details
SIMPLE mode must fill in android.statistics.faceRectangles and android.statistics.faceScores. FULL mode must also fill in android.statistics.faceIds, and android.statistics.faceLandmarks.
android.statistics.faceIds | int32 x n [ndk_public] [legacy] | List of unique IDs for detected faces. |  |  | 3.2 | BC
Details
Each detected face is given a unique ID that is valid for as long as the face is visible to the camera device. A face that leaves the field of view and later returns may be assigned a new ID. Only available if android.statistics.faceDetectMode == FULL
android.statistics.faceLandmarks | int32 x n x 6 [ndk_public] [legacy] (leftEyeX, leftEyeY, rightEyeX, rightEyeY, mouthX, mouthY) | List of landmarks for detected faces. |  |  | 3.2 | BC
Details
For devices not supporting android.distortionCorrection.mode control, the coordinate system always follows that of android.sensor.info.activeArraySize, with `(0, 0)` being the top-left pixel of the active array. For devices supporting android.distortionCorrection.mode control, the coordinate system depends on the mode being set. When the distortion correction mode is OFF, the coordinate system follows android.sensor.info.preCorrectionActiveArraySize, with `(0, 0)` being the top-left pixel of the pre-correction active array. When the distortion correction mode is not OFF, the coordinate system follows android.sensor.info.activeArraySize, with `(0, 0)` being the top-left pixel of the active array. Only available if android.statistics.faceDetectMode == FULL. Starting from API level 30, the coordinate system of activeArraySize or preCorrectionActiveArraySize is used to represent post-zoomRatio field of view, not pre-zoomRatio field of view. This means that if the relative position of faces and the camera device doesn't change, when zooming in by increasing android.control.zoomRatio, the face landmarks move farther away from the center of the activeArray or preCorrectionActiveArray. If android.control.zoomRatio is set to 1.0 (default), the face landmarks coordinates won't change as android.scaler.cropRegion changes. See android.control.zoomRatio for details. Whether to use activeArraySize or preCorrectionActiveArraySize still depends on distortion correction mode.
HAL Implementation Details
HAL must always report face landmarks in the coordinate system of pre-correction active array.
android.statistics.faceRectangles | int32 x n x 4 [ndk_public as rectangle] [legacy] (xmin, ymin, xmax, ymax). (0,0) is top-left of active pixel area | List of the bounding rectangles for detected faces. |  |  | 3.2 | BC
Details
For devices not supporting android.distortionCorrection.mode control, the coordinate system always follows that of android.sensor.info.activeArraySize, with `(0, 0)` being the top-left pixel of the active array. For devices supporting android.distortionCorrection.mode control, the coordinate system depends on the mode being set. When the distortion correction mode is OFF, the coordinate system follows android.sensor.info.preCorrectionActiveArraySize, with `(0, 0)` being the top-left pixel of the pre-correction active array. When the distortion correction mode is not OFF, the coordinate system follows android.sensor.info.activeArraySize, with `(0, 0)` being the top-left pixel of the active array. Only available if android.statistics.faceDetectMode != OFF. Starting from API level 30, the coordinate system of activeArraySize or preCorrectionActiveArraySize is used to represent post-zoomRatio field of view, not pre-zoomRatio field of view. This means that if the relative position of faces and the camera device doesn't change, when zooming in by increasing android.control.zoomRatio, the face rectangles grow larger and move farther away from the center of the activeArray or preCorrectionActiveArray. If android.control.zoomRatio is set to 1.0 (default), the face rectangles won't change as android.scaler.cropRegion changes. See android.control.zoomRatio for details. Whether to use activeArraySize or preCorrectionActiveArraySize still depends on distortion correction mode.
HAL Implementation Details
HAL must always report face rectangles in the coordinate system of pre-correction active array.
android.statistics.faceScores | byte x n [ndk_public] [legacy] | List of the face confidence scores for detected faces |  | 1-100 | 3.2 | BC
Details
Only available if android.statistics.faceDetectMode != OFF.
HAL Implementation Details
The value should be meaningful (for example, setting 100 at all times is illegal).
android.statistics.faces | int32 x n [java_public as face] [synthetic] [legacy] | List of the faces detected through camera face detection in this capture. |  |  | 3.2 |
Details
Only available if android.statistics.faceDetectMode `!=` OFF.
android.statistics.histogram | int32 x n x 3 [system] count of pixels for each color channel that fall into each histogram bucket, scaled to be between 0 and maxHistogramCount | A 3-channel histogram based on the raw sensor data |  |  | 3.2 | FUTURE
Details
The k'th bucket (0-based) covers the input range (with w = android.sensor.info.whiteLevel) of [ k * w/N, (k + 1) * w / N ). If only a monochrome sharpness map is supported, all channels should have the same data
android.statistics.histogramMode | byte [system as boolean] OFF (v3.2) ON (v3.2) | Operating mode for histogram generation |  |  | 3.2 | FUTURE
android.statistics.sharpnessMap | int32 x n x m x 3 [system] estimated sharpness for each region of the input image. Normalized to be between 0 and maxSharpnessMapValue. Higher values mean sharper (better focused) | A 3-channel sharpness map, based on the raw sensor data |  |  | 3.2 | FUTURE
Details
If only a monochrome sharpness map is supported, all channels should have the same data
android.statistics.sharpnessMapMode | byte [system as boolean] OFF (v3.2) ON (v3.2) | Operating mode for sharpness map generation |  |  | 3.2 | FUTURE
android.statistics.lensShadingCorrectionMap | byte [java_public as lensShadingMap] [full] | The shading map is a low-resolution floating-point map that lists the coefficients used to correct for vignetting, for each Bayer color channel. |  | Each gain factor is >= 1 | 3.2 |
Details
The map provided here is the same map that is used by the camera device to correct both color shading and vignetting for output non-RAW images. When there is no lens shading correction applied to RAW output images (android.sensor.info.lensShadingApplied `==` false), this map is the complete lens shading correction map; when there is some lens shading correction applied to the RAW output image (android.sensor.info.lensShadingApplied`==` true), this map reports the remaining lens shading correction map that needs to be applied to get shading corrected images that match the camera device's output for non-RAW formats. For a complete shading correction map, the least shaded section of the image will have a gain factor of 1; all other sections will have gains above 1. When android.colorCorrection.mode = TRANSFORM_MATRIX, the map will take into account the colorCorrection settings. The shading map is for the entire active pixel array, and is not affected by the crop region specified in the request. Each shading map entry is the value of the shading compensation map over a specific pixel on the sensor. Specifically, with a (N x M) resolution shading map, and an active pixel array size (W x H), shading map entry (x,y) ϵ (0 ... N-1, 0 ... M-1) is the value of the shading map at pixel ( ((W-1)/(N-1)) * x, ((H-1)/(M-1)) * y) for the four color channels. The map is assumed to be bilinearly interpolated between the sample points. The channel order is [R, Geven, Godd, B], where Geven is the green channel for the even rows of a Bayer pattern, and Godd is the odd rows. The shading map is stored in a fully interleaved format. The shading map will generally have on the order of 30-40 rows and columns, and will be smaller than 64x64. As an example, given a very small map defined as:
    width,height = [ 4, 3 ]
    values =
    [ 1.3, 1.2, 1.15, 1.2,  1.2, 1.2, 1.15, 1.2,
        1.1, 1.2, 1.2, 1.2,  1.3, 1.2, 1.3, 1.3,
      1.2, 1.2, 1.25, 1.1,  1.1, 1.1, 1.1, 1.0,
        1.0, 1.0, 1.0, 1.0,  1.2, 1.3, 1.25, 1.2,
      1.3, 1.2, 1.2, 1.3,   1.2, 1.15, 1.1, 1.2,
        1.2, 1.1, 1.0, 1.2,  1.3, 1.15, 1.2, 1.3 ]
The low-resolution scaling map images for each channel are (displayed using nearest-neighbor interpolation): As a visualization only, inverting the full-color map to recover an image of a gray wall (using bicubic interpolation for visual quality) as captured by the sensor gives: For a MONOCHROME camera, all of the 2x2 channels must have the same values. An example shading map for such a camera is defined as:
    android.lens.info.shadingMapSize = [ 4, 3 ]
    android.statistics.lensShadingMap =
    [ 1.3, 1.3, 1.3, 1.3,  1.2, 1.2, 1.2, 1.2,
        1.1, 1.1, 1.1, 1.1,  1.3, 1.3, 1.3, 1.3,
      1.2, 1.2, 1.2, 1.2,  1.1, 1.1, 1.1, 1.1,
        1.0, 1.0, 1.0, 1.0,  1.2, 1.2, 1.2, 1.2,
      1.3, 1.3, 1.3, 1.3,   1.2, 1.2, 1.2, 1.2,
        1.2, 1.2, 1.2, 1.2,  1.3, 1.3, 1.3, 1.3 ]
android.statistics.lensShadingMap | float x 4 x n x m [ndk_public] [full] 2D array of float gain factors per channel to correct lens shading | The shading map is a low-resolution floating-point map that lists the coefficients used to correct for vignetting and color shading, for each Bayer color channel of RAW image data. |  | Each gain factor is >= 1 | 3.2 |
Details
The map provided here is the same map that is used by the camera device to correct both color shading and vignetting for output non-RAW images. When there is no lens shading correction applied to RAW output images (android.sensor.info.lensShadingApplied `==` false), this map is the complete lens shading correction map; when there is some lens shading correction applied to the RAW output image (android.sensor.info.lensShadingApplied`==` true), this map reports the remaining lens shading correction map that needs to be applied to get shading corrected images that match the camera device's output for non-RAW formats. For a complete shading correction map, the least shaded section of the image will have a gain factor of 1; all other sections will have gains above 1. When android.colorCorrection.mode = TRANSFORM_MATRIX, the map will take into account the colorCorrection settings. The shading map is for the entire active pixel array, and is not affected by the crop region specified in the request. Each shading map entry is the value of the shading compensation map over a specific pixel on the sensor. Specifically, with a (N x M) resolution shading map, and an active pixel array size (W x H), shading map entry (x,y) ϵ (0 ... N-1, 0 ... M-1) is the value of the shading map at pixel ( ((W-1)/(N-1)) * x, ((H-1)/(M-1)) * y) for the four color channels. The map is assumed to be bilinearly interpolated between the sample points. For a Bayer camera, the channel order is [R, Geven, Godd, B], where Geven is the green channel for the even rows of a Bayer pattern, and Godd is the odd rows. The shading map is stored in a fully interleaved format, and its size is provided in the camera static metadata by android.lens.info.shadingMapSize. The shading map will generally have on the order of 30-40 rows and columns, and will be smaller than 64x64. As an example, given a very small map for a Bayer camera defined as:
    android.lens.info.shadingMapSize = [ 4, 3 ]
    android.statistics.lensShadingMap =
    [ 1.3, 1.2, 1.15, 1.2,  1.2, 1.2, 1.15, 1.2,
        1.1, 1.2, 1.2, 1.2,  1.3, 1.2, 1.3, 1.3,
      1.2, 1.2, 1.25, 1.1,  1.1, 1.1, 1.1, 1.0,
        1.0, 1.0, 1.0, 1.0,  1.2, 1.3, 1.25, 1.2,
      1.3, 1.2, 1.2, 1.3,   1.2, 1.15, 1.1, 1.2,
        1.2, 1.1, 1.0, 1.2,  1.3, 1.15, 1.2, 1.3 ]
The low-resolution scaling map images for each channel are (displayed using nearest-neighbor interpolation): As a visualization only, inverting the full-color map to recover an image of a gray wall (using bicubic interpolation for visual quality) as captured by the sensor gives: For a MONOCHROME camera, all of the 2x2 channels must have the same values. An example shading map for such a camera is defined as:
    android.lens.info.shadingMapSize = [ 4, 3 ]
    android.statistics.lensShadingMap =
    [ 1.3, 1.3, 1.3, 1.3,  1.2, 1.2, 1.2, 1.2,
        1.1, 1.1, 1.1, 1.1,  1.3, 1.3, 1.3, 1.3,
      1.2, 1.2, 1.2, 1.2,  1.1, 1.1, 1.1, 1.1,
        1.0, 1.0, 1.0, 1.0,  1.2, 1.2, 1.2, 1.2,
      1.3, 1.3, 1.3, 1.3,   1.2, 1.2, 1.2, 1.2,
        1.2, 1.2, 1.2, 1.2,  1.3, 1.3, 1.3, 1.3 ]
Note that the RAW image data might be subject to lens shading correction not reported on this map. Query android.sensor.info.lensShadingApplied to see if RAW image data has subject to lens shading correction. If android.sensor.info.lensShadingApplied is TRUE, the RAW image data is subject to partial or full lens shading correction. In the case full lens shading correction is applied to RAW images, the gain factor map reported in this key will contain all 1.0 gains. In other words, the map reported in this key is the remaining lens shading that needs to be applied on the RAW image to get images without lens shading artifacts. See android.request.maxNumOutputRaw for a list of RAW image formats.
HAL Implementation Details
The lens shading map calculation may depend on exposure and white balance statistics. When AE and AWB are in AUTO modes (android.control.aeMode `!=` OFF and android.control.awbMode `!=` OFF), the HAL may have all the information it need to generate most accurate lens shading map. When AE or AWB are in manual mode (android.control.aeMode `==` OFF or android.control.awbMode `==` OFF), the shading map may be adversely impacted by manual exposure or white balance parameters. To avoid generating unreliable shading map data, the HAL may choose to lock the shading map with the latest known good map generated when the AE and AWB are in AUTO modes.
android.statistics.predictedColorGains | float x 4 [hidden] [deprecated] A 1D array of floats for 4 color channel gains | The best-fit color channel gains calculated by the camera device's statistics units for the current output frame. |  | Deprecated. Do not use. | 3.2 |
Details
This may be different than the gains used for this frame, since statistics processing on data from a new frame typically completes after the transform has already been applied to that frame. The 4 channel gains are defined in Bayer domain, see android.colorCorrection.gains for details. This value should always be calculated by the auto-white balance (AWB) block, regardless of the android.control.* current values.
android.statistics.predictedColorTransform | rational x 3 x 3 [hidden] [deprecated] 3x3 rational matrix in row-major order | The best-fit color transform matrix estimate calculated by the camera device's statistics units for the current output frame. |  | Deprecated. Do not use. | 3.2 |
Details
The camera device will provide the estimate from its statistics unit on the white balance transforms to use for the next frame. These are the values the camera device believes are the best fit for the current output frame. This may be different than the transform used for this frame, since statistics processing on data from a new frame typically completes after the transform has already been applied to that frame. These estimates must be provided for all frames, even if capture settings and color transforms are set by the application. This value should always be calculated by the auto-white balance (AWB) block, regardless of the android.control.* current values.
android.statistics.sceneFlicker | byte [public] [full] NONE (v3.2) The camera device does not detect any flickering illumination in the current scene. 50HZ (v3.2) The camera device detects illumination flickering at 50Hz in the current scene. 60HZ (v3.2) The camera device detects illumination flickering at 60Hz in the current scene. | The camera device estimated scene illumination lighting frequency. |  |  | 3.2 |
Details
Many light sources, such as most fluorescent lights, flicker at a rate that depends on the local utility power standards. This flicker must be accounted for by auto-exposure routines to avoid artifacts in captured images. The camera device uses this entry to tell the application what the scene illuminant frequency is. When manual exposure control is enabled (`android.control.aeMode == OFF` or `android.control.mode == OFF`), the android.control.aeAntibandingMode doesn't perform antibanding, and the application can ensure it selects exposure times that do not cause banding issues by looking into this metadata field. See android.control.aeAntibandingMode for more details. Reports NONE if there doesn't appear to be flickering illumination.
android.statistics.hotPixelMapMode | byte [public as boolean] OFF (v3.2) Hot pixel map production is disabled. ON (v3.2) Hot pixel map production is enabled. | Operating mode for hot pixel map generation. |  | android.statistics.info.availableHotPixelMapModes | 3.2 | V1 RAW
Details
If set to `true`, a hot pixel map is returned in android.statistics.hotPixelMap. If set to `false`, no hot pixel map will be returned.
android.statistics.hotPixelMap | int32 x 2 x n [public as point] list of coordinates based on android.sensor.pixelArraySize | List of `(x, y)` coordinates of hot/defective pixels on the sensor. |  | n <= number of pixels on the sensor. The `(x, y)` coordinates must be bounded by android.sensor.info.pixelArraySize. | 3.2 | V1 RAW
Details
A coordinate `(x, y)` must lie between `(0, 0)`, and `(width - 1, height - 1)` (inclusive), which are the top-left and bottom-right of the pixel array, respectively. The width and height dimensions are given in android.sensor.info.pixelArraySize. This may include hot pixels that lie outside of the active array bounds given by android.sensor.info.activeArraySize.
HAL Implementation Details
A hotpixel map contains the coordinates of pixels on the camera sensor that do report valid values (usually due to defects in the camera sensor). This includes pixels that are stuck at certain values, or have a response that does not accuractly encode the incoming light from the scene. To avoid performance issues, there should be significantly fewer hot pixels than actual pixels on the camera sensor.
android.statistics.lensShadingMapMode | byte [public] [full] OFF (v3.2) Do not include a lens shading map in the capture result. ON (v3.2) Include a lens shading map in the capture result. | Whether the camera device will output the lens shading map in output result metadata. |  | android.statistics.info.availableLensShadingMapModes | 3.2 | RAW
Details
When set to ON, android.statistics.lensShadingMap will be provided in the output result metadata. ON is always supported on devices with the RAW capability.
android.statistics.oisDataMode | byte [public] OFF (v3.3) Do not include OIS data in the capture result. ON (v3.3) Include OIS data in the capture result. | A control for selecting whether optical stabilization (OIS) position information is included in output result metadata. |  | android.statistics.info.availableOisDataModes | 3.3 |
Details
Since optical image stabilization generally involves motion much faster than the duration of individualq image exposure, multiple OIS samples can be included for a single capture result. For example, if the OIS reporting operates at 200 Hz, a typical camera operating at 30fps may have 6-7 OIS samples per capture result. This information can be combined with the rolling shutter skew to account for lens motion during image exposure in post-processing algorithms.
android.statistics.oisTimestamps | int64 x n [ndk_public] | An array of timestamps of OIS samples, in nanoseconds. | nanoseconds |  | 3.3 |
Details
The array contains the timestamps of OIS samples. The timestamps are in the same timebase as and comparable to android.sensor.timestamp.
android.statistics.oisXShifts | float x n [ndk_public] | An array of shifts of OIS samples, in x direction. | Pixels in active array. |  | 3.3 |
Details
The array contains the amount of shifts in x direction, in pixels, based on OIS samples. A positive value is a shift from left to right in the pre-correction active array coordinate system. For example, if the optical center is (1000, 500) in pre-correction active array coordinates, a shift of (3, 0) puts the new optical center at (1003, 500). The number of shifts must match the number of timestamps in android.statistics.oisTimestamps. The OIS samples are not affected by whether lens distortion correction is enabled (on supporting devices). They are always reported in pre-correction active array coordinates, since the scaling of OIS shifts would depend on the specific spot on the sensor the shift is needed.
android.statistics.oisYShifts | float x n [ndk_public] | An array of shifts of OIS samples, in y direction. | Pixels in active array. |  | 3.3 |
Details
The array contains the amount of shifts in y direction, in pixels, based on OIS samples. A positive value is a shift from top to bottom in pre-correction active array coordinate system. For example, if the optical center is (1000, 500) in active array coordinates, a shift of (0, 5) puts the new optical center at (1000, 505). The number of shifts must match the number of timestamps in android.statistics.oisTimestamps. The OIS samples are not affected by whether lens distortion correction is enabled (on supporting devices). They are always reported in pre-correction active array coordinates, since the scaling of OIS shifts would depend on the specific spot on the sensor the shift is needed.
android.statistics.oisSamples | float x n [java_public as oisSample] [synthetic] | An array of optical stabilization (OIS) position samples. |  |  | 3.3 |
Details
Each OIS sample contains the timestamp and the amount of shifts in x and y direction, in pixels, of the OIS sample. A positive value for a shift in x direction is a shift from left to right in the pre-correction active array coordinate system. For example, if the optical center is (1000, 500) in pre-correction active array coordinates, a shift of (3, 0) puts the new optical center at (1003, 500). A positive value for a shift in y direction is a shift from top to bottom in pre-correction active array coordinate system. For example, if the optical center is (1000, 500) in active array coordinates, a shift of (0, 5) puts the new optical center at (1000, 505). The OIS samples are not affected by whether lens distortion correction is enabled (on supporting devices). They are always reported in pre-correction active array coordinates, since the scaling of OIS shifts would depend on the specific spot on the sensor the shift is needed.
tonemap
controls
Property Name | Type | Description | Units | Range | Initial HIDL HAL version | Tags
android.tonemap.curveBlue | float x n x 2 [ndk_public] [full] 1D array of float pairs (P_IN, P_OUT). The maximum number of pairs is specified by android.tonemap.maxCurvePoints. | Tonemapping / contrast / gamma curve for the blue channel, to use when android.tonemap.mode is CONTRAST_CURVE. |  |  | 3.2 |
Details
See android.tonemap.curveRed for more details.
android.tonemap.curveGreen | float x n x 2 [ndk_public] [full] 1D array of float pairs (P_IN, P_OUT). The maximum number of pairs is specified by android.tonemap.maxCurvePoints. | Tonemapping / contrast / gamma curve for the green channel, to use when android.tonemap.mode is CONTRAST_CURVE. |  |  | 3.2 |
Details
See android.tonemap.curveRed for more details.
android.tonemap.curveRed | float x n x 2 [ndk_public] [full] 1D array of float pairs (P_IN, P_OUT). The maximum number of pairs is specified by android.tonemap.maxCurvePoints. | Tonemapping / contrast / gamma curve for the red channel, to use when android.tonemap.mode is CONTRAST_CURVE. |  | 0-1 on both input and output coordinates, normalized as a floating-point value such that 0 == black and 1 == white. | 3.2 |
Details
Each channel's curve is defined by an array of control points:
    android.tonemap.curveRed =
      [ P0in, P0out, P1in, P1out, P2in, P2out, P3in, P3out, ..., PNin, PNout ]
    2 <= N <= android.tonemap.maxCurvePoints
These are sorted in order of increasing `Pin`; it is required that input values 0.0 and 1.0 are included in the list to define a complete mapping. For input values between control points, the camera device must linearly interpolate between the control points. Each curve can have an independent number of points, and the number of points can be less than max (that is, the request doesn't have to always provide a curve with number of points equivalent to android.tonemap.maxCurvePoints). For devices with MONOCHROME capability, all three channels must have the same set of control points. A few examples, and their corresponding graphical mappings; these only specify the red channel and the precision is limited to 4 digits, for conciseness. Linear mapping:
    android.tonemap.curveRed = [ 0, 0, 1.0, 1.0 ]
Invert mapping:
    android.tonemap.curveRed = [ 0, 1.0, 1.0, 0 ]
Gamma 1/2.2 mapping, with 16 control points:
    android.tonemap.curveRed = [
      0.0000, 0.0000, 0.0667, 0.2920, 0.1333, 0.4002, 0.2000, 0.4812,
      0.2667, 0.5484, 0.3333, 0.6069, 0.4000, 0.6594, 0.4667, 0.7072,
      0.5333, 0.7515, 0.6000, 0.7928, 0.6667, 0.8317, 0.7333, 0.8685,
      0.8000, 0.9035, 0.8667, 0.9370, 0.9333, 0.9691, 1.0000, 1.0000 ]
Standard sRGB gamma mapping, per IEC 61966-2-1:1999, with 16 control points:
    android.tonemap.curveRed = [
      0.0000, 0.0000, 0.0667, 0.2864, 0.1333, 0.4007, 0.2000, 0.4845,
      0.2667, 0.5532, 0.3333, 0.6125, 0.4000, 0.6652, 0.4667, 0.7130,
      0.5333, 0.7569, 0.6000, 0.7977, 0.6667, 0.8360, 0.7333, 0.8721,
      0.8000, 0.9063, 0.8667, 0.9389, 0.9333, 0.9701, 1.0000, 1.0000 ]
HAL Implementation Details
For good quality of mapping, at least 128 control points are preferred. A typical use case of this would be a gamma-1/2.2 curve, with as many control points used as are available.
android.tonemap.curve | float [java_public as tonemapCurve] [synthetic] [full] | Tonemapping / contrast / gamma curve to use when android.tonemap.mode is CONTRAST_CURVE. |  |  | 3.2 |
Details
The tonemapCurve consist of three curves for each of red, green, and blue channels respectively. The following example uses the red channel as an example. The same logic applies to green and blue channel. Each channel's curve is defined by an array of control points:
    curveRed =
      [ P0(in, out), P1(in, out), P2(in, out), P3(in, out), ..., PN(in, out) ]
    2 <= N <= android.tonemap.maxCurvePoints
These are sorted in order of increasing `Pin`; it is always guaranteed that input values 0.0 and 1.0 are included in the list to define a complete mapping. For input values between control points, the camera device must linearly interpolate between the control points. Each curve can have an independent number of points, and the number of points can be less than max (that is, the request doesn't have to always provide a curve with number of points equivalent to android.tonemap.maxCurvePoints). For devices with MONOCHROME capability, all three channels must have the same set of control points. A few examples, and their corresponding graphical mappings; these only specify the red channel and the precision is limited to 4 digits, for conciseness. Linear mapping:
    curveRed = [ (0, 0), (1.0, 1.0) ]
Invert mapping:
    curveRed = [ (0, 1.0), (1.0, 0) ]
Gamma 1/2.2 mapping, with 16 control points:
    curveRed = [
      (0.0000, 0.0000), (0.0667, 0.2920), (0.1333, 0.4002), (0.2000, 0.4812),
      (0.2667, 0.5484), (0.3333, 0.6069), (0.4000, 0.6594), (0.4667, 0.7072),
      (0.5333, 0.7515), (0.6000, 0.7928), (0.6667, 0.8317), (0.7333, 0.8685),
      (0.8000, 0.9035), (0.8667, 0.9370), (0.9333, 0.9691), (1.0000, 1.0000) ]
Standard sRGB gamma mapping, per IEC 61966-2-1:1999, with 16 control points:
    curveRed = [
      (0.0000, 0.0000), (0.0667, 0.2864), (0.1333, 0.4007), (0.2000, 0.4845),
      (0.2667, 0.5532), (0.3333, 0.6125), (0.4000, 0.6652), (0.4667, 0.7130),
      (0.5333, 0.7569), (0.6000, 0.7977), (0.6667, 0.8360), (0.7333, 0.8721),
      (0.8000, 0.9063), (0.8667, 0.9389), (0.9333, 0.9701), (1.0000, 1.0000) ]
HAL Implementation Details
This entry is created by the framework from the curveRed, curveGreen and curveBlue entries.
android.tonemap.mode | byte [public] [full] CONTRAST_CURVE (v3.2) Use the tone mapping curve specified in the android.tonemap.curve* entries. All color enhancement and tonemapping must be disabled, except for applying the tonemapping curve specified by android.tonemap.curve. Must not slow down frame rate relative to raw sensor output. FAST (v3.2) Advanced gamma mapping and color enhancement may be applied, without reducing frame rate compared to raw sensor output. HIGH_QUALITY (v3.2) High-quality gamma mapping and color enhancement will be applied, at the cost of possibly reduced frame rate compared to raw sensor output. GAMMA_VALUE (v3.2) Use the gamma value specified in android.tonemap.gamma to peform tonemapping. All color enhancement and tonemapping must be disabled, except for applying the tonemapping curve specified by android.tonemap.gamma. Must not slow down frame rate relative to raw sensor output. PRESET_CURVE (v3.2) Use the preset tonemapping curve specified in android.tonemap.presetCurve to peform tonemapping. All color enhancement and tonemapping must be disabled, except for applying the tonemapping curve specified by android.tonemap.presetCurve. Must not slow down frame rate relative to raw sensor output. | High-level global contrast/gamma/tonemapping control. |  | android.tonemap.availableToneMapModes | 3.2 |
Details
When switching to an application-defined contrast curve by setting android.tonemap.mode to CONTRAST_CURVE, the curve is defined per-channel with a set of `(in, out)` points that specify the mapping from input high-bit-depth pixel value to the output low-bit-depth value. Since the actual pixel ranges of both input and output may change depending on the camera pipeline, the values are specified by normalized floating-point numbers. More-complex color mapping operations such as 3D color look-up tables, selective chroma enhancement, or other non-linear color transforms will be disabled when android.tonemap.mode is CONTRAST_CURVE. When using either FAST or HIGH_QUALITY, the camera device will emit its own tonemap curve in android.tonemap.curve. These values are always available, and as close as possible to the actually used nonlinear/nonglobal transforms. If a request is sent with CONTRAST_CURVE with the camera device's provided curve in FAST or HIGH_QUALITY, the image's tonemap will be roughly the same.
android.tonemap.gamma | float [public] | Tonemapping curve to use when android.tonemap.mode is GAMMA_VALUE |  |  | 3.2 |
Details
The tonemap curve will be defined the following formula: * OUT = pow(IN, 1.0 / gamma) where IN and OUT is the input pixel value scaled to range [0.0, 1.0], pow is the power function and gamma is the gamma value specified by this key. The same curve will be applied to all color channels. The camera device may clip the input gamma value to its supported range. The actual applied value will be returned in capture result. The valid range of gamma value varies on different devices, but values within [1.0, 5.0] are guaranteed not to be clipped.
android.tonemap.presetCurve | byte [public] SRGB (v3.2) Tonemapping curve is defined by sRGB REC709 (v3.2) Tonemapping curve is defined by ITU-R BT.709 | Tonemapping curve to use when android.tonemap.mode is PRESET_CURVE |  |  | 3.2 |
Details
The tonemap curve will be defined by specified standard. sRGB (approximated by 16 control points): Rec. 709 (approximated by 16 control points): Note that above figures show a 16 control points approximation of preset curves. Camera devices may apply a different approximation to the curve.
static
Property Name | Type | Description | Units | Range | Initial HIDL HAL version | Tags
android.tonemap.maxCurvePoints | int32 [public] [full] | Maximum number of supported points in the tonemap curve that can be used for android.tonemap.curve. |  |  | 3.2 |
Details
If the actual number of points provided by the application (in android.tonemap.curve*) is less than this maximum, the camera device will resample the curve to its internal representation, using linear interpolation. The output curves in the result metadata may have a different number of points than the input curves, and will represent the actual hardware curves used as closely as possible when linearly interpolated.
HAL Implementation Details
This value must be at least 64. This should be at least 128.
android.tonemap.availableToneMapModes | byte x n [public as enumList] [full] list of enums | List of tonemapping modes for android.tonemap.mode that are supported by this camera device. |  | Any value listed in android.tonemap.mode | 3.2 |
Details
Camera devices that support the MANUAL_POST_PROCESSING capability will always contain at least one of below mode combinations: CONTRAST_CURVE, FAST and HIGH_QUALITY GAMMA_VALUE, PRESET_CURVE, FAST and HIGH_QUALITY This includes all FULL level devices.
HAL Implementation Details
HAL must support both FAST and HIGH_QUALITY if automatic tonemap control is available on the camera device, but the underlying implementation can be the same for both modes. That is, if the highest quality implementation on the camera device does not slow down capture rate, then FAST and HIGH_QUALITY will generate the same output.
dynamic
Property Name | Type | Description | Units | Range | Initial HIDL HAL version | Tags
android.tonemap.curveBlue | float x n x 2 [ndk_public] [full] 1D array of float pairs (P_IN, P_OUT). The maximum number of pairs is specified by android.tonemap.maxCurvePoints. | Tonemapping / contrast / gamma curve for the blue channel, to use when android.tonemap.mode is CONTRAST_CURVE. |  |  | 3.2 |
Details
See android.tonemap.curveRed for more details.
android.tonemap.curveGreen | float x n x 2 [ndk_public] [full] 1D array of float pairs (P_IN, P_OUT). The maximum number of pairs is specified by android.tonemap.maxCurvePoints. | Tonemapping / contrast / gamma curve for the green channel, to use when android.tonemap.mode is CONTRAST_CURVE. |  |  | 3.2 |
Details
See android.tonemap.curveRed for more details.
android.tonemap.curveRed | float x n x 2 [ndk_public] [full] 1D array of float pairs (P_IN, P_OUT). The maximum number of pairs is specified by android.tonemap.maxCurvePoints. | Tonemapping / contrast / gamma curve for the red channel, to use when android.tonemap.mode is CONTRAST_CURVE. |  | 0-1 on both input and output coordinates, normalized as a floating-point value such that 0 == black and 1 == white. | 3.2 |
Details
Each channel's curve is defined by an array of control points:
    android.tonemap.curveRed =
      [ P0in, P0out, P1in, P1out, P2in, P2out, P3in, P3out, ..., PNin, PNout ]
    2 <= N <= android.tonemap.maxCurvePoints
These are sorted in order of increasing `Pin`; it is required that input values 0.0 and 1.0 are included in the list to define a complete mapping. For input values between control points, the camera device must linearly interpolate between the control points. Each curve can have an independent number of points, and the number of points can be less than max (that is, the request doesn't have to always provide a curve with number of points equivalent to android.tonemap.maxCurvePoints). For devices with MONOCHROME capability, all three channels must have the same set of control points. A few examples, and their corresponding graphical mappings; these only specify the red channel and the precision is limited to 4 digits, for conciseness. Linear mapping:
    android.tonemap.curveRed = [ 0, 0, 1.0, 1.0 ]
Invert mapping:
    android.tonemap.curveRed = [ 0, 1.0, 1.0, 0 ]
Gamma 1/2.2 mapping, with 16 control points:
    android.tonemap.curveRed = [
      0.0000, 0.0000, 0.0667, 0.2920, 0.1333, 0.4002, 0.2000, 0.4812,
      0.2667, 0.5484, 0.3333, 0.6069, 0.4000, 0.6594, 0.4667, 0.7072,
      0.5333, 0.7515, 0.6000, 0.7928, 0.6667, 0.8317, 0.7333, 0.8685,
      0.8000, 0.9035, 0.8667, 0.9370, 0.9333, 0.9691, 1.0000, 1.0000 ]
Standard sRGB gamma mapping, per IEC 61966-2-1:1999, with 16 control points:
    android.tonemap.curveRed = [
      0.0000, 0.0000, 0.0667, 0.2864, 0.1333, 0.4007, 0.2000, 0.4845,
      0.2667, 0.5532, 0.3333, 0.6125, 0.4000, 0.6652, 0.4667, 0.7130,
      0.5333, 0.7569, 0.6000, 0.7977, 0.6667, 0.8360, 0.7333, 0.8721,
      0.8000, 0.9063, 0.8667, 0.9389, 0.9333, 0.9701, 1.0000, 1.0000 ]
HAL Implementation Details
For good quality of mapping, at least 128 control points are preferred. A typical use case of this would be a gamma-1/2.2 curve, with as many control points used as are available.
android.tonemap.curve | float [java_public as tonemapCurve] [synthetic] [full] | Tonemapping / contrast / gamma curve to use when android.tonemap.mode is CONTRAST_CURVE. |  |  | 3.2 |
Details
The tonemapCurve consist of three curves for each of red, green, and blue channels respectively. The following example uses the red channel as an example. The same logic applies to green and blue channel. Each channel's curve is defined by an array of control points:
    curveRed =
      [ P0(in, out), P1(in, out), P2(in, out), P3(in, out), ..., PN(in, out) ]
    2 <= N <= android.tonemap.maxCurvePoints
These are sorted in order of increasing `Pin`; it is always guaranteed that input values 0.0 and 1.0 are included in the list to define a complete mapping. For input values between control points, the camera device must linearly interpolate between the control points. Each curve can have an independent number of points, and the number of points can be less than max (that is, the request doesn't have to always provide a curve with number of points equivalent to android.tonemap.maxCurvePoints). For devices with MONOCHROME capability, all three channels must have the same set of control points. A few examples, and their corresponding graphical mappings; these only specify the red channel and the precision is limited to 4 digits, for conciseness. Linear mapping:
    curveRed = [ (0, 0), (1.0, 1.0) ]
Invert mapping:
    curveRed = [ (0, 1.0), (1.0, 0) ]
Gamma 1/2.2 mapping, with 16 control points:
    curveRed = [
      (0.0000, 0.0000), (0.0667, 0.2920), (0.1333, 0.4002), (0.2000, 0.4812),
      (0.2667, 0.5484), (0.3333, 0.6069), (0.4000, 0.6594), (0.4667, 0.7072),
      (0.5333, 0.7515), (0.6000, 0.7928), (0.6667, 0.8317), (0.7333, 0.8685),
      (0.8000, 0.9035), (0.8667, 0.9370), (0.9333, 0.9691), (1.0000, 1.0000) ]
Standard sRGB gamma mapping, per IEC 61966-2-1:1999, with 16 control points:
    curveRed = [
      (0.0000, 0.0000), (0.0667, 0.2864), (0.1333, 0.4007), (0.2000, 0.4845),
      (0.2667, 0.5532), (0.3333, 0.6125), (0.4000, 0.6652), (0.4667, 0.7130),
      (0.5333, 0.7569), (0.6000, 0.7977), (0.6667, 0.8360), (0.7333, 0.8721),
      (0.8000, 0.9063), (0.8667, 0.9389), (0.9333, 0.9701), (1.0000, 1.0000) ]
HAL Implementation Details
This entry is created by the framework from the curveRed, curveGreen and curveBlue entries.
android.tonemap.mode | byte [public] [full] CONTRAST_CURVE (v3.2) Use the tone mapping curve specified in the android.tonemap.curve* entries. All color enhancement and tonemapping must be disabled, except for applying the tonemapping curve specified by android.tonemap.curve. Must not slow down frame rate relative to raw sensor output. FAST (v3.2) Advanced gamma mapping and color enhancement may be applied, without reducing frame rate compared to raw sensor output. HIGH_QUALITY (v3.2) High-quality gamma mapping and color enhancement will be applied, at the cost of possibly reduced frame rate compared to raw sensor output. GAMMA_VALUE (v3.2) Use the gamma value specified in android.tonemap.gamma to peform tonemapping. All color enhancement and tonemapping must be disabled, except for applying the tonemapping curve specified by android.tonemap.gamma. Must not slow down frame rate relative to raw sensor output. PRESET_CURVE (v3.2) Use the preset tonemapping curve specified in android.tonemap.presetCurve to peform tonemapping. All color enhancement and tonemapping must be disabled, except for applying the tonemapping curve specified by android.tonemap.presetCurve. Must not slow down frame rate relative to raw sensor output. | High-level global contrast/gamma/tonemapping control. |  | android.tonemap.availableToneMapModes | 3.2 |
Details
When switching to an application-defined contrast curve by setting android.tonemap.mode to CONTRAST_CURVE, the curve is defined per-channel with a set of `(in, out)` points that specify the mapping from input high-bit-depth pixel value to the output low-bit-depth value. Since the actual pixel ranges of both input and output may change depending on the camera pipeline, the values are specified by normalized floating-point numbers. More-complex color mapping operations such as 3D color look-up tables, selective chroma enhancement, or other non-linear color transforms will be disabled when android.tonemap.mode is CONTRAST_CURVE. When using either FAST or HIGH_QUALITY, the camera device will emit its own tonemap curve in android.tonemap.curve. These values are always available, and as close as possible to the actually used nonlinear/nonglobal transforms. If a request is sent with CONTRAST_CURVE with the camera device's provided curve in FAST or HIGH_QUALITY, the image's tonemap will be roughly the same.
android.tonemap.gamma | float [public] | Tonemapping curve to use when android.tonemap.mode is GAMMA_VALUE |  |  | 3.2 |
Details
The tonemap curve will be defined the following formula: * OUT = pow(IN, 1.0 / gamma) where IN and OUT is the input pixel value scaled to range [0.0, 1.0], pow is the power function and gamma is the gamma value specified by this key. The same curve will be applied to all color channels. The camera device may clip the input gamma value to its supported range. The actual applied value will be returned in capture result. The valid range of gamma value varies on different devices, but values within [1.0, 5.0] are guaranteed not to be clipped.
android.tonemap.presetCurve | byte [public] SRGB (v3.2) Tonemapping curve is defined by sRGB REC709 (v3.2) Tonemapping curve is defined by ITU-R BT.709 | Tonemapping curve to use when android.tonemap.mode is PRESET_CURVE |  |  | 3.2 |
Details
The tonemap curve will be defined by specified standard. sRGB (approximated by 16 control points): Rec. 709 (approximated by 16 control points): Note that above figures show a 16 control points approximation of preset curves. Camera devices may apply a different approximation to the curve.
led
controls
Property Name | Type | Description | Units | Range | Initial HIDL HAL version | Tags
android.led.transmit | byte [hidden as boolean] OFF (v3.2) ON (v3.2) | This LED is nominally used to indicate to the user that the camera is powered on and may be streaming images back to the Application Processor. In certain rare circumstances, the OS may disable this when video is processed locally and not transmitted to any untrusted applications. In particular, the LED must always be on when the data could be transmitted off the device. The LED should always be on whenever data is stored locally on the device. The LED may be off if a trusted application is using the data that doesn't violate the above rules. |  |  | 3.2 |
dynamic
Property Name | Type | Description | Units | Range | Initial HIDL HAL version | Tags
android.led.transmit | byte [hidden as boolean] OFF (v3.2) ON (v3.2) | This LED is nominally used to indicate to the user that the camera is powered on and may be streaming images back to the Application Processor. In certain rare circumstances, the OS may disable this when video is processed locally and not transmitted to any untrusted applications. In particular, the LED must always be on when the data could be transmitted off the device. The LED should always be on whenever data is stored locally on the device. The LED may be off if a trusted application is using the data that doesn't violate the above rules. |  |  | 3.2 |
static
Property Name | Type | Description | Units | Range | Initial HIDL HAL version | Tags
android.led.availableLeds | byte x n [hidden] TRANSMIT (v3.2) android.led.transmit control is used. | A list of camera LEDs that are available on this system. |  |  | 3.2 |
info
static
Property Name | Type | Description | Units | Range | Initial HIDL HAL version | Tags
android.info.supportedHardwareLevel | byte [public] [legacy] LIMITED (v3.2) This camera device does not have enough capabilities to qualify as a `FULL` device or better. Only the stream configurations listed in the `LEGACY` and `LIMITED` tables in the createCaptureSession documentation are guaranteed to be supported. All `LIMITED` devices support the `BACKWARDS_COMPATIBLE` capability, indicating basic support for color image capture. The only exception is that the device may alternatively support only the `DEPTH_OUTPUT` capability, if it can only output depth measurements and not color images. `LIMITED` devices and above require the use of android.control.aePrecaptureTrigger to lock exposure metering (and calculate flash power, for cameras with flash) before capturing a high-quality still image. A `LIMITED` device that only lists the `BACKWARDS_COMPATIBLE` capability is only required to support full-automatic operation and post-processing (`OFF` is not supported for android.control.aeMode, android.control.afMode, or android.control.awbMode) Additional capabilities may optionally be supported by a `LIMITED`-level device, and can be checked for in android.request.availableCapabilities. FULL (v3.2) This camera device is capable of supporting advanced imaging applications. The stream configurations listed in the `FULL`, `LEGACY` and `LIMITED` tables in the createCaptureSession documentation are guaranteed to be supported. A `FULL` device will support below capabilities: `BURST_CAPTURE` capability (android.request.availableCapabilities contains `BURST_CAPTURE`) Per frame control (android.sync.maxLatency `==` PER_FRAME_CONTROL) Manual sensor control (android.request.availableCapabilities contains `MANUAL_SENSOR`) Manual post-processing control (android.request.availableCapabilities contains `MANUAL_POST_PROCESSING`) The required exposure time range defined in android.sensor.info.exposureTimeRange The required maxFrameDuration defined in android.sensor.info.maxFrameDuration Note: Pre-API level 23, FULL devices also supported arbitrary cropping region (android.scaler.croppingType `== FREEFORM`); this requirement was relaxed in API level 23, and `FULL` devices may only support `CENTERED` cropping. LEGACY (v3.2) This camera device is running in backward compatibility mode. Only the stream configurations listed in the `LEGACY` table in the createCaptureSession documentation are supported. A `LEGACY` device does not support per-frame control, manual sensor control, manual post-processing, arbitrary cropping regions, and has relaxed performance constraints. No additional capabilities beyond `BACKWARD_COMPATIBLE` will ever be listed by a `LEGACY` device in android.request.availableCapabilities. In addition, the android.control.aePrecaptureTrigger is not functional on `LEGACY` devices. Instead, every request that includes a JPEG-format output target is treated as triggering a still capture, internally executing a precapture trigger. This may fire the flash for flash power metering during precapture, and then fire the flash for the final capture, if a flash is available on the device and the AE mode is set to enable the flash. Devices that initially shipped with Android version Q or newer will not include any LEGACY-level devices. 3 (v3.2) This camera device is capable of YUV reprocessing and RAW data capture, in addition to FULL-level capabilities. The stream configurations listed in the `LEVEL_3`, `RAW`, `FULL`, `LEGACY` and `LIMITED` tables in the createCaptureSession documentation are guaranteed to be supported. The following additional capabilities are guaranteed to be supported: `YUV_REPROCESSING` capability (android.request.availableCapabilities contains `YUV_REPROCESSING`) `RAW` capability (android.request.availableCapabilities contains `RAW`) EXTERNAL (v3.3) This camera device is backed by an external camera connected to this Android device. The device has capability identical to a LIMITED level device, with the following exceptions: The device may not report lens/sensor related information such as android.lens.focalLength android.lens.info.hyperfocalDistance android.sensor.info.physicalSize android.sensor.info.whiteLevel android.sensor.blackLevelPattern android.sensor.info.colorFilterArrangement android.sensor.rollingShutterSkew The device will report 0 for android.sensor.orientation The device has less guarantee on stable framerate, as the framerate partly depends on the external camera being used. | Generally classifies the overall set of the camera device functionality. |  |  | 3.2 |
Details
The supported hardware level is a high-level description of the camera device's capabilities, summarizing several capabilities into one field. Each level adds additional features to the previous one, and is always a strict superset of the previous level. The ordering is `LEGACY < LIMITED < FULL < LEVEL_3`. Starting from `LEVEL_3`, the level enumerations are guaranteed to be in increasing numerical value as well. To check if a given device is at least at a given hardware level, the following code snippet can be used:
    // Returns true if the device supports the required hardware level, or better.
    boolean isHardwareLevelSupported(CameraCharacteristics c, int requiredLevel) {
        final int[] sortedHwLevels = {
            CameraCharacteristics.INFO_SUPPORTED_HARDWARE_LEVEL_LEGACY,
            CameraCharacteristics.INFO_SUPPORTED_HARDWARE_LEVEL_EXTERNAL,
            CameraCharacteristics.INFO_SUPPORTED_HARDWARE_LEVEL_LIMITED,
            CameraCharacteristics.INFO_SUPPORTED_HARDWARE_LEVEL_FULL,
            CameraCharacteristics.INFO_SUPPORTED_HARDWARE_LEVEL_3
        };
        int deviceLevel = c.get(CameraCharacteristics.INFO_SUPPORTED_HARDWARE_LEVEL);
        if (requiredLevel == deviceLevel) {
            return true;
        }

        for (int sortedlevel : sortedHwLevels) {
            if (sortedlevel == requiredLevel) {
                return true;
            } else if (sortedlevel == deviceLevel) {
                return false;
            }
        }
        return false; // Should never reach here
    }
At a high level, the levels are: `LEGACY` devices operate in a backwards-compatibility mode for older Android devices, and have very limited capabilities. `LIMITED` devices represent the baseline feature set, and may also include additional capabilities that are subsets of `FULL`. `FULL` devices additionally support per-frame manual control of sensor, flash, lens and post-processing settings, and image capture at a high rate. `LEVEL_3` devices additionally support YUV reprocessing and RAW image capture, along with additional output stream configurations. `EXTERNAL` devices are similar to `LIMITED` devices with exceptions like some sensor or lens information not reported or less stable framerates. See the individual level enums for full descriptions of the supported capabilities. The android.request.availableCapabilities entry describes the device's capabilities at a finer-grain level, if needed. In addition, many controls have their available settings or ranges defined in individual entries from CameraCharacteristics. Some features are not part of any particular hardware level or capability and must be queried separately. These include: Calibrated timestamps (android.sensor.info.timestampSource `==` REALTIME) Precision lens control (android.lens.info.focusDistanceCalibration `==` CALIBRATED) Face detection (android.statistics.info.availableFaceDetectModes) Optical or electrical image stabilization (android.lens.info.availableOpticalStabilization, android.control.availableVideoStabilizationModes)
HAL Implementation Details
A camera HALv3 device can implement one of three possible operational modes; LIMITED, FULL, and LEVEL_3. FULL support or better is expected from new higher-end devices. Limited mode has hardware requirements roughly in line with those for a camera HAL device v1 implementation, and is expected from older or inexpensive devices. Each level is a strict superset of the previous level, and they share the same essential operational flow. For full details refer to "S3. Operational Modes" in camera3.h Camera HAL3+ must not implement LEGACY mode. It is there for backwards compatibility in the `android.hardware.camera2` user-facing API only on legacy HALv1 devices, and is implemented by the camera framework code. EXTERNAL level devices have lower peformance bar in CTS since the peformance might depend on the external camera being used and is not fully controlled by the device manufacturer. The ITS test suite is exempted for the same reason.
android.info.version | byte [public as string] | A short string for manufacturer version information about the camera device, such as ISP hardware, sensors, etc. |  |  | 3.3 |
Details
This can be used in TAG_IMAGE_DESCRIPTION in jpeg EXIF. This key may be absent if no version information is available on the device.
HAL Implementation Details
The string must consist of only alphanumeric characters, punctuation, and whitespace, i.e. it must match regular expression "[\p{Alnum}\p{Punct}\p{Space}]*". It must not exceed 256 characters.
android.info.supportedBufferManagementVersion | byte [system] HIDL_DEVICE_3_5 (v3.4) This camera device supports and opts in to the buffer management APIs provided by HIDL ICameraDevice version 3.5. | The version of buffer management API this camera device supports and opts into. |  |  | 3.4 |
Details
When this key is not present, camera framework will interact with this camera device without any buffer management HAL API. When this key is present and camera framework supports the buffer management API version, camera framework will interact with camera HAL using such version of buffer management API.
blackLevel
controls
Property Name | Type | Description | Units | Range | Initial HIDL HAL version | Tags
android.blackLevel.lock | byte [public as boolean] [full] OFF (v3.2) ON (v3.2) | Whether black-level compensation is locked to its current values, or is free to vary. |  |  | 3.2 | HAL2
Details
When set to `true` (ON), the values used for black-level compensation will not change until the lock is set to `false` (OFF). Since changes to certain capture parameters (such as exposure time) may require resetting of black level compensation, the camera device must report whether setting the black level lock was successful in the output result metadata. For example, if a sequence of requests is as follows: Request 1: Exposure = 10ms, Black level lock = OFF Request 2: Exposure = 10ms, Black level lock = ON Request 3: Exposure = 10ms, Black level lock = ON Request 4: Exposure = 20ms, Black level lock = ON Request 5: Exposure = 20ms, Black level lock = ON Request 6: Exposure = 20ms, Black level lock = ON And the exposure change in Request 4 requires the camera device to reset the black level offsets, then the output result metadata is expected to be: Result 1: Exposure = 10ms, Black level lock = OFF Result 2: Exposure = 10ms, Black level lock = ON Result 3: Exposure = 10ms, Black level lock = ON Result 4: Exposure = 20ms, Black level lock = OFF Result 5: Exposure = 20ms, Black level lock = ON Result 6: Exposure = 20ms, Black level lock = ON This indicates to the application that on frame 4, black levels were reset due to exposure value changes, and pixel values may not be consistent across captures. The camera device will maintain the lock to the extent possible, only overriding the lock to OFF when changes to other request parameters require a black level recalculation or reset.
HAL Implementation Details
If for some reason black level locking is no longer possible (for example, the analog gain has changed, which forces black level offsets to be recalculated), then the HAL must override this request (and it must report 'OFF' when this does happen) until the next capture for which locking is possible again.
dynamic
Property Name | Type | Description | Units | Range | Initial HIDL HAL version | Tags
android.blackLevel.lock | byte [public as boolean] [full] OFF (v3.2) ON (v3.2) | Whether black-level compensation is locked to its current values, or is free to vary. |  |  | 3.2 | HAL2
Details
Whether the black level offset was locked for this frame. Should be ON if android.blackLevel.lock was ON in the capture request, unless a change in other capture settings forced the camera device to perform a black level reset.
HAL Implementation Details
If for some reason black level locking is no longer possible (for example, the analog gain has changed, which forces black level offsets to be recalculated), then the HAL must override this request (and it must report 'OFF' when this does happen) until the next capture for which locking is possible again.
sync
dynamic
Property Name | Type | Description | Units | Range | Initial HIDL HAL version | Tags
android.sync.frameNumber | int64 [ndk_public] [legacy] CONVERGING (v3.2) -1 The current result is not yet fully synchronized to any request. Synchronization is in progress, and reading metadata from this result may include a mix of data that have taken effect since the last synchronization time. In some future result, within android.sync.maxLatency frames, this value will update to the actual frame number frame number the result is guaranteed to be synchronized to (as long as the request settings remain constant). UNKNOWN (v3.2) -2 The current result's synchronization status is unknown. The result may have already converged, or it may be in progress. Reading from this result may include some mix of settings from past requests. After a settings change, the new settings will eventually all take effect for the output buffers and results. However, this value will not change when that happens. Altering settings rapidly may provide outcomes using mixes of settings from recent requests. This value is intended primarily for backwards compatibility with the older camera implementations (for android.hardware.Camera). | The frame number corresponding to the last request with which the output result (metadata + buffers) has been fully synchronized. |  | Either a non-negative value corresponding to a `frame_number`, or one of the two enums (CONVERGING / UNKNOWN). | 3.2 | V1
Details
When a request is submitted to the camera device, there is usually a delay of several frames before the controls get applied. A camera device may either choose to account for this delay by implementing a pipeline and carefully submit well-timed atomic control updates, or it may start streaming control changes that span over several frame boundaries. In the latter case, whenever a request's settings change relative to the previous submitted request, the full set of changes may take multiple frame durations to fully take effect. Some settings may take effect sooner (in less frame durations) than others. While a set of control changes are being propagated, this value will be CONVERGING. Once it is fully known that a set of control changes have been finished propagating, and the resulting updated control settings have been read back by the camera device, this value will be set to a non-negative frame number (corresponding to the request to which the results have synchronized to). Older camera device implementations may not have a way to detect when all camera controls have been applied, and will always set this value to UNKNOWN. FULL capability devices will always have this value set to the frame number of the request corresponding to this result. Further details: Whenever a request differs from the last request, any future results not yet returned may have this value set to CONVERGING (this could include any in-progress captures not yet returned by the camera device, for more details see pipeline considerations below). Submitting a series of multiple requests that differ from the previous request (e.g. r1, r2, r3 s.t. r1 != r2 != r3) moves the new synchronization frame to the last non-repeating request (using the smallest frame number from the contiguous list of repeating requests). Submitting the same request repeatedly will not change this value to CONVERGING, if it was already a non-negative value. When this value changes to non-negative, that means that all of the metadata controls from the request have been applied, all of the metadata controls from the camera device have been read to the updated values (into the result), and all of the graphics buffers corresponding to this result are also synchronized to the request. Pipeline considerations: Submitting a request with updated controls relative to the previously submitted requests may also invalidate the synchronization state of all the results corresponding to currently in-flight requests. In other words, results for this current request and up to android.request.pipelineMaxDepth prior requests may have their android.sync.frameNumber change to CONVERGING.
HAL Implementation Details
Using UNKNOWN here is illegal unless android.sync.maxLatency is also UNKNOWN. FULL capability devices should simply set this value to the `frame_number` of the request this result corresponds to.
static
Property Name | Type | Description | Units | Range | Initial HIDL HAL version | Tags
android.sync.maxLatency | int32 [public] [legacy] PER_FRAME_CONTROL (v3.2) 0 Every frame has the requests immediately applied. Changing controls over multiple requests one after another will produce results that have those controls applied atomically each frame. All FULL capability devices will have this as their maxLatency. UNKNOWN (v3.2) -1 Each new frame has some subset (potentially the entire set) of the past requests applied to the camera settings. By submitting a series of identical requests, the camera device will eventually have the camera settings applied, but it is unknown when that exact point will be. All LEGACY capability devices will have this as their maxLatency. | The maximum number of frames that can occur after a request (different than the previous) has been submitted, and before the result's state becomes synchronized. | Frame counts | A positive value, PER_FRAME_CONTROL, or UNKNOWN. | 3.2 | V1
Details
This defines the maximum distance (in number of metadata results), between the frame number of the request that has new controls to apply and the frame number of the result that has all the controls applied. In other words this acts as an upper boundary for how many frames must occur before the camera device knows for a fact that the new submitted camera settings have been applied in outgoing frames.
HAL Implementation Details
For example if maxLatency was 2,
    initial request = X (repeating)
    request1 = X
    request2 = Y
    request3 = Y
    request4 = Y

    where requestN has frameNumber N, and the first of the repeating
    initial request's has frameNumber F (and F < 1).

    initial result = X' + { android.sync.frameNumber == F }
    result1 = X' + { android.sync.frameNumber == F }
    result2 = X' + { android.sync.frameNumber == CONVERGING }
    result3 = X' + { android.sync.frameNumber == CONVERGING }
    result4 = X' + { android.sync.frameNumber == 2 }

    where resultN has frameNumber N.
Since `result4` has a `frameNumber == 4` and `android.sync.frameNumber == 2`, the distance is clearly `4 - 2 = 2`. Use `frame_count` from camera3_request_t instead of android.request.frameCount or `CaptureResult#getFrameNumber`. LIMITED devices are strongly encouraged to use a non-negative value. If UNKNOWN is used here then app developers do not have a way to know when sensor settings have been applied.
reprocess
controls
Property Name | Type | Description | Units | Range | Initial HIDL HAL version | Tags
android.reprocess.effectiveExposureFactor | float [java_public] [limited] | The amount of exposure time increase factor applied to the original output frame by the application processing before sending for reprocessing. | Relative exposure time increase factor. | >= 1.0 | 3.2 | REPROC
Details
This is optional, and will be supported if the camera device supports YUV_REPROCESSING capability (android.request.availableCapabilities contains YUV_REPROCESSING). For some YUV reprocessing use cases, the application may choose to filter the original output frames to effectively reduce the noise to the same level as a frame that was captured with longer exposure time. To be more specific, assuming the original captured images were captured with a sensitivity of S and an exposure time of T, the model in the camera device is that the amount of noise in the image would be approximately what would be expected if the original capture parameters had been a sensitivity of S/effectiveExposureFactor and an exposure time of T*effectiveExposureFactor, rather than S and T respectively. If the captured images were processed by the application before being sent for reprocessing, then the application may have used image processing algorithms and/or multi-frame image fusion to reduce the noise in the application-processed images (input images). By using the effectiveExposureFactor control, the application can communicate to the camera device the actual noise level improvement in the application-processed image. With this information, the camera device can select appropriate noise reduction and edge enhancement parameters to avoid excessive noise reduction (android.noiseReduction.mode) and insufficient edge enhancement (android.edge.mode) being applied to the reprocessed frames. For example, for multi-frame image fusion use case, the application may fuse multiple output frames together to a final frame for reprocessing. When N image are fused into 1 image for reprocessing, the exposure time increase factor could be up to square root of N (based on a simple photon shot noise model). The camera device will adjust the reprocessing noise reduction and edge enhancement parameters accordingly to produce the best quality images. This is relative factor, 1.0 indicates the application hasn't processed the input buffer in a way that affects its effective exposure time. This control is only effective for YUV reprocessing capture request. For noise reduction reprocessing, it is only effective when `android.noiseReduction.mode != OFF`. Similarly, for edge enhancement reprocessing, it is only effective when `android.edge.mode != OFF`.
dynamic
Property Name | Type | Description | Units | Range | Initial HIDL HAL version | Tags
android.reprocess.effectiveExposureFactor | float [java_public] [limited] | The amount of exposure time increase factor applied to the original output frame by the application processing before sending for reprocessing. | Relative exposure time increase factor. | >= 1.0 | 3.2 | REPROC
Details
This is optional, and will be supported if the camera device supports YUV_REPROCESSING capability (android.request.availableCapabilities contains YUV_REPROCESSING). For some YUV reprocessing use cases, the application may choose to filter the original output frames to effectively reduce the noise to the same level as a frame that was captured with longer exposure time. To be more specific, assuming the original captured images were captured with a sensitivity of S and an exposure time of T, the model in the camera device is that the amount of noise in the image would be approximately what would be expected if the original capture parameters had been a sensitivity of S/effectiveExposureFactor and an exposure time of T*effectiveExposureFactor, rather than S and T respectively. If the captured images were processed by the application before being sent for reprocessing, then the application may have used image processing algorithms and/or multi-frame image fusion to reduce the noise in the application-processed images (input images). By using the effectiveExposureFactor control, the application can communicate to the camera device the actual noise level improvement in the application-processed image. With this information, the camera device can select appropriate noise reduction and edge enhancement parameters to avoid excessive noise reduction (android.noiseReduction.mode) and insufficient edge enhancement (android.edge.mode) being applied to the reprocessed frames. For example, for multi-frame image fusion use case, the application may fuse multiple output frames together to a final frame for reprocessing. When N image are fused into 1 image for reprocessing, the exposure time increase factor could be up to square root of N (based on a simple photon shot noise model). The camera device will adjust the reprocessing noise reduction and edge enhancement parameters accordingly to produce the best quality images. This is relative factor, 1.0 indicates the application hasn't processed the input buffer in a way that affects its effective exposure time. This control is only effective for YUV reprocessing capture request. For noise reduction reprocessing, it is only effective when `android.noiseReduction.mode != OFF`. Similarly, for edge enhancement reprocessing, it is only effective when `android.edge.mode != OFF`.
static
Property Name | Type | Description | Units | Range | Initial HIDL HAL version | Tags
android.reprocess.maxCaptureStall | int32 [java_public] [limited] | The maximal camera capture pipeline stall (in unit of frame count) introduced by a reprocess capture request. | Number of frames. | <= 4 | 3.2 | REPROC
Details
The key describes the maximal interference that one reprocess (input) request can introduce to the camera simultaneous streaming of regular (output) capture requests, including repeating requests. When a reprocessing capture request is submitted while a camera output repeating request (e.g. preview) is being served by the camera device, it may preempt the camera capture pipeline for at least one frame duration so that the camera device is unable to process the following capture request in time for the next sensor start of exposure boundary. When this happens, the application may observe a capture time gap (longer than one frame duration) between adjacent capture output frames, which usually exhibits as preview glitch if the repeating request output targets include a preview surface. This key gives the worst-case number of frame stall introduced by one reprocess request with any kind of formats/sizes combination. If this key reports 0, it means a reprocess request doesn't introduce any glitch to the ongoing camera repeating request outputs, as if this reprocess request is never issued. This key is supported if the camera device supports PRIVATE or YUV reprocessing ( i.e. android.request.availableCapabilities contains PRIVATE_REPROCESSING or YUV_REPROCESSING).
depth
static
Property Name | Type | Description | Units | Range | Initial HIDL HAL version | Tags
android.depth.maxDepthSamples | int32 [system] [limited] | Maximum number of points that a depth point cloud may contain. |  |  | 3.2 | DEPTH
Details
If a camera device supports outputting depth range data in the form of a depth point cloud (ImageFormat#DEPTH_POINT_CLOUD), this is the maximum number of points an output buffer may contain. Any given buffer may contain between 0 and maxDepthSamples points, inclusive. If output in the depth point cloud format is not supported, this entry will not be defined.
android.depth.availableDepthStreamConfigurations | int32 x n x 4 [ndk_public as streamConfiguration] [limited] OUTPUT (v3.2) INPUT (v3.2) | The available depth dataspace stream configurations that this camera device supports (i.e. format, width, height, output/input stream). |  |  | 3.2 | DEPTH
Details
These are output stream configurations for use with dataSpace HAL_DATASPACE_DEPTH. The configurations are listed as `(format, width, height, input?)` tuples. Only devices that support depth output for at least the HAL_PIXEL_FORMAT_Y16 dense depth map may include this entry. A device that also supports the HAL_PIXEL_FORMAT_BLOB sparse depth point cloud must report a single entry for the format in this list as `(HAL_PIXEL_FORMAT_BLOB, android.depth.maxDepthSamples, 1, OUTPUT)` in addition to the entries for HAL_PIXEL_FORMAT_Y16.
android.depth.availableDepthMinFrameDurations | int64 x 4 x n [ndk_public as streamConfigurationDuration] [limited] | This lists the minimum frame duration for each format/size combination for depth output formats. | (format, width, height, ns) x n |  | 3.2 | DEPTH
Details
This should correspond to the frame duration when only that stream is active, with all processing (typically in android.*.mode) set to either OFF or FAST. When multiple streams are used in a request, the minimum frame duration will be max(individual stream min durations). The minimum frame duration of a stream (of a particular format, size) is the same regardless of whether the stream is input or output. See android.sensor.frameDuration and android.scaler.availableStallDurations for more details about calculating the max frame rate.
android.depth.availableDepthStallDurations | int64 x 4 x n [ndk_public as streamConfigurationDuration] [limited] | This lists the maximum stall duration for each output format/size combination for depth streams. | (format, width, height, ns) x n |  | 3.2 | DEPTH
Details
A stall duration is how much extra time would get added to the normal minimum frame duration for a repeating request that has streams with non-zero stall. This functions similarly to android.scaler.availableStallDurations for depth streams. All depth output stream formats may have a nonzero stall duration.
android.depth.depthIsExclusive | byte [public as boolean] [limited] FALSE (v3.2) TRUE (v3.2) | Indicates whether a capture request may target both a DEPTH16 / DEPTH_POINT_CLOUD output, and normal color outputs (such as YUV_420_888, JPEG, or RAW) simultaneously. |  |  | 3.2 |
Details
If TRUE, including both depth and color outputs in a single capture request is not supported. An application must interleave color and depth requests. If FALSE, a single request can target both types of output. Typically, this restriction exists on camera devices that need to emit a specific pattern or wavelength of light to measure depth values, which causes the color image to be corrupted during depth measurement.
android.depth.availableRecommendedDepthStreamConfigurations | int32 x n x 5 [ndk_public as recommendedStreamConfiguration] | Recommended depth stream configurations for common client use cases. |  |  | 3.4 |
Details
Optional subset of the android.depth.availableDepthStreamConfigurations that contains similar tuples listed as (i.e. width, height, format, output/input stream, usecase bit field). Camera devices will be able to suggest particular depth stream configurations which are power and performance efficient for specific use cases. For more information about retrieving the suggestions see CameraCharacteristics#getRecommendedStreamConfigurationMap.
HAL Implementation Details
Recommended depth configurations are expected to be declared with SNAPSHOT and/or ZSL if supported by the device. For additional details on how to declare recommended stream configurations, check android.scaler.availableRecommendedStreamConfigurations. For additional requirements on depth streams please consider android.depth.availableDepthStreamConfigurations.
android.depth.availableDynamicDepthStreamConfigurations | int32 x n x 4 [ndk_public as streamConfiguration] OUTPUT (v3.4) INPUT (v3.4) | The available dynamic depth dataspace stream configurations that this camera device supports (i.e. format, width, height, output/input stream). |  |  | 3.4 | DEPTH
Details
These are output stream configurations for use with dataSpace DYNAMIC_DEPTH. The configurations are listed as `(format, width, height, input?)` tuples. Only devices that support depth output for at least the HAL_PIXEL_FORMAT_Y16 dense depth map along with HAL_PIXEL_FORMAT_BLOB with the same size or size with the same aspect ratio can have dynamic depth dataspace stream configuration. android.depth.depthIsExclusive also needs to be set to FALSE.
HAL Implementation Details
Do not set this property directly. It is populated by camera framework and must not be set at the HAL layer.
android.depth.availableDynamicDepthMinFrameDurations | int64 x 4 x n [ndk_public as streamConfigurationDuration] | This lists the minimum frame duration for each format/size combination for dynamic depth output streams. | (format, width, height, ns) x n |  | 3.4 | DEPTH
Details
This should correspond to the frame duration when only that stream is active, with all processing (typically in android.*.mode) set to either OFF or FAST. When multiple streams are used in a request, the minimum frame duration will be max(individual stream min durations). The minimum frame duration of a stream (of a particular format, size) is the same regardless of whether the stream is input or output.
HAL Implementation Details
Do not set this property directly. It is populated by camera framework and must not be set at the HAL layer.
android.depth.availableDynamicDepthStallDurations | int64 x 4 x n [ndk_public as streamConfigurationDuration] | This lists the maximum stall duration for each output format/size combination for dynamic depth streams. | (format, width, height, ns) x n |  | 3.4 | DEPTH
Details
A stall duration is how much extra time would get added to the normal minimum frame duration for a repeating request that has streams with non-zero stall. All dynamic depth output streams may have a nonzero stall duration.
HAL Implementation Details
Do not set this property directly. It is populated by camera framework and must not be set at the HAL layer.
logicalMultiCamera
static
Property Name | Type | Description | Units | Range | Initial HIDL HAL version | Tags
android.logicalMultiCamera.physicalIds | byte x n [ndk_public] [limited] | String containing the ids of the underlying physical cameras. | UTF-8 null-terminated string |  | 3.3 | LOGICALCAMERA
Details
For a logical camera, this is concatenation of all underlying physical camera IDs. The null terminator for physical camera ID must be preserved so that the whole string can be tokenized using '\0' to generate list of physical camera IDs. For example, if the physical camera IDs of the logical camera are "2" and "3", the value of this tag will be ['2', '\0', '3', '\0']. The number of physical camera IDs must be no less than 2.
android.logicalMultiCamera.sensorSyncType | byte [public] [limited] APPROXIMATE (v3.3) A software mechanism is used to synchronize between the physical cameras. As a result, the timestamp of an image from a physical stream is only an approximation of the image sensor start-of-exposure time. CALIBRATED (v3.3) The camera device supports frame timestamp synchronization at the hardware level, and the timestamp of a physical stream image accurately reflects its start-of-exposure time. | The accuracy of frame timestamp synchronization between physical cameras |  |  | 3.3 | LOGICALCAMERA
Details
The accuracy of the frame timestamp synchronization determines the physical cameras' ability to start exposure at the same time. If the sensorSyncType is CALIBRATED, the physical camera sensors usually run in leader/follower mode where one sensor generates a timing signal for the other, so that their shutter time is synchronized. For APPROXIMATE sensorSyncType, the camera sensors usually run in leader/leader mode, where both sensors use their own timing generator, and there could be offset between their start of exposure. In both cases, all images generated for a particular capture request still carry the same timestamps, so that they can be used to look up the matching frame number and onCaptureStarted callback. This tag is only applicable if the logical camera device supports concurrent physical streams from different physical cameras.
dynamic
Property Name | Type | Description | Units | Range | Initial HIDL HAL version | Tags
android.logicalMultiCamera.activePhysicalId | byte [public as string] | String containing the ID of the underlying active physical camera. | UTF-8 null-terminated string |  | 3.4 | LOGICALCAMERA
Details
The ID of the active physical camera that's backing the logical camera. All camera streams and metadata that are not physical camera specific will be originating from this physical camera. For a logical camera made up of physical cameras where each camera's lenses have different characteristics, the camera device may choose to switch between the physical cameras when application changes FOCAL_LENGTH or SCALER_CROP_REGION. At the time of lens switch, this result metadata reflects the new active physical camera ID. This key will be available if the camera device advertises this key via CameraCharacteristics#getAvailableCaptureResultKeys. When available, this must be one of valid physical IDs backing this logical multi-camera. If this key is not available for a logical multi-camera, the camera device implementation may still switch between different active physical cameras based on use case, but the current active physical camera information won't be available to the application.
HAL Implementation Details
Staring from HIDL ICameraDevice version 3.5, the tag must be available in the capture result metadata to indicate current active physical camera ID.
distortionCorrection
controls
Property Name | Type | Description | Units | Range | Initial HIDL HAL version | Tags
android.distortionCorrection.mode | byte [public] OFF (v3.3) No distortion correction is applied. FAST (v3.3) Lens distortion correction is applied without reducing frame rate relative to sensor output. It may be the same as OFF if distortion correction would reduce frame rate relative to sensor. HIGH_QUALITY (v3.3) High-quality distortion correction is applied, at the cost of possibly reduced frame rate relative to sensor output. | Mode of operation for the lens distortion correction block. |  | android.distortionCorrection.availableModes | 3.3 |
Details
The lens distortion correction block attempts to improve image quality by fixing radial, tangential, or other geometric aberrations in the camera device's optics. If available, the android.lens.distortion field documents the lens's distortion parameters. OFF means no distortion correction is done. FAST/HIGH_QUALITY both mean camera device determined distortion correction will be applied. HIGH_QUALITY mode indicates that the camera device will use the highest-quality correction algorithms, even if it slows down capture rate. FAST means the camera device will not slow down capture rate when applying correction. FAST may be the same as OFF if any correction at all would slow down capture rate. Every output stream will have a similar amount of enhancement applied. The correction only applies to processed outputs such as YUV, Y8, JPEG, or DEPTH16; it is not applied to any RAW output. This control will be on by default on devices that support this control. Applications disabling distortion correction need to pay extra attention with the coordinate system of metering regions, crop region, and face rectangles. When distortion correction is OFF, metadata coordinates follow the coordinate system of android.sensor.info.preCorrectionActiveArraySize. When distortion is not OFF, metadata coordinates follow the coordinate system of android.sensor.info.activeArraySize. The camera device will map these metadata fields to match the corrected image produced by the camera device, for both capture requests and results. However, this mapping is not very precise, since rectangles do not generally map to rectangles when corrected. Only linear scaling between the active array and precorrection active array coordinates is performed. Applications that require precise correction of metadata need to undo that linear scaling, and apply a more complete correction that takes into the account the app's own requirements. The full list of metadata that is affected in this way by distortion correction is: android.control.afRegions android.control.aeRegions android.control.awbRegions android.scaler.cropRegion android.statistics.faces
static
Property Name | Type | Description | Units | Range | Initial HIDL HAL version | Tags
android.distortionCorrection.availableModes | byte x n [public as enumList] list of enums | List of distortion correction modes for android.distortionCorrection.mode that are supported by this camera device. |  | Any value listed in android.distortionCorrection.mode | 3.3 | V1 REPROC
Details
No device is required to support this API; such devices will always list only 'OFF'. All devices that support this API will list both FAST and HIGH_QUALITY.
HAL Implementation Details
HAL must support both FAST and HIGH_QUALITY if distortion correction is available on the camera device, but the underlying implementation can be the same for both modes. That is, if the highest quality implementation on the camera device does not slow down capture rate, then FAST and HIGH_QUALITY will generate the same output.
dynamic
Property Name | Type | Description | Units | Range | Initial HIDL HAL version | Tags
android.distortionCorrection.mode | byte [public] OFF (v3.3) No distortion correction is applied. FAST (v3.3) Lens distortion correction is applied without reducing frame rate relative to sensor output. It may be the same as OFF if distortion correction would reduce frame rate relative to sensor. HIGH_QUALITY (v3.3) High-quality distortion correction is applied, at the cost of possibly reduced frame rate relative to sensor output. | Mode of operation for the lens distortion correction block. |  | android.distortionCorrection.availableModes | 3.3 |
Details
The lens distortion correction block attempts to improve image quality by fixing radial, tangential, or other geometric aberrations in the camera device's optics. If available, the android.lens.distortion field documents the lens's distortion parameters. OFF means no distortion correction is done. FAST/HIGH_QUALITY both mean camera device determined distortion correction will be applied. HIGH_QUALITY mode indicates that the camera device will use the highest-quality correction algorithms, even if it slows down capture rate. FAST means the camera device will not slow down capture rate when applying correction. FAST may be the same as OFF if any correction at all would slow down capture rate. Every output stream will have a similar amount of enhancement applied. The correction only applies to processed outputs such as YUV, Y8, JPEG, or DEPTH16; it is not applied to any RAW output. This control will be on by default on devices that support this control. Applications disabling distortion correction need to pay extra attention with the coordinate system of metering regions, crop region, and face rectangles. When distortion correction is OFF, metadata coordinates follow the coordinate system of android.sensor.info.preCorrectionActiveArraySize. When distortion is not OFF, metadata coordinates follow the coordinate system of android.sensor.info.activeArraySize. The camera device will map these metadata fields to match the corrected image produced by the camera device, for both capture requests and results. However, this mapping is not very precise, since rectangles do not generally map to rectangles when corrected. Only linear scaling between the active array and precorrection active array coordinates is performed. Applications that require precise correction of metadata need to undo that linear scaling, and apply a more complete correction that takes into the account the app's own requirements. The full list of metadata that is affected in this way by distortion correction is: android.control.afRegions android.control.aeRegions android.control.awbRegions android.scaler.cropRegion android.statistics.faces
heic
static
Property Name | Type | Description | Units | Range | Initial HIDL HAL version | Tags
android.heic.info.supported | byte [system as boolean] [limited] FALSE (v3.4) TRUE (v3.4) | Whether this camera device can support identical set of stream combinations involving HEIC image format, compared to the table of combinations involving JPEG image format required for the device's hardware level and capabilities. |  |  | 3.4 | HEIC
Details
All the static, control and dynamic metadata tags related to JPEG apply to HEIC formats as well. For example, the same android.jpeg.orientation and android.jpeg.quality are used to control the orientation and quality of the HEIC image. Configuring JPEG and HEIC streams at the same time is not supported. If a camera device supports HEIC format (ISO/IEC 23008-12), not only does it support the existing mandatory stream combinations required for the device's hardware level and capabilities, it also supports swapping each JPEG stream with HEIC stream in all guaranteed combinations. For every HEIC stream configured by the application, the camera framework sets up 2 internal streams with camera HAL: A YUV_420_888 or IMPLEMENTATION_DEFINED HAL stream as input to HEIC or HEVC encoder. A BLOB stream with JPEG_APPS_SEGMENTS dataspace to extract application markers including EXIF and thumbnail to be saved in HEIF container. A camera device can output HEIC format to the application if and only if: The system contains a HEIC or HEVC encoder with constant quality mode, and This tag is set to TRUE, meaning that camera HAL supports replacing JPEG streams in all mandatory stream combinations with a [YUV_420_888/IMPLEMENTATION_DEFINED stream + JPEG_APPS_SEGMENT BLOB stream] combo. As an example, if the camera device's hardware level is LIMITED, and it supports HEIC, in addition to the required stream combinations, HAL must support below stream combinations as well: IMPLEMENTATION_DEFINED/YUV_420_888 MAXIMUM + JPEG_SEGMENTS_BLOB, PRIV PREVIEW + IMPLEMENTATION_DEFINED/YUV_420_888 MAXIMUM + JPEG_SEGMENTS_BLOB, YUV PREVIEW + IMPLEMENTATION_DEFINED/YUV_420_888 MAXIMUM + JPEG_SEGMENTS_BLOB, PRIV PREVIEW + YUV PREVIEW + IMPLEMENTATION_DEFINED/YUV_420_888 MAXIMUM + JPEG_SEGMENTS_BLOB The selection logic between YUV_420_888 and IMPLEMENTATION_DEFINED for HAL internal stream is as follows:
    if (HEIC encoder exists and supports the size) {
        use IMPLEMENTATION_DEFINED with GRALLOC_USAGE_HW_IMAGE_ENCODER usage flag;
    } else {
        // HVC encoder exists
        if (size is less than framework predefined tile size) {
            use IMPLEMENTATINO_DEFINED with GRALLOC_USAGE_HW_VIDEO_ENCODER usage flag;
        } else {
            use YUV_420_888;
        }
    }
android.heic.info.maxJpegAppSegmentsCount | byte [system] [limited] | The maximum number of Jpeg APP segments supported by the camera HAL device. |  |  | 3.4 | HEIC
Details
The camera framework will use this value to derive the size of the BLOB buffer with JPEG_APP_SEGMENTS dataspace, with each APP segment occupying at most 64K bytes. If the value of this tag is n, the size of the framework allocated buffer will be:
    n * (2 + 0xFFFF) + sizeof(struct CameraBlob)
where 2 is number of bytes for APP marker, 0xFFFF is the maximum size per APP segment (including segment size). The value of this tag must be at least 1, and APP1 marker (0xFFE1) segment must be the first segment stored in the JPEG_APPS_SEGMENTS BLOB buffer. APP1 segment stores EXIF and thumbnail. Since media encoder embeds the orientation in the metadata of the output image, to be consistent between main image and thumbnail, camera HAL must not rotate the thumbnail image data based on android.jpeg.orientation. The framework will write the orientation into EXIF and HEIC container. APP1 segment is followed immediately by one or multiple APP2 segments, and APPn segments. After the HAL fills and returns the JPEG_APP_SEGMENTS buffer, the camera framework modifies the APP1 segment by filling in the EXIF tags that are related to main image bitstream and the tags that can be derived from capture result metadata, before saving them into the HEIC container. The value of this tag must not be more than 16.
android.heic.availableHeicStreamConfigurations | int32 x n x 4 [ndk_public as streamConfiguration] [limited] OUTPUT (v3.4) INPUT (v3.4) | The available HEIC (ISO/IEC 23008-12) stream configurations that this camera device supports (i.e. format, width, height, output/input stream). |  |  | 3.4 | HEIC
Details
The configurations are listed as `(format, width, height, input?)` tuples. If the camera device supports HEIC image format, it will support identical set of stream combinations involving HEIC image format, compared to the combinations involving JPEG image format as required by the device's hardware level and capabilities. All the static, control, and dynamic metadata tags related to JPEG apply to HEIC formats. Configuring JPEG and HEIC streams at the same time is not supported.
HAL Implementation Details
These are output stream configurations for use with dataSpace HAL_DATASPACE_HEIF. Do not set this property directly. It is populated by camera framework and must not be set by the HAL layer.
android.heic.availableHeicMinFrameDurations | int64 x 4 x n [ndk_public as streamConfigurationDuration] [limited] | This lists the minimum frame duration for each format/size combination for HEIC output formats. | (format, width, height, ns) x n |  | 3.4 | HEIC
Details
This should correspond to the frame duration when only that stream is active, with all processing (typically in android.*.mode) set to either OFF or FAST. When multiple streams are used in a request, the minimum frame duration will be max(individual stream min durations). See android.sensor.frameDuration and android.scaler.availableStallDurations for more details about calculating the max frame rate.
HAL Implementation Details
Do not set this property directly. It is populated by camera framework and must not be set by the HAL layer.
android.heic.availableHeicStallDurations | int64 x 4 x n [ndk_public as streamConfigurationDuration] [limited] | This lists the maximum stall duration for each output format/size combination for HEIC streams. | (format, width, height, ns) x n |  | 3.4 | HEIC
Details
A stall duration is how much extra time would get added to the normal minimum frame duration for a repeating request that has streams with non-zero stall. This functions similarly to android.scaler.availableStallDurations for HEIC streams. All HEIC output stream formats may have a nonzero stall duration.
HAL Implementation Details
Do not set this property directly. It is populated by camera framework and must not be set by the HAL layer.

## Tags

- BC - Needed for backwards compatibility with old Java API
  - android.control.aeAntibandingMode (controls)
  - android.control.aeExposureCompensation (controls)
  - android.control.aeLock (controls)
  - android.control.aeMode (controls)
  - android.control.aeRegions (controls)
  - android.control.aeTargetFpsRange (controls)
  - android.control.aePrecaptureTrigger (controls)
  - android.control.afMode (controls)
  - android.control.afRegions (controls)
  - android.control.afTrigger (controls)
  - android.control.awbLock (controls)
  - android.control.awbMode (controls)
  - android.control.awbRegions (controls)
  - android.control.captureIntent (controls)
  - android.control.effectMode (controls)
  - android.control.mode (controls)
  - android.control.sceneMode (controls)
  - android.control.videoStabilizationMode (controls)
  - android.control.aeAvailableAntibandingModes (static)
  - android.control.aeAvailableModes (static)
  - android.control.aeAvailableTargetFpsRanges (static)
  - android.control.aeCompensationRange (static)
  - android.control.aeCompensationStep (static)
  - android.control.afAvailableModes (static)
  - android.control.availableEffects (static)
  - android.control.availableSceneModes (static)
  - android.control.availableVideoStabilizationModes (static)
  - android.control.awbAvailableModes (static)
  - android.control.maxRegions (static)
  - android.control.sceneModeOverrides (static)
  - android.control.aeLockAvailable (static)
  - android.control.awbLockAvailable (static)
  - android.flash.mode (controls)
  - android.flash.info.available (static)
  - android.jpeg.gpsCoordinates (controls)
  - android.jpeg.gpsProcessingMethod (controls)
  - android.jpeg.gpsTimestamp (controls)
  - android.jpeg.orientation (controls)
  - android.jpeg.quality (controls)
  - android.jpeg.thumbnailQuality (controls)
  - android.jpeg.thumbnailSize (controls)
  - android.jpeg.availableThumbnailSizes (static)
  - android.lens.focusDistance (controls)
  - android.lens.info.availableFocalLengths (static)
  - android.lens.focusRange (dynamic)
  - android.request.maxNumOutputStreams (static)
  - android.scaler.cropRegion (controls)
  - android.scaler.availableFormats (static)
  - android.scaler.availableJpegMinDurations (static)
  - android.scaler.availableJpegSizes (static)
  - android.scaler.availableMaxDigitalZoom (static)
  - android.scaler.availableProcessedMinDurations (static)
  - android.scaler.availableProcessedSizes (static)
  - android.scaler.availableRawMinDurations (static)
  - android.sensor.info.sensitivityRange (static)
  - android.sensor.info.physicalSize (static)
  - android.sensor.info.pixelArraySize (static)
  - android.sensor.orientation (static)
  - android.sensor.timestamp (dynamic)
  - android.statistics.faceDetectMode (controls)
  - android.statistics.info.maxFaceCount (static)
  - android.statistics.faceIds (dynamic)
  - android.statistics.faceLandmarks (dynamic)
  - android.statistics.faceRectangles (dynamic)
  - android.statistics.faceScores (dynamic)
  - android.lens.focalLength (dynamic)
  - android.lens.focusDistance (dynamic)
- V1 - New features for first camera 2 release (API1)
  - android.colorCorrection.availableAberrationModes (static)
  - android.control.availableHighSpeedVideoConfigurations (static)
  - android.edge.mode (controls)
  - android.edge.availableEdgeModes (static)
  - android.hotPixel.mode (controls)
  - android.hotPixel.availableHotPixelModes (static)
  - android.lens.aperture (controls)
  - android.lens.filterDensity (controls)
  - android.lens.focalLength (controls)
  - android.lens.focusDistance (controls)
  - android.lens.opticalStabilizationMode (controls)
  - android.lens.info.availableApertures (static)
  - android.lens.info.availableFilterDensities (static)
  - android.lens.info.availableFocalLengths (static)
  - android.lens.info.availableOpticalStabilization (static)
  - android.lens.info.minimumFocusDistance (static)
  - android.lens.info.shadingMapSize (static)
  - android.lens.info.focusDistanceCalibration (static)
  - android.lens.state (dynamic)
  - android.noiseReduction.mode (controls)
  - android.noiseReduction.availableNoiseReductionModes (static)
  - android.request.id (controls)
  - android.scaler.availableMinFrameDurations (static)
  - android.scaler.availableStallDurations (static)
  - android.sensor.exposureTime (controls)
  - android.sensor.frameDuration (controls)
  - android.sensor.sensitivity (controls)
  - android.sensor.info.sensitivityRange (static)
  - android.sensor.info.exposureTimeRange (static)
  - android.sensor.info.maxFrameDuration (static)
  - android.sensor.info.physicalSize (static)
  - android.sensor.info.timestampSource (static)
  - android.sensor.maxAnalogSensitivity (static)
  - android.sensor.rollingShutterSkew (dynamic)
  - android.statistics.hotPixelMapMode (controls)
  - android.statistics.info.availableHotPixelMapModes (static)
  - android.statistics.hotPixelMap (dynamic)
  - android.sync.frameNumber (dynamic)
  - android.sync.maxLatency (static)
  - android.distortionCorrection.availableModes (static)
  - android.edge.mode (dynamic)
  - android.hotPixel.mode (dynamic)
  - android.lens.aperture (dynamic)
  - android.lens.filterDensity (dynamic)
  - android.lens.opticalStabilizationMode (dynamic)
  - android.noiseReduction.mode (dynamic)
- RAW - Needed for useful RAW image processing and DNG file support
  - android.hotPixel.mode (controls)
  - android.hotPixel.availableHotPixelModes (static)
  - android.sensor.info.activeArraySize (static)
  - android.sensor.info.colorFilterArrangement (static)
  - android.sensor.info.pixelArraySize (static)
  - android.sensor.info.whiteLevel (static)
  - android.sensor.info.preCorrectionActiveArraySize (static)
  - android.sensor.referenceIlluminant1 (static)
  - android.sensor.referenceIlluminant2 (static)
  - android.sensor.calibrationTransform1 (static)
  - android.sensor.calibrationTransform2 (static)
  - android.sensor.colorTransform1 (static)
  - android.sensor.colorTransform2 (static)
  - android.sensor.forwardMatrix1 (static)
  - android.sensor.forwardMatrix2 (static)
  - android.sensor.blackLevelPattern (static)
  - android.sensor.profileHueSatMapDimensions (static)
  - android.sensor.neutralColorPoint (dynamic)
  - android.sensor.noiseProfile (dynamic)
  - android.sensor.profileHueSatMap (dynamic)
  - android.sensor.profileToneCurve (dynamic)
  - android.sensor.greenSplit (dynamic)
  - android.sensor.dynamicBlackLevel (dynamic)
  - android.sensor.dynamicWhiteLevel (dynamic)
  - android.statistics.hotPixelMapMode (controls)
  - android.statistics.info.availableHotPixelMapModes (static)
  - android.statistics.hotPixelMap (dynamic)
  - android.statistics.lensShadingMapMode (controls)
  - android.hotPixel.mode (dynamic)
- HAL2 - Entry is only used by camera device legacy HAL 2.x
  - android.request.inputStreams (controls)
  - android.request.outputStreams (controls)
  - android.request.type (controls)
  - android.request.maxNumReprocessStreams (static)
  - android.blackLevel.lock (controls)
- FULL - Entry is required for full hardware level devices, and optional for other hardware levels
  - android.sensor.maxAnalogSensitivity (static)
- DEPTH - Entry is required for the depth capability.
  - android.lens.poseRotation (static)
  - android.lens.poseTranslation (static)
  - android.lens.intrinsicCalibration (static)
  - android.lens.radialDistortion (static)
  - android.lens.distortion (static)
  - android.depth.maxDepthSamples (static)
  - android.depth.availableDepthStreamConfigurations (static)
  - android.depth.availableDepthMinFrameDurations (static)
  - android.depth.availableDepthStallDurations (static)
  - android.depth.availableDynamicDepthStreamConfigurations (static)
  - android.depth.availableDynamicDepthMinFrameDurations (static)
  - android.depth.availableDynamicDepthStallDurations (static)
- REPROC - Entry is required for the YUV or PRIVATE reprocessing capability.
  - android.edge.mode (controls)
  - android.edge.availableEdgeModes (static)
  - android.noiseReduction.mode (controls)
  - android.noiseReduction.availableNoiseReductionModes (static)
  - android.request.maxNumInputStreams (static)
  - android.scaler.availableInputOutputFormatsMap (static)
  - android.scaler.availableRecommendedInputOutputFormatsMap (static)
  - android.reprocess.effectiveExposureFactor (controls)
  - android.reprocess.maxCaptureStall (static)
  - android.distortionCorrection.availableModes (static)
  - android.edge.mode (dynamic)
  - android.noiseReduction.mode (dynamic)
- LOGICALCAMERA - Entry is required for logical multi-camera capability.
  - android.logicalMultiCamera.physicalIds (static)
  - android.logicalMultiCamera.sensorSyncType (static)
  - android.logicalMultiCamera.activePhysicalId (dynamic)
- HEIC - Entry is required for devices with HEIC (High Efficiency Image Format) support.
  - android.heic.info.supported (static)
  - android.heic.info.maxJpegAppSegmentsCount (static)
  - android.heic.availableHeicStreamConfigurations (static)
  - android.heic.availableHeicMinFrameDurations (static)
  - android.heic.availableHeicStallDurations (static)
- FUTURE - Entry is under-specified and is not required for now. This is for book-keeping purpose, do not implement or use it, it may be revised for future.
  - android.demosaic.mode (controls)
  - android.edge.strength (controls)
  - android.flash.firingPower (controls)
  - android.flash.firingTime (controls)
  - android.flash.info.chargeDuration (static)
  - android.flash.colorTemperature (static)
  - android.flash.maxEnergy (static)
  - android.jpeg.size (dynamic)
  - android.noiseReduction.strength (controls)
  - android.request.metadataMode (controls)
  - android.sensor.baseGainFactor (static)
  - android.sensor.temperature (dynamic)
  - android.shading.strength (controls)
  - android.statistics.histogramMode (controls)
  - android.statistics.sharpnessMapMode (controls)
  - android.statistics.info.histogramBucketCount (static)
  - android.statistics.info.maxHistogramCount (static)
  - android.statistics.info.maxSharpnessMapValue (static)
  - android.statistics.info.sharpnessMapSize (static)
  - android.statistics.histogram (dynamic)
  - android.statistics.sharpnessMap (dynamic)

[ top ]