--- Configure.help-2.2.13	Fri Oct 22 01:35:01 1999
+++ Configure.help-2.2.14	Thu Jan  6 01:45:57 2000
@@ -1202 +1202 @@
-  ftp://koobera.math.uic.edu/pub/docs/syncookies-archive.
+  ftp://koobera.math.uic.edu/syncookies.html .
@@ -2534,0 +2535,2 @@
+  Enabling masquerading automagically enables ip_always_defrag too.
+
@@ -2646,19 +2647,0 @@
-IP: always defragment (required for masquerading)
-CONFIG_IP_ALWAYS_DEFRAG
-  If you say Y here, then all incoming fragments (parts of IP packets
-  that arose when some host between origin and destination decided
-  that the packets were too large and cut them into pieces) will be
-  reassembled (defragmented) before being processed, even if they are
-  about to be forwarded.
-
-  You must say Y here if you want to enable "IP: masquerading" or "IP:
-  transparent proxying".
-
-  When using "IP: firewalling" support, you might also want to say Y
-  here, to have a more reliable firewall (otherwise second and further
-  fragments must be dealt with by the firewall, which can be tricky).
-
-  Only say Y here if running either a firewall that is the sole link
-  to your network or a transparent proxy; never ever say Y here for a
-  normal router or host.
-
@@ -3518,2 +3501,3 @@
-  module, say M here and read Documentation/modules.txt. If unsure,
-  say Y.
+  module, say M here and read Documentation/modules.txt.  You will
+  need to add 'alias net-pf-17 af_packet' to your /etc/conf.modules
+  file for the module version to function automatically.  If unsure, say Y.
@@ -5269 +5253 @@
-  The WAN routing support is also available as a module called
+  The WAN routing support is only available as a module called
@@ -5292,0 +5277 @@
+
@@ -5551,3 +5536,6 @@
-  and designated S502E(A), S503 or S508. These cards support the X.25,
-  Frame Relay, and PPP protocols. If you have one or more of these
-  cards, say Y to this option; you may then also want to read the file
+  and designated S503 or S508. These cards support the X.25, Frame
+  Relay, PPP, Cisco HDLC protocols. The driver also offers API support
+  for protocols like HDLC (LAPB), HDLC Streaming and BiSync. 
+
+  If you have one or more of these cards, say M to this option; you
+  may then also want to read the file
@@ -5573,4 +5561,3 @@
-  to an X.25 network. You should then also have said Y to "CCITT X.25
-  Packet Layer" and "LAPB Data Link Driver", above. If you say N, the
-  X.25 support will not be included in the driver (saves about 16 KB
-  of kernel memory).
+  to an X.25 network. If you say N, the X.25 support will not be
+  included in the driver. The X.25 option is ONLY supported on S508
+  cards.
@@ -5581,4 +5568,3 @@
-  to a frame relay network. You should then also have said Y to "Frame
-  Relay (DLCI) support", above. If you say N, the frame relay
-  support will not be included in the driver (saves about 16 KB of
-  kernel memory).
+  to a frame relay network. If you say N, the frame relay support will
+  not be included in the driver. The Frame Relay option is ONLY
+  supported on S508 cards.
@@ -5589,4 +5575,83 @@
-  to a leased line using Point-to-Point protocol (PPP). You should
-  then also have said Y to "PPP (point-to-point) support", above. If
-  you say N, the PPP support will not be included in the driver (saves
-  about 16 KB of kernel memory).
+  to a leased line using Point-to-Point protocol (PPP). If you say N,
+  the PPP support will not be included in the driver. The PPP option
+  is ONLY supported on S508 cards.
+
+WANPIPE Cisco HDLC support
+CONFIG_WANPIPE_CHDLC
+  Say Y to this option if you are planning to connect a WANPIPE card
+  to a leased line using the Cisco HDLC protocol. This now supports
+  Dual Port Cisco HDLC on the S508 card ONLY. This support also allows
+  user to build applications using the HDLC streaming API. If you say
+  N, the Cisco HDLC support and HDLC streaming API will not be
+  included in the driver.
+
+MultiGate/COMX support
+CONFIG_COMX
+  Say Y if you want to use any board from the MultiGate (COMX) family. 
+  These boards are synchronous serial adapters for the PC, manufactured 
+  by ITConsult-Pro Co, Hungary. 
+
+  Read linux/Documentation/networking/comx.txt  for help on configuring 
+  and using COMX interfaces. Further info on these cards can be found at 
+  http://www.itc.hu or <info@itc.hu>.
+
+  If you want to compile this as a module, say M and read
+  Documentation/modules.txt. The module will be called comx.o.
+
+COMX/CMX/HiCOMX board support
+CONFIG_COMX_HW_COMX
+  Hardware driver for the 'CMX', 'COMX' and 'HiCOMX' boards from the
+  MultiGate family. Say Y if you have one of these. 
+
+  You will need additional firmware to use these cards, which are
+  downloadable from ftp://ftp.itc.hu/.
+
+  If you want to compile this as a module, say M and read
+  Documentation/modules.txt. The module will be called comx-hw-comx.o.
+
+LoCOMX board support
+CONFIG_COMX_HW_LOCOMX
+  Hardware driver for the 'LoCOMX' board from the MultiGate family. Say Y
+  if you have a board like this. 
+
+  If you want to compile this as a module, say M and read
+  Documentation/modules.txt. The module will be called comx-hw-locomx.o.
+
+MixCOM board support
+CONFIG_COMX_HW_MIXCOM
+  Hardware driver for the 'MixCOM' board from the MultiGate family. Say Y
+  if you have a board like this.
+
+  If you want to use the watchdog device on this card, you should
+  select it in the Watchdog Cards section of the Character Devices
+  configuration. The ISDN interface of this card is Teles 16.3 compatible,
+  you should enable it in the ISDN configuration menu. The driver for the 
+  flash ROM of this card is available separately on ftp://ftp.itc.hu/.
+
+  If you want to compile this as a module, say M and read
+  Documentation/modules.txt. The module will be called comx-hw-mixcom.o.
+
+MultiGate Cisco-HDLC and synchronous PPP protocol support
+CONFIG_COMX_PROTO_PPP
+  Cisco-HDLC and synchronous PPP protocol driver for all MultiGate boards. 
+  Say Y if you want to use either protocol on your MultiGate boards.
+
+  If you want to compile this as a module, say M and read
+  Documentation/modules.txt. The module will be called 
+  comx-proto-ppp.o.
+
+MultiGate LAPB protocol support
+CONFIG_COMX_PROTO_LAPB
+  LAPB protocol driver for all MultiGate boards. Say Y if you 
+  want to use this protocol on your MultiGate boards.
+
+  If you want to compile this as a module, say M and read
+  Documentation/modules.txt. The module will be called comx-proto-lapb.o.
+
+MultiGate Frame Relay protocol support
+CONFIG_COMX_PROTO_FR
+  Frame Relay protocol driver for all MultiGate boards. Say Y if you 
+  want to use this protocol on your MultiGate boards.
+
+  If you want to compile this as a module, say M and read
+  Documentation/modules.txt. The module will be called comx-proto-fr.o.
@@ -5804,0 +5870,18 @@
+SiS 900/7016 support
+CONFIG_SIS900
+  This is a driver for the Fast Ethernet PCI network cards based on
+  the SiS 900 and SiS 7016 chips. The SiS 900 core is also embedded in
+  SiS 630 and SiS 540 chipsets. If you have one of those, say Y and
+  read the Ethernet-HOWTO, available via FTP (user: anonymous) in   
+  ftp://metalab.unc.edu/pub/Linux/docs/HOWTO. Please read 
+  Documentation/networking/sis900.txt and comments at the beginning
+  of drivers/net/sis900.c for more information.
+
+  This driver also supports AMD 79C901 HomePNA such that you can use
+  your phone line as network cable.
+
+  If you want to compile this driver as a module ( = code which can be
+  inserted in and removed from the running kernel whenever you want), 
+  say M here and read Documentation/modules.txt. This is recommended. 
+  The module will be called sis900.o.
+
@@ -5850,0 +5934,21 @@
+SysKonnect SK-98xx support
+CONFIG_SK98LIN
+  Say Y here if you have a SysKonnect SK-98xx Gigabit Ethernet Server
+  Adapter. The following adapters are supported by this driver:
+  - SK-9841 (single link 1000Base-LX)
+  - SK-9842 (dual link   1000Base-LX)
+  - SK-9843 (single link 1000Base-SX)
+  - SK-9844 (dual link   1000Base-SX)
+  - SK-9821 (single link 1000Base-T)
+  - SK-9822 (dual link   1000Base-T)
+  The dual link adapters support a link-failover feature.
+  Read Documentation/networking/sk98lin.txt for information about
+  optional driver parameters.
+  Questions concerning this driver may be addresse to:
+    linux@syskonnect.de
+
+  If you want to compile this driver as a module ( = code which can be
+  inserted in and removed from the running kernel whenever you want),
+  say M here and read Documentation/modules.txt. This is recommended.
+  The module will be called sk98lin.o.
+
@@ -6394,0 +6499,26 @@
+  This is the new version of this driver. If it does not work for
+  you please try older version which is also available.
+
+  This driver is also available as a module ( = code which can be
+  inserted in and removed from the running kernel whenever you want).
+  The module will be called tulip.o. If you want to compile it as a
+  module, say M here and read Documentation/modules.txt as well as
+  Documentation/networking/net-modules.txt.
+
+Old DECchip Tulip (dc21x4x) PCI support
+CONFIG_DEC_ELCP_OLD
+  This driver is developed for the SMC EtherPower series Ethernet
+  cards and also works with cards based on the DECchip
+  21040/21041/21140 (Tulip series) chips. Some LinkSys PCI cards are
+  of this type. (If your card is NOT SMC EtherPower 10/100 PCI
+  (smc9332dst), you can also try the driver for "Generic DECchip"
+  cards, above. However, most people with a network card of this type
+  will say Y here.) Do read the Ethernet-HOWTO, available via FTP
+  (user: anonymous) in ftp://metalab.unc.edu/pub/Linux/docs/HOWTO.
+  More specific information is contained in
+  Documentation/networking/tulip.txt.
+
+  This an older version of the driver which supports some cards the
+  new version does not (yet) support. Use it if the new driver does
+  not work for you.
+
@@ -8887,3 +9017,9 @@
-  reset after a USER RESUME operation, the /proc/apm device will
-  provide battery status information, and user-space programs will
-  receive notification of APM "events" (e.g., battery status change).
+  reset after a RESUME operation, the /proc/apm device will provide
+  battery status information, and user-space programs will receive
+  notification of APM "events" (e.g. battery status change).
+
+  If you select "Y" here, you can disable actual use of the APM
+  BIOS by passing the "apm=off" option to the kernel at boot time.
+
+  Note that the APM support is almost completely disabled for
+  machines with more than one CPU.
@@ -8902,3 +9038 @@
-  will cause those machines to panic during the boot phase (typically,
-  these machines are using a data segment of 0040, which is reserved
-  for the Linux kernel). 
+  may cause those machines to panic during the boot phase.
@@ -9194,6 +9328,7 @@
-  If you have a joystick, you can say Y here to enable generic
-  joystick support. You will also need to say Y or M to at least one
-  of the hardware specific joystick drivers. This will make the
-  joysticks available as /dev/jsX devices. Please read the file
-  Documentation/joystick.txt which contains more information and the
-  location of the joystick package that you'll need.
+  If you have a joystick, 6dof controller, gamepad, steering wheel,
+  weapon control system or something like that you can say Y here to
+  enable generic support for these controllers. You will also need to
+  say Y or M to at least one of the hardware specific drivers. This
+  will make the controllers available as /dev/jsX devices. Please read
+  the file Documentation/joystick.txt which contains more information
+  and the location of the joystick package that you'll need.
@@ -9201,6 +9336 @@
-  This driver is also available as a module ( = code which can be
-  inserted in and removed from the running kernel whenever you want).
-  The module will be called joystick.o. If you want to compile it as a
-  module, say M here and read Documentation/modules.txt.
-
-Classic PC analog joysticks and gamepads
+Classic PC analog
@@ -9208,4 +9338,4 @@
-  Say Y here if you have an analog joystick or gamepad that connects
-  to the PC gameport. This supports many different types, including
-  joysticks with throttle control, with rudders, or with extensions
-  like additional hats and buttons compatible with CH Flightstick Pro,
+  Say Y here if you have a controller that connects to the PC
+  gameport. This supports many different types, including joysticks
+  with throttle control, with rudders, or with extensions like
+  additional hats and buttons compatible with CH Flightstick Pro,
@@ -9215,5 +9345,5 @@
-FPGaming and MadCatz A3D controllers
-CONFIG_JOY_ASSASIN
-  Say Y here if you have an FPGaming Assasin 3D, MadCatz Panther or
-  MadCatz Panther XL. For more information on how to use the driver
-  please read Documentation/joystick.txt
+FPGaming and MadCatz A3D
+CONFIG_JOY_ASSASSIN
+  Say Y here if you have an FPGaming or MadCatz controller using the
+  A3D protocol over the PC gameport. For more information on how to
+  use the driver please read Documentation/joystick.txt
@@ -9221 +9351 @@
-Gravis GrIP joysticks and gamepads
+Gravis GrIP
@@ -9223,3 +9353,9 @@
-  Say Y here if you have a Gravis GamePad Pro, Gravis Xterminator or
-  Gravis Blackhawk Digital. For more information on how to use the
-  driver please read Documentation/joystick.txt
+  Say Y here if you have a Gravis controller using the GrIP protocol
+  over the PC gameport. For more information on how to use the driver
+  please read Documentation/joystick.txt
+
+Logitech ADI
+CONFIG_JOY_LOGITECH
+  Say Y here if you have a Logitech controller using the ADI
+  protocol over the PC gameport. For more information on how to use
+  the driver please read Documentation/joystick.txt
@@ -9227 +9363,20 @@
-PDPI Lightning 4 gamecards
+Microsoft SideWinder
+CONFIG_JOY_SIDEWINDER
+  Say Y here if you have a Microsoft controller using the Digital
+  Overdrive protocol over PC gameport. For more information on how to
+  use the driver please read Documentation/joystick.txt
+
+ThrustMaster DirectConnect
+CONFIG_JOY_THRUSTMASTER
+  Say Y here if you have a ThrustMaster controller using the
+  DirectConnect (BSP) protocol over the PC gameport. For more
+  information on how to use the driver please read
+  Documentation/joystick.txt
+
+Creative Labs Blaster
+CONFIG_JOY_CREATIVE
+  Say Y here if you have a Creative Labs controller using the
+  Blaster protocol over the PC gameport. For more information on how
+  to use the driver please read Documentation/joystick.txt
+
+PDPI Lightning 4 card
@@ -9233,4 +9388,17 @@
-Logitech Digital joysticks and gamepads
-CONFIG_JOY_LOGITECH
-  Say Y here if you have a Logitech WingMan Extreme Digital,
-  Logitech ThunderPad Digital or Logitech CyberMan 2. For more
+Trident 4DWave and Aureal Vortex gameport
+CONFIG_JOY_PCI
+  Say Y here if you have a Trident 4DWave DX/NX or Aureal Vortex 1/2
+  card and want to use its gameport in its enhanced digital mode
+  with and ordinary analog joystick. For more information on how to
+  use the driver please read Documentation/joystick.txt
+
+Magellan and Space Mouse
+CONFIG_JOY_MAGELLAN
+  Say Y here if you have a Magellan or Space Mouse 6DOF controller
+  connected to your computer's serial port.  For more information on
+  how to use the driver please read Documentation/joystick.txt
+
+SpaceTec SpaceOrb 360 and SpaceBall Avenger
+CONFIG_JOY_SPACEORB
+  Say Y here if you have a SpaceOrb 360 or SpaceBall Avenger 6DOF
+  controller connected to your computer's serial port.  For more
@@ -9240,6 +9408,5 @@
-Microsoft SideWinder, Genius Digital joysticks and gamepads
-CONFIG_JOY_SIDEWINDER
-  Say Y here if you have a Microsoft SideWinder 3d Pro, Microsoft
-  SideWinder Precision Pro, Microsoft SideWinder Force Feedback Pro,
-  Microsoft Sidewinder GamePad or Genius Flight2000 F-23 Digital. For
-  more information on how to use the driver please read
+SpaceTec SpaceBall 4000 FLX
+CONFIG_JOY_SPACEBALL
+  Say Y here if you have a SpaceTec SpaceBall 4000 FLX
+  controller connected to your computer's serial port.  For more
+  information on how to use the driver please read
@@ -9248,5 +9415,5 @@
-ThrustMaster DirectConnect joysticks and gamepads
-CONFIG_JOY_THRUSTMASTER
-  Say Y here if you have a ThrustMaster Millenium 3D Inceptor or a
-  ThrustMaster 3D Rage Pad. For more information on how to use the
-  driver please read Documentation/joystick.txt
+Logitech WingMan Warrior
+CONFIG_JOY_WARRIOR
+  Say Y here if you have a Logitech WingMan Warrior controller
+  connected to your computer's serial port.  For more information on
+  how to use the driver please read Documentation/joystick.txt
@@ -9254 +9421 @@
-NES, SNES, PSX, Multisystem joysticks and gamepads
+NES, SNES, N64, PSX, Multi
@@ -9257,3 +9424,4 @@
-  Super Nintendo Entertainment System gamepad, Sony PlayStation
-  gamepad or a Multisystem -- Atari, Amiga, Commodore, Amstrad CPC
-  joystick. For more information on how to use the driver please read
+  Super Nintendo Entertainment System gamepad, Nintendo 64 gamepad,
+  Sony PlayStation gamepad or a Multisystem -- Atari, Amiga,
+  Commodore, Amstrad CPC joystick connected to your parallel port.
+  For more information on how to use the driver please read
@@ -9262 +9430 @@
-Sega, Multisystem joysticks and gamepads
+Sega, Multi
@@ -9266,3 +9434,3 @@
-  Commodore, Amstrad CPC joystick. For more information on how to use
-  the driver please read Documentation/joystick.txt and
-  Documentation/joystick-parport.txt
+  Commodore, Amstrad CPC joystick connected to your parallel port. For
+  more information on how to use the driver please read
+  Documentation/joystick.txt and Documentation/joystick-parport.txt
@@ -9270 +9438 @@
-TurboGraFX Multisystem joystick interface
+TurboGraFX interface
@@ -9425,14 +9592,0 @@
-Generic OPL2/OPL3 FM synthesizer support
-CONFIG_SOUND_ADLIB
-  Answer Y if your card has a FM chip made by Yamaha (OPL2/OPL3/OPL4).
-  Answering Y is usually a safe and recommended choice, however some
-  cards may have software (TSR) FM emulation. Enabling FM support with
-  these cards may cause trouble (I don't currently know of any such
-  cards, however). 
-
-  Please read the file Documentation/sound/OPL3 if your card has an
-  OPL3 chip.
-
-  If unsure, say Y.
-  
-
@@ -9718 +9872,9 @@
-  Answer Y here, unless you know you will not need the option.
+  Answer Y if your card has a FM chip made by Yamaha (OPL2/OPL3/OPL4).
+  Answering Y is usually a safe and recommended choice, however some
+  cards may have software (TSR) FM emulation. Enabling FM support with
+  these cards may cause trouble (I don't currently know of any such
+  cards, however).
+  Please read the file Documentation/sound/OPL3 if your card has an
+  OPL3 chip.
+
+  If unsure, say Y.
@@ -9924,0 +10087,6 @@
+ESS Maestro sound chipsets
+CONFIG_SOUND_MAESTRO
+  Say Y or M if you have a sound system driven by ESS's Maestro line
+  of PCI sound chips.  These include the Maestro 1, Maestro 2, and
+  Maestro 2E.  See Documentation/sound/Maestro for more details.
+
@@ -9956,5 +10123,0 @@
-  CAUTION: the ISDN driver shipped with this kernel distribution
-  is outdated and might not work without problems. An updated driver
-  is available for download. Please read http://www.isdn4linux.de
-  on the WWW for a list of servers.
-
@@ -9969,3 +10132 @@
-  read http://alumni.caltech.edu/~dank/isdn/ on the WWW. (To browse
-  the WWW, you need to have access to a machine on the Internet that
-  has a program like lynx or netscape.)
+  read http://alumni.caltech.edu/~dank/isdn/ on the WWW.
@@ -10021 +10182 @@
-X.25 PLP on top of ISDN (EXPERIMENTAL)
+X.25 PLP on top of ISDN
@@ -10023,2 +10184,2 @@
-  This experimental feature provides the X.25 protocol over ISDN
-  connections. See Documentation/isdn/README.x25 for more information
+  This feature provides the X.25 protocol over ISDN connections.
+  See Documentation/isdn/README.x25 for more information
@@ -10031,9 +10192,12 @@
-  line. Supported options are CD (call deflection), CFU (Call 
-  forward unconditional), CFB (Call forward when busy) and CFNR 
-  (call forward not reachable).
-  Additionally the actual CFU, CFB and CFNR state may be 
-  interrogated. The use of CFU, CFB, CFNR and interrogation may
-  be limited to some countries. The keypad protocol is still not
-  implemented.
-  CD should work in all countries if this service has been sub-
-  scribed.
+  line. 
+
+  Supported options are CD (call deflection), CFU (Call forward
+  unconditional), CFB (Call forward when busy) and CFNR (call forward
+  not reachable). Additionally the actual CFU, CFB and CFNR state may
+  be interrogated.
+
+  The use of CFU, CFB, CFNR and interrogation may be limited to some
+  countries. The keypad protocol is still not implemented. CD should
+  work in all countries if the service has been subscribed to.
+
+  Please read the file Documentation/isdn/README.diversion.
@@ -10281 +10445 @@
-HiSax Support for Winbond W6692 based cards (EXPERIMENTAL)
+HiSax Support for Winbond W6692 based cards
@@ -10314,3 +10478 @@
-  http://www.spellcast.com for more information (to browse the WWW,
-  you need to have access to a machine on the Internet that has a
-  program like lynx or netscape).
+  http://www.spellcast.com for more information.
@@ -10322,2 +10484,2 @@
-  into the card using the eiconctrl utility which is part of the latest
-  isdn4k-utils package. Please read the file
+  into the card using the eiconctrl utility which is part of the
+  latest isdn4k-utils package. Please read the file
@@ -10328,4 +10490,4 @@
-  Say Y here if you have an old-type Eicon active ISDN card. In order to
-  use this card, additional firmware is necessary, which has to be loaded
-  into the card using the eiconctrl utility which is part of the latest
-  isdn4k-utils package. Please read the file
+  Say Y here if you have an old-type Eicon active ISDN card. In order
+  to use this card, additional firmware is necessary, which has to be
+  loaded into the card using the eiconctrl utility which is part of
+  the latest isdn4k-utils package. Please read the file
@@ -10338,2 +10500,2 @@
-  (mgetty+sendfax, hylafax), you will be able to use your Linux box 
-  as an ISDN-fax-machine. This must be supported by the lowlevel driver
+  (mgetty+sendfax, hylafax), you will be able to use your Linux box as
+  an ISDN-fax-machine. This must be supported by the lowlevel driver
@@ -10342 +10504 @@
-AVM-B1 with CAPI2.0 support
+AVM CAPI2.0 support
@@ -10353 +10515 @@
-
+  
@@ -10367 +10529 @@
-AVM T1/T1B ISA support
+AVM T1/T1-B ISA support
@@ -10375,0 +10538,5 @@
+AVM T1/T1-B PCI support
+CONFIG_ISDN_DRV_AVMB1_T1PCI
+  Enable support for the AVM T1 T1B card.
+  Note: This is a PRI card and handle 30 B-channels.
+
@@ -10381,0 +10549 @@
+
@@ -10521,0 +10690 @@
+Amiga 1200/600 PCMCIA support
@@ -11785,0 +11955,62 @@
+IBM's S/390 architecture
+CONFIG_ARCH_S390
+  Select this option, if you want to run the Kernel on one of IBM's
+  mainframes of the S/390 generation. You should have installed the
+  s390-compiler released by IBM (based on gcc-2.95.1) before.
+
+Merge some code into the kernel to make the image IPLable
+CONFIG_IPLABLE
+  If you want to use the produced kernel to IPL directly from a
+  device, you have to merge a bootsector specific to the device
+  into the first bytes of the kernel. You will have to select the
+  IPL device on another question, that pops up, when you select
+  CONFIG_IPLABE.
+
+IPL from a S/390 tape unit
+CONFIG_IPL_TAPE
+  Select this option if you want to IPL the image from a tape.
+
+IPL from a virtual card reader emulated by VM/ESA
+CONFIG_IPL_RDR_VM
+  Select this option if you are running under VM/ESA and want 
+  to IPL the image from the emulated card reader.
+
+IPL from a real card reader
+CONFIG_IPL_RDR
+  Select this option if you want to IPL the image from a real
+  card reader. Maybe you still got one and want to try. We didn't
+  test.
+
+IBMs S/390 Harddisks (DASDs)
+CONFIG_DASD
+  Enable this option if you want to access DASDs directly utilizing
+  S/390s channel subsystem commands. This is necessary for running
+  natively on a single image or an LPAR.
+
+Enable DASD fast write
+CONFIG_DASD_FAST_IO
+  Enable fast I/O for DASDs. That means that the next I/O command
+  is already issued at interrupt time, if an I/O request is pending.
+  This option gives significant speedup of I/O, because we don't
+  schedule the bottom-halves as often as Intel.
+
+Support for IBM-style disk-labels (S/390)
+CONFIG_S390_PARTITION
+  Enable this option to assure standard IBM labels on the DASDs.
+  You must enable it, if you are planning to access DASDs also
+  attached to another IBM mainframe operation system (OS/390, 
+  VM/ESA, VSE/ESA).
+
+ECKD devices
+CONFIG_DASD_ECKD
+  ECKD devices are the most commonly used devices. you should enable
+  this option unless you are very sure to have no ECKD device.
+
+CKD devices
+CONFIG_DASD_CKD
+  CKD devices are currently unsupported.
+
+FBA devices
+CONFIG_DASD_FBA
+  FBA devices are currently unsupported.
+
@@ -11792,0 +12024,18 @@
+
+QuickNet Internet LineJack/PhoneJack support
+CONFIG_PHONE_IXJ
+  Say M if you have a telephony card manufactured by Quicknet
+  Technologies, Inc.  These include the Internet PhoneJACK and
+  Internet LineJACK Telephony Cards.
+
+  For the ISA versions of these products, you can configure the
+  cards using the isapnp tools (pnpdump/isapnp) or you can use the
+  backported isapnp module.  Please read:
+
+  /usr/src/linux/Documentation/telephony/ixj.txt.
+
+  For more information on these cards, see Quicknet's website at:
+  http://www.quicknet.net/
+
+  If you do not have any Quicknet telephony cards, you can safely
+  ignore this option.
