--- Configure.help-2.2.15	Thu Jun  8 14:45:49 2000
+++ Configure.help-2.2.16	Thu Jun  8 14:44:51 2000
@@ -12,2 +12,2 @@
-#   - French, by David Bourgin (dbourgin@wsc.com), at
-#     http://www.linux-kheops.com/traduc/kernels/
+#   - French, by Pierre Tane (tanep@bigfoot.com), at
+#     http://www.traduc.org/kernelfr
@@ -209,0 +210,5 @@
+Default RAM disk size
+CONFIG_BLK_DEV_RAM_SIZE
+  The default value is 4096. Only change this if you know what are
+  you doing. If you are using IBM S/390, then set this to 8192.
+
@@ -2377 +2382 @@
-  http://www.rustcorp.com/linux/ipchains/) to allow selective blocking
+  http://netfilter.kernelnotes.org/ipchains/) to allow selective blocking
@@ -2446,3 +2451,20 @@
-  command line, you can say N here. If unsure, say Y. Note that if you
-  want to use BOOTP, a BOOTP server must be operating on your network.
-  Read Documentation/nfsroot.txt for details.
+  command line, you can say N here.
+
+  If unsure, say Y. Note that if you want to use BOOTP, a BOOTP server
+  must be operating on your network.  Read Documentation/nfsroot.txt
+  for details.
+
+DHCP support
+CONFIG_IP_PNP_DHCP
+  If you want your Linux box to mount its whole root filesystem (the
+  one containing the directory /) from some other computer over the
+  net via NFS and you want the IP address of your computer to be
+  discovered automatically at boot time using the DHCP protocol (a
+  special protocol designed for doing this job), say Y here. In case
+  the boot ROM of your network card was designed for booting Linux and
+  does DHCP itself, providing all necessary information on the kernel
+  command line, you can say N here.
+
+  If unsure, say Y. Note that if you want to use DHCP, a DHCP server
+  must be operating on your network.  Read Documentation/nfsroot.txt
+  for details.
@@ -3847,5 +3869,4 @@
-  Consult the SCSI-HOWTO, available via anonymous FTP from
-  ftp://metalab.unc.edu/pub/Linux/docs/HOWTO, and the file
-  README.ips in drivers/scsi for more information.  If this driver
-  does not work correctly without modification please contact the
-  author by email at ipslinux@us.ibm.com.
+  See http://www.developer.ibm.com/welcome/netfinity/serveraid.html
+  for more information.  If this driver does not work correctly
+  without modification please contact the author by email at
+  ipslinux@us.ibm.com.
@@ -5696,0 +5718,40 @@
+Generic HDLC driver
+CONFIG_HDLC
+  Say Y to this option if your Linux box contains a WAN card supported
+  by this driver and you are planning to connect the box to a WAN
+  ( = Wide Area Network). You will need supporting software from
+  ftp://ftp.pm.waw.pl/pub/Linux/hdlc/
+
+  If unsure, say N here.
+
+SDL RISCom/N2 driver
+CONFIG_N2
+  This driver is for RISCom/N2 single or dual channel ISA cards
+  made by SDL Communications Inc.
+  If you have such a card, say Y here. This driver requires
+  Generic HDLC driver and its supporting utility available from
+  ftp://ftp.pm.waw.pl/pub/Linux/hdlc/
+  Note that N2csu and N2dds cards are not supported by this driver.
+
+  If unsure, say N here.
+
+Moxa C101 driver
+CONFIG_C101
+  This driver is for C101 SuperSync ISA cards made by Moxa
+  Technologies Co., Ltd.
+  If you have such a card, say Y here. This driver requires
+  Generic HDLC driver and its supporting utility available from
+  ftp://ftp.pm.waw.pl/pub/Linux/hdlc/
+
+  If unsure, say N here.
+
+SBE wanXL driver
+CONFIG_WANXL
+  This driver is for wanXL PCI cards made by SBE Inc.
+  If you have such a card, say Y here. This driver requires
+  Generic HDLC driver and its supporting utility available from
+  ftp://ftp.pm.waw.pl/pub/Linux/hdlc/ and a firmware available
+  from SBE Inc.
+
+  If unsure, say N here.
+
@@ -6323,3 +6384,4 @@
-  If you have a network (Ethernet) card of this type, say Y. Note
-  however that the EtherExpress PRO/100 Ethernet card has its own
-  separate driver. Please read the Ethernet-HOWTO, available via FTP
+  If you have a network (Ethernet) card of this type, say Y. This
+  driver supports intel i82595{FX,TX} based boards. Note however 
+  that the EtherExpress PRO/100 Ethernet card has its own separate
+  driver. Please read the Ethernet-HOWTO, available via FTP
@@ -7931,0 +7994,12 @@
+nls default codepage
+CONFIG_NLS_DEFAULT
+  The default NLS used when mounting filesystem. Currently, the valid
+  values are cp437, cp737, cp775, cp850, cp852, cp855, cp857, cp860,
+  cp861, cp862, cp863, cp864, cp865, cp866, cp869, cp874, cp932, cp936,
+  cp949, cp950, iso8859-1, iso8859-2, iso8859-3, iso8859-4, iso8859-5,
+  iso8859-6, iso8859-7, iso8859-8, iso8859-9, iso8859-14, iso8859-15, 
+  koi8-r.  If you specify a wrong value, it will use the built-in NLS; 
+  compatible with iso8859-1.
+
+  If unsure, specify it as "cp437".
+
@@ -8109,0 +8184,42 @@
+nls codepage 932
+CONFIG_NLS_CODEPAGE_932
+  The Microsoft fat filesystem family can deal with filenames in
+  native language character sets. These character sets are stored in
+  so-called DOS codepages. You need to include the appropriate
+  codepage if you want to be able to read/write these filenames on
+  DOS/Windows partitions correctly. This does apply to the filenames
+  only, not to the file contents. You can include several codepages;
+  say Y here if you want to include the DOS codepage for Shift-JIS.
+
+nls codepage 936
+CONFIG_NLS_CODEPAGE_936
+  The Microsoft fat filesystem family can deal with filenames in
+  native language character sets. These character sets are stored in
+  so-called DOS codepages. You need to include the appropriate
+  codepage if you want to be able to read/write these filenames on
+  DOS/Windows partitions correctly. This does apply to the filenames
+  only, not to the file contents. You can include several codepages;
+  say Y here if you want to include the DOS codepage for Simplified
+  Chinese(GBK).
+
+nls codepage 949
+CONFIG_NLS_CODEPAGE_949
+  The Microsoft fat filesystem family can deal with filenames in
+  native language character sets. These character sets are stored in
+  so-called DOS codepages. You need to include the appropriate
+  codepage if you want to be able to read/write these filenames on
+  DOS/Windows partitions correctly. This does apply to the filenames
+  only, not to the file contents. You can include several codepages;
+  say Y here if you want to include the DOS codepage for UHC.
+
+nls codepage 950
+CONFIG_NLS_CODEPAGE_950
+  The Microsoft fat filesystem family can deal with filenames in
+  native language character sets. These character sets are stored in
+  so-called DOS codepages. You need to include the appropriate
+  codepage if you want to be able to read/write these filenames on
+  DOS/Windows partitions correctly. This does apply to the filenames
+  only, not to the file contents. You can include several codepages;
+  say Y here if you want to include the DOS codepage for Traditional
+  Chinese(Big5).
+
@@ -9209,8 +9324,0 @@
-Ignore multiple suspend/standby events
-CONFIG_APM_IGNORE_MULTIPLE_SUSPEND
-  This option is necessary on the IBM Thinkpad 560, but should work on
-  all other laptops. When the APM BIOS returns multiple suspend or
-  standby events while one is already being processed they will be
-  ignored. Without this the Thinkpad 560 has troubles with the user
-  level daemon apmd, and with the PCMCIA package pcmcia-cs.
-
@@ -9351,0 +9460,12 @@
+SBC-60XX Watchdog Timer
+CONFIG_60XX_WDT
+ This driver can be used with the watchdog timer found on some
+ single board computers, namely the 6010 PII based computer.
+ It may well work with other cards.  It reads port 0x443 to enable
+ and re-set the watchdog timer, and reads port 0x45 to disable
+ the watchdog.  If you have a card that behave in similar ways,
+ you can probably make this driver work with your card as well.
+
+ You can compile this driver directly into the kernel, or use
+ it as a module.  The module will be called sbc60xxwdt.o.
+
@@ -10171,0 +10292,16 @@
+  
+Trident 4DWave DX/NX or SiS 7018 PCI Audio Core or ALi 5451
+CONFIG_SOUND_TRIDENT
+  Say Y or M if you have a PCI sound card utilizing the Trident
+  4DWave-DX/NX chipset or your mother board chipset has SiS 7018
+  built-in, or if you have an ALi 5451. The SiS 7018 PCI Audio Core
+  is embedded in SiS960 Super South Bridge and SiS540/630 Single
+  Chipset.
+
+  Use lspci -n to find out if your sound card or chipset uses
+  Trident 4DWave or SiS 7018. PCI ID 1023:2000 or 1023:2001 stands
+  for Trident 4Dwave. PCI ID 1039:7018 stands for SiS7018.
+  PCI ID 10b9:5451 stands for ALi 5451.
+
+  This driver differs slightly from OSS/Free, so PLEASE READ the
+  comments at the beginning of driver/sound/trident.c
@@ -12121 +12257,7 @@
-  FBA devices are currently unsupported.
+  FBA devices are e.g. the Vitual disk in storage under VM/ESA and others.
+
+Diag access to CMS formatted minidisk
+CONFIG_DASD_MDSK
+  By using this access method you can acess any disk supported by VM/ESA.
+  You have to format the disk using CMS and then specify the parameter
+  dasd_force_diag=<devno> in the parameter line of the kernel.
