--- Configure.help-2.2.12	Fri Sep 10 00:28:29 1999
+++ Configure.help-2.2.13	Fri Oct 22 01:33:06 1999
@@ -3632,8 +3632,9 @@
-  talk to these devices using the SCSI protocol. For CD-writers, you
-  would need the program cdwrite, available via FTP (user: anonymous)
-  from ftp://metalab.unc.edu/pub/Linux/utils/disk-management; for
-  other devices, it's possible that you'll have to write the driver
-  software yourself, so have a look at the SCSI-HOWTO and at the
-  SCSI-Programming-HOWTO, both available via FTP (user: anonymous) in
-  ftp://metalab.unc.edu/pub/Linux/docs/HOWTO. Please read the file
-  Documentation/scsi-generic.txt for more information.
+  talk to these devices using the SCSI protocol. For scanners, look at
+  SANE (www.mostang.com/sane). For CD writer software look at cdrecord
+  (www.fokus.gmd.de/research/cc/glone/employees/joerg.schilling/private
+  /cdrecord.html) and for burning a "disk at once": cdrdao
+  (www.ping.de/sites/daneb/cdrdao.html). Cdparanoia is a high quality
+  digital reader of audio CDs (www.xiph.org/paranoia).
+  For other devices, it's possible that you'll have to write the driver
+  software yourself. Please read the file Documentation/scsi-generic.txt
+  for more information.
@@ -3845,0 +3847,9 @@
+IBM ServeRAID Support
+CONFIG_SCSI_IPS
+  This is support for the IBM ServeRAID hardware RAID controllers.
+  Consult the SCSI-HOWTO, available via anonymous FTP from
+  ftp://metalab.unc.edu/pub/Linux/docs/HOWTO, and the file
+  README.ips in drivers/scsi for more information.  If this driver
+  does not work correctly without modification please contact the
+  author by email at ipslinux@us.ibm.com.
+
@@ -5507,0 +5518,12 @@
+SBNI Leased Line Adapters
+CONFIG_SBNI
+  This is a driver for ISA SBNI12-xx cards that is a low cost
+  alternative to leased line modems. Say Y if you want to insert
+  driver into kernel or say M to compile driver as a module. 
+  
+  You can find more information and last versions of drivers and 
+  utilities at http://www.granch.ru. If you have any question you
+  can mail to sbni@granch.ru.
+  
+  Say N if unsure.
+  
@@ -5709,0 +5732,12 @@
+PCI DM9102 support
+CONFIG_DM9102
+  This driver is for DM9102 compatible PCI cards from Davicom 
+  (http://www.davicom.com.tw) 
+  If you have a PCI DM9102 network (Ethernet) card, say Y.
+
+  This driver is also available as a module ( = code which can be
+  inserted in and removed from the running kernel whenever you want).
+  The module will be called dmfe.o. If you want to compile it as a
+  module, say M here and read Documentation/modules.txt as well as
+  Documentation/networking/net-modules.txt.
+
@@ -9011,5 +9045,6 @@
-  The watchdog is usually used together with the watchdog daemon 
-  which is available via FTP (user: anonymous) from
-  ftp://tsx-11.mit.edu/pub/linux/sources/sbin/. This daemon can also
-  monitor NFS connections and can reboot the machine when the process
-  table is full.
+  The watchdog is usually used together with the watchdog daemon which is
+  available via FTP (user: anonymous) from
+  ftp://metalab.unc.edu/pub/linux/system/daemons/watchdog. This daemon can
+  check a larger part of the system. For instance it can monitor NFS
+  connections and reboot the machine when the process table is full or the
+  workload exceeds a predefined value.
@@ -9318 +9353 @@
-  package, available at http://www.imladris.demon.co.uk/pcsp/.
+  package, available at ftp://ftp.infradead.org/pub/pcsp/.
@@ -9503,0 +9539,5 @@
+SoundPro chip support
+CONFIG_SOUND_SPRO
+  If you have a (usually Taiwanese) motherboard with the SoundPro chip
+  on board, say Y here. Otherwise say N.
+
@@ -9541,0 +9582,5 @@
+VIA 82Cxxx audio support
+CONFIG_SOUND_VIA82CXXX
+  Answer Y if you have a VIA82C686 chip, typically found built
+  onto a motherboard.
+
@@ -9869,0 +9915,10 @@
+NeoMagic 256AV/256ZX sound chipsets
+CONFIG_SOUND_NM256
+  Say M here to include audio support for the NeoMagic 256AV/256ZX
+  chipsets.  These are the audio chipsets found in the Sony Z505S/SX/DX,
+  some Sony F-series, and the Dell Latitude CPi and CPt laptops. It includes 
+  support for an AC97-compatible mixer and an apparently proprietary sound 
+  engine.
+
+  See Documentation/sound/NM256 for further information.
+
@@ -10045,0 +10101,4 @@
+HiSax Support for german 1TR6
+CONFIG_HISAX_1TR6
+  Enable this if you have a old german 1TR6 line.
+
@@ -10215,0 +10275,13 @@
+HiSax Support for HFC PCI-Bus cards
+CONFIG_HISAX_HFC_PCI
+  This enables HiSax support for the HFC-S PCI 2BDS0 based cards.
+  
+  For more informations see under Documentation/isdn/README.hfc-pci.
+
+HiSax Support for Winbond W6692 based cards (EXPERIMENTAL)
+CONFIG_HISAX_W6692
+  This enables HiSax support for Winbond W6692 based PCI ISDN cards.
+  
+  See Documentation/isdn/README.HiSax on how to configure it using a
+  different D-channel protocol, or non-standard IRQ/port settings.
+
@@ -10272 +10344 @@
-  This enables support for the AVM B1 ISDN networking cards. In
+  This enables support for the AVM B1/T1 ISDN networking cards.In
@@ -10286,0 +10359,17 @@
+AVM B1 ISA support
+CONFIG_ISDN_DRV_AVMB1_B1ISA
+  Enable support for the ISA version of the AVM B1 card.
+
+AVM B1 PCI support
+CONFIG_ISDN_DRV_AVMB1_B1PCI
+  Enable support for the PCI version of the AVM B1 card.
+
+AVM T1/T1B ISA support
+CONFIG_ISDN_DRV_AVMB1_T1ISA
+  Enable support for the AVM T1 T1B card.
+  Note: This is a PRI card and handle 30 B-channels.
+
+AVM B1/M1/M2 PCMCIA support
+CONFIG_ISDN_DRV_AVMB1_B1PCMCIA
+  Enable support for the PCMCIA version of the AVM B1 card.
+
@@ -11149,0 +11239,19 @@
+Trust FM Radio Card
+CONFIG_RADIO_TRUST
+  Choose Y here if you have this FM radio card, and then fill in the 
+  port address below.
+
+  In order to control your radio card, you will need to use programs
+  that are compatible with the Video for Linux API. Information on
+  this API and pointers to "v4l" programs may be found at
+  http://roadrunner.swansea.uk.linux.org/v4l.shtml.
+
+  If you want to compile this driver as a module ( = code which can be
+  inserted in and removed from the running kernel whenever you want),
+  say M here and read Documentation/modules.txt. The module will be
+  called radio-trust.o.
+
+Trust FM Radio I/O port
+CONFIG_RADIO_TRUST_PORT
+  Enter the I/O port of your card (usually 0x350 or 0x358).
+
@@ -11638,0 +11747,7 @@
+
+Simple 53c710 SCSI support (Compaq, NCR machines)
+CONFIG_SCSI_SIM710
+  This is a driver for the NCR53C710 chip commonly found in Compaq and
+  NCR machines.  If you are looking for 53C710 support for an Amiga or
+  some 680x0 based VME card then you probably want the other NCR53C710
+  driver.
