--- Configure.help-2.2.14	Thu Jan  6 02:03:12 2000
+++ Configure.help-2.2.15	Sun May  7 01:21:59 2000
@@ -2552,0 +2553,14 @@
+IP: UDP masquerading loose checking
+CONFIG_IP_MASQUERADE_UDP_LOOSE
+  Whether UDP masquerading does address checking in a loose fashion.
+
+  If you say Y here, then UDP masqueraded connections will allow
+  any external system to be connect back through the firewall to the
+  port on the internal machine.  However it will allow the more
+  efficient use of masqueraded ports, and may be required for some
+  gaming uses.
+
+  You should only say Y here if you understand the consequences since
+  it will open your internal network to external probing and potential
+  attacks.  In all other cases choose N
+
@@ -2576 +2590 @@
-  http://juanjox.linuxhq.com/
+  http://juanjox.kernelnotes.org/
@@ -2591 +2605 @@
-  http://juanjox.linuxhq.com/ .
+  http://juanjox.kernelnotes.org/ .
@@ -2622 +2636 @@
-  downloaded from http://juanjox.linuxhq.com/
+  downloaded from http://juanjox.kernelnotes.org/
@@ -3484,6 +3498,5 @@
-  available via FTP (user: anonymous) from
-  ftp://shadow.cabi.net/pub/Linux. Please read the Bridge mini-HOWTO
-  for more information. Note that if your box acts as a bridge, it
-  probably contains several Ethernet devices, but the kernel is not
-  able to recognize more than one at boot time without help; for
-  details read the Ethernet-HOWTO, available via FTP (user: anonymous)
+  available from http://lrp.plain.co.nz/tarballs/bridgex-0.30.tar.gz
+  Note that if your box acts as a bridge, it probably contains several
+  Ethernet devices, but the kernel is not able to recognize more than 
+  one ISA ethernet card at boot time without help; for  details read 
+  the Ethernet-HOWTO, available via FTP (user: anonymous)
@@ -5492,0 +5506,25 @@
+Lan Media sync serial boards support
+CONFIG_LANMEDIA
+  This is a driver for the following Lan Media family of serial boards.
+
+  LMC 1000 board allows you to connect synchronous serial devices (for
+  example base-band modems, or any other device with the X.21, V.24,
+  V.35 or V.36 interface) to your Linux box. 
+
+  LMC 1200 with on board DSU board allows you to connect your Linux
+  box dirrectly to a T1 or E1 circuit. 
+
+  LMC 5200 board provides a HSSI interface capable of runnig up to
+  52 mbits per second.
+
+  LMC 5245 board connects directly to a T3 circuit saving the
+  additional external hardware.
+
+  To change setting such as syncPPP vs cisco HDLC or clock source you
+  will need lmcctl.  It it available at ftp.lanmedia.com.
+
+  The driver will be compiled as a module ( = code which can be
+  inserted in and removed from the running kernel whenever you want).
+  The module will be called lmc.o. For general information about
+  modules read Documentation/modules.txt.
+
@@ -5943,0 +5982 @@
+  The adapters support Jumbo Frames.
@@ -5947 +5986 @@
-  Questions concerning this driver may be addresse to:
+  Questions concerning this driver may be addressed to:
@@ -6527,2 +6566,2 @@
-  The module will be called tulip.o. If you want to compile it as a
-  module, say M here and read Documentation/modules.txt as well as
+  The module will be called old_tulip.o. If you want to compile it as
+  a module, say M here and read Documentation/modules.txt as well as
@@ -6587 +6626 @@
-  Please email feedback to james.banks@caldera.com.
+  Please email feedback to torben.mathiasen@compaq.com.
@@ -6744,0 +6784,13 @@
+IBM Lanstreamer chipset PCI adapter support
+CONFIG_IBMLS
+  This is support for IBM Lanstreamer PCI Token Ring Cards.
+
+  If you have such an adapter, say Y and read the Token-Ring mini-HOWTO
+  available via FTP (user:anonymous) from
+  ftp://metalab.unc/edu/pub/Linux/docs/HOWTO.
+
+  This driver is also available as a modules ( = code which can be
+  inserted in and removed from the running kernel whenever you want).
+  The modules will be called lanstreamer.o. If you want to compile it as
+  a module, say M here and read Documentation/modules.txt.
+
@@ -6749,0 +6802,2 @@
+  It also supports Compaq PCI Token Ring adapters and Proteon ISA
+  Token Ring adapters (1392 and 1392+).
@@ -7542 +7596 @@
-QNX filesystem support (EXPERIMENTAL)
+QNX4 filesystem support (EXPERIMENTAL)
@@ -7546 +7600 @@
-  "QNXFS read-write support" below, you will only be able to read
+  "QNX4FS write support" below, you will only be able to read
@@ -7554 +7608,2 @@
-  If unsure, say N.
+  If you don't know whether you need it, then you don't need it:
+  answer N.
@@ -7556 +7611 @@
-QNXFS read-write support (FOR TESTING ONLY)
+QNX4FS write support (DANGEROUS)
@@ -7558 +7613 @@
-  Say Y if you want to test write support for QNX filesystems.
+  Say Y if you want to test write support for QNX4 filesystems.
@@ -8367,0 +8423,38 @@
+Specialix SX card support
+CONFIG_SX
+  This is a driver for the Specialix SX multiport card (both the
+  ISA and the PCI version of both the older SI/XIO and the newer SX
+  variants of the card) which gives you many serial ports. You
+  would need something like this to connect more than two modems to 
+  your Linux box, for instance in order to become a dial-in server.
+  You will also need the specialix_sxtools package to be able to 
+  initialize and use the SX system. This driver does NOT support 
+  the rev 1 cards (+/- 1990), or the EISA version of the card. Sorry.
+
+  If you have one of these cards, say Y here and read the file
+  Documentation/sx.txt. Also it's possible to say M here and
+  compile this driver as kernel loadable module which will be called
+  sx.o.
+
+Specialix RIO system support
+CONFIG_RIO
+  This is a driver for the Specialix RIO hostcard (both the
+  ISA and the PCI versions of the card). This hostcard allows you
+  to connect many remote terminal adapters, each supporting 8 or 16
+  serial ports. These cards are ideal if you have more than 100 
+  terminals that need to be connected to your server. (But don't 
+  worry if you have only 32 ports.... That works too). You will 
+  also need the specialix_riotools to be able to initialize and
+  configure your rio system.  
+
+  If you have one of these cards, say Y here. Also it's possible to 
+  say M here and compile this driver as kernel loadable module which 
+  will be called rio.o.
+
+Specialix OLD RIO/PCI support 
+CONFIG_RIO_OLDPCI
+  This turns on support for the older PCI card. If you include
+  this support, performance on the newer cards will suffer a bit.
+
+  If you have one of these cards, say Y here.
+
@@ -8979,3 +9072,6 @@
-  
-  The Centaur C6 (WinChip) has 8 MCRs, allowing write-combining. These
-  are supported.
+
+  The Centaur C6 (WinChip) and WinChip 2&3 processors have 8 MCRs. 
+  These are supported. Note that, due to the design of the WinChip 2&3, 
+  setting the access for normal memory to uncachable or write-combine
+  on these processors will result in instant kernel panic. It is okay 
+  to set this for non-cacheable (video) memory.
@@ -9000,2 +9096,2 @@
-  This driver does not exist at this point, so you might as well 
-  say N.
+  If you are asked this question, something is wrong with config scripts.
+  Zilog serial driver is always enabled in sparc architecture.
@@ -9028,2 +9124,2 @@
-  Battery Powered Linux mini-HOWTO, available via FTP (user:
-  anonymous) from ftp://metalab.unc.edu/pub/Linux/docs/HOWTO/mini.
+  Battery Powered Linux mini-HOWTO, available from
+  http://www.linuxdoc.org/docs.html#howto .
@@ -9042,3 +9138 @@
-  http://www.cs.utexas.edu/users/kharker/linux-laptop/ (to browse the
-  WWW, you need to have access to a machine on the Internet that has a
-  program like lynx or netscape). 
+  http://www.cs.utexas.edu/users/kharker/linux-laptop/ .
@@ -9115,12 +9208,0 @@
-Power off on shutdown 
-CONFIG_APM_POWER_OFF
-  Enable the ability to power off the computer after the Linux kernel
-  is halted. You will need software (e.g., a suitable version of the
-  halt(8) command ("man 8 halt")) to cause the computer to power down.
-  Recent versions of the sysvinit package available from
-  ftp://metalab.unc.edu/pub/Linux/system/daemons/init/ (user:
-  anonymous) contain support for this ("halt -p" shuts down Linux and
-  powers off the computer, if executed from runlevel 0). As with the
-  other APM options, this option may not work reliably with some APM
-  BIOS implementations.
-
@@ -9163,0 +9246,6 @@
+Use real mode APM BIOS call to power off
+CONFIG_APM_REAL_MODE_POWER_OFF
+  Use real mode APM BIOS calls to switch off the computer. This is
+  a work-around for a number of buggy BIOSes. Switch this option on if
+  your computer crashes instead of powering off properly.
+
@@ -9905,0 +9994,13 @@
+Micronas Intermetall MSP 3400 support
+CONFIG_VIDEO_MSP3400
+  This option enables the driver for the Micronas Intermetall MSP 3400 
+  series sound decoder/mixer chips often found on BT848-style TV cards.
+
+  Say Y here if your sound card has a MSP 3400 series sound decoder or 
+  mixer chip.
+
+  This driver is also available as a module ( = code which can be
+  inserted in and removed from the running kernel whenever you want).
+  If you want to compile it as a module, say M here and read
+  Documentation/modules.txt. The module will be called msp3400.o.
+
@@ -10264,0 +10366,5 @@
+Disable keypad protocol option
+CONFIG_HISAX_NO_KEYPAD
+  If you like to send special dialstrings including * or # without
+  using the keypad protocol, select this option.
+
@@ -10269 +10375 @@
-HiSax Support for Teles 16.0/8.0
+Teles 16.0/8.0
@@ -10278 +10384 @@
-HiSax Support for Teles 16.3 or PNP or PCMCIA
+Teles 16.3 or PNP or PCMCIA
@@ -10287 +10393 @@
-HiSax Support for Teles PCI
+Teles PCI
@@ -10292 +10398 @@
-HiSax Support for Teles S0Box
+Teles S0Box
@@ -10297 +10403 @@
-HiSax Support for AVM A1 (Fritz)
+AVM A1 (Fritz)
@@ -10305 +10411 @@
-HiSax Support for AVM PnP/PCI (Fritz!PNP/PCI)
+AVM PnP/PCI (Fritz!PNP/PCI)
@@ -10310 +10416 @@
-HiSax Support for AVM A1 PCMCIA (Fritz)
+AVM A1 PCMCIA (Fritz)
@@ -10315 +10421 @@
-HiSax Support for Elsa cards
+Elsa cards
@@ -10324 +10430 @@
-HiSax Support for ITK ix1-micro Revision 2
+ITK ix1-micro Revision 2
@@ -10332 +10438 @@
-HiSax Support for Eicon.Diehl Diva cards
+Eicon.Diehl Diva cards
@@ -10341 +10447 @@
-HiSax Support for ASUSCOM cards
+ASUSCOM ISA cards
@@ -10344 +10450 @@
-  passive ISDN cards.
+  passive ISDN ISA cards.
@@ -10350 +10456 @@
-HiSax Support for TELEINT cards
+TELEINT cards
@@ -10358 +10464 @@
-HiSax Support for HFC-S based cards
+HFC-S based cards
@@ -10367 +10473 @@
-HiSax Support for Sedlbauer cards
+Sedlbauer cards
@@ -10375 +10481 @@
-HiSax Support for USR Sportster internal TA
+USR Sportster internal TA
@@ -10382 +10488 @@
-HiSax Support for MIC card
+MIC card
@@ -10389 +10495 @@
-HiSax Support for NETjet card
+NETjet card
@@ -10397 +10503 @@
-HiSax Support for Niccy PnP/PCI card
+Niccy PnP/PCI card
@@ -10404 +10510 @@
-HiSax Support for Siemens I-Surf card
+Siemens I-Surf card
@@ -10411 +10517 @@
-HiSax Support for HST Saphir card
+HST Saphir card
@@ -10418 +10524 @@
-HiSax Support for Telekom A4T card
+Telekom A4T card
@@ -10425 +10531 @@
-HiSax Support for Scitel Quadro card
+Scitel Quadro card
@@ -10432 +10538 @@
-HiSax Support for Gazel cards
+Gazel cards
@@ -10439 +10545 @@
-HiSax Support for HFC PCI-Bus cards
+HFC PCI-Bus cards
@@ -10445 +10551 @@
-HiSax Support for Winbond W6692 based cards
+Winbond W6692 based cards
@@ -10452 +10558,6 @@
-HiSax Support for Am7930 (EXPERIMENTAL)
+HFC-S+, HFC-SP, HFC-PCMCIA cards (EXPERIMENTAL)
+CONFIG_HISAX_HFC_SX
+  This enables HiSax support for the HFC-S+, HFC-SP and HFC-PCMCIA cards.
+  This code is not finished yet.
+
+Am7930 (EXPERIMENTAL)
@@ -10528,0 +10640,4 @@
+AVM B1 PCI V4 support
+CONFIG_ISDN_DRV_AVMB1_B1PCIV4
+  Enable support for the V4 version of AVM B1 PCI card.
+
@@ -10542,0 +10658,5 @@
+AVM C4 support
+CONFIG_ISDN_DRV_AVMB1_C4
+  Enable support for the AVM C4 PCI card.
+  This card handle 4 BRI ISDN lines (8 channels).
+
@@ -10587,2 +10707,8 @@
-#Mostek real time clock support
-#CONFIG_SUN_MOSTEK_RTC
+Mostek real time clock support
+CONFIG_SUN_MOSTEK_RTC
+  The Mostek RTC chip is used on all knows Sun computers except
+  some JavaStation-s. For a JavaStation you need to say Y both here
+  and to CONFIG_RTC.
+
+  Say Y here unless you are building a special purpose kernel.
+
@@ -11203,5 +11328,0 @@
-  If you have GemTeks combined (PnP) sound- and radio card you must use
-  this driver as a module and setup the card with isapnptools. You must
-  also pass the module a suitable io parameter, 0x248 has been reported
-  to be used by these cards.
-
@@ -11390,0 +11512,6 @@
+  If you have GemTeks combined (PnP) sound- and radio card you might want
+  to use this driver as a module and setup the card with isapnptools. You
+  must also pass the module a suitable io parameter. If you have trouble
+  getting the driver to work with the card as a module, please try building
+  it into the kernel by answering Y.
+
@@ -11405,2 +11532,3 @@
-  Enter either 0x20c, 0x30c, 0x24c or 0x34c here. The card default is
-  0x34c, if you haven't changed the jumper setting on the card.
+  Enter either 0x20c, 0x30c, 0x24c or 0x34c here. 0x20c and 0x248 have
+  been reported to work with the combined sound/radio card. The card
+  default is 0x34c, if you haven't changed the jumper setting on the card.
@@ -11739,27 +11867 @@
-  will create two modules called ircomm and ircomm_tty. For more
-  information go to http://www.pluto.dti.ne.jp/~thiguchi/irda/
-
-IrLPT Protocol
-CONFIG_IRLPT
-  Say Y here if you want to build support for the IrLPT protocol. If
-  you want to compile it as a module, say M here and read
-  Documentation/modules.txt. IrLPT makes it possible to print
-  documents to IrDA capable printers.
-
-IrLPT Client Protocol 
-CONFIG_IRLPT_CLIENT
-  Say Y here if you want to build support for the IrLPT client
-  protocol. If you want to compile it as a module, say M here and read
-  Documentation/modules.txt. The IrLPT client protocol can be used to
-  print documents to IrDA compatible printers like the HP-5MP, or
-  IrLPT printer adapters like the ACTiSYS IR-100M.
-
-IrLPT Server Protocol 
-CONFIG_IRLPT_SERVER
-  Say Y here if you want to build support for the IrLPT server
-  protocol. If you want to compile it as a module, say M here and read
-  Documentation/modules.txt. The IrLPT server protocol makes it
-  possible to use a Linux machine as an infrared printer server for
-  other laptops. So if your Linux machine has a cable connection to a
-  printer, then other laptops can use the Linux machine to print out 
-  documents using infrared communication.
+  will create two modules called ircomm and ircomm-tty.
@@ -11802 +11904 @@
-NSC PC87108 IrDA Device Driver
+NSC IrDA Device Driver
@@ -11804,12 +11906,4 @@
-  Say Y here if you want to build support for the NSC PC87108 IrDA
-  chipset. If you want to compile it as a module, say M here and
-  read Documentation/modules.txt. This drivers currently only supports
-  the ACTiSYS IR2000B ISA card and supports SIR, MIR and FIR (4Mbps)
-  speeds.
-
-Sharp UIRCC IrDA Device Driver
-CONFIG_SHARP_FIR
-  Say Y here if you want to build support for the Sharp UIRCC IrDA
-  chipset. If you want to compile it as a module, say M here and
-  read Documentation/modules.txt. This chipset is used by the Toshiba
-  Tecra laptops.
+  Say Y here if you want to build support for the NSC PC87108 and
+  PC87338 IrDA chipsets. If you want to compile it as a module, say M 
+  here and read Documentation/modules.txt. This driver supports SIR, 
+  MIR and FIR (4Mbps) speeds.
@@ -11831 +11925 @@
-  insert "irattach -d esi" in the /etc/irda/drivers script.
+  start irattach like this: "irattach -d esi".
@@ -11840,2 +11934,2 @@
-  dongles you will have to insert "irattach -d actisys" or
-  "irattach -d actisys_plus" in the/etc/irda/drivers script.
+  dongles you will have to start irattach like this: 
+  "irattach -d actisys" or "irattach -d actisys+".
@@ -11850 +11944 @@
-  to insert "irattach -d tekram" in the /etc/irda/drivers script.
+  to start irattach like this: "irattach -d tekram".
@@ -11868 +11962,13 @@
-  insert "irattach -d litelink" in the /etc/irda/drivers script.
+  start irattach like this "irattach -d litelink".
+
+Old Belking dongle
+CONFIG_OLD_BELKING_DONGLE
+  Say Y here if you want to build support for the old Belkin SmartBeam
+  dongle. If you want to compile it as a module, say M here and read
+  Documentation/modules.txt. The Belkin SmartBeam dongle (F5F500) come 
+  in two variants. The only way to distinguish those is to open the 
+  dongle and check the presence of a jumper (the jumper, on the new 
+  dongle, toggle between IrDA and ASK modes). This driver only support 
+  the old dongle. The old dongle is also limited to 9600 b/s (which is 
+  not very fun). To activate support for old Belkin dongles you will 
+  have to start irattach like this: "irattach -d old_dongle".
@@ -12042,0 +12149,27 @@
+CPiA Video For Linux
+CONFIG_VIDEO_CPIA
+  This is the video4linux driver for cameras based on Vision's CPiA
+  (Colour Processor Interface ASIC), such as the Creative Labs Video
+  Blaster Webcam II. If you have one of these cameras, say Y here
+  and select parallel port lowlevel support below (the USB-version,
+  is not supported on this kernel-version) otherwise say N. This will
+  not work with the Creative Webcam III. It is also available as a
+  module (cpia.o).
+
+  For more information (supported camera models, module autoloading, DMA
+  interrupt settings, supported applications, etc.) read
+  Documentation/video4linux/README.cpia.
+
+CPiA Parallel Port Lowlevel Support
+CONFIG_VIDEO_CPIA_PP
+  This is the lowlevel parallel port support for cameras based on
+  Vision's CPiA (Colour Processor Interface ASIC), such as the
+  Creative Webcam II. If you have the parallel port version of one
+  of these cameras, say Y here, otherwise say N. It is also available
+  as a module (cpia_pp.o).
+
+CPiA Parallel Port DMA Support
+CONFIG_VIDEO_CPIA_PP_DMA
+  This will use DMA if possible to reduce CPU usage.  If in doubt,
+  say Y here.
+   
@@ -12268 +12401 @@
-# LocalWords:  QNXFS ISI isicom xterms Apollos VPN RCPCI rcpci sgi visws pcmcia
+# LocalWords:  QNX4FS ISI isicom xterms Apollos VPN RCPCI rcpci sgi visws pcmcia
