--- Configure.help-2.0.35	Mon Oct  4 14:07:31 1999
+++ Configure.help-2.0.36	Mon Oct  4 14:07:31 1999
@@ -15 +15 @@
-# via ftp (user: anonymous) from sunsite.unc.edu in the directory
+# via FTP (user: anonymous) from sunsite.unc.edu in the directory
@@ -74 +74 @@
-  procedure is also explained in the SCSI-HOWTO, available via ftp
+  procedure is also explained in the SCSI-HOWTO, available via FTP
@@ -96 +96 @@
-  devices (such as harddrives) can do.  It is usually used to load and
+  devices (such as hard drives) can do. It is usually used to load and
@@ -98,7 +98,7 @@
-  during the initial install of Linux.  Note that the kernel command
-  line option "ramdisk=XX" is now obsolete.  For details, read
-  Documentation/ramdisk.txt. If you want to compile this as a module (
-  = code which can be inserted in and removed from the running kernel
-  whenever you want), say M and read Documentation/modules.txt.  Most
-  normal users won't need the RAM disk functionality, and can thus say
-  N here.
+  during the initial install of Linux. Note that the kernel command
+  line option "ramdisk=XX" is now obsolete. For details, read
+  Documentation/ramdisk.txt. If you want to compile this as a module
+  ( = code which can be inserted in and removed from the running
+  kernel whenever you want), say M and read Documentation/modules.txt.
+  Most normal users won't need the RAM disk functionality, and can
+  thus say N here.
@@ -131 +131 @@
-  (>540MB) IDE disks, soundcard IDE ports, and other topics, is all
+  (>540MB) IDE disks, sound card IDE ports, and other topics, is all
@@ -135 +135 @@
-  select the Old harddisk driver instead to save about 13kB of
+  select the Old hard disk driver instead to save about 13kB of
@@ -140 +140 @@
-Old harddisk (MFM/RLL/IDE) driver
+Old hard disk (MFM/RLL/IDE) driver
@@ -158 +158 @@
-  harddisk driver to control the primary IDE/disk interface in the
+  hard disk driver to control the primary IDE/disk interface in the
@@ -179 +179 @@
-  CDROM-HOWTO, available via ftp (user: anonymous) in
+  CDROM-HOWTO, available via FTP (user: anonymous) in
@@ -182 +182 @@
-  linux boot loader) cannot properly deal with IDE/ATAPI CDROMs, so
+  Linux boot loader) cannot properly deal with IDE/ATAPI CDROMs, so
@@ -262 +262 @@
-  enhanced support may be necessary for linux to be able to access the
+  enhanced support may be necessary for Linux to be able to access the
@@ -314 +314 @@
-XT harddisk support
+XT hard disk support
@@ -329,10 +329,10 @@
-  Read linux/Documentation/paride.txt for more information.  If you 
-  built PARIDE support into your kernel,  you may still build the 
-  individual protocol modules and high-level drivers as loadable 
-  modules. If you build this support as a module, it will be called 
-  paride.o.  To use the PARIDE support, you must say Y or M here 
-  and also to at least one high-level driver (e.g. "Parallel port 
-  IDE disks", "Parallel port ATAPI CD-ROMs", "Parallel port ATAPI 
-  disks" etc.) and to at least one protocol driver (e.g. "ATEN 
-  EH-100 protocol", "MicroSolutions backpack protocol", "DataStor 
-  Commuter protocol" etc.).
+  Read linux/Documentation/paride.txt for more information.
+  If you built PARIDE support into your kernel, you may still build
+  the individual protocol modules and high-level drivers as loadable
+  modules. If you build this support as a module, it will be called
+  paride.o. To use the PARIDE support, you must say Y or M here and
+  also to at least one high-level driver (e.g. "Parallel port IDE
+  disks", "Parallel port ATAPI CD-ROMs", "Parallel port ATAPI disks"
+  etc.) and to at least one protocol driver (e.g. "ATEN EH-100
+  protocol", "MicroSolutions backpack protocol", "DataStor Commuter
+  protocol" etc.).
@@ -341 +341 @@
-CONFIG_PARIDE_PD 
+CONFIG_PARIDE_PD
@@ -353 +353 @@
-CONFIG_PARIDE_PCD 
+CONFIG_PARIDE_PCD
@@ -367 +367 @@
-CONFIG_PARIDE_PF 
+CONFIG_PARIDE_PF
@@ -393,10 +393,10 @@
-  programs, such as cdrecord, to send ATAPI commands directly to a
-  device. If you chose to build PARIDE support into your kernel, you 
-  may answer Y here to build in the parallel port generic ATAPI driver, 
-  otherwise you should answer M to build it as a loadable module.
-  The module will be called pg.o.  You must also have at least one 
-  parallel port protocol driver in your system.  This driver 
-  implements an API loosely related to the generic SCSI driver.  
-  See /usr/include/linux/pg.h for details, or visit 
-  http://www.torque.net/parport/cdr.html for more information and
-  the required patches to cdrecord.
+  programs, such as cdrecord, to send ATAPI commands directly to
+  a device.  If you chose to build PARIDE support into your kernel,
+  you may answer Y here to build in the parallel port generic ATAPI
+  driver, otherwise you should answer M to build it as a loadable
+  module.  The module will be called pg.o.  You must also have at
+  least one parallel port protocol driver in your system.  This driver
+  implements an API loosely related to the generic SCSI driver.  See
+  /usr/include/linux/pg.h for details.  You can obtain the most recent
+  version of cdrecord from ftp://ftp.fokus.gmd.de/pub/unix/cdrecord/ .
+  Versions 1.6.1a3 and later fully support the pg driver.
@@ -408 +408 @@
-  parallel port kits made in Hong Kong. If you chose to build PARIDE 
+  parallel port kits made in Hong Kong.  If you chose to build PARIDE 
@@ -425,2 +425,2 @@
-CONFIG_PARIDE_COMM 
-  This option enables support for the Commuter parallel port IDE 
+CONFIG_PARIDE_COMM
+  This option enables support for the Commuter parallel port IDE
@@ -434,2 +434,2 @@
-CONFIG_PARIDE_DSTR 
-  This option enables support for the EP-2000 parallel port IDE 
+CONFIG_PARIDE_DSTR
+  This option enables support for the EP-2000 parallel port IDE
@@ -443,2 +443,2 @@
-CONFIG_PARIDE_EPAT 
-  This option enables support for the EPAT parallel port IDE 
+CONFIG_PARIDE_EPAT
+  This option enables support for the EPAT parallel port IDE
@@ -447,5 +447,5 @@
-  such as Hewlett-Packard, SyQuest, Imation and Avatar. If you 
-  chose to build PARIDE support into your kernel, you may answer Y 
-  here to build in the protocol driver, otherwise you should answer M 
-  to build it as a loadable module.  The module will be called epat.o.  
-  You must also have a high-level driver for the type of device that 
+  such as Hewlett-Packard, SyQuest, Imation and Avatar.  If you
+  chose to build PARIDE support into your kernel, you may answer Y
+  here to build in the protocol driver, otherwise you should answer M
+  to build it as a loadable module.  The module will be called epat.o.
+  You must also have a high-level driver for the type of device that
@@ -455,8 +455,8 @@
-CONFIG_PARIDE_EPIA 
-  This option enables support for the (obsolete) EPIA parallel port 
-  IDE protocol from Shuttle Technology.  This adapter can still be found
-  in some no-name kits. If you chose to build PARIDE support into your 
-  kernel, you may answer Y here to build in the protocol driver,
-  otherwise you should answer M to build it as a loadable module.  
-  The module will be called epia.o.  You must also have a high-level 
-  driver for the type of device that you want to support.
+CONFIG_PARIDE_EPIA
+  This option enables support for the (obsolete) EPIA parallel port
+  IDE protocol from Shuttle Technology.  This adapter can still be
+  found in some no-name kits.  If you chose to build PARIDE support
+  into your kernel, you may answer Y here to build in the protocol
+  driver, otherwise you should answer M to build it as a loadable
+  module.  The module will be called epia.o.  You must also have a
+  high-level driver for the type of device that you want to support.
@@ -466,8 +466,8 @@
-  This option enables support for the TD-2000 parallel port IDE protocol
-  from Fidelity International Technology.  This is a simple (low speed) 
-  adapter that is used in some portable hard drives.  If you chose to 
-  build PARIDE support into your kernel, you may answer Y here to 
-  build in the protocol driver, otherwise you should answer M to 
-  build it as a loadable module.  The module will be called fit2.o.
-  You must also have a high-level driver for the type of device 
-  that you want to support.
+  This option enables support for the TD-2000 parallel port IDE
+  protocol from Fidelity International Technology.  This is a simple
+  (low speed) adapter that is used in some portable hard drives.
+  If you chose to build PARIDE support into your kernel, you may
+  answer Y here to build in the protocol driver, otherwise you should
+  answer M to build it as a loadable module.  The module will be
+  called fit2.o.  You must also have a high-level driver for the type
+  of device that you want to support.
@@ -477,8 +477,8 @@
-  This option enables support for the TD-3000 parallel port IDE protocol
-  from Fidelity International Technology. This protocol is used in newer
-  models of their portable disk, CD-ROM and PD/CD devices.   If you chose
-  to build PARIDE support into your kernel, you may answer Y here to
-  build in the protocol driver, otherwise you should answer M to
-  build it as a loadable module.  The module will be called fit3.o.
-  You must also have a high-level driver for the type of device
-  that you want to support.
+  This option enables support for the TD-3000 parallel port IDE
+  protocol from Fidelity International Technology.  This protocol is
+  used in newer models of their portable disk, CD-ROM and PD/CD
+  devices.  If you chose to build PARIDE support into your kernel, you
+  may answer Y here to build in the protocol driver, otherwise you
+  should answer M to build it as a loadable module.  The module will
+  be called fit3.o.  You must also have a high-level driver for the
+  type of device that you want to support.
@@ -487,7 +487,7 @@
-CONFIG_PARIDE_FRPW 
-  This option enables support for the Freecom power parallel port IDE 
-  protocol.  If you chose to build PARIDE support into your kernel, you 
-  may answer Y here to build in the protocol driver, otherwise you 
-  should answer M to build it as a loadable module.  The module will be 
-  called frpw.o.  You must also have a high-level driver for the type 
-  of device that you want to support.
+CONFIG_PARIDE_FRPW
+  This option enables support for the Freecom power parallel port IDE
+  protocol.  If you chose to build PARIDE support into your kernel,
+  you may answer Y here to build in the protocol driver, otherwise you
+  should answer M to build it as a loadable module.  The module will
+  be called frpw.o.  You must also have a high-level driver for the
+  type of device that you want to support.
@@ -496,9 +496,9 @@
-CONFIG_PARIDE_KBIC 
-  This option enables support for the KBIC-951A and KBIC-971A parallel 
-  port IDE protocols from KingByte Information Corp.  KingByte's adapters
-  appear in many no-name portable disk and CD-ROM products, especially 
-  in Europe. If you chose to build PARIDE support into your kernel, you 
-  may answer Y here to build in the protocol driver, otherwise you should 
-  answer M to build it as a loadable module.  The module will be called 
-  kbic.o.  You must also have a high-level driver for the type of device 
-  that you want to support.
+CONFIG_PARIDE_KBIC
+  This option enables support for the KBIC-951A and KBIC-971A parallel
+  port IDE protocols from KingByte Information Corp.  KingByte's
+  adapters appear in many no-name portable disk and CD-ROM products,
+  especially in Europe.  If you chose to build PARIDE support into
+  your kernel, you may answer Y here to build in the protocol driver,
+  otherwise you should answer M to build it as a loadable module.
+  The module will be called kbic.o.  You must also have a high-level
+  driver for the type of device that you want to support.
@@ -510,4 +510,4 @@
-  used in some 2.5" portable hard drives.  If you chose to build PARIDE 
-  support into your kernel, you may answer Y here to build in the 
-  protocol driver, otherwise you should answer M to build it as a 
-  loadable module.  The module will be called ktti.o.  You must also 
+  used in some 2.5" portable hard drives.  If you chose to build
+  PARIDE support into your kernel, you may answer Y here to build in
+  the protocol driver, otherwise you should answer M to build it as a
+  loadable module.  The module will be called ktti.o.  You must also
@@ -518,2 +518,2 @@
-CONFIG_PARIDE_ON20 
-  This option enables support for the (obsolete) 90c20 parallel port 
+CONFIG_PARIDE_ON20
+  This option enables support for the (obsolete) 90c20 parallel port
@@ -521,4 +521,4 @@
-  name).  If you chose to build PARIDE support into your kernel, you 
-  may answer Y here to build in the protocol driver, otherwise you 
-  should answer M to build it as a loadable module.  The module will 
-  be called on20.o.  You must also have a high-level driver for the 
+  name).  If you chose to build PARIDE support into your kernel, you
+  may answer Y here to build in the protocol driver, otherwise you
+  should answer M to build it as a loadable module.  The module will
+  be called on20.o.  You must also have a high-level driver for the
@@ -528,2 +528,2 @@
-CONFIG_PARIDE_ON26 
-  This option enables support for the 90c26 parallel port IDE protocol 
+CONFIG_PARIDE_ON26
+  This option enables support for the 90c26 parallel port IDE protocol
@@ -531,4 +531,4 @@
-  name).  If you chose to build PARIDE support into your kernel, you 
-  may answer Y here to build in the protocol driver, otherwise you 
-  should answer M to build it as a loadable module.  The module will 
-  be called on26.o.  You must also have a high-level driver for the 
+  name).  If you chose to build PARIDE support into your kernel, you
+  may answer Y here to build in the protocol driver, otherwise you
+  should answer M to build it as a loadable module.  The module will
+  be called on26.o.  You must also have a high-level driver for the
@@ -539 +539 @@
-  This driver lets you combine several harddisk partitions into one
+  This driver lets you combine several hard disk partitions into one
@@ -541 +541 @@
-  the necessary tools are available over ftp (user: anonymous) from
+  the necessary tools are available over FTP (user: anonymous) from
@@ -549 +549 @@
-  to use the so-called linear mode, i.e. it will combine the harddisk
+  to use the so-called linear mode, i.e. it will combine the hard disk
@@ -558 +558 @@
-  to use the so-called raid0 mode, i.e. it will combine the harddisk
+  to use the so-called raid0 mode, i.e. it will combine the hard disk
@@ -707,2 +707,2 @@
-  If you are SYN flooded, the source address reported by the kernel is 
-  likely to have been forged by the attacker.  The source address is 
+  If you are SYN flooded, the source address reported by the kernel is
+  likely to have been forged by the attacker.  The source address is
@@ -713 +713 @@
-  This is support for floppy drives on Sun Sparc workstations. Say Y
+  This is support for floppy drives on Sun SPARC workstations. Say Y
@@ -719 +719 @@
-  want to read the Linux/Alpha homepage on the WWW at
+  want to read the Linux/Alpha home page on the WWW at
@@ -763 +763 @@
-  via ftp (user: anonymous) in sunsite.unc.edu:/pub/Linux/docs/HOWTO.
+  via FTP (user: anonymous) in sunsite.unc.edu:/pub/Linux/docs/HOWTO.
@@ -818 +818 @@
-  this option). The PCI-HOWTO, available via ftp (user: anonymous) in
+  this option). The PCI-HOWTO, available via FTP (user: anonymous) in
@@ -833 +833 @@
-  If your PCI system uses an IDE harddrive (as opposed to SCSI, say)
+  If your PCI system uses an IDE hard drive (as opposed to SCSI, say)
@@ -844 +844 @@
-  system calls which let processes (= running programs) synchronize
+  system calls which let processes ( = running programs) synchronize
@@ -848 +848 @@
-  (read the DOSEMU-HOWTO, available via ftp (user: anonymous) in
+  (read the DOSEMU-HOWTO, available via FTP (user: anonymous) in
@@ -881 +881 @@
-Compile kernel as ELF - if your GCC is ELF-GCC
+Compile kernel as ELF -- if your GCC is ELF-GCC
@@ -922,2 +922,2 @@
-  even execute HTML files containing JAVA applets (= JAVA binaries) if
-  those files start with the string "<!--applet-->". If you want to
+  even execute HTML files containing JAVA applets ( = JAVA binaries)
+  if those files start with the string "<!--applet-->". If you want to
@@ -925 +925 @@
-  available via ftp (user: anonymous) at
+  available via FTP (user: anonymous) at
@@ -938,10 +938,22 @@
-  This is the processor type of your CPU. It is used for optimizing
-  purposes. In order to compile a kernel that can run on all CPU types
-  (albeit not optimally fast), you can specify "386" here.  If you
-  specify "486" or "Pentium" or "PPro", then the kernel will run on
-  486 and Pentium (=586) and Pentium Pro (=686) CPUs. In rare cases,
-  it can make sense to specify "Pentium" even if running a 486: the
-  kernel will be smaller but slower. On the other hand, if you use a
-  compiler before gcc 2.7 (say "gcc -v" to find out), then you have to
-  say "386" or "486" here even if running on a Pentium or PPro
-  machine. If you don't know what to do, say "386".
+  This is the processor type of your CPU.  It is used for optimizing
+  purposes.  In order to compile a kernel that can run on all CPU
+  types (albeit not optimally fast), you can specify "386" here.  If
+  you specify "486" or "Pentium" or "PPro", then the kernel will run
+  on all of these CPUs: 486 and Pentium (=586) and Pentium Pro (=686).
+  Here are the settings recommended for greatest speed:
+   - "386" for the AMD/Cyrix/Intel 386DX/DXL/SL/SLC/SX and
+     Cyrix/TI 486DLC/DLC2. Only "386" kernels will run on a 386 class
+     machine.
+   - "486" for the AMD/Cyrix/IBM/Intel DX4 or 486DX/DX2/SL/SX/SX2,
+     AMD/Cyrix 5x86, NexGen Nx586 and UMC U5D or U5S
+   - "Pentium" for the AMD K5, K6 and K6-3D, Cyrix MediaGX,
+     Cyrix/IBM/National Semiconductor 6x86 and GXm, IDT Centaur
+     WinChip C6, and Intel Pentium/Pentium MMX
+   - "PPro" for the Cyrix/IBM/National Semiconductor 6x86MX, MII and
+     Intel Pentium II/Pentium Pro
+  In rare cases, it can make sense to specify "Pentium" even if
+  running a 486: the kernel will be smaller but slightly slower.  On
+  the other hand, if you use a compiler before gcc 2.7 (say "gcc -v"
+  to find out), then you have to say "386" or "486" here even if
+  running on a Pentium or PPro machine.
+  If you don't know what to do, say "386".
@@ -959,2 +971,2 @@
-  If you have a linuxelf-gcc as opposed to linux-gcc, say Y, otherwise
-  N.
+  If you have a linuxelf-gcc as opposed to linux-gcc, say Y,
+  otherwise N.
@@ -1007 +1019 @@
-  available via ftp (user: anonymous) from
+  available via FTP (user: anonymous) from
@@ -1039 +1051 @@
-  computer. Read the Term-HOWTO, available via ftp (user: anonymous)
+  computer. Read the Term-HOWTO, available via FTP (user: anonymous)
@@ -1048 +1060 @@
-  about 5 kB). Note that in this case, you possibly have two ethernet
+  about 5 kB). Note that in this case, you possibly have two Ethernet
@@ -1052 +1064 @@
-  Multiple-Ethernet-mini-HOWTO, available via ftp (user: anonymous) in
+  Multiple-Ethernet-mini-HOWTO, available via FTP (user: anonymous) in
@@ -1056 +1068 @@
-  local network from the internet. The Firewall-HOWTO tells you how to
+  local network from the Internet. The Firewall-HOWTO tells you how to
@@ -1072 +1084 @@
-  used on the MBONE (a high bandwidth network on top of the internet
+  used on the MBONE (a high bandwidth network on top of the Internet
@@ -1084 +1096 @@
-  of the internet which carries audio and video broadcasts. More
+  of the Internet which carries audio and video broadcasts. More
@@ -1105 +1117 @@
-  ftp (user: anonymous) in sunsite.unc.edu:/pub/Linux/docs/HOWTO.
+  FTP (user: anonymous) in sunsite.unc.edu:/pub/Linux/docs/HOWTO.
@@ -1177 +1189 @@
-  have the computers on the local network participate on the internet
+  have the computers on the local network participate on the Internet
@@ -1208,6 +1220,6 @@
-  This option means that all incoming fragments (= parts of IP packets
-  that arose when some host between origin and destination decided
-  that the IP packets were too large and cut them in pieces) will be
-  reassembled (defragmented) before being processed, even if they are
-  about to be forwarded.  This option is highly recommended if you
-  have enabled the masquerading support (CONFIG_IP_MASQUERADE),
+  This option means that all incoming fragments ( = parts of IP
+  packets that arose when some host between origin and destination
+  decided that the IP packets were too large and cut them in pieces)
+  will be reassembled (defragmented) before being processed, even if
+  they are about to be forwarded.  This option is highly recommended
+  if you have enabled the masquerading support (CONFIG_IP_MASQUERADE),
@@ -1229,4 +1241,4 @@
-  interface (= serial port or ethernet card).  The most common case is
-  that you want to serve different WWW documents to the outside
-  according to which of your host names they used to connect to
-  you.  This is explained in detail on the WWW at
+  interface ( = serial port or Ethernet card).  The most common case
+  is that you want to serve different WWW documents to the outside
+  according to which of your host names they used to connect to you.
+  This is explained in detail on the WWW at
@@ -1236,2 +1248,2 @@
-  there are two logical networks living on your local ethernet and you
-  want to access them both with the same ethernet card.  The
+  there are two logical networks living on your local Ethernet and you
+  want to access them both with the same Ethernet card.  The
@@ -1246 +1258 @@
-  MBONE, a high bandwidth network on top of the internet which carries
+  MBONE, a high bandwidth network on top of the Internet which carries
@@ -1255,4 +1267,4 @@
-  If you have been having difficulties telnetting to your Linux machine
-  from a DOS system that uses (broken) PC/TCP networking software (all
-  versions up to OnNet 2.0) over your local ethernet try enabling this
-  option.  Everyone else says N.
+  If you have been having difficulties telnetting to your Linux
+  machine from a DOS system that uses (broken) PC/TCP networking
+  software (all versions up to OnNet 2.0) over your local Ethernet try
+  enabling this option.  Everyone else says N.
@@ -1265 +1277 @@
-  machines on your local network that know their hardware ethernet
+  machines on your local network that know their hardware Ethernet
@@ -1307 +1319 @@
-  sending small IP frames (= packets).  This keeps tiny telnet and
+  sending small IP frames ( = packets).  This keeps tiny telnet and
@@ -1315,11 +1327,11 @@
-  Usually, the originator of an IP frame (= packet) specifies only the
-  destination, and the hosts along the way do the routing, i.e. they
-  decide how to forward the frame.  However, there is a feature of the
-  IP protocol that allows to specify the full route for a given frame
-  already at its origin. A frame with such a fully specified route is
-  called "source routed".  The question now is whether we should
-  honour these route requests when such frames arrive, or if we should
-  drop all those frames instead.  Honouring them can introduce
-  security problems (and is rarely a useful feature), and hence it is
-  recommended that you say Y here unless you really know what you're
-  doing.
+  Usually, the originator of an IP frame ( = packet) specifies only
+  the destination, and the hosts along the way do the routing, i.e.
+  they decide how to forward the frame.  However, there is a feature
+  of the IP protocol that allows to specify the full route for a given
+  frame already at its origin. A frame with such a fully specified
+  route is called "source routed".  The question now is whether we
+  should honour these route requests when such frames arrive, or if
+  we should drop all those frames instead.  Honouring them can
+  introduce security problems (and is rarely a useful feature), and
+  hence it is recommended that you say Y here unless you really know
+  what you're doing.
@@ -1327 +1339 @@
-IP: Allow large windows (not recommend if <16Mb of memory)
+IP: Allow large windows (not recommend if <16MB of memory)
@@ -1335 +1347 @@
-  thus this option is best only used on machines with 16Mb of
+  thus this option is best only used on machines with 16MB of
@@ -1345,2 +1357,2 @@
-  to access Novell Netware file or print servers using the Linux
-  Novell client ncpfs (available via ftp (user: anonymous) from
+  to access Novell NetWare file or print servers using the Linux
+  Novell client ncpfs (available via FTP (user: anonymous) from
@@ -1351 +1363 @@
-  turn your Linux box into a fully featured Netware file server and
+  turn your Linux box into a fully featured NetWare file server and
@@ -1379 +1391 @@
-Appletalk DDP
+AppleTalk DDP
@@ -1381,4 +1393,4 @@
-  Appletalk is the way Apple computers speak to each other on a
-  network.  EtherTalk is the name used for appletalk over ethernet
-  and Localtalk is appletalk over the apple serial links.  If your
-  linux box is connected to such a network and you want to join the
+  AppleTalk is the way Apple computers speak to each other on a
+  network.  EtherTalk is the name used for AppleTalk over Ethernet
+  and LocalTalk is AppleTalk over the Apple serial links.  If your
+  Linux box is connected to such a network and you want to join the
@@ -1387 +1399 @@
-  macs as well as access appletalk printers.  Check out
+  macs as well as access AppleTalk printers.  Check out
@@ -1391 +1403 @@
-  netscape or Mosaic).  The NET-2-HOWTO, available via ftp (user:
+  netscape or Mosaic).  The NET-2-HOWTO, available via FTP (user:
@@ -1394,5 +1406,5 @@
-  module (= code which can be inserted in and removed from the running
-  kernel whenever you want).  If you want to compile it as a module,
-  say M here and read Documentation/modules.txt.  I hear that the GNU
-  boycott of Apple is over, so even politically correct people are
-  allowed to say Y here.  At the time the kernel is released the
+  module ( = code which can be inserted in and removed from the
+  running kernel whenever you want).  If you want to compile it as a
+  module, say M here and read Documentation/modules.txt.  I hear that
+  the GNU boycott of Apple is over, so even politically correct people
+  are allowed to say Y here.  At the time the kernel is released the
@@ -1401 +1413 @@
-  will need to do is download and install the localtalk driver.  
+  will need to do is download and install the localtalk driver.
@@ -1407 +1419 @@
-  carry other protocols such as tcp/ip. To use it, you need a device
+  carry other protocols such as TCP/IP. To use it, you need a device
@@ -1418 +1430 @@
-  AX.25 port is contained in the HAM-HOWTO, available via ftp (user:
+  AX.25 port is contained in the HAM-HOWTO, available via FTP (user:
@@ -1432 +1444 @@
-  AX.25 port is contained in the HAM-HOWTO, available via ftp (user:
+  AX.25 port is contained in the HAM-HOWTO, available via FTP (user:
@@ -1445 +1457 @@
-  traffic over ethernet (also called "BPQ AX.25"), which could be
+  traffic over Ethernet (also called "BPQ AX.25"), which could be
@@ -1452,2 +1464,2 @@
-  ethernet bridge, which means that the different ethernet segments it
-  is connected to will appear as one ethernet to the participants.
+  Ethernet bridge, which means that the different Ethernet segments it
+  is connected to will appear as one Ethernet to the participants.
@@ -1455 +1467 @@
-  networks of ethernets using the IEEE802.1 spanning tree algorithm.
+  networks of Ethernets using the IEEE802.1 spanning tree algorithm.
@@ -1458 +1470 @@
-  the bridge configuration tools available via ftp (user: anonymous)
+  the bridge configuration tools available via FTP (user: anonymous)
@@ -1460 +1472 @@
-  probably contains several ethernet devices, but the kernel is not
+  probably contains several Ethernet devices, but the kernel is not
@@ -1462 +1474 @@
-  details read the Multiple-Ethernet-mini-HOWTO, available via ftp
+  details read the Multiple-Ethernet-mini-HOWTO, available via FTP
@@ -1489 +1501 @@
-  If you want to use a SCSI harddisk, SCSI tapedrive, SCSI CDROM or
+  If you want to use a SCSI hard disk, SCSI tapedrive, SCSI CDROM or
@@ -1495 +1507 @@
-  SCSI-HOWTO, available via ftp (user: anonymous) in sunsite.unc.edu:
+  SCSI-HOWTO, available via FTP (user: anonymous) in sunsite.unc.edu:
@@ -1497,3 +1509,4 @@
-  (= code which can be inserted in and removed from the running kernel
-  whenever you want).  If you want to compile it as a module, say M
-  here and read Documentation/modules.txt and Documentation/scsi.txt.
+  ( = code which can be inserted in and removed from the running
+  kernel whenever you want).  If you want to compile it as a module,
+  say M here and read Documentation/modules.txt and
+  Documentation/scsi.txt.
@@ -1503,4 +1516,4 @@
-  If you want to use a SCSI harddisk or the SCSI or parallel port
-  version of the IOMEGA ZIP drive under Linux, say Y and read
-  the SCSI-HOWTO, available via ftp (user: anonymous) in
-  sunsite.unc.edu:/pub/Linux/docs/HOWTO. This is NOT for SCSI CDROMs.
+  If you want to use a SCSI hard disk or the SCSI or parallel port
+  version of the IOMEGA ZIP drive under Linux, say Y and read the
+  SCSI-HOWTO, available via FTP (user: anonymous) in sunsite.unc.edu:
+  /pub/Linux/docs/HOWTO. This is NOT for SCSI CDROMs.
@@ -1515,7 +1528,7 @@
-  SCSI-HOWTO, available via ftp (user: anonymous) in
-  sunsite.unc.edu:/pub/Linux/docs/HOWTO and drivers/scsi/README.st in
-  the kernel source. This is NOT for SCSI CDROMs. This driver is also
-  available as a module ( = code which can be inserted in and removed
-  from the running kernel whenever you want). If you want to compile
-  it as a module, say M here and read Documentation/modules.txt and
-  Documentation/scsi.txt .
+  SCSI-HOWTO, available via FTP (user: anonymous) in sunsite.unc.edu:
+  /pub/Linux/docs/HOWTO and drivers/scsi/README.st in the kernel
+  source. This is NOT for SCSI CDROMs. This driver is also available
+  as a module ( = code which can be inserted in and removed from the
+  running kernel whenever you want). If you want to compile it as a
+  module, say M here and read Documentation/modules.txt and
+  Documentation/scsi.txt.
@@ -1536 +1549 @@
-  about anything having "SCSI" in its name other than harddisks,
+  about anything having "SCSI" in its name other than hard disks,
@@ -1540 +1553 @@
-  would need the program cdwrite, available via ftp (user: anonymous)
+  would need the program cdwrite, available via FTP (user: anonymous)
@@ -1544 +1557 @@
-  SCSI-Programming-HOWTO, both available via ftp (user: anonymous) in
+  SCSI-Programming-HOWTO, both available via FTP (user: anonymous) in
@@ -1570,4 +1583,4 @@
-  drivers/scsi/advansys.c. This driver is also available as a module (
-  = code which can be inserted in and removed from the running kernel
-  whenever you want). If you want to compile it as a module, say M
-  here and read Documentation/modules.txt.
+  drivers/scsi/advansys.c. This driver is also available as a module
+  ( = code which can be inserted in and removed from the running
+  kernel whenever you want). If you want to compile it as a module,
+  say M here and read Documentation/modules.txt.
@@ -1579,7 +1592,6 @@
-  SCSI-HOWTO, available via ftp (user: anonymous) at
-  sunsite.unc.edu:/pub/Linux/docs/HOWTO. You might also want to read
-  the comments at the top of drivers/scsi/aha152x.c. This driver is
-  also available as a module ( = code which can be inserted in and
-  removed from the running kernel whenever you want). If you want to
-  compile it as a module, say M here and read
-  Documentation/modules.txt.
+  SCSI-HOWTO, available via FTP (user: anonymous) at sunsite.unc.edu:
+  /pub/Linux/docs/HOWTO. You might also want to read the comments at
+  the top of drivers/scsi/aha152x.c. This driver is also available as
+  a module ( = code which can be inserted in and removed from the
+  running kernel whenever you want). If you want to compile it as a
+  module, say M here and read Documentation/modules.txt.
@@ -1590 +1602 @@
-  3.4 of the SCSI-HOWTO, available via ftp (user: anonymous) at
+  3.4 of the SCSI-HOWTO, available via FTP (user: anonymous) at
@@ -1602 +1614 @@
-  section 3.5 of the SCSI-HOWTO, available via ftp (user: anonymous)
+  section 3.5 of the SCSI-HOWTO, available via FTP (user: anonymous)
@@ -1670 +1682 @@
-  interactions between the aic7xxx driver and the rest of the linux
+  interactions between the aic7xxx driver and the rest of the Linux
@@ -1677 +1689 @@
-  Adapters.  Consult the SCSI-HOWTO, available via anonymous ftp from
+  Adapters.  Consult the SCSI-HOWTO, available via anonymous FTP from
@@ -1697 +1709 @@
-  the SCSI-HOWTO, available via ftp (user: anonymous) at
+  the SCSI-HOWTO, available via FTP (user: anonymous) at
@@ -1700,3 +1712,3 @@
-  module (= code which can be inserted in and removed from the running
-  kernel whenever you want). If you want to compile it as a module,
-  say M here and read Documentation/modules.txt.
+  module ( = code which can be inserted in and removed from the
+  running kernel whenever you want). If you want to compile it as a
+  module, say M here and read Documentation/modules.txt.
@@ -1709 +1721 @@
-  SCSI-HOWTO, available via ftp (user: anonymous) at
+  SCSI-HOWTO, available via FTP (user: anonymous) at
@@ -1711 +1723 @@
-  available as a module (= code which can be inserted in and removed
+  available as a module ( = code which can be inserted in and removed
@@ -1720 +1732 @@
-  doing so, since this driver only supports harddisks and lacks
+  doing so, since this driver only supports hard disks and lacks
@@ -1722 +1734 @@
-  available via ftp (user: anonymous) at
+  available via FTP (user: anonymous) at
@@ -1734 +1746 @@
-  Read the SCSI-HOWTO, available via ftp (user: anonymous) at
+  Read the SCSI-HOWTO, available via FTP (user: anonymous) at
@@ -1749 +1761 @@
-  It is explained in section 3.7 of the SCSI-HOWTO, available via ftp
+  It is explained in section 3.7 of the SCSI-HOWTO, available via FTP
@@ -1760 +1772 @@
-  section 3.8 of the SCSI-HOWTO, available via ftp (user: anonymous)
+  section 3.8 of the SCSI-HOWTO, available via FTP (user: anonymous)
@@ -1770 +1782 @@
-  This enables certain optimizations for the NCR53c400 scsi cards. You
+  This enables certain optimizations for the NCR53c400 SCSI cards. You
@@ -1788 +1800 @@
-  3.8 of the SCSI-HOWTO, available via ftp (user: anonymous) at
+  3.8 of the SCSI-HOWTO, available via FTP (user: anonymous) at
@@ -1791,4 +1803,4 @@
-  drivers/scsi/53c7,8xx.h. This driver is also available as a module (
-  = code which can be inserted in and removed from the running kernel
-  whenever you want). If you want to compile it as a module, say M
-  here and read Documentation/modules.txt.
+  drivers/scsi/53c7,8xx.h. This driver is also available as a module
+  ( = code which can be inserted in and removed from the running
+  kernel whenever you want). If you want to compile it as a module,
+  say M here and read Documentation/modules.txt.
@@ -1822 +1834 @@
-  This is the BSD ncr driver adapted to linux for the NCR53C8XX family
+  This is the BSD ncr driver adapted to Linux for the NCR53C8XX family
@@ -1824,2 +1836,2 @@
-  tagged command queuing, fast scsi II transfer up to 10 MB/s with
-  narrow scsi devices and 20 MB/s with wide scsi devices.
+  tagged command queuing, fast SCSI II transfer up to 10 MB/s with
+  narrow SCSI devices and 20 MB/s with wide SCSI devices.
@@ -1833 +1845 @@
-  SCSI-2 specifications allow scsi devices to negotiate a synchronous
+  SCSI-2 specifications allow SCSI devices to negotiate a synchronous
@@ -1837 +1849 @@
-  MB/second throughput with 8 bits scsi-2 devices and 20 MB/second
+  MB/second throughput with 8 bits SCSI-2 devices and 20 MB/second
@@ -1845 +1857 @@
-  However, a flawless singled-ended scsi bus supports 10 MHz data
+  However, a flawless singled-ended SCSI bus supports 10 MHz data
@@ -1864 +1876 @@
-  This option is only provided for safety if you suspect some scsi
+  This option is only provided for safety if you suspect some SCSI
@@ -1868 +1880 @@
-  than 1 device on a scsi bus.  The normal answer therefore is N.
+  than 1 device on a SCSI bus.  The normal answer therefore is N.
@@ -1873 +1885 @@
-  linux start-up.  Some scsi devices do not properly support this
+  Linux start-up.  Some SCSI devices do not properly support this
@@ -1926 +1938 @@
-  53C8XX based scsi board with a vendor-specific BIOS (example: Tekram
+  53C8XX based SCSI board with a vendor-specific BIOS (example: Tekram
@@ -1945 +1957 @@
-  3.10 of the SCSI-HOWTO, available via ftp (user: anonymous) at
+  3.10 of the SCSI-HOWTO, available via FTP (user: anonymous) at
@@ -1957 +1969 @@
-  the SCSI-HOWTO, available via ftp (user: anonymous) at
+  the SCSI-HOWTO, available via FTP (user: anonymous) at
@@ -1970 +1982 @@
-  You should also read the SCSI-HOWTO, available via ftp (user:
+  You should also read the SCSI-HOWTO, available via FTP (user:
@@ -1981 +1993 @@
-  available via ftp (user: anonymous) at sunsite.unc.edu:
+  available via FTP (user: anonymous) at sunsite.unc.edu:
@@ -1992 +2004 @@
-  3.11 of the SCSI-HOWTO, available via ftp (user: anonymous) at
+  3.11 of the SCSI-HOWTO, available via FTP (user: anonymous) at
@@ -2002,6 +2014,6 @@
-  SCSI-HOWTO, available via ftp (user: anonymous) at
-  sunsite.unc.edu:/pub/Linux/docs/HOWTO.  If it doesn't work out of
-  the box, you may have to change some settings in
-  drivers/scsi/ultrastor.h.  If you want to compile this as a module
-  (= code which can be inserted in and removed from the running kernel
-  whenever you want), say M here and read Documentation/modules.txt.
+  SCSI-HOWTO, available via FTP (user: anonymous) at sunsite.unc.edu:
+  /pub/Linux/docs/HOWTO.  If it doesn't work out of the box, you may
+  have to change some settings in drivers/scsi/ultrastor.h.  If you
+  want to compile this as a module ( = code which can be inserted in
+  and removed from the running kernel whenever you want), say M here
+  and read Documentation/modules.txt.
@@ -2030 +2042 @@
-  SCSI-HOWTO, available via ftp (user: anonymous) at
+  SCSI-HOWTO, available via FTP (user: anonymous) at
@@ -2040 +2052 @@
-  kernel source.  Also read the SCSI-HOWTO, available via ftp (user:
+  kernel source.  Also read the SCSI-HOWTO, available via FTP (user:
@@ -2057 +2069 @@
-  available via ftp (user: anonymous) at
+  available via FTP (user: anonymous) at
@@ -2069 +2081 @@
-  it as a module, say M here and read Documentation/modules.txt. 
+  it as a module, say M here and read Documentation/modules.txt.
@@ -2077 +2089 @@
-  is available via anonymous ftp from sunsite.unc.edu in the directory
+  is available via anonymous FTP from sunsite.unc.edu in the directory
@@ -2088 +2100 @@
-IOMEGA ZIP drive - Buggy EPP chipset support
+IOMEGA ZIP drive -- Buggy EPP chipset support
@@ -2102 +2114 @@
-  telephone lines; read the UUCP-HOWTO, available via ftp (user:
+  telephone lines; read the UUCP-HOWTO, available via FTP (user:
@@ -2108 +2120 @@
-  network card that you want to use under linux (make sure you know
+  network card that you want to use under Linux (make sure you know
@@ -2111 +2123 @@
-  under linux, read the Multiple-Ethernet-mini-HOWTO, available from
+  under Linux, read the Multiple-Ethernet-mini-HOWTO, available from
@@ -2127,2 +2139,2 @@
-  100-base-<whatever> are common types of ethernet. If your Linux
-  machine will be connected to an Ethernet and you have an ethernet
+  100-base-<whatever> are common types of Ethernet. If your Linux
+  machine will be connected to an Ethernet and you have an Ethernet
@@ -2130 +2142 @@
-  Ethernet-HOWTO, available via ftp (user: anonymous) from
+  Ethernet-HOWTO, available via FTP (user: anonymous) from
@@ -2143 +2155 @@
-  in the Network Administrator's Guide, available via ftp (user:
+  in the Network Administrator's Guide, available via FTP (user:
@@ -2163 +2175 @@
-  around (available via ftp (user: anonymous) from sunsite.unc.edu:
+  around (available via FTP (user: anonymous) from sunsite.unc.edu:
@@ -2166 +2178 @@
-  sure to say Y to CSLIP, below.  The NET-2-HOWTO, available via ftp
+  sure to say Y to CSLIP, below.  The NET-2-HOWTO, available via FTP
@@ -2182,3 +2194,3 @@
-  on both ends. Ask your access provider if you are not sure and say
-  Y, just in case.  You will still be able to use plain SLIP.  If you
-  plan to use SLiRP, the SLIP emulator (available via ftp (user:
+  on both ends.  Ask your access provider if you are not sure and
+  say Y, just in case.  You will still be able to use plain SLIP.  If
+  you plan to use SLiRP, the SLIP emulator (available via FTP (user:
@@ -2187,2 +2199,2 @@
-  connection, you definitely want to say Y here.  The NET-2-HOWTO,
-  available via ftp (user: anonymous) in
+  connection, you definitely want to say Y here.
+  The NET-2-HOWTO, available via FTP (user: anonymous) in
@@ -2211 +2223 @@
-  (AX.25), support for wireless ethernet and other systems.  Note that
+  (AX.25), support for wireless Ethernet and other systems.  Note that
@@ -2216 +2228 @@
-  ftp (user: anonymous) from shadow.cabi.net.  If unsure, say N.
+  FTP (user: anonymous) from shadow.cabi.net.  If unsure, say N.
@@ -2225 +2237 @@
-  up shell account on some UNIX computer; get it via ftp (user:
+  up shell account on some UNIX computer; get it via FTP (user:
@@ -2251 +2263 @@
-  linux box to act as a dial-in PPP server.  Most people can say N.
+  Linux box to act as a dial-in PPP server.  Most people can say N.
@@ -2281 +2293 @@
-  available via ftp (user: anonymous) at
+  available via FTP (user: anonymous) at
@@ -2292,3 +2304,3 @@
-  configure the driver, use the sethdlc utility available
-  in the standard ax25 utilities package. For information on the modems,
-  see http://www.baycom.de and drivers/net/README.baycom.
+  configure the driver, use the sethdlc utility available in the
+  standard ax25 utilities package. For information on the modems, see
+  http://www.baycom.de and drivers/net/README.baycom.
@@ -2302,4 +2314,3 @@
-  WindowsSoundSystem compatible sound card to be used as a packet radio
-  modem (NOT as a telephone modem!), to send digital traffic over
-  amateur radio. 
-
+  WindowsSoundSystem compatible sound card to be used as a packet
+  radio modem (NOT as a telephone modem!), to send digital traffic
+  over amateur radio.
@@ -2312,2 +2323 @@
-  Documentation/networking/soundmodem.txt. 
-
+  Documentation/networking/soundmodem.txt.
@@ -2325,2 +2335,2 @@
-  this usually results in better performance. This option also supports
-  SB16/32/64 in full duplex mode.
+  this usually results in better performance. This option also
+  supports SB16/32/64 in full duplex mode.
@@ -2340,3 +2350,4 @@
-  This option enables the soundmodem driver 1200 baud AFSK modem, 
-  compatible to popular modems using TCM3105 or AM7911. The demodulator
-  requires about 12% of the CPU power of a Pentium 75 CPU per channel.
+  This option enables the soundmodem driver 1200 baud AFSK modem,
+  compatible to popular modems using TCM3105 or AM7911.
+  The demodulator requires about 12% of the CPU power of a Pentium 75
+  CPU per channel.
@@ -2348 +2359 @@
-  crystal.  Note that the availability of this driver does _not_ imply
+  crystal. Note that the availability of this driver does _not_ imply
@@ -2359,2 +2370,2 @@
-  Note that the availability of this driver does _not_ imply that I
-  recommend building such links. It is only here since users
+  Note that the availability of this driver does _not_ imply that
+  I recommend building such links. It is only here since users
@@ -2408 +2419 @@
-  read the PLIP mini-HOWTO, available via ftp (user: anonymous) in
+  read the PLIP mini-HOWTO, available via FTP (user: anonymous) in
@@ -2413,18 +2424,20 @@
-  your kernel by about 8kB. If you want to compile this as a module (
-  = code which can be inserted in and removed from the running kernel
-  whenever you want), say M here and read Documentation/modules.txt as
-  well as Documentation/networking/net-modules.txt. If you want to use
-  both a parallel printer and PLIP, there are two cases: 1) If the
-  printer and the PLIP cable are to use the same parallel port
-  (presumably because you have just one), it is best to compile both
-  drivers as modules and load and unload them as needed. 2) To use
-  different parallel ports for the printer and the PLIP cable, you can
-  say Y to the printer driver, specify the base address of the
-  parallel port(s) to use for the printer(s) with the "lp" kernel
-  command line option. (See the documentation of your boot loader
-  (lilo or loadlin) about how to pass options to the kernel at boot
-  time. The lilo procedure is also explained in the SCSI-HOWTO,
-  available via ftp (user: anonymous) in
-  sunsite.unc.edu:/pub/Linux/docs/HOWTO.) The standard base addresses
-  as well as the syntax of the "lp" command line option can be found
-  in drivers/char/lp.c. You can then say Y to this PLIP driver or,
+  your kernel by about 8kB.
+  If you want to compile this as a module ( = code which can be
+  inserted in and removed from the running kernel whenever you want),
+  say M here and read Documentation/modules.txt as well as
+  Documentation/networking/net-modules.txt.
+  If you want to use both a parallel printer and PLIP, there are two
+  cases:
+  1) If the printer and the PLIP cable are to use the same parallel
+  port (presumably because you have just one), it is best to compile
+  both drivers as modules and load and unload them as needed.
+  2) To use different parallel ports for the printer and the PLIP
+  cable, you can say Y to the printer driver, specify the base address
+  of the parallel port(s) to use for the printer(s) with the "lp"
+  kernel command line option. (See the documentation of your boot
+  loader (lilo or loadlin) about how to pass options to the kernel at
+  boot time. The lilo procedure is also explained in the SCSI-HOWTO,
+  available via FTP (user: anonymous) in sunsite.unc.edu:
+  /pub/Linux/docs/HOWTO.) The standard base addresses as well as the
+  syntax of the "lp" command line option can be found in
+  drivers/char/lp.c. You can then say Y to this PLIP driver or,
@@ -2440,2 +2453,2 @@
-  SLIP (= the protocol for sending internet traffic over telephone
-  lines) or PPP (= a better SLIP) on them, you can make them behave
+  SLIP ( = the protocol for sending internet traffic over telephone
+  lines) or PPP ( = a better SLIP) on them, you can make them behave
@@ -2453 +2466 @@
-  low-cost way to connect to a remote internet access provider or to
+  low-cost way to connect to a remote Internet access provider or to
@@ -2494,2 +2507,2 @@
-  This is support for lance ethernet cards on Sun workstations such as
-  the Sparcstation IPC (any Sparc with a network interface 'le0' under
+  This is support for lance Ethernet cards on Sun workstations such as
+  the SPARCstation IPC (any SPARC with a network interface 'le0' under
@@ -2500 +2513 @@
-  This is support for the intel ethernet cards on some Sun
+  This is support for the Intel Ethernet cards on some Sun
@@ -2505,2 +2518,2 @@
-  If you have a network (ethernet) card belonging to this class, say Y
-  and read the Ethernet-HOWTO, available via ftp (user: anonymous) in
+  If you have a network (Ethernet) card belonging to this class, say Y
+  and read the Ethernet-HOWTO, available via FTP (user: anonymous) in
@@ -2508 +2521 @@
-  one network card under linux, read the Multiple-Ethernet-mini-HOWTO,
+  one network card under Linux, read the Multiple-Ethernet-mini-HOWTO,
@@ -2513,3 +2526,3 @@
-  asked for your specific card in the following questions. If you plan
-  to use more than one network card under linux, read the
-  Multiple-Ethernet-mini-HOWTO, available from
+  asked for your specific card in the following questions.
+  If you plan to use more than one network card under Linux,
+  read the Multiple-Ethernet-mini-HOWTO, available from
@@ -2520,2 +2533,2 @@
-  If you have a network (ethernet) card of this type, say Y and read
-  the Ethernet-HOWTO, available via ftp (user: anonymous) in
+  If you have a network (Ethernet) card of this type, say Y and read
+  the Ethernet-HOWTO, available via FTP (user: anonymous) in
@@ -2526,3 +2539,3 @@
-  Documentation/networking/net-modules.txt. If you plan to use more
-  than one network card under linux, read the
-  Multiple-Ethernet-mini-HOWTO, available from
+  Documentation/networking/net-modules.txt.
+  If you plan to use more than one network card under Linux,
+  read the Multiple-Ethernet-mini-HOWTO, available from
@@ -2533,2 +2546,2 @@
-  If you have a network (ethernet) card of this type, say Y and read
-  the Ethernet-HOWTO, available via ftp (user: anonymous) in
+  If you have a network (Ethernet) card of this type, say Y and read
+  the Ethernet-HOWTO, available via FTP (user: anonymous) in
@@ -2540 +2553 @@
-  more than one network card under linux, read the
+  more than one network card under Linux, read the
@@ -2550,2 +2563,2 @@
-  If you have a network (ethernet) card of this type, say Y and read
-  the Ethernet-HOWTO, available via ftp (user: anonymous) in
+  If you have a network (Ethernet) card of this type, say Y and read
+  the Ethernet-HOWTO, available via FTP (user: anonymous) in
@@ -2557 +2570 @@
-  more than one network card under linux, read the
+  more than one network card under Linux, read the
@@ -2566,2 +2579,2 @@
-  into the kernel, and read the the file drivers/net/README.smc9 and
-  the Ethernet-HOWTO, available via ftp (user: anonymous) in
+  into the kernel, and read the file drivers/net/README.smc9 and
+  the Ethernet-HOWTO, available via FTP (user: anonymous) in
@@ -2573 +2586 @@
-  more than one network card under linux, read the
+  more than one network card under Linux, read the
@@ -2579,2 +2592,2 @@
-  If you have a network (ethernet) card of this type, say Y and read
-  the Ethernet-HOWTO, available via ftp (user: anonymous) in
+  If you have a network (Ethernet) card of this type, say Y and read
+  the Ethernet-HOWTO, available via FTP (user: anonymous) in
@@ -2582 +2595 @@
-  one network card under linux, read the Multiple-Ethernet-mini-HOWTO,
+  one network card under Linux, read the Multiple-Ethernet-mini-HOWTO,
@@ -2587,2 +2600,2 @@
-  If you have a network (ethernet) card belonging to this class, say Y
-  and read the Ethernet-HOWTO, available via ftp (user: anonymous) in
+  If you have a network (Ethernet) card belonging to this class, say Y
+  and read the Ethernet-HOWTO, available via FTP (user: anonymous) in
@@ -2594 +2607 @@
-  under linux, read the Multiple-Ethernet-mini-HOWTO, available from
+  under Linux, read the Multiple-Ethernet-mini-HOWTO, available from
@@ -2599,2 +2612,2 @@
-  If you have a network (ethernet) card of this type, say Y and read
-  the Ethernet-HOWTO, available via ftp (user: anonymous) in
+  If you have a network (Ethernet) card of this type, say Y and read
+  the Ethernet-HOWTO, available via FTP (user: anonymous) in
@@ -2607 +2620 @@
-  If you plan to use more than one network card under linux,
+  If you plan to use more than one network card under Linux,
@@ -2609 +2622 @@
-  sunsite.unc.edu:/pub/Linux/docs/HOWTO/mini---and don't use 3c501s.
+  sunsite.unc.edu:/pub/Linux/docs/HOWTO/mini -- and don't use 3c501s.
@@ -2613,2 +2626,2 @@
-  If you have a network (ethernet) card of this type, say Y and read
-  the Ethernet-HOWTO, available via ftp (user: anonymous) in
+  If you have a network (Ethernet) card of this type, say Y and read
+  the Ethernet-HOWTO, available via FTP (user: anonymous) in
@@ -2620 +2633 @@
-  If you plan to use more than one network card under linux,
+  If you plan to use more than one network card under Linux,
@@ -2626 +2639 @@
-  Information about this network (ethernet) card can be found in
+  Information about this network (Ethernet) card can be found in
@@ -2628 +2641 @@
-  say Y and read the Ethernet-HOWTO, available via ftp (user:
+  say Y and read the Ethernet-HOWTO, available via FTP (user:
@@ -2634 +2647 @@
-  If you plan to use more than one network card under linux,
+  If you plan to use more than one network card under Linux,
@@ -2640,2 +2653,2 @@
-  If you have a network (ethernet) card of this type, say Y and read
-  the Ethernet-HOWTO, available via ftp (user: anonymous) in
+  If you have a network (Ethernet) card of this type, say Y and read
+  the Ethernet-HOWTO, available via FTP (user: anonymous) in
@@ -2646,3 +2659,3 @@
-  Documentation/networking/net-modules.txt. If you plan to use more
-  than one network card under linux, read the
-  Multiple-Ethernet-mini-HOWTO, available from
+  Documentation/networking/net-modules.txt.
+  If you plan to use more than one network card under Linux,
+  read the Multiple-Ethernet-mini-HOWTO, available from
@@ -2653 +2666 @@
-  If you have a network (ethernet) card belonging to the 3Com
+  If you have a network (Ethernet) card belonging to the 3Com
@@ -2655 +2668 @@
-  via ftp (user: anonymous) in sunsite.unc.edu:/pub/Linux/docs/HOWTO.
+  via FTP (user: anonymous) in sunsite.unc.edu:/pub/Linux/docs/HOWTO.
@@ -2660 +2673 @@
-  than one network card under linux, read the
+  than one network card under Linux, read the
@@ -2668,2 +2681,2 @@
-  If you have a network (ethernet) card of this type, say Y and read
-  the Ethernet-HOWTO, available via ftp (user: anonymous) in
+  If you have a network (Ethernet) card of this type, say Y and read
+  the Ethernet-HOWTO, available via FTP (user: anonymous) in
@@ -2677 +2690 @@
-  than one network card under linux, read the
+  than one network card under Linux, read the
@@ -2679 +2692 @@
-  sunsite.unc.edu:/pub/Linux/docs/HOWTO/mini
+  sunsite.unc.edu:/pub/Linux/docs/HOWTO/mini.
@@ -2683 +2696 @@
-  If your network (ethernet) card hasn't been mentioned yet and its
+  If your network (Ethernet) card hasn't been mentioned yet and its
@@ -2687 +2700 @@
-  ftp (user: anonymous) in sunsite.unc.edu:/pub/Linux/docs/HOWTO. If
+  FTP (user: anonymous) in sunsite.unc.edu:/pub/Linux/docs/HOWTO. If
@@ -2693 +2706 @@
-  linux, read the Multiple-Ethernet-mini-HOWTO, available from
+  Linux, read the Multiple-Ethernet-mini-HOWTO, available from
@@ -2701,2 +2714,2 @@
-  via ftp (user: anonymous) in sunsite.unc.edu:/pub/Linux/docs/HOWTO
-  (even though ARCnet is not really ethernet).  This driver is also
+  via FTP (user: anonymous) in sunsite.unc.edu:/pub/Linux/docs/HOWTO
+  (even though ARCnet is not really Ethernet).  This driver is also
@@ -2707 +2720 @@
-  use more than one network card under linux, read the
+  use more than one network card under Linux, read the
@@ -2713 +2726 @@
-  This allows you to use "ethernet encapsulation" with your ARCnet
+  This allows you to use "Ethernet encapsulation" with your ARCnet
@@ -2739,2 +2752,2 @@
-  If you have a network (ethernet) card of this type, say Y and read
-  the Ethernet-HOWTO, available via ftp (user: anonymous) in
+  If you have a network (Ethernet) card of this type, say Y and read
+  the Ethernet-HOWTO, available via FTP (user: anonymous) in
@@ -2745,3 +2758,3 @@
-  Documentation/networking/net-modules.txt. If you plan to use more
-  than one network card under linux, read the
-  Multiple-Ethernet-mini-HOWTO, available from
+  Documentation/networking/net-modules.txt.
+  If you plan to use more than one network card under Linux,
+  read the Multiple-Ethernet-mini-HOWTO, available from
@@ -2752,2 +2765,2 @@
-  If you have a network (ethernet) card of this type, say Y and read
-  the Ethernet-HOWTO, available via ftp (user: anonymous) in
+  If you have a network (Ethernet) card of this type, say Y and read
+  the Ethernet-HOWTO, available via FTP (user: anonymous) in
@@ -2755,2 +2768,2 @@
-  drivers/net/depca.c.  If you want to compile this as a module ( =
-  code which can be inserted in and removed from the running kernel
+  drivers/net/depca.c.  If you want to compile this as a module
+  (= code which can be inserted in and removed from the running kernel
@@ -2759 +2772 @@
-  more than one network card under linux, read the
+  more than one network card under Linux, read the
@@ -2765 +2778 @@
-  This driver supports the DE203, DE204 and DE205 network (ethernet)
+  This driver supports the DE203, DE204 and DE205 network (Ethernet)
@@ -2768 +2781 @@
-  ftp (user: anonymous) from sunsite.unc.edu:/pub/Linux/docs/HOWTO.
+  FTP (user: anonymous) from sunsite.unc.edu:/pub/Linux/docs/HOWTO.
@@ -2773 +2786 @@
-  than one network card under linux, read the
+  than one network card under Linux, read the
@@ -2779,2 +2792,2 @@
-  This is a driver for the SEEQ 8005 network (ethernet) card. If this
-  is for you, read the Ethernet-HOWTO, available via ftp (user:
+  This is a driver for the SEEQ 8005 network (Ethernet) card. If this
+  is for you, read the Ethernet-HOWTO, available via FTP (user:
@@ -2782 +2795 @@
-  to use more than one network card under linux, read the
+  to use more than one network card under Linux, read the
@@ -2788,2 +2801,2 @@
-  If you have a network (ethernet) card of this type, say Y and read
-  the Ethernet-HOWTO, available via ftp (user: anonymous) in
+  If you have a network (Ethernet) card of this type, say Y and read
+  the Ethernet-HOWTO, available via FTP (user: anonymous) in
@@ -2794,3 +2807,3 @@
-  Documentation/networking/net-modules.txt. If you plan to use more
-  than one network card under linux, read the
-  Multiple-Ethernet-mini-HOWTO, available from
+  Documentation/networking/net-modules.txt.
+  If you plan to use more than one network card under Linux,
+  read the Multiple-Ethernet-mini-HOWTO, available from
@@ -2801,2 +2814,2 @@
-  If you have a Fujitsu FMV-181/182/183/184 network (ethernet) card,
-  say Y and read the Ethernet-HOWTO, available via ftp (user:
+  If you have a Fujitsu FMV-181/182/183/184 network (Ethernet) card,
+  say Y and read the Ethernet-HOWTO, available via FTP (user:
@@ -2809 +2822 @@
-  If you plan to use more than one network card under linux,
+  If you plan to use more than one network card under Linux,
@@ -2823,2 +2836,2 @@
-  If you have a network (ethernet) card of this type, say Y and read
-  the Ethernet-HOWTO, available via ftp (user: anonymous) in
+  If you have a network (Ethernet) card of this type, say Y and read
+  the Ethernet-HOWTO, available via FTP (user: anonymous) in
@@ -2829,3 +2842,3 @@
-  Documentation/networking/net-modules.txt. If you plan to use more
-  than one network card under linux, read the
-  Multiple-Ethernet-mini-HOWTO, available from
+  Documentation/networking/net-modules.txt.
+  If you plan to use more than one network card under Linux,
+  read the Multiple-Ethernet-mini-HOWTO, available from
@@ -2836,2 +2849,2 @@
-  If you have an EtherExpress16 network (ethernet) card, say Y and
-  read the Ethernet-HOWTO, available via ftp (user: anonymous) in
+  If you have an EtherExpress16 network (Ethernet) card, say Y and
+  read the Ethernet-HOWTO, available via FTP (user: anonymous) in
@@ -2846 +2859 @@
-  than one network card under linux, read the
+  than one network card under Linux, read the
@@ -2852,2 +2865,2 @@
-  If you have a network (ethernet) card of this type, say Y and read
-  the Ethernet-HOWTO, available via ftp (user: anonymous) in
+  If you have a network (Ethernet) card of this type, say Y and read
+  the Ethernet-HOWTO, available via FTP (user: anonymous) in
@@ -2855 +2868 @@
-  one network card under linux, read the Multiple-Ethernet-mini-HOWTO,
+  one network card under Linux, read the Multiple-Ethernet-mini-HOWTO,
@@ -2860,2 +2873,2 @@
-  If you have a network (ethernet) card of this type, say Y and read
-  the Ethernet-HOWTO, available via ftp (user: anonymous) in
+  If you have a network (Ethernet) card of this type, say Y and read
+  the Ethernet-HOWTO, available via FTP (user: anonymous) in
@@ -2863 +2876 @@
-  one network card under linux, read the Multiple-Ethernet-mini-HOWTO,
+  one network card under Linux, read the Multiple-Ethernet-mini-HOWTO,
@@ -2874 +2887 @@
-  you can say Y here and should read the HAM-HOWTO, available via ftp
+  you can say Y here and should read the HAM-HOWTO, available via FTP
@@ -2891 +2904 @@
-  is a Radio LAN (wireless ethernet-like) at 900 MHz and 2.4 GHz.
+  is a Radio LAN (wireless Ethernet-like) at 900 MHz and 2.4 GHz.
@@ -2905,2 +2918,2 @@
-  If you have a network (ethernet) card of this type, say Y and read
-  the Ethernet-HOWTO, available via ftp (user: anonymous) in
+  If you have a network (Ethernet) card of this type, say Y and read
+  the Ethernet-HOWTO, available via FTP (user: anonymous) in
@@ -2911,3 +2924,3 @@
-  Documentation/networking/net-modules.txt. If you plan to use more
-  than one network card under linux, read the
-  Multiple-Ethernet-mini-HOWTO, available from
+  Documentation/networking/net-modules.txt.
+  If you plan to use more than one network card under Linux,
+  read the Multiple-Ethernet-mini-HOWTO, available from
@@ -2918,2 +2931,2 @@
-  If you have a network (ethernet) card of this type, say Y and read
-  the Ethernet-HOWTO, available via ftp (user: anonymous) in
+  If you have a network (Ethernet) card of this type, say Y and read
+  the Ethernet-HOWTO, available via FTP (user: anonymous) in
@@ -2924,3 +2937,3 @@
-  Documentation/networking/net-modules.txt. If you plan to use more
-  than one network card under linux, read the
-  Multiple-Ethernet-mini-HOWTO, available from
+  Documentation/networking/net-modules.txt.
+  If you plan to use more than one network card under Linux,
+  read the Multiple-Ethernet-mini-HOWTO, available from
@@ -2931,2 +2944,2 @@
-  If you have a network (ethernet) card of this type, say Y and read
-  the Ethernet-HOWTO, available via ftp (user: anonymous) in
+  If you have a network (Ethernet) card of this type, say Y and read
+  the Ethernet-HOWTO, available via FTP (user: anonymous) in
@@ -2938 +2951 @@
-  than one network card under linux, read the
+  than one network card under Linux, read the
@@ -2944,2 +2957,2 @@
-  If you have a network (ethernet) card of this type, say Y and read
-  the Ethernet-HOWTO, available via ftp (user: anonymous) in
+  If you have a network (Ethernet) card of this type, say Y and read
+  the Ethernet-HOWTO, available via FTP (user: anonymous) in
@@ -2950,3 +2963,3 @@
-  Documentation/networking/net-modules.txt. If you plan to use more
-  than one network card under linux, read the
-  Multiple-Ethernet-mini-HOWTO, available from
+  Documentation/networking/net-modules.txt.
+  If you plan to use more than one network card under Linux,
+  read the Multiple-Ethernet-mini-HOWTO, available from
@@ -2957,2 +2970,2 @@
-  If you have a network (ethernet) card of this type, say Y and read
-  the Ethernet-HOWTO, available via ftp (user: anonymous) in
+  If you have a network (Ethernet) card of this type, say Y and read
+  the Ethernet-HOWTO, available via FTP (user: anonymous) in
@@ -2960 +2973 @@
-  one network card under linux, read the Multiple-Ethernet-mini-HOWTO,
+  one network card under Linux, read the Multiple-Ethernet-mini-HOWTO,
@@ -2967,3 +2980,3 @@
-  available via ftp (user: anonymous) from
-  sunsite.unc.edu:/pub/Linux/docs/HOWTO; if you are unsure, say
-  Y. Note that the answer to this question doesn't directly affect the
+  available via FTP (user: anonymous) from sunsite.unc.edu:
+  /pub/Linux/docs/HOWTO; if you are unsure, say Y.
+  Note that the answer to this question doesn't directly affect the
@@ -2972,2 +2985,2 @@
-  will be asked for your specific card in the following questions.  If
-  you plan to use more than one network card under linux, read the
+  will be asked for your specific card in the following questions.
+  If you plan to use more than one network card under Linux, read the
@@ -2979,2 +2992,2 @@
-  If you have a network (ethernet) card of this type, say Y and read
-  the Ethernet-HOWTO, available via ftp (user: anonymous) in
+  If you have a network (Ethernet) card of this type, say Y and read
+  the Ethernet-HOWTO, available via FTP (user: anonymous) in
@@ -2985,3 +2998,3 @@
-  Documentation/networking/net-modules.txt. If you plan to use more
-  than one network card under linux, read the
-  Multiple-Ethernet-mini-HOWTO, available from
+  Documentation/networking/net-modules.txt.
+  If you plan to use more than one network card under Linux,
+  read the Multiple-Ethernet-mini-HOWTO, available from
@@ -2990 +3003 @@
-Apricot Xen-II on board ethernet
+Apricot Xen-II on board Ethernet
@@ -2992,2 +3005,2 @@
-  If you have a network (ethernet) controller of this type, say Y and
-  read the Ethernet-HOWTO, available via ftp (user: anonymous) in
+  If you have a network (Ethernet) controller of this type, say Y and
+  read the Ethernet-HOWTO, available via FTP (user: anonymous) in
@@ -2999 +3012 @@
-  than one network card under linux, read the
+  than one network card under Linux, read the
@@ -3005 +3018 @@
-  This is support for the DIGITAL series of PCI/EISA ethernet
+  This is support for the DIGITAL series of PCI/EISA Ethernet
@@ -3008 +3021 @@
-  the Ethernet-HOWTO, available via ftp (user: anonymous) in
+  the Ethernet-HOWTO, available via FTP (user: anonymous) in
@@ -3014,3 +3027,3 @@
-  Documentation/networking/net-modules.txt. If you plan to use more
-  than one network card under linux, read the
-  Multiple-Ethernet-mini-HOWTO, available from
+  Documentation/networking/net-modules.txt.
+  If you plan to use more than one network card under Linux,
+  read the Multiple-Ethernet-mini-HOWTO, available from
@@ -3021 +3034 @@
-  This driver is developed for the SMC EtherPower series ethernet
+  This driver is developed for the SMC EtherPower series Ethernet
@@ -3027 +3040 @@
-  Ethernet-HOWTO, available via ftp (user: anonymous) in
+  Ethernet-HOWTO, available via FTP (user: anonymous) in
@@ -3038 +3051 @@
-  PCI/EISA ethernet switch cards.  These include the SE-4 and the SE-6
+  PCI/EISA Ethernet switch cards.  These include the SE-4 and the SE-6
@@ -3040 +3053 @@
-  the Ethernet-HOWTO, available via ftp (user: anonymous) in
+  the Ethernet-HOWTO, available via FTP (user: anonymous) in
@@ -3046,3 +3059,3 @@
-  Documentation/networking/net-modules.txt. If you plan to use more
-  than one network card under linux, read the
-  Multiple-Ethernet-mini-HOWTO, available from
+  Documentation/networking/net-modules.txt.
+  If you plan to use more than one network card under Linux,
+  read the Multiple-Ethernet-mini-HOWTO, available from
@@ -3053,2 +3066,2 @@
-  If you have a network (ethernet) card of this type, say Y and read
-  the Ethernet-HOWTO, available via ftp (user: anonymous) in
+  If you have a network (Ethernet) card of this type, say Y and read
+  the Ethernet-HOWTO, available via FTP (user: anonymous) in
@@ -3059,3 +3072,3 @@
-  Documentation/networking/net-modules.txt. If you plan to use more
-  than one network card under linux, read the
-  Multiple-Ethernet-mini-HOWTO, available from
+  Documentation/networking/net-modules.txt.
+  If you plan to use more than one network card under Linux,
+  read the Multiple-Ethernet-mini-HOWTO, available from
@@ -3064 +3077 @@
-TI ThunderLAN support (EXPERIMENTAL)
+TI ThunderLAN support
@@ -3071,0 +3085,6 @@
+VIA Rhine support
+CONFIG_VIA_RHINE
+  If you have a VIA "rhine" based network card (Rhine-I (3043) or
+  Rhine-2 (VT86c100A)), say Y here. To build this driver as a module
+  say M.
+
@@ -3075 +3094 @@
-  (ethernet) card, and this is the Linux driver for it. Note that the
+  (Ethernet) card, and this is the Linux driver for it. Note that the
@@ -3077 +3096 @@
-  by this driver. Read the Ethernet-HOWTO, available via ftp (user:
+  by this driver. Read the Ethernet-HOWTO, available via FTP (user:
@@ -3082 +3101 @@
-  Cute little network (ethernet) devices which attach to the parallel
+  Cute little network (Ethernet) devices which attach to the parallel
@@ -3084 +3103 @@
-  one of those, say Y and read the Ethernet-HOWTO, available via ftp
+  one of those, say Y and read the Ethernet-HOWTO, available via FTP
@@ -3094 +3113 @@
-  plan to use more than one network device under linux, read the
+  plan to use more than one network device under Linux, read the
@@ -3102 +3121 @@
-  This is a network (ethernet) device which attaches to your parallel
+  This is a network (Ethernet) device which attaches to your parallel
@@ -3104 +3123 @@
-  available via ftp (user: anonymous) from
+  available via FTP (user: anonymous) from
@@ -3106 +3125 @@
-  you plan to use more than one network card under linux, read the
+  you plan to use more than one network card under Linux, read the
@@ -3114 +3133 @@
-  This is a network (ethernet) device which attaches to your parallel
+  This is a network (Ethernet) device which attaches to your parallel
@@ -3116 +3135 @@
-  available via ftp (user: anonymous) from
+  available via FTP (user: anonymous) from
@@ -3123 +3142 @@
-  card under linux, read the Multiple-Ethernet-mini-HOWTO, available
+  card under Linux, read the Multiple-Ethernet-mini-HOWTO, available
@@ -3128 +3147 @@
-  This is a network (ethernet) device which attaches to your parallel
+  This is a network (Ethernet) device which attaches to your parallel
@@ -3130 +3149 @@
-  available via ftp (user: anonymous) from
+  available via FTP (user: anonymous) from
@@ -3137 +3156 @@
-  card under linux, read the Multiple-Ethernet-mini-HOWTO, available
+  card under Linux, read the Multiple-Ethernet-mini-HOWTO, available
@@ -3143 +3162 @@
-  rest of the world uses ethernet. If you are connected to a token
+  rest of the world uses Ethernet. If you are connected to a token
@@ -3160 +3179 @@
-  here, otherwise N. Read the CDROM-HOWTO, available via ftp (user:
+  here, otherwise N. Read the CDROM-HOWTO, available via FTP (user:
@@ -3251,2 +3270,2 @@
-  CR540 CDROM drive.  This driver - just like all these CDROM drivers
-  - is NOT for CDROM drives with IDE/ATAPI interface, such as Aztech
+  CR540 CDROM drive. This driver -- just like all these CDROM drivers
+  -- is NOT for CDROM drives with IDE/ATAPI interface, such as Aztech
@@ -3301,2 +3320,2 @@
-  Here 'port','irq' and 'dma' are the base i/o address, irq number and
-  dma line assumed to be used by the attached cdrom
+  Here 'port','irq' and 'dma' are the base i/o address, IRQ number and
+  DMA line assumed to be used by the attached cdrom
@@ -3319,2 +3338,2 @@
-  quota support is only useful for multi user systems. If unsure, say
-  N.
+  quota support is only useful for multi user systems. If unsure,
+  say N.
@@ -3336,2 +3355,2 @@
-  Minix is a simple operating system used in many classes about
-  OS's. The minix filesystem (= method to organize files on a harddisk
+  Minix is a simple operating system used in many classes about OS's.
+  The minix filesystem ( = method to organize files on a hard disk
@@ -3341,5 +3360,5 @@
-  leaner. You don't want to use it on your harddisk because of certain
-  built-in restrictions. This option will enlarge your kernel by about
-  25 kB. Everyone should say Y or M so that they are able to read this
-  common floppy format.  If you want to compile this as a module
-  ( = code which can be inserted in and removed from the
+  leaner. You don't want to use it on your hard disk because of
+  certain built-in restrictions. This option will enlarge your kernel
+  by about 25 kB. Everyone should say Y or M so that they are able to
+  read this common floppy format. If you want to compile this as
+  a module ( = code which can be inserted in and removed from the
@@ -3352,4 +3371,4 @@
-  This is the old Linux filesystem (= method to organize files on a
-  harddisk partition or a floppy disk) and not in use anymore. It
-  enlarges your kernel by about 25 kB. Let's all kill this beast. Say
-  N.
+  This is the old Linux filesystem ( = method to organize files on a
+  hard disk partition or a floppy disk) and not in use anymore.
+  It enlarges your kernel by about 25 kB. Let's all kill this beast.
+  Say N.
@@ -3359,16 +3378,16 @@
-  This is the de facto standard Linux filesystem (= method to organize
-  files on a storage device) for harddisks. You want to say Y, unless
-  you intend to use Linux exclusively from inside a DOS partition
-  using the umsdos filesystem. The advantage of the latter is that you
-  can get away without repartitioning your hard drive (which often
-  implies backing everything up and restoring afterwards); the
-  disadvantage is that Linux becomes susceptible to DOS viruses and
-  that umsdos is somewhat slower than ext2fs. Even if you want to run
-  Linux in this fashion, it might be a good idea to have ext2fs
-  around: it enables you to read more floppy disks and facilitates the
-  transition to a *real* Linux partition later. Another (rare) case
-  which doesn't require ext2fs is a diskless Linux box which mounts
-  all files over the network using NFS (in this case it's sufficient
-  to enable NFS filesystem support below; if you are planning to do
-  this, have a look at the netboot package in
-  /pub/Linux/system/Linux-boot/, available via ftp (user: anonymous)
+  This is the de facto standard Linux filesystem ( = method to
+  organize files on a storage device) for hard disks. You want to
+  say Y, unless you intend to use Linux exclusively from inside a DOS
+  partition using the umsdos filesystem. The advantage of the latter
+  is that you can get away without repartitioning your hard drive
+  (which often implies backing everything up and restoring
+  afterwards); the disadvantage is that Linux becomes susceptible to
+  DOS viruses and that umsdos is somewhat slower than ext2fs. Even if
+  you want to run Linux in this fashion, it might be a good idea to
+  have ext2fs around: it enables you to read more floppy disks and
+  facilitates the transition to a *real* Linux partition later.
+  Another (rare) case which doesn't require ext2fs is a diskless Linux
+  box which mounts all files over the network using NFS (in this case
+  it's sufficient to enable NFS filesystem support below; if you are
+  planning to do this, have a look at the netboot package in
+  /pub/Linux/system/Linux-boot/, available via FTP (user: anonymous)
@@ -3376 +3395 @@
-  short ext2fs-FAQ, available via ftp (user: anonymous) in
+  short ext2fs-FAQ, available via FTP (user: anonymous) in
@@ -3382,2 +3401,2 @@
-  This is an old filesystem (= method to organize files on a harddisk
-  partition or a floppy disk) and not in use anymore. This option
+  This is an old filesystem ( = method to organize files on a hard
+  disk partition or a floppy disk) and not in use anymore. This option
@@ -3385 +3404 @@
-  say N.  If you want to compile this as a module ( = code which can
+  say N. If you want to compile this as a module ( = code which can
@@ -3400,2 +3419,2 @@
-  support as a module, you cannot compile any of the FAT-based file-
-  systems into the kernel - they will have to be modules as well.
+  support as a module, you cannot compile any of the FAT-based
+  filesystems into the kernel -- they will have to be modules as well.
@@ -3406 +3425 @@
-  This allows you to mount MSDOS partitions of your harddrive (unless
+  This allows you to mount MSDOS partitions of your hard drive (unless
@@ -3409 +3428 @@
-  DOSEMU-HOWTO, available via ftp (user: anonymous) at
+  DOSEMU-HOWTO, available via FTP (user: anonymous) at
@@ -3433 +3452 @@
-  This allows you to mount MSDOS partitions of your harddrive. It
+  This allows you to mount MSDOS partitions of your hard drive. It
@@ -3448 +3467 @@
-  partition of your harddrive. The advantage of this is that you can
+  partition of your hard drive. The advantage of this is that you can
@@ -3462,3 +3481,2 @@
-  whenever you want), say M here and read
-  Documentation/modules.txt. Note that the filesystem of your root
-  partition cannot be a module.
+  whenever you want), say M here and read Documentation/modules.txt.
+  Note that the filesystem of your root partition cannot be a module.
@@ -3560 +3578 @@
-  This is the DOS codepage that is used in much of Europe--United
+  This is the DOS codepage that is used in much of Europe -- United
@@ -3622 +3640 @@
-  your harddisk: the files are created on the fly when you access
+  your hard disk: the files are created on the fly when you access
@@ -3625 +3643 @@
-  Guide, available via ftp (user: anonymous) in
+  Guide, available via FTP (user: anonymous) in
@@ -3631,2 +3649,2 @@
-  that are used by the periphery to gain the CPU's attention - often a
-  source of trouble if two devices are mistakenly configured to use
+  that are used by the periphery to gain the CPU's attention -- often
+  a source of trouble if two devices are mistakenly configured to use
@@ -3639 +3657 @@
-  (using SLIP, PLIP, PPP or ethernet) and want to mount files
+  (using SLIP, PLIP, PPP or Ethernet) and want to mount files
@@ -3643 +3661 @@
-  sitting on the client's harddisk. For this to work, the server must
+  sitting on the client's hard disk. For this to work, the server must
@@ -3646,13 +3664,12 @@
-  Administrator's Guide, available via ftp (user: anonymous) in
-  sunsite.unc.edu:/pub/Linux/docs/LDP, and on its man page: "man
-  nfs". There is also a NFS-FAQ in
-  sunsite.unc.edu:/pub/Linux/docs/faqs which presumes that you know
-  the basics of NFS already. If you say Y here, you should have said Y
-  to TCP/IP networking also. This option would enlarge your kernel by
-  about 27 kB. This filesystem is also available as a module ( = code
-  which can be inserted in and removed from the running kernel
-  whenever you want). If you want to compile it as a module, say M
-  here and read Documentation/modules.txt. If you configure a diskless
-  machine which will mount its root filesystem over nfs, you cannot
-  compile this driver as a module. If you don't know what all this is
-  about, say N.
+  Administrator's Guide, available via FTP (user: anonymous) in
+  sunsite.unc.edu:/pub/Linux/docs/LDP, and on its man page: "man nfs".
+  There is also a NFS-FAQ in sunsite.unc.edu:/pub/Linux/docs/faqs
+  which presumes that you know the basics of NFS already. If you say Y
+  here, you should have said Y to TCP/IP networking also. This option
+  would enlarge your kernel by about 27 kB. This filesystem is also
+  available as a module ( = code which can be inserted in and removed
+  from the running kernel whenever you want). If you want to compile
+  it as a module, say M here and read Documentation/modules.txt.
+  If you configure a diskless machine which will mount its root
+  filesystem over NFS, you cannot compile this driver as a module.
+  If you don't know what all this is about, say N.
@@ -3664 +3681 @@
-  box doesn't have a harddisk), say Y. Read Documentation/nfsroot.txt
+  box doesn't have a hard disk), say Y. Read Documentation/nfsroot.txt
@@ -3698,5 +3715,5 @@
-  via ftp (user: anonymous) from
-  sunsite.unc.edu:/pub/Linux/docs/HOWTO), thereby enlarging your
-  kernel by about 27 kB; otherwise say N.  If you want to compile this
-  as a module ( = code which can be inserted in and removed from the
-  running kernel whenever you want), say M here and read
+  via FTP (user: anonymous) from sunsite.unc.edu:
+  /pub/Linux/docs/HOWTO), thereby enlarging your kernel by about
+  27 kB; otherwise say N. If you want to compile this as a module
+  ( = code which can be inserted in and removed from the running
+  kernel whenever you want), say M here and read
@@ -3708 +3725 @@
-  is the filesystem used for organizing files on OS/2 harddisk
+  is the filesystem used for organizing files on OS/2 hard disk
@@ -3710 +3727 @@
-  HPFS partition of your harddrive. OS/2 floppies however are in
+  HPFS partition of your hard drive. OS/2 floppies however are in
@@ -3720 +3737 @@
-  SCO, Xenix and Coherent are commercial Unix systems for intel
+  SCO, Xenix and Coherent are commercial Unix systems for Intel
@@ -3722,2 +3739,2 @@
-  and from their floppies and harddisk partitions. If you have a
-  floppy or harddisk partition like that, it is probable that they
+  and from their floppies and hard disk partitions. If you have a
+  floppy or hard disk partition like that, it is probable that they
@@ -3732 +3749 @@
-  nfs filesystem support obviously). Note that this option is
+  NFS filesystem support obviously). Note that this option is
@@ -3741,3 +3758,2 @@
-  whenever you want), say M here and read
-  Documentation/modules.txt. If you haven't heard about all of this
-  before, it's safe to say N.
+  whenever you want), say M here and read Documentation/modules.txt.
+  If you haven't heard about all of this before, it's safe to say N.
@@ -3764 +3780 @@
-  UFS filesystem support (but you need nfs filesystem support
+  UFS filesystem support (but you need NFS filesystem support
@@ -3793 +3809 @@
-  This is mainly used to carry data from a Sparc under SunOS to your
+  This is mainly used to carry data from a SPARC under SunOS to your
@@ -3797 +3813 @@
-SMB filesystem support (to mount WfW shares etc..)
+SMB filesystem support (to mount WfW shares etc...)
@@ -3801 +3817 @@
-  ethernet. Enabling this allows you to mount their filesystems and
+  Ethernet. Enabling this allows you to mount their filesystems and
@@ -3807 +3823 @@
-  program samba (available via ftp (user: anonymous) in
+  program samba (available via FTP (user: anonymous) in
@@ -3828 +3844 @@
-  what nfs is to tcp/ip, if that helps. Enabling this option allows
+  what NFS is to TCP/IP, if that helps. Enabling this option allows
@@ -3840 +3856 @@
-  harddisks by Amiga (tm) Systems since AmigaOS Version 1.3 (34.20).
+  hard disks by Amiga (tm) Systems since AmigaOS Version 1.3 (34.20).
@@ -3846 +3862 @@
-  and to an Amiga FFS partition of your harddrive.  Amiga floppies
+  and to an Amiga FFS partition of your hard drive.  Amiga floppies
@@ -3860 +3876 @@
-  setting up dedicated ethernet WWW/ftp servers, or users that have
+  setting up dedicated Ethernet WWW/FTP servers, or users that have
@@ -3877 +3893 @@
-  to connect more than two modems to your linux box, for instance in
+  to connect more than two modems to your Linux box, for instance in
@@ -3885 +3901 @@
-  to connect more than two modems to your linux box, for instance in
+  to connect more than two modems to your Linux box, for instance in
@@ -3889,0 +3906,18 @@
+Specialix IO8+ card support
+CONFIG_SPECIALIX
+  This is a driver for the Specialix IO8+ multiport card (both the
+  ISA and the PCI version), that gives you 8 serial ports. You would 
+  need a card like this to connect more than two modems to your linux 
+  box, for instance in order to become a BBS. If you have a card like 
+  that, say Y here and read the file Documentation/specialix.txt. Also 
+  it's possible to say M here and compile this driver as kernel 
+  loadable module.
+
+Specialix DTR/RTS pin is RTS
+CONFIG_SPECIALIX_RTSCTS
+  The Specialix card can only support either RTS or DTR. When this
+  option is off, the driver will use the pin as "DTR" when the tty is
+  in software handshake mode. When this option is on or hardware 
+  handshake is on, it will always be RTS. Read the file 
+  Documentation/specialix.txt for more information. 
+
@@ -3894 +3928 @@
-  your linux box, for instance in order to become a BBS. If you want
+  your Linux box, for instance in order to become a BBS. If you want
@@ -3904 +3938 @@
-  like this to connect more than two modems to your linux box, for
+  like this to connect more than two modems to your Linux box, for
@@ -3932 +3966 @@
-  read the Printing-HOWTO, available via ftp (user: anonymous) in
+  read the Printing-HOWTO, available via FTP (user: anonymous) in
@@ -3946 +3980 @@
-  explained in the SCSI-HOWTO, available via ftp (user: anonymous) in
+  explained in the SCSI-HOWTO, available via FTP (user: anonymous) in
@@ -3961 +3995 @@
-  have something else, read the Busmouse-HOWTO, available via ftp
+  have something else, read the Busmouse-HOWTO, available via FTP
@@ -3966,3 +4000,3 @@
-  the answer to this question won't directly affect the kernel: saying
-  N will just cause this configure script to skip all the questions
-  about non-serial mice.  If unsure, say Y.
+  the answer to this question won't directly affect the kernel:
+  saying N will just cause this configure script to skip all the
+  questions about non-serial mice.  If unsure, say Y.
@@ -3976 +4010 @@
-  available via ftp (user: anonymous) in
+  available via FTP (user: anonymous) in
@@ -3993 +4027 @@
-  explained in detail in the Busmouse-HOWTO, available via ftp (user:
+  explained in detail in the Busmouse-HOWTO, available via FTP (user:
@@ -4004 +4038 @@
-  doesn't work. Read the Busmouse-HOWTO, available via ftp (user:
+  doesn't work. Read the Busmouse-HOWTO, available via FTP (user:
@@ -4011 +4045 @@
-  you have, say Y and read the Busmouse-HOWTO, available via ftp
+  you have, say Y and read the Busmouse-HOWTO, available via FTP
@@ -4018 +4052 @@
-  actually mean PS/2 busmouse - so count the pins on the connector.
+  actually mean PS/2 busmouse -- so count the pins on the connector.
@@ -4024 +4058 @@
-  busmice. Read the Busmouse-HOWTO, available via ftp (user:
+  busmice. Read the Busmouse-HOWTO, available via FTP (user:
@@ -4047 +4081 @@
-  program via anonymous ftp which is able to configure this driver
+  program via anonymous FTP which is able to configure this driver
@@ -4068,2 +4102,2 @@
-  This driver does not exist at this point, so you might as well say
-  N.
+  This driver does not exist at this point, so you might as well
+  say N.
@@ -4130 +4164 @@
-  Further, this option doesn't work for all laptops---it might not
+  Further, this option doesn't work for all laptops -- it might not
@@ -4227,6 +4261,6 @@
-  /proc/rtc and its behaviour is set by various ioctls on
-  /dev/rtc. People running SMP (= multiprocessor) versions of Linux
-  should enable this option to read and set the RTC clock in a SMP
-  compatible fashion. If you think you have a use for such a device
-  (such as periodic data sampling), then say Y here, and go read the
-  file Documentation/rtc.txt for details.
+  /proc/rtc and its behaviour is set by various ioctls on /dev/rtc.
+  People running SMP ( = multiprocessor) versions of Linux should
+  enable this option to read and set the RTC clock in a SMP compatible
+  fashion. If you think you have a use for such a device (such as
+  periodic data sampling), then say Y here, and go read the file
+  Documentation/rtc.txt for details.
@@ -4240 +4274 @@
-  want to read the Sound-HOWTO, available via ftp (user: anonymous)
+  want to read the Sound-HOWTO, available via FTP (user: anonymous)
@@ -4285 +4319 @@
-  all soundcards. However, some natively supported cards have their
+  all sound cards. However, some natively supported cards have their
@@ -4341 +4375 @@
-  Answer Y if you have a soundcard based on the Ensoniq SoundScape
+  Answer Y if you have a sound card based on the Ensoniq SoundScape
@@ -4386 +4420 @@
-  This is support for the soundcards on Sun workstations. The code
+  This is support for the sound cards on Sun workstations. The code
@@ -4397 +4431 @@
-  Guide, available via ftp (user: anonymous) from
+  Guide, available via FTP (user: anonymous) from
@@ -4439,2 +4473,2 @@
-  by bundling several ISDN-connections, using this protocol. See
-  Documentation/isdn/README.syncppp for more information.
+  by bundling several ISDN-connections, using this protocol.
+  See Documentation/isdn/README.syncppp for more information.
@@ -4473,2 +4507 @@
-  many compatibles). It's a complete rewrite of the original Teles
-  driver.
+  many compatibles). It supports other chipsets too.
@@ -4477,0 +4511,23 @@
+HiSax Support for EURO/DSS1
+CONFIG_HISAX_EURO
+  Enable this if you have a EURO ISDN line.
+
+Support for german chargeinfo
+CONFIG_DE_AOC
+  If you have german AOC, you can enable this to get the charginfo.
+
+Disable sending complete
+CONFIG_HISAX_NO_SENDCOMPLETE
+  If you have trouble with some ugly exchanges or you live in
+  Australia select this option.
+
+Disable sending low layer compatibility
+CONFIG_HISAX_NO_LLC
+  If you have trouble with some ugly exchanges try to select this
+  option.
+
+HiSax Support for german 1TR6
+CONFIG_HISAX_1TR6
+  Enable this if you have a old german 1TR6 line.
+  Note: Many older local switches are using 1TR6 on internal S0.
+
@@ -4482,3 +4538,3 @@
-  See Documentation/isdn/README.HiSax on how to configure it
-  using the different cards, a different D-channel protocol, or
-  non-standard irq/port/shmem settings.
+  See Documentation/isdn/README.HiSax on how to configure it using the
+  different cards, a different D-channel protocol, or non-standard
+  IRQ/port/shmem settings.
@@ -4490,3 +4546,18 @@
-  See Documentation/isdn/README.HiSax on how to configure it
-  using the different cards, a different D-channel protocol, or
-  non-standard irq/port/shmem settings.
+  See Documentation/isdn/README.HiSax on how to configure it using the
+  different cards, a different D-channel protocol, or non-standard
+  IRQ/port settings.
+
+HiSax Support for Teles 16.3c
+CONFIG_HISAX_TELES3C
+  This enables HiSax support for the Teles 16.3c PnP.
+  See Documentation/isdn/README.HiSax on how to configure it.
+
+HiSax Support for Teles PCI
+CONFIG_HISAX_TELESPCI
+  This enables HiSax support for the Teles PCI.
+  See Documentation/isdn/README.HiSax on how to configure it.
+
+HiSax Support for Teles S0Box
+CONFIG_HISAX_S0BOX
+  This enables HiSax support for the Teles/Creatix parallel port
+  S0BOX.  See Documentation/isdn/README.HiSax on how to configure it.
@@ -4496,4 +4567,14 @@
-  This enables HiSax support for the AVM A1 (aka "Fritz").
-  See Documentation/isdn/README.HiSax on how to configure it
-  using the different cards, a different D-channel protocol, or
-  non-standard irq/port/shmem settings.
+  This enables HiSax support for the AVM A1 (aka "Fritz!").
+  See Documentation/isdn/README.HiSax on how to configure it using the
+  different cards, a different D-channel protocol, or non-standard
+  IRQ/port settings.
+
+HiSax Support for AVM PnP/PCI (Fritz!PNP/PCI)
+CONFIG_HISAX_FRITZPCI
+  This enables HiSax support for the AVM "Fritz!PnP" and "Fritz!PCI".
+  See Documentation/isdn/README.HiSax on how to configure it.
+
+HiSax Support for AVM A1 PCMCIA (Fritz)
+CONFIG_HISAX_AVM_A1_PCMCIA
+  This enables HiSax support for the AVM A1 "Fritz!PCMCIA").
+  See Documentation/isdn/README.HiSax on how to configure it.
@@ -4502,17 +4583,6 @@
-CONFIG_HISAX_ELSA_PCC
-  This enables HiSax support for the Elsa Mircolink cards and
-  for the Elsa Quickstep series cards for the ISA bus.
-  You don't have to select "HiSax Support for Elsa PCMCIA card"
-  at the same time.
-  See Documentation/isdn/README.HiSax on how to configure it
-  using the different cards, a different D-channel protocol, or
-  non-standard irq/port/shmem settings.
-
-HiSax Support for Elsa PCMCIA card
-CONFIG_HISAX_ELSA_PCMCIA
-  This enables HiSax support for the Elsa PCMCIA card.
-  You don't have to select "HiSax Support for Elsa ISA cards" at
-  the same time.
-  See Documentation/isdn/README.HiSax on how to configure it
-  using the different cards, a different D-channel protocol, or
-  non-standard irq/port/shmem settings.
+CONFIG_HISAX_ELSA
+  This enables HiSax support for all Elsa cards.
+  See Documentation/isdn/README.HiSax on how to configure it using the
+  different cards, a different D-channel protocol, or non-standard
+  IRQ/port settings.
+
@@ -4523,3 +4593 @@
-  See Documentation/isdn/README.HiSax on how to configure it
-  using the different cards, a different D-channel protocol, or
-  non-standard irq/port/shmem settings.
+  See Documentation/isdn/README.HiSax on how to configure it.
@@ -4527,23 +4595,49 @@
-HiSax Support for EURO/DSS1
-CONFIG_HISAX_EURO
-  You should choose your D-channel protocol your local
-  telephone service provider uses here by saying Y or N.
-  NOTE: This is mutually exclusive with HiSax Support for
-  german 1TR6 and US/NI-1 if you have only one ISDN card
-  installed.
-
-HiSax Support for US/NI-1
-CONFIG_HISAX_NI1
-  You should choose your D-channel protocol your local
-  telephone service provider uses here by saying Y or N.
-  NOTE: This is mutually exclusive with HiSax Support for
-  german 1TR6 and EURO/DSS1 if you have only one ISDN card
-  installed. (not working yet, under developement)
-
-HiSax Support for german 1TR6
-CONFIG_HISAX_1TR6
-  You should choose your D-channel protocol your local
-  telephone service provider uses here by saying Y or N.
-  NOTE: This is mutually exclusive with HiSax Support for
-  EURO/DSS1 and US/NI-1 if you have only one ISDN card
-  installed.
+HiSax Support for Eicon.Diehl Diva cards
+CONFIG_HISAX_DIEHLDIVA
+  This enables HiSax support for all none Pro versions of
+  Eicon.Diehl's Diva series passiv cards.
+  See Documentation/isdn/README.HiSax on how to configure it.
+
+HiSax Support for ASUSCOM cards
+CONFIG_HISAX_ASUSCOM
+  This enables HiSax support for all passiv AsusCom and AsusComs OEM cards,
+  e.g PCBIT-DP, Dynalink and much more.
+  See Documentation/isdn/README.HiSax on how to configure it.
+
+HiSax Support for TELEINT cards
+CONFIG_HISAX_TELEINT
+  This enables HiSax support for TeleInts semi-activ card and for
+  other HFC-2BS0 based cards.
+  See Documentation/isdn/README.HiSax on how to configure it.
+
+HiSax Support for Sedlbauer cards
+CONFIG_HISAX_SEDLBAUER
+  This enables HiSax support for all Sedlbauer passiv cards such as
+  Sedlbauer Speed Card (Speed Win, Teledat 100), Speed Star
+  and Speed Star2 (PCMCIA), ISDN-Controller PC/104, Speed PCI and
+  Speed Fax+.
+  
+  See Documentation/isdn/README.HiSax on how to configure it.
+
+HiSax Support for USR Sportster internal TA
+CONFIG_HISAX_SPORTSTER
+  This enables HiSax support for the USR (3Com) Sportster internal TA
+  passiv card.
+  See Documentation/isdn/README.HiSax on how to configure it.
+
+HiSax Support for MIC card
+CONFIG_HISAX_MIC
+  This enables HiSax support for the MIC passiv card.
+  See Documentation/isdn/README.HiSax on how to configure it.
+
+HiSax Support for NETjet card
+CONFIG_HISAX_NETJET
+  This enables HiSax support for the NetJet PCI and maybe for other
+  Tiger300 based passiv cards.
+  See Documentation/isdn/README.HiSax on how to configure it.
+
+HiSax Support for Niccy PnP/PCI card
+CONFIG_HISAX_NICCY
+  This enables HiSax support for Dr. Neuhaus (Sagem) Niccy series
+  passiv cards.
+  See Documentation/isdn/README.HiSax on how to configure it.
@@ -4556,3 +4650,3 @@
-  using a utility which is distributed separately.  See
-  Documentation/isdn/README and Documentation/isdn/README.pcbit for
-  more information.
+  using a utility which is distributed separately.
+  See Documentation/isdn/README and Documentation/isdn/README.pcbit
+  for more information.
@@ -4577 +4671 @@
-  This enables support for a sparc based parallel multi-computer
+  This enables support for a SPARC based parallel multi-computer
@@ -4582 +4676 @@
-Sparc ESP SCSI support
+SPARC ESP SCSI support
@@ -4587 +4681 @@
-Sparc /dev/openprom compatibility driver
+SPARC /dev/openprom compatibility driver
@@ -4589 +4683 @@
-  This driver provides user programs with an interface to the Sparc
+  This driver provides user programs with an interface to the SPARC
@@ -4595,0 +4690,7 @@
+Handle buggy SMP BIOSes with bad MTRR setup
+CONFIG_MTRR
+  Some BIOSes for MP1.1/MP1.4 SMP machines fail to set the MTRR
+  registers in the chips up correctly as the specification and Intel
+  rules require. If you have a PPro or later SMP and one or more CPU's
+  report a value of about 2-3 bogomips enable this.
+
@@ -4603,2 +4704,2 @@
-# LocalWords:  cdrom harddisk diskless netboot nfs xzvf ATAPI MB harddrives ide
-# LocalWords:  HD harddisks CDROMs IDECD NEC MITSUMI filesystem XT XD PCI bios
+# LocalWords:  cdrom diskless netboot nfs xzvf ATAPI MB ide
+# LocalWords:  HD CDROMs IDECD NEC MITSUMI filesystem XT XD PCI bios
@@ -4606 +4707 @@
-# LocalWords:  BINFMT Linkable http ac uk jo html GCC Sparc AVANTI CABRIOLET EB
+# LocalWords:  BINFMT Linkable http ac uk jo html GCC SPARC AVANTI CABRIOLET EB
@@ -4608 +4709 @@
-# LocalWords:  genksyms INET loopback gatewaying ethernet internet PPP ARP Arp
+# LocalWords:  genksyms INET loopback gatewaying Ethernet internet PPP ARP Arp
@@ -4612 +4713 @@
-# LocalWords:  Mb SKB IPX Novell Netware dosemu Appletalk DDP ATALK tapedrive
+# LocalWords:  Mb SKB IPX Novell NetWare dosemu AppleTalk DDP ATALK tapedrive
@@ -4625 +4726 @@
-# LocalWords:  LMS OPTCD Sanyo SJCD minix faqs xiafs XIA msdos harddrive mtools
+# LocalWords:  LMS OPTCD Sanyo SJCD minix faqs xiafs XIA msdos mtools
@@ -4627 +4728 @@
-# LocalWords:  hpfs SYSV SCO intel iBCS Wyse WordPerfect tsx mit unixes sysv NR
+# LocalWords:  hpfs SYSV SCO Intel iBCS Wyse WordPerfect tsx mit unixes sysv NR
@@ -4633 +4734 @@
-# LocalWords:  mcdx gscd optcd sjcd ISP soundcard hdparm Workgroups Lan samba
+# LocalWords:  mcdx gscd optcd sjcd ISP hdparm Workgroups Lan samba
@@ -4635 +4736 @@
-# LocalWords:  chipset FB multicast MROUTE appletalk ifconfig IBMTR multiport
+# LocalWords:  chipset FB multicast MROUTE ifconfig IBMTR multiport
@@ -4639 +4740 @@
-# LocalWords:  pppd Zilog ZS soundcards SRM bootloader ez mainmenu rarp ipfwadm
+# LocalWords:  pppd Zilog ZS SRM bootloader ez mainmenu rarp ipfwadm
@@ -4644 +4745 @@
-# LocalWords:  bsd comp Sparcstation le SunOS ie Gracilis PackeTwin PT pt LU FX
+# LocalWords:  bsd comp SPARCstation le SunOS ie Gracilis PackeTwin PT pt LU FX
