"eHC-40" - EPSON HC-40/PX-4 Emulator for Win32
								2/29/2008

--- Internal ROM images

	SYS.ROM		CP/M ROM ($0000-$7FFF in system bank)
	BASIC.ROM	32KBytes ROM capsule bank1 (usually for BASIC)
	UTIL.ROM	32KBytes ROM capsule bank2 (usually for UTILITY)
	EXT.ROM		128KBytes ROM capsule on External RAM disk

--- Optional devices

	A:	External RAM disk
	B:	32KBytes ROM capsule bank1
	C:	32KBytes ROM capsule bank2
	D:	TF-20 floopy drive #1
	E:	TF-20 floopy drive #2
	F:	TF-20 floopy drive #3
	G:	TF-20 floopy drive #4
	CAS0:	External cassette

	NOTE: ROM capsule on External RAM disk is not supported by CP/M.

--- Key maps

	Virtual		PC
	--------------------------------
	STOP		Break/Pause
	PAUSE		F11
	HELP		F12

----------------------------------------
TAKEDA, toshiya
t-takeda@m1.interq.or.jp
http://homepage3.nifty.com/takeda-toshiya/
